# Atmel EDBG-based Tools Protocols
AVR8 generic protocol

Sidebar | Prev | Up | Next

## AVR8GENERIC ID definitions

This section includes the header file defining the different command, response and event IDs for the AVR8 protocol. It also defines the different possible failure codes.

    enum Avr8GenericCommands {
        CMD_AVR8_QUERY                      = 0x00, //! Capability discovery
        CMD_AVR8_SET                        = 0x01, //! Set parameters
        CMD_AVR8_GET                        = 0x02, //! Get parameters
        CMD_AVR8_ACTIVATE_PHYSICAL          = 0x10, //! Connect physically
        CMD_AVR8_DEACTIVATE_PHYSICAL        = 0x11, //! Disconnect physically
        CMD_AVR8_GET_ID                     = 0x12, //! Read the ID
        CMD_AVR8_ATTACH                     = 0x13, //! Attach to OCD module
        CMD_AVR8_DETACH                     = 0x14, //! Detach from OCD module
        CMD_AVR8_PROG_MODE_ENTER            = 0x15, //! Enter programming mode
        CMD_AVR8_PROG_MODE_LEAVE            = 0x16, //! Leave programming mode
        CMD_AVR8_DISABLE_DEBUGWIRE          = 0x17, //! Disable debugWIRE interface
        CMD_AVR8_ERASE                      = 0x20, //! Erase the chip
        CMD_AVR8_MEMORY_READ                = 0x21, //! Read memory
        CMD_AVR8_MEMORY_READ_MASKED         = 0x22, //! Read memory while via a mask
        CMD_AVR8_MEMORY_WRITE               = 0x23, //! Write memory
        CMD_AVR8_CRC                        = 0x24, //! Calculate CRC
        CMD_AVR8_RESET                      = 0x30, //! Reset the MCU
        CMD_AVR8_STOP                       = 0x31, //! Stop the MCU
        CMD_AVR8_RUN                        = 0x32, //! Resume execution
        CMD_AVR8_RUN_TO_ADDRESS             = 0x33, //! Resume with breakpoint
        CMD_AVR8_STEP                       = 0x34, //! Single step
        CMD_AVR8_PC_READ                    = 0x35, //! Read PC
        CMD_AVR8_PC_WRITE                   = 0x36, //! Write PC
        CMD_AVR8_HW_BREAK_SET               = 0x40, //! Set breakpoints
        CMD_AVR8_HW_BREAK_CLEAR             = 0x41, //! Clear breakpoints
        CMD_AVR8_SW_BREAK_SET               = 0x43, //! Set software breakpoints
        CMD_AVR8_SW_BREAK_CLEAR             = 0x44, //! Clear software breakpoints
        CMD_AVR8_SW_BREAK_CLEAR_ALL         = 0x45, //! Clear all software breakpoints
        CMD_AVR8_PAGE_ERASE                 = 0x50  //! Erase page
    };

    // Protocol responses
    enum Avr8GenericResponses {
        RSP_AVR8_OK                         = 0x80, //! All OK
        RSP_AVR8_LIST                       = 0x81, //! List of items returned
        RSP_AVR8_DATA                       = 0x84, //! Data returned
        RSP_AVR8_PC                         = 0x83, //! PC value returned
        RSP_AVR8_FAILED                     = 0xA0  //! Command failed to execute
    };

    // Protocol events
    enum Avr8GenericEvents {
        EVT_AVR8_BREAK                      = 0x40, //! Break message
        EVT_AVR8_IDR                        = 0x41  //! IO Data Register message
    };

    // Failure response codes (RSP_FAILED)
    enum Avr8GenericFailureCodes {
        AVR8_FAILURE_OK                      = 0x00, //! All OK
        AVR8_FAILURE_DW_PHY_ERROR            = 0x10, //! debugWIRE physical error
        AVR8_FAILURE_JTAGM_INIT_ERROR        = 0x11, //! JTAGM failed to initialise
        AVR8_FAILURE_JTAGM_ERROR             = 0x12, //! JTAGM did something strange
        AVR8_FAILURE_JTAG_ERROR              = 0x13, //! JTAG low level error
        AVR8_FAILURE_JTAGM_VERSION           = 0x14, //! Unsupported version of JTAGM
        AVR8_FAILURE_JTAGM_TIMEOUT           = 0x15, //! JTAG master timed out
        AVR8_FAILURE_JTAG_BIT_BANGER_TIMEOUT = 0x16, //! JTAG bit banger timed out
        AVR8_FAILURE_PARITY_ERROR            = 0x17, //! Parity error in received data
        AVR8_FAILURE_EB_ERROR                = 0x18, //! Did not receive EMPTY byte
        AVR8_FAILURE_PDI_TIMEOUT             = 0x19, //! PDI physical timed out
        AVR8_FAILURE_COLLISION               = 0x1A, //! Collision on physical level
        AVR8_FAILURE_PDI_ENABLE              = 0x1B, //! PDI enable failed
        AVR8_FAILURE_NO_DEVICE_FOUND         = 0x20, //! devices == 0!
        AVR8_FAILURE_CLOCK_ERROR             = 0x21, //! Failure when increasing baud
        AVR8_FAILURE_NO_TARGET_POWER         = 0x22, //! Target power not detected
        AVR8_FAILURE_NOT_ATTACHED            = 0x23, //! Must run attach command first
        AVR8_FAILURE_INVALID_PHYSICAL_STATE  = 0x31, //! Physical not activated
        AVR8_FAILURE_ILLEGAL_STATE           = 0x32, //! Illegal run / stopped state
        AVR8_FAILURE_INVALID_CONFIG          = 0x33, //! Invalid config for activate phy
        AVR8_FAILURE_INVALID_MEMTYPE         = 0x34, //! Not a valid memtype
        AVR8_FAILURE_INVALID_SIZE            = 0x35, //! Too many or too few bytes
        AVR8_FAILURE_INVALID_ADDRESS         = 0x36, //! Asked for a bad address
        AVR8_FAILURE_INVALID_ALIGNMENT       = 0x37, //! Asked for badly aligned data
        AVR8_FAILURE_ILLEGAL_MEMORY_RANGE    = 0x38, //! Address not within legal range
        AVR8_FAILURE_ILLEGAL_VALUE           = 0x39, //! Illegal value given
        AVR8_FAILURE_ILLEGAL_ID              = 0x3A, //! Illegal target ID
        AVR8_FAILURE_INVALID_CLOCK_SPEED     = 0x3B, //! Clock value out of range
        AVR8_FAILURE_TIMEOUT                 = 0x3C, //! A timeout occurred
        AVR8_FAILURE_ILLEGAL_OCD_STATUS      = 0x3D, //! Read an illegal OCD status
        AVR8_FAILURE_NVM_ENABLE              = 0x40, //! NVM failed to be enabled
        AVR8_FAILURE_NVM_DISABLE             = 0x41, //! NVM failed to be disabled
        AVR8_FAILURE_CS_ERROR                = 0x42, //! Illegal control/status bits
        AVR8_FAILURE_CRC_FAILURE             = 0x43, //! CRC mismatch
        AVR8_FAILURE_OCD_LOCKED              = 0x44, //! Failed to enable OCD
        AVR8_FAILURE_NO_OCD_CONTROL          = 0x50, //! Device is not under control
        AVR8_FAILURE_PC_READ_FAILED          = 0x60, //! Error when reading PC
        AVR8_FAILURE_REGISTER_READ_FAILED    = 0x61, //! Error when reading register
        AVR8_FAILURE_READ_ERROR              = 0x70, //! Error while reading
        AVR8_FAILURE_WRITE_ERROR             = 0x71, //! Error while writing
        AVR8_FAILURE_WRITE_TIMEOUT           = 0x72, //! Timeout while reading
        AVR8_FAILURE_ILLEGAL_BREAKPOINT      = 0x80, //! Invalid breakpoint configuration
        AVR8_FAILURE_TOO_MANY_BREAKPOINTS    = 0x81, //! Not enough available resources
        AVR8_FAILURE_NOT_SUPPORTED           = 0x90, //! This feature is not available
        AVR8_FAILURE_NOT_IMPLEMENTED         = 0x91, //! Command has not been implemented
        AVR8_FAILURE_UNKNOWN                 = 0xFF  //! Disaster.
    };

    // QUERY types on this protocol
    enum Avr8GenericQueryContexts {
        AVR8_QUERY_COMMANDS                 = 0x00, //! Supported command list
        AVR8_QUERY_CONFIGURATION            = 0x05, //! Supported configuration list
        AVR8_QUERY_READ_MEMTYPES            = 0x07, //! Supported read memtypes list
        AVR8_QUERY_WRITE_MEMTYPES           = 0x08  //! Supported write memtypes list
    };

    // Context definitions
    enum Avr8GenericSetGetContexts {
        AVR8_CTXT_CONFIG                    = 0x00, //! Configuration
        AVR8_CTXT_PHYSICAL                  = 0x01, //! Physical interface related
        AVR8_CTXT_DEVICE                    = 0x02, //! Device specific settings
        AVR8_CTXT_OPTIONS                   = 0x03, //! Option-related settings
        AVR8_CTXT_SESSION                   = 0x04, //! Session-related settings
    };

    enum Avr8GenericConfigContextParameters {
        AVR8_CONFIG_VARIANT                 = 0x00, //! Device family/variant
        AVR8_CONFIG_FUNCTION                = 0x01  //! Functional intent
    };

    enum Avr8GenericPhysicalContextParameters {
        AVR8_PHY_INTERFACE                  = 0x00, //! Physical interface selector
        AVR8_PHY_JTAG_DAISY                 = 0x01, //! JTAG daisy chain settings
        AVR8_PHY_DW_CLK_DIV                 = 0x10, //! debugWIRE clock divide ratio
        AVR8_PHY_MEGA_PRG_CLK               = 0x20, //! Clock for programming megaAVR
        AVR8_PHY_MEGA_DBG_CLK               = 0x21, //! Clock for debugging megaAVR
        AVR8_PHY_XM_JTAG_CLK                = 0x30, //! JTAG clock for AVR XMEGA
        AVR8_PHY_XM_PDI_CLK                 = 0x31  //! PDI clock for AVR XMEGA
    };

    enum Avr8GenericOptionsContextParameters {
        AVR8_OPT_RUN_TIMERS                 = 0x00, //! Keep timers running when stopped
        AVR8_OPT_DISABLE_DBP                = 0x01, //! No data breaks during reset
        AVR8_OPT_ENABLE_IDR                 = 0x03, //! Relay IDR messages
        AVR8_OPT_POLL_INT                   = 0x04  //! Configure polling speed
    };

    enum Avr8GenericSessionContextParameters {
        AVR8_SESS_MAIN_PC                   = 0x00  //! Address of main() function
    };

    enum Avr8GenericConfigTestParameters {
        AVR8_TEST_TGT_RUNNING               = 0x00  //! Is target running?
    };

    enum Avr8GenericVariantValues {
        AVR8_VARIANT_LOOPBACK               = 0x00, //! Dummy device
        AVR8_VARIANT_TINYOCD                = 0x01, //! tinyAVR or megaAVR with debugWIRE
        AVR8_VARIANT_MEGAOCD                = 0x02, //! megaAVR with JTAG
        AVR8_VARIANT_XMEGA                  = 0x03, //! AVR XMEGA
        AVR8_VARIANT_NONE                   = 0xFF  //! No device
    };

    enum Avr8GenericFunctionValues {
        AVR8_FUNC_NONE                      = 0x00, //! Not configured
        AVR8_FUNC_PROGRAMMING               = 0x01, //! I want to program only
        AVR8_FUNC_DEBUGGING                 = 0x02  //! I want a debug session
    };

    // Physical modes
    enum Avr8GenericPhysicalInterfaces {
        AVR8_PHY_INTF_NONE                  = 0x00, //! Not configured
        AVR8_PHY_INTF_JTAG                  = 0x04, //! JTAG
        AVR8_PHY_INTF_DW                    = 0x05, //! debugWIRE
        AVR8_PHY_INTF_PDI                   = 0x06  //! PDI
    };

    enum Avr8GenericMegaBreakpointTypes {
        AVR8_HWBP_PROG_BP               = 0x01  //! Program breaks

    };

    enum Avr8GenericMegaBreakCauses {
        AVR8_BREAK_CAUSE_UNKNOWN        = 0x00, //! Unspecified
        AVR8_BREAK_CAUSE_PROGRAM        = 0x01  //! Program break

    };

    enum Avr8GenericXmegaEraseModes {
        XMEGA_ERASE_CHIP                = 0x00, //! Erase entire chip
        XMEGA_ERASE_APP                 = 0x01, //! Erase application section only
        XMEGA_ERASE_BOOT                = 0x02, //! Erase boot section only
        XMEGA_ERASE_EEPROM              = 0x03, //! Erase EEPROM section only
        XMEGA_ERASE_APP_PAGE            = 0x04, //! Erase a single app section page
        XMEGA_ERASE_BOOT_PAGE           = 0x05, //! Erase a single boot section page
        XMEGA_ERASE_EEPROM_PAGE         = 0x06, //! Erase a single EEPROM page
        XMEGA_ERASE_USERSIG             = 0x07  //! Erase the user signature section
    };

    // Memory types
    enum Avr8GenericMemtypes {
        MEMTYPE_SRAM                    = 0x20, //! SRAM
        MEMTYPE_EEPROM                  = 0x22, //! EEPROM memory
        MEMTYPE_SPM                     = 0xA0, //! Flash memory in a debug session
        MEMTYPE_FLASH_PAGE              = 0xB0, //! Flash memory programming
        MEMTYPE_EEPROM_PAGE             = 0xB1, //! EEPROM memory pages
        MEMTYPE_FUSES                   = 0xB2, //! Fuse memory
        MEMTYPE_LOCKBITS                = 0xB3, //! Lock bits
        MEMTYPE_SIGNATURE               = 0xB4, //! Device signature
        MEMTYPE_OSCCAL                  = 0xB5, //! Oscillator calibration values
        MEMTYPE_REGFILE                 = 0xB8, //! Register file
        MEMTYPE_APPL_FLASH              = 0xC0, //! Application section flash
        MEMTYPE_BOOT_FLASH              = 0xC1, //! Boot section flash
        MEMTYPE_APPL_FLASH_ATOMIC       = 0xC2, //! Application page with auto-erase
        MEMTYPE_BOOT_FLASH_ATOMIC       = 0xC3, //! Boot page with auto-erase
        MEMTYPE_EEPROM_ATOMIC           = 0xC4, //! EEPROM page with auto-erase
        MEMTYPE_USER_SIGNATURE          = 0xC5, //! User signature secion
        MEMTYPE_CALIBRATION_SIGNATURE   = 0xC6  //! Calibration section
        };

Prev | Up | Next
| Home |