---
tag: m0552
title: Ethernet IP Address, Network IF
brief: Set Ethernet IP Address, Network Interface state
author: thinkyhead

group: ethernet
since: 2.0.8
requires: HAS_ETHERNET
eeprom: true

codes: [ M552 ]

parameters:
- tag: P
  optional: true
  description: Set IP Address. Set 0.0.0.0 to set the IP Address via DHCP.
  values:
  - tag: ip-address
    type: string
- tag: S
  optional: true
  description: Reset, Disable, or Enable the Network Interface.
  values:
  - tag: -1
    description: Reset
  - tag: 0
    description: Disable
  - tag: 1
    description: Enable

example:
- pre: Set the IP address and Reset the Network Interface
  code: M552 S-1 P192.168.1.55

---

Reset / enable / disable the Ethernet Interface and set the IP Address.
