---
tag: m0192
title: Wait for Probe temperature
brief: Wait for the probe temperature sensor to reach a target
author: thinkyhead

group: calibration
since: 2.0.6.2
requires: PROBE_TEMP_COMPENSATION

codes: [ M192 ]
related: [ G76, M871 ]

parameters:

- tag: R
  optional: true
  description: Temperature to wait for, whether heating or cooling.
  values:
  - tag: temp
    type: int

- tag: S
  optional: true
  description: A minimum temperature to wait for. No wait if already higher.
  values:
  - tag: temp
    type: int

example:
- code:
  - M192 S44 ; Wait for probe temperature to go above 44C
  - M192 R28 ; Wait for probe temperature to get close to 28C

---

Use this command to dwell until the probe reaches a given target temperature.
