---
tag: m0141
title: Set Chamber Temperature
brief: Set a new target chamber temperature.
author: GMagician

group: thermal

codes: [ M141 ]
related: [ M191 ]

parameters:

- tag: S
  optional: true
  description: 'Target temperature.<br/>`AUTOTEMP`: the min auto-temperature.'
  values:
  - tag: temp
    type: float

example:
- pre: Set chamber target temperature to 40°C
  code: M141 S40

---

Set a new target heated chamber temperature and continue without waiting. The firmware will continue to try to reach and hold the temperature in the background.
