---
tag: m0430
title: Power Monitor
brief: Read and display current (A), voltage (V), and power (W)
author: shitcreek

group: thermal
requires: POWER_MONITOR_CURRENT | POWER_MONITOR_VOLTAGE
eeprom: true

codes: [ M430 ]

notes:
- Requires either `POWER_MONITOR_CURRENT` or `POWER_MONITOR_VOLTAGE`

parameters:

- tag: I
  optional: true
  description: display current (A) on LCD
  values:
  - type: bool

- tag: V
  optional: true
  description: toggle display voltage (V) on LCD
  values:
  - type: bool

- tag: W
  optional: true
  description: display power/watts (W) on LCD
  values:
  - type: bool


examples:
- pre: report current LCD display power draw
  code: M430
- pre: Display all power monitor on LCD
  code: M430 I1 V1 W1

---
Enable/disable power monitor on LCD display. Report current/amps (A), voltage (V) and watts (W) if no parameters.

