---
tag: m0402
title: Stow Probe
brief: Stow the bed probe
author: thinkyhead

group: calibration
requires: HAS_BED_PROBE

codes: [ M402 ]
related: [ G30, M401 ]

notes: Requires some kind of bed probe. This command has no visible effect for probes that don't move; they are just deactivated.

parameters:

- tag: R
  optional: true
  since: 2.1.3
  description: Remain in place after stowing (and before deactivating) the probe.
  values:
  - type: bool

examples:
- pre: Deactivate and stow the probe
  code: M402
- pre: Deactivate and stow, remaining in place
  code: M402 R1

---

Stow the bed probe. The Z axis may raise up to make room for the probe to stow.
