---
tag: m0010
title: Vacuum / Blower Control
brief: Enable and disable the Cutter Vacuum or Laser Blower Motor.
author: descipher

group: control
since: 2.0.8
requires: AIR_EVACUATION

codes: [ M10, M11 ]

notes: These G-codes can only be enabled for use with a spindle or laser setup.

examples:

- pre: Turn laser blower motor on
  code: M10

- pre: Turn laser blower motor off
  code: M11

---

Immediately turn the cutter's vacuum or laser's blower motor on or off.
