Mesa 17.0.2 Release Notes / March 20, 2017
==========================================

Mesa 17.0.2 is a bug fix release which fixes bugs found since the 17.0.1
release.

Mesa 17.0.2 implements the OpenGL 4.5 API, but the version reported by
glGetString(GL_VERSION) or glGetIntegerv(GL_MAJOR_VERSION) /
glGetIntegerv(GL_MINOR_VERSION) depends on the particular driver being
used. Some drivers don't support all the features required in OpenGL
4.5. OpenGL 4.5 is **only** available if requested at context creation
because compatibility contexts are not supported.

SHA256 checksums
----------------

::

   2e0f41e7974ba7a36ca32bbeaf8ebcd65c8fd4d2dc9872f04d4becbd5e7a8cb5  mesa-17.0.2.tar.gz
   f8f191f909e01e65de38d5bdea5fb057f21649a3aed20948be02348e77a689d4  mesa-17.0.2.tar.xz

New features
------------

None

Bug fixes
---------

-  `Bug 68504 <https://bugs.freedesktop.org/show_bug.cgi?id=68504>`__ -
   9.2-rc1 workaround for clover build failure on ppc/altivec: cannot
   convert 'bool' to '__vector(4) \__bool int' in return
-  `Bug 97988 <https://bugs.freedesktop.org/show_bug.cgi?id=97988>`__ -
   [radeonsi] playing back videos with VDPAU exhibits
   deinterlacing/anti-aliasing issues not visible with VA-API
-  `Bug 99484 <https://bugs.freedesktop.org/show_bug.cgi?id=99484>`__ -
   Crusader Kings 2 - Loading bars, siege bars, morale bars, etc. do not
   render correctly
-  `Bug 99715 <https://bugs.freedesktop.org/show_bug.cgi?id=99715>`__ -
   Don't print: "Note: Buggy applications may crash, if they do please
   report to vendor"
-  `Bug 100049 <https://bugs.freedesktop.org/show_bug.cgi?id=100049>`__
   - "ralloc: Make sure ralloc() allocations match malloc()'s
   alignment." causes seg fault in 32bit build

Changes
-------

Alex Smith (3):

-  radv: Emit pending flushes before executing a secondary command
   buffer
-  radv: Flush before copying with PKT3_WRITE_DATA in CmdUpdateBuffer
-  radv/ac: Fix shared memory offset calculation

Bas Nieuwenhuizen (3):

-  radv: Disable HTILE for textures with multiple layers/levels.
-  radv: Emit cache flushes before CP DMA.
-  Revert "radv: Emit cache flushes before CP DMA."

Dave Airlie (3):

-  radv: drop Z24 support.
-  radv: disable mip point pre clamping.
-  radv: setup llvm target data layout

Emil Velikov (4):

-  docs: add sha256 checksums for 17.0.1
-  cherry-ignore: add the swizzle blorp_clear fix
-  i965: move brw_define.h ifndef guard to the top
-  Update version to 17.0.2

Fredrik Höglund (2):

-  radv: fix the dynamic buffer index in vkCmdBindDescriptorSets
-  radv/ac: fix multiple descriptor sets with dynamic buffers

Gregory Hainaut (1):

-  glapi: fix typo in count_scale

Ilia Mirkin (2):

-  nvc0: take extra pushbuf space into account for pushbuf_space calls
-  nvc0: increase alignment to 256 for texture buffers on fermi

Jacob Lifshay (1):

-  vulkan/wsi: Improve the DRI3 error message

James Legg (1):

-  radv: Fix using more than 4 bound descriptor sets

Faith Ekstrand (7):

-  anv/blorp/clear_subpass: Only set surface clear color for fast clears
-  anv: Accurately advertise dynamic descriptor limits
-  anv: Stall before fast-clear operations
-  anv: Properly handle destroying NULL devices and instances
-  anv/blorp: Turn off AUX after doing a CCS_D resolve
-  anv/blorp: Only set a clear color for resolves if fast-cleared
-  nir/intrinsics: Make load_barycentric_input take a 2-component coor

Jonas Pfeil (1):

-  ralloc: Make sure ralloc() allocations match malloc()'s alignment.

Kenneth Graunke (1):

-  egl: Ensure ResetNotificationStrategy matches for shared contexts.

Marek Olšák (3):

-  st/mesa: reset sample_mask, min_sample, and render_condition for PBO
   ops
-  st/mesa: set blend state for PBO readbacks
-  radeonsi: mark all bound shader buffer ranges as initialized

Matt Turner (1):

-  clover: Work around build failure with AltiVec.

Nanley Chery (2):

-  anv/pass: Avoid accessing attachment array out of bounds
-  anv/image: Remove extra dependency on HiZ-specific variable

Nicolai Hähnle (2):

-  st/glsl_to_tgsi: avoid iterating past the head of the instruction
   list
-  st/mesa: inform the driver of framebuffer changes before compute
   dispatches

Robert Foss (1):

-  mesa: Avoid read of uninitialized variable

Samuel Iglesias Gonsálvez (5):

-  i965/fs: mark last DF uniform array element as 64 bit live one
-  i965/fs: detect different bit size accesses to uniforms to push them
   in proper locations
-  i965/fs: fix indirect load DF uniforms on BSW/BXT
-  i965/fs: fix source type when emitting MOV_INDIRECT to read ICP
   handles
-  i965/fs: emit MOV_INDIRECT with the source with the right register
   type

Samuel Pitoiset (1):

-  radeonsi: disable sinking common instructions down to the end block
