Mesa 24.0.9 Release Notes / 2024-06-06
======================================

Mesa 24.0.9 is a bug fix release which fixes bugs found since the 24.0.8 release.

Mesa 24.0.9 implements the OpenGL 4.6 API, but the version reported by
glGetString(GL_VERSION) or glGetIntegerv(GL_MAJOR_VERSION) /
glGetIntegerv(GL_MINOR_VERSION) depends on the particular driver being used.
Some drivers don't support all the features required in OpenGL 4.6. OpenGL
4.6 is **only** available if requested at context creation.
Compatibility contexts may report a lower version depending on each driver.

Mesa 24.0.9 implements the Vulkan 1.3 API, but the version reported by
the apiVersion property of the VkPhysicalDeviceProperties struct
depends on the particular driver being used.

SHA256 checksum
---------------

::

    51aa686ca4060e38711a9e8f60c8f1efaa516baf411946ed7f2c265cd582ca4c  mesa-24.0.9.tar.xz


New features
------------

- None


Bug fixes
---------

- RustiCL: deadlock when calling clGetProfilingInfo() on callbacks
- dEQP-VK.pipeline.pipeline_library.shader_module_identifier.pipeline_from_id.graphics regression
- anv: unbounded shader cache
- radv: Crash due to nir validation fail in Enshrouded
- radv: Crash due to nir validation fail in Enshrouded
- panforst: T604 issue with using u32 for flat varyings


Changes
-------

Alexandre Marquet (1):

- pan/mdg: quirk to disable auto32

David Heidelberg (2):

- subprojects: uprev perfetto to v45.0
- ci/nouveau: move disabled jobs back from include into main gitlab-ci.yml

David Rosca (1):

- frontends/va: Fix leak when destroying VAEncCodedBufferType

Eric Engestrom (11):

- docs: add sha256sum for 24.0.8
- .pick_status.json: Update to 18c736bcfc55b8fa309ede02332b9c7a2ca22e78
- .pick_status.json: Mark 01bac643f6c088f7537edf18f2d4094881c1ecda as denominated
- .pick_status.json: Update to 4b6f7613c0bd161548f1bd45d42b65b4841a278a
- .pick_status.json: Mark eefe34127f8e8ae2ba91a7837b9dfef999dc3f87 as denominated
- .pick_status.json: Update to a1ea0956b46778d0331e4ef60ebd2be057fd0e9f
- .pick_status.json: Mark 410ca6a3e99c5c1c9c91f0f79bf43a35103cbd98 as denominated
- freedreno/a6xx: fix kernel -> compute handling
- panfrost: mark tests as fixed
- panfrost/ci: add missing genxml trigger path
- .pick_status.json: Update to 6f713a764fb412567caaabd9ae574822e79da383

Eric R. Smith (4):

- get_color_read_type: make sure format/type combo is legal for gles
- glsl: test both inputs when sorting varyings for xfb
- panfrost: fix some omissions in valhall flow control
- panfrost: change default rounding mode for samplers

Friedrich Vock (2):

- radv: Use max_se instead of num_se where appropriate
- radeonsi: Use max_se instead of num_se where appropriate

Iago Toral Quiroga (4):

- broadcom/compiler: make add_node return the node index
- broadcom/compiler: don't assign payload registers to spilling setup temps
- broadcom/compiler: apply payload conflict to spill setup before RA
- v3dv: fix incorrect index buffer size

Iván Briano (1):

- anv: check cmd_buffer is on a transfer queue more properly

Jose Maria Casanova Crespo (8):

- v3d: fix CLE MMU errors avoiding using last bytes of CL BOs.
- v3dv: fix CLE MMU errors avoiding using last bytes of CL BOs.
- v3d: Increase alignment to 16k on CL BO on RPi5
- v3dv: Increase alignment to 16k on CL BO on RPi5
- v3dv: V3D_CL_MAX_INSTR_SIZE bytes in last CL instruction not needed
- v3dv: Emit stencil draw clear if needed for GFXH-1461
- v3dv: really fix CLE MMU errors on 7.1HW Rpi5
- v3d: really fix CLE MMU errors on 7.1HW Rpi5

Juan A. Suarez Romero (1):

- ci: define SNMP base interface on runner

Karol Herbst (5):

- gallium/vl: stub vl_video_buffer_create_as_resource
- gallium/vl: remove stubs which are defined in mesa_util
- meson: centralize galliumvl_stub handling
- rusticl: link against libgalliumvl_stub
- rusticl/event: fix deadlock when calling clGetEventProfilingInfo inside callbacks

Kevin Chuang (1):

- anv: Properly fetch partial results in vkGetQueryPoolResults

Lionel Landwerlin (5):

- anv: use weak_ref mode for global pipeline caches
- anv: fix shader identifier handling
- intel/brw: ensure find_live_channel don't access arch register without sync
- anv: fix utrace compute walker timestamp captures
- anv: fix timestamp copies from secondary buffers

Renato Pereyra (1):

- anv: Attempt to compile all pipelines even after errors

Rhys Perry (3):

- aco: create lcssa phis for continue_or_break loops when necessary
- aco: create lcssa phis for continue_or_break loops when necessary
- radv: malloc graphics pipeline stages

Samuel Pitoiset (6):

- radv: allow 3d views with VK_IMAGE_CREATE_2D_VIEW_COMPATIBLE_BIT_EXT
- radv: set image view descriptors as buffer for non-graphics GPU
- radv: mark some formats as unsupported on GFX8/CARRIZO
- radv: only set ALPHA_IS_ON_MSB if the image has DCC on GFX6-9
- radv: fix setting a custom pitch for CB on GFX10_3+
- radv: fix flushing DB meta cache on GFX11.5

Tapani Pälli (1):

- anv/android: enable emulated astc for applications

Yusuf Khan (1):

- zink/query: begin time elapsed queries even if we arent in a rp
