# General

# Identification

## Product identification

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50000 | 0xC350 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50000 | 0xC350 | 4 | "SOCO" | - | STRING_16
50004 | 0xC354 | 1 | Product order ID (Countis:100, Protection:200, Atys:300, Diris:400) | - | U16
50005 | 0xC355 | 1 | Product ID (EX: 1000 ATS3) | - | U16
50006 | 0xC356 | 1 | JBUS Table Version (EX: 101 Version 1.01) | - | U16
50007 | 0xC357 | 1 | Product software version (EX: 100 Version 1.00) | - | U16
50008 | 0xC358 | 1 | Serial_AA_SS | - | U16_HEX
50009 | 0xC359 | 1 | Serial_SST_L | - | U16_HEX
50010 | 0xC35A | 1 | Serial_order | - | U16
50011 | 0xC35B | 2 | Serial_Reserve | - | U32
50013 | 0xC35D | 4 | See "Code table" tab for more details | - | U64_HEX
50017 | 0xC361 | 1 | Reserved | - | -
50018 | 0xC362 | 1 | Product version (Major) | - | U16
50019 | 0xC363 | 1 | Product version (Minor) | - | U16
50020 | 0xC364 | 1 | Reserved | - | -
50021 | 0xC365 | 1 | Reserved | - | -
50022 | 0xC366 | 3 | Reserved | - | -
50025 | 0xC369 | 1 | Reserved | - | -
50026 | 0xC36A | 1 | Reserved | - | -
50027 | 0xC36B | 1 | Reserved | - | -
50028 | 0xC36C | 1 | Reserved | - | -
50029 | 0xC36D | 1 | Reserved | - | -
50030 | 0xC36E | 4 | Product VLO (EX : "880100") | - | STRING_NORM
50034 | 0xC372 | 4 | Reserved | - | -
50038 | 0xC376 | 4 | Reserved | - | -
50042 | 0xC37A | 8 | Vendor name (EX : "SOCOMEC") | - | STRING_NORM
50050 | 0xC382 | 8 | Product name (EX : "DIRIS A40R") | - | STRING_NORM
50058 | 0xC38A | 8 | Extended name | - | STRING_NORM

## Communication board information

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38912 | 0x9800 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38912 | 0x9800 | 1 | Communication Board version (Major) | - | U16
38913 | 0x9801 | 1 | Communication Board version (Minor) | - | U16
38914 | 0x9802 | 1 | Communication Board version (Revision) | - | U16
38915 | 0x9803 | 1 | Communication Board version (Build) | - | U16
38916 | 0x9804 | 3 | Communication Board build date | - | DATETIME_3
38919 | 0x9807 | 4 | Communication Board VLO (EX : "880100") | - | STRING_NORM

# Common settings

## Network Setting

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57344 | 0xE000 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57344 | 0xE000 | 1 | Network Type : 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8
57345 | 0xE001 | 1 | Current Transformer secondary : 1 : 1 A 5 : 5 A | - | U8
57346 | 0xE002 | 1 | Current Transformer primary | A | U16
57347 | 0xE003 | 1 | Reserved | - | -
57348 | 0xE004 | 1 | Reserved | - | -
57349 | 0xE005 | 1 | Reserved | - | -
57350 | 0xE006 | 1 | Reserved | - | -
57351 | 0xE007 | 1 | Reserved | - | -
57352 | 0xE008 | 2 | Reserved | - | -
57354 | 0xE00A | 1 | Reserved | - | -
57355 | 0xE00B | 1 | Synchronisation Top for P+/- Q+/- : time in seconds ( 1mn, 5mn, 8mn, 10mn, 15mn, 20mn, 30mn, 60mn) | - | U16

## Hour/Date setting ( Write 6 words in one time Function 16)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57600 | 0xE100 | Settings | 6 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57600 | 0xE100 | 1 | Day | - | U8
57601 | 0xE101 | 1 | Month | - | U8
57602 | 0xE102 | 1 | Year | - | U16
57603 | 0xE103 | 1 | Hour | - | U8
57604 | 0xE104 | 1 | Minute | - | U8
57605 | 0xE105 | 1 | Second | - | U8

# Actions

## Action system

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57856 | 0xE200 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57856 | 0xE200 | 1 | Action : 0xA1 : Product Configuration storage 0xB2 : Produit reset | - | U8_HEX

## Value reset

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57888 | 0xE220 | Commands | 5 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57888 | 0xE220 | 1 | Reset :0x0001 : Min/Max and AVG 4V0x0002 : Min/Max and AVG 3U0x0004 : Min/Max and AVG 4I0x0008 : Min/Max and AVG F0x0010 : Min/Max and AVG P+0x0020 : Min/Max and AVG P-0x0040 : Min/Max and AVG Q+0x0080 : Min/Max and AVG Q-0x0100 : Min/Max and AVG S0x0200 : Min/Max and AVG PF0x0400 : Min/Max and AVG THD 4V0x0800 : Min/Max and AVG THD 3U0x1000 : Min/Max and AVG THD 4I0x2000 : Min/Max and AVG TIHD 4V0x4000 : Min/Max and AVG TIHD 3U0x8000 : Min/Max and AVG TIHD 4I | - | U16_HEX
57889 | 0xE221 | 1 | Reset : 0x0001 : Instantaneous Min/Max 4V0x0002 : Instantaneous Min/Max 3U0x0004 : Instantaneous Min/Max 4I0x0008 : Instantaneous Min/Max F0x0010 : Instantaneous Min/Max P+0x0020 : Instantaneous Min/Max P-0x0040 : Instantaneous Min/Max Q+0x0080 : Instantaneous Min/Max Q-0x0100 : Instantaneous Min/Max S0x0200 : Instantaneous Min/Max PF0x0400 : Instantaneous Min/Max THD 4V0x0800 : Instantaneous Min/Max THD 3U0x1000 : Instantaneous Min/Max THD 4I0x2000 : Instantaneous Min/Max TIHD 4V0x4000 : Instantaneous Min/Max TIHD 3U0x8000 : Instantaneous Min/Max TIHD 4I | - | U16_HEX
57890 | 0xE222 | 1 | Reset : 0x0001 : Ea+0x0002 : Er+0x0004 : Es0x0008 : Ea-0x0010 : Er-0x0020 : Hour counter0x0040 : All average P/Q/S0x0080 : All events and all curves0x0100 : All alarms | - | U16_HEX
57891 | 0xE223 | 1 | Reset : 0x0001 : Input pulse counter 10x0002 : Input pulse counter 20x0004 : Input pulse counter 30x0008 : Input pulse counter 40x0010 : Input pulse counter 50x0020 : Input pulse counter 60x0040 : Input pulse counter 70x0080 : Input pulse counter 80x0100 : Input pulse counter 90x0200 : Input pulse counter 100xFFFF : All | - | U16_HEX
57892 | 0xE224 | 1 | Reset : 0x0001 : Tariff counter 10x0002 : Tariff counter 20x0004 : Tariff counter 30x0008 : Tariff counter 40x0010 : Tariff counter 50x0020 : Tariff counter 60x0040 : Tariff counter 70x0080 : Tariff counter 80xFFFF : All | - | U16_HEX

# Application

# Measurement

# Common

## Metrology Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50512 | 0xC550 | Info | 62 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50512 | 0xC550 | 2 | Reserved | - | -
50514 | 0xC552 | 2 | Phase to Phase Voltage: U12 | V / 100 | U32
50516 | 0xC554 | 2 | Phase to Phase Voltage: U23 | V / 100 | U32
50518 | 0xC556 | 2 | Phase to Phase Voltage: U31 | V / 100 | U32
50520 | 0xC558 | 2 | Simple voltage : V1 | V / 100 | U32
50522 | 0xC55A | 2 | Simple voltage : V2 | V / 100 | U32
50524 | 0xC55C | 2 | Simple voltage : V3 | V / 100 | U32
50526 | 0xC55E | 2 | Frequency : F | Hz / 100 | U32
50528 | 0xC560 | 2 | Current : I1 | A / 1000 | U32
50530 | 0xC562 | 2 | Current : I2 | A / 1000 | U32
50532 | 0xC564 | 2 | Current : I3 | A / 1000 | U32
50534 | 0xC566 | 2 | Neutral Current : In | A / 1000 | U32
50536 | 0xC568 | 2 | ? Active Power +/- : P | W / 0.1 | S32
50538 | 0xC56A | 2 | ? Reactive Power +/- : Q | var / 0.1 | S32
50540 | 0xC56C | 2 | ? Apparent Power : S | VA / 0.1 | U32
50542 | 0xC56E | 2 | ? Power Factor : -: leading et + : lagging : PF | - / 1000 | S32
50544 | 0xC570 | 2 | Active Power phase 1 +/- : P1 | W / 0.1 | S32
50546 | 0xC572 | 2 | Active Power phase 2 +/- : P2 | W / 0.1 | S32
50548 | 0xC574 | 2 | Active Power phase 3 +/- : P3 | W / 0.1 | S32
50550 | 0xC576 | 2 | Reactive Power phase 1 +/- : Q1 | var / 0.1 | S32
50552 | 0xC578 | 2 | Reactive Power phase 2 +/- : Q2 | var / 0.1 | S32
50554 | 0xC57A | 2 | Reactive Power phase 3 +/- : Q3 | var / 0.1 | S32
50556 | 0xC57C | 2 | Apparent Power phase 1 : S1 | VA / 0.1 | U32
50558 | 0xC57E | 2 | Apparent Power phase 2 : S2 | VA / 0.1 | U32
50560 | 0xC580 | 2 | Apparent Power phase 3 : S3 | VA / 0.1 | U32
50562 | 0xC582 | 2 | Power Factor phase 1 -: leading and + : lagging : PF1 | - / 1000 | S32
50564 | 0xC584 | 2 | Power Factor phase 2 -: leading and + : lagging : PF2 | - / 1000 | S32
50566 | 0xC586 | 2 | Power Factor phase 3 -: leading and + : lagging : PF3 | - / 1000 | S32
50568 | 0xC588 | 2 | Reserved | - | -
50570 | 0xC58A | 2 | Reserved | - | -
50572 | 0xC58C | 2 | Reserved | - | -

## Energies

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50768 | 0xC650 | Info | 65 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50768 | 0xC650 | 2 | Reserved | - | -
50770 | 0xC652 | 2 | Total Positive Active Energy (no resetable) : Ea+ | Wh / 0.001 | U32
50772 | 0xC654 | 2 | Total Positive Reactive Energy (no resetable) : Er + | varh / 0.001 | U32
50774 | 0xC656 | 2 | Reserved | - | -
50776 | 0xC658 | 2 | Total Negative Active Energy (no resetable) : Ea- | Wh / 0.001 | U32
50778 | 0xC65A | 2 | Reserved | - | -
50780 | 0xC65C | 2 | Partial Positive Active Energy: Ea+ | Wh / 0.001 | U32
50782 | 0xC65E | 2 | Partial Positive Reactive Energy: Er + | varh / 0.001 | U32
50784 | 0xC660 | 2 | Reserved | - | -
50786 | 0xC662 | 2 | Partial Negative Active Energy : Ea- | Wh / 0.001 | U32
50788 | 0xC664 | 2 | Reserved | - | -
50790 | 0xC666 | 2 | Reserved | - | -
50792 | 0xC668 | 2 | Reserved | - | -
50794 | 0xC66A | 2 | Reserved | - | -
50796 | 0xC66C | 2 | Reserved | - | -
50798 | 0xC66E | 2 | Reserved | - | -
50800 | 0xC670 | 2 | Reserved | - | -
50802 | 0xC672 | 2 | Reserved | - | -
50804 | 0xC674 | 2 | Reserved | - | -
50806 | 0xC676 | 2 | Reserved | - | -
50808 | 0xC678 | 2 | Reserved | - | -
50810 | 0xC67A | 2 | Reserved | - | -
50812 | 0xC67C | 2 | Reserved | - | -
50814 | 0xC67E | 2 | Reserved | - | -
50816 | 0xC680 | 2 | Reserved | - | -
50818 | 0xC682 | 2 | Reserved | - | -
50820 | 0xC684 | 2 | Reserved | - | -
50822 | 0xC686 | 2 | Reserved | - | -
50824 | 0xC688 | 2 | Reserved | - | -
50826 | 0xC68A | 2 | Last date for Record average P/Q/S in second since 01/01/2000 | - | DATETIME
50828 | 0xC68C | 1 | Last average (P+) | W | U16
50829 | 0xC68D | 1 | Reserved | - | -
50830 | 0xC68E | 1 | Reserved | - | -
50831 | 0xC68F | 1 | Reserved | - | -
50832 | 0xC690 | 1 | Reserved | - | -

## Energies in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50944 | 0xC700 | Info | 65 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50944 | 0xC700 | 2 | Reserved | - | -
50946 | 0xC702 | 2 | Total Positive Active Energy (no resetable) : Ea+ | Wh / 0.1 | U32
50948 | 0xC704 | 2 | Total Positive Reactive Energy (no resetable) : Er + | varh / 0.1 | U32
50950 | 0xC706 | 2 | Reserved | - | -
50952 | 0xC708 | 2 | Total Negative Active Energy (no resetable) : Ea- | Wh / 0.1 | U32
50954 | 0xC70A | 2 | Reserved | - | -
50956 | 0xC70C | 2 | Partial Positive Active Energy: Ea+ | Wh / 0.1 | U32
50958 | 0xC70E | 2 | Partial Positive Reactive Energy: Er + | varh / 0.1 | U32
50960 | 0xC710 | 2 | Reserved | - | -
50962 | 0xC712 | 2 | Partial Negative Active Energy : Ea- | Wh / 0.1 | U32
50964 | 0xC714 | 2 | Reserved | - | -
50966 | 0xC716 | 2 | Reserved | - | -
50968 | 0xC718 | 2 | Reserved | - | -
50970 | 0xC71A | 2 | Reserved | - | -
50972 | 0xC71C | 2 | Reserved | - | -
50974 | 0xC71E | 2 | Reserved | - | -
50976 | 0xC720 | 2 | Reserved | - | -
50978 | 0xC722 | 2 | Reserved | - | -
50980 | 0xC724 | 2 | Reserved | - | -
50982 | 0xC726 | 2 | Reserved | - | -
50984 | 0xC728 | 2 | Reserved | - | -
50986 | 0xC72A | 2 | Reserved | - | -
50988 | 0xC72C | 2 | Reserved | - | -
50990 | 0xC72E | 2 | Reserved | - | -
50992 | 0xC730 | 2 | Reserved | - | -
50994 | 0xC732 | 2 | Reserved | - | -
50996 | 0xC734 | 2 | Reserved | - | -
50998 | 0xC736 | 2 | Reserved | - | -
51000 | 0xC738 | 2 | Reserved | - | -
51002 | 0xC73A | 2 | Last date for Record average P/Q/S in second since 01/01/2000 | - | DATETIME
51004 | 0xC73C | 1 | Last average (P+) | W | U16
51005 | 0xC73D | 1 | Reserved | - | -
51006 | 0xC73E | 1 | Reserved | - | -
51007 | 0xC73F | 1 | Reserved | - | -
51008 | 0xC740 | 1 | Reserved | - | -

## Statistique Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51024 | 0xC750 | Info | 70 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51024 | 0xC750 | 2 | Reserved | - | -
51026 | 0xC752 | 2 | Reserved | - | -
51028 | 0xC754 | 2 | Reserved | - | -
51030 | 0xC756 | 2 | Reserved | - | -
51032 | 0xC758 | 2 | Reserved | - | -
51034 | 0xC75A | 2 | Reserved | - | -
51036 | 0xC75C | 2 | Reserved | - | -
51038 | 0xC75E | 2 | Reserved | - | -
51040 | 0xC760 | 2 | Reserved | - | -
51042 | 0xC762 | 2 | Reserved | - | -
51044 | 0xC764 | 2 | Reserved | - | -
51046 | 0xC766 | 2 | Reserved | - | -
51048 | 0xC768 | 2 | Reserved | - | -
51050 | 0xC76A | 2 | Reserved | - | -
51052 | 0xC76C | 2 | Reserved | - | -
51054 | 0xC76E | 2 | Reserved | - | -
51056 | 0xC770 | 2 | Reserved | - | -
51058 | 0xC772 | 2 | Reserved | - | -
51060 | 0xC774 | 2 | Reserved | - | -
51062 | 0xC776 | 2 | Reserved | - | -
51064 | 0xC778 | 2 | Reserved | - | -
51066 | 0xC77A | 2 | Reserved | - | -
51068 | 0xC77C | 2 | Reserved | - | -
51070 | 0xC77E | 2 | Reserved | - | -
51072 | 0xC780 | 2 | Reserved | - | -
51074 | 0xC782 | 2 | Reserved | - | -
51076 | 0xC784 | 2 | Reserved | - | -
51078 | 0xC786 | 2 | Reserved | - | -
51080 | 0xC788 | 2 | Reserved | - | -
51082 | 0xC78A | 2 | Reserved | - | -
51084 | 0xC78C | 2 | Reserved | - | -
51086 | 0xC78E | 2 | Reserved | - | -
51088 | 0xC790 | 1 | Reserved | - | -
51089 | 0xC791 | 1 | Reserved | - | -
51090 | 0xC792 | 1 | Reserved | - | -
51091 | 0xC793 | 1 | Reserved | - | -
51092 | 0xC794 | 1 | Reserved | - | -
51093 | 0xC795 | 1 | Reserved | - | -

## Metrology No Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51280 | 0xC850 | Info | 35 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51280 | 0xC850 | 1 | Reserved | - | -
51281 | 0xC851 | 1 | Phase to Phase Voltage: U12 | V / 100 | U16
51282 | 0xC852 | 1 | Phase to Phase Voltage: U23 | V / 100 | U16
51283 | 0xC853 | 1 | Phase to Phase Voltage: U31 | V / 100 | U16
51284 | 0xC854 | 1 | Simple voltage : V1 | V / 100 | U16
51285 | 0xC855 | 1 | Simple voltage : V2 | V / 100 | U16
51286 | 0xC856 | 1 | Simple voltage : V3 | V / 100 | U16
51287 | 0xC857 | 1 | Reserved | - | -
51288 | 0xC858 | 1 | Reserved | - | -
51289 | 0xC859 | 1 | Reserved | - | -
51290 | 0xC85A | 1 | Reserved | - | -
51291 | 0xC85B | 1 | Reserved | - | -
51292 | 0xC85C | 1 | ? active Power +/- : P | W / 0.1 | S16
51293 | 0xC85D | 1 | ? reactive Power +/- : Q | var / 0.1 | S16
51294 | 0xC85E | 1 | ? apparent power : S | VA / 0.1 | U16
51295 | 0xC85F | 1 | ? power factor : -: leading and + : lagging : PF | - / 1000 | S16
51296 | 0xC860 | 1 | Active Power phase 1 +/- : P1 | W / 0.1 | S16
51297 | 0xC861 | 1 | Active Power phase 2 +/- : P2 | W / 0.1 | S16
51298 | 0xC862 | 1 | Active Power phase 3 +/- : P3 | W / 0.1 | S16
51299 | 0xC863 | 1 | Reactive Power phase 1 +/- : Q1 | var / 0.1 | S16
51300 | 0xC864 | 1 | Reactive Power phase 2 +/- : Q2 | var / 0.1 | S16
51301 | 0xC865 | 1 | Reactive Power phase 3 +/- : Q3 | var / 0.1 | S16
51302 | 0xC866 | 1 | Apparent power phase 1 : S1 | VA / 0.1 | U16
51303 | 0xC867 | 1 | Apparent power phase 2 : S2 | VA / 0.1 | U16
51304 | 0xC868 | 1 | Apparent power phase 3 : S3 | VA / 0.1 | U16
51305 | 0xC869 | 1 | Power Factor phase 1 -: leading and + : lagging : PF1 | - / 1000 | S16
51306 | 0xC86A | 1 | Power Factor phase 2 -: leading and + : lagging : PF2 | - / 1000 | S16
51307 | 0xC86B | 1 | Power Factor phase 3 -: leading and + : lagging : PF3 | - / 1000 | S16
51308 | 0xC86C | 1 | Reserved | - | -
51309 | 0xC86D | 1 | Reserved | - | -
51310 | 0xC86E | 1 | Reserved | - | -
51311 | 0xC86F | 1 | Total Positive Active Energy (no resetable) : Ea+ | Wh / 1E-06 | U16
51312 | 0xC870 | 1 | Total Positive Reactive Energy (no resetable) : Er + | varh / 1E-06 | U16
51313 | 0xC871 | 1 | Total Negative Active Energy (no resetable) : Ea- | Wh / 1E-06 | U16
51314 | 0xC872 | 1 | Reserved | - | -

## Load curve P+

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61440 | 0xF000 | Command | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61440 | 0xF000 | 1 | Action 0x0001 : Reset read pointer 0xFFFE : Get next data | - | U16_HEX

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61456 | 0xF010 | Header | 6 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61456 | 0xF010 | 1 | Record count ( Maximum 29 ) | - | U8
61457 | 0xF011 | 1 | Record size : 4 see below the data record description | W | U8
61458 | 0xF012 | 1 | Integration period | s | U16
61459 | 0xF013 | 1 | Physical Unit : 0 0 : W 1 : W 2 : var 3 : var 4 : VA 5 : None 6 : J 7 : Pulse 8 : m3 9 : Nm3 20 : kW 22 : kVAr 24 : kVA 26 : kJ 27 : kilo-Pulse | - | U8
61460 | 0xF014 | 1 | Numerator Rate | - | U16
61461 | 0xF015 | 1 | Denominator Rate | - | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61462 | 0xF016 | Data | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61462 | 0xF016 | 2 | Date | s | DATETIME
61464 | 0xF018 | 1 | Full/incomplete period 0 : full integration period 1 : incomplete integration period | - | U8
61465 | 0xF019 | 1 | Value without CT*VT rate | W | U16

## Energies per tariff

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50848 | 0xC6A0 | Info | 50 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50848 | 0xC6A0 | 1 | 0 >: Tariff number <: 8 | - | U8
50849 | 0xC6A1 | 1 | Tariff number in progress ( 1 to 8 ) | - | U8
50850 | 0xC6A2 | 2 | Positive Active Energies 1 | Wh / 0.001 | U32
50852 | 0xC6A4 | 2 | Positive Active Energies 2 | Wh / 0.001 | U32
50854 | 0xC6A6 | 2 | Positive Active Energies 3 | Wh / 0.001 | U32
50856 | 0xC6A8 | 2 | Positive Active Energies 4 | Wh / 0.001 | U32
50858 | 0xC6AA | 2 | Reserved | - | -
50860 | 0xC6AC | 2 | Reserved | - | -
50862 | 0xC6AE | 2 | Reserved | - | -
50864 | 0xC6B0 | 2 | Reserved | - | -
50866 | 0xC6B2 | 2 | Reserved | - | -
50868 | 0xC6B4 | 2 | Reserved | - | -
50870 | 0xC6B6 | 2 | Reserved | - | -
50872 | 0xC6B8 | 2 | Reserved | - | -
50874 | 0xC6BA | 2 | Reserved | - | -
50876 | 0xC6BC | 2 | Reserved | - | -
50878 | 0xC6BE | 2 | Reserved | - | -
50880 | 0xC6C0 | 2 | Reserved | - | -
50882 | 0xC6C2 | 2 | Reserved | - | -
50884 | 0xC6C4 | 2 | Reserved | - | -
50886 | 0xC6C6 | 2 | Reserved | - | -
50888 | 0xC6C8 | 2 | Reserved | - | -
50890 | 0xC6CA | 2 | Reserved | - | -
50892 | 0xC6CC | 2 | Reserved | - | -
50894 | 0xC6CE | 2 | Reserved | - | -
50896 | 0xC6D0 | 2 | Reserved | - | -

## Energies per tariff in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51200 | 0xC800 | Info | 50 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51200 | 0xC800 | 1 | 0 >: Tariff number <: 8 | - | U8
51201 | 0xC801 | 1 | Tariff number in progress ( 1 to 8 ) | - | U8
51202 | 0xC802 | 2 | Positive Active Energies 1 | Wh / 0.1 | U32
51204 | 0xC804 | 2 | Positive Active Energies 2 | Wh / 0.1 | U32
51206 | 0xC806 | 2 | Positive Active Energies 3 | Wh / 0.1 | U32
51208 | 0xC808 | 2 | Positive Active Energies 4 | Wh / 0.1 | U32
51210 | 0xC80A | 2 | Reserved | - | -
51212 | 0xC80C | 2 | Reserved | - | -
51214 | 0xC80E | 2 | Reserved | - | -
51216 | 0xC810 | 2 | Reserved | - | -
51218 | 0xC812 | 2 | Reserved | - | -
51220 | 0xC814 | 2 | Reserved | - | -
51222 | 0xC816 | 2 | Reserved | - | -
51224 | 0xC818 | 2 | Reserved | - | -
51226 | 0xC81A | 2 | Reserved | - | -
51228 | 0xC81C | 2 | Reserved | - | -
51230 | 0xC81E | 2 | Reserved | - | -
51232 | 0xC820 | 2 | Reserved | - | -
51234 | 0xC822 | 2 | Reserved | - | -
51236 | 0xC824 | 2 | Reserved | - | -
51238 | 0xC826 | 2 | Reserved | - | -
51240 | 0xC828 | 2 | Reserved | - | -
51242 | 0xC82A | 2 | Reserved | - | -
51244 | 0xC82C | 2 | Reserved | - | -
51246 | 0xC82E | 2 | Reserved | - | -
51248 | 0xC830 | 2 | Reserved | - | -

# Specific

## Table Overflow

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36864 | 0x9000 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36864 | 0x9000 | 2 | Value of the meter overflow (10Wh) : 999 999 999 | Wh / 0.1 | U32
36866 | 0x9002 | 1 | Nb Overflow Total Ea + | - | U8
36867 | 0x9003 | 1 | Nb Overflow Total Er + | - | U8
36868 | 0x9004 | 1 | Nb Overflow Total Ea - | - | U8
36869 | 0x9005 | 1 | Reserved | - | U8
36870 | 0x9006 | 1 | Reserved | - | U8
36871 | 0x9007 | 1 | Nb Overflow Total Ea T1 | - | U8
36872 | 0x9008 | 1 | Nb Overflow Total Ea T2 | - | U8
36873 | 0x9009 | 1 | Nb Overflow Total Ea T3 | - | U8
36874 | 0x900A | 1 | Nb Overflow Total Ea T4 | - | U8

## Temporal Active Index

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36896 | 0x9020 | Info | 24 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36896 | 0x9020 | 2 | Ea + for day n-1 | Wh / 0.001 | U32
36898 | 0x9022 | 2 | Ea - for day n-1 | Wh / 0.001 | U32
36900 | 0x9024 | 2 | Ea + for day n | Wh / 0.001 | U32
36902 | 0x9026 | 2 | Ea - for day n | Wh / 0.001 | U32
36904 | 0x9028 | 2 | Ea + for Week n-1 | Wh / 0.001 | U32
36906 | 0x902A | 2 | Ea - for Week n-1 | Wh / 0.001 | U32
36908 | 0x902C | 2 | Ea + for Week n | Wh / 0.001 | U32
36910 | 0x902E | 2 | Ea - for Week n | Wh / 0.001 | U32
36912 | 0x9030 | 2 | Ea + for Month n-1 | Wh / 0.001 | U32
36914 | 0x9032 | 2 | Ea - for Month n-1 | Wh / 0.001 | U32
36916 | 0x9034 | 2 | Ea + for Month n | Wh / 0.001 | U32
36918 | 0x9036 | 2 | Ea - for Month n | Wh / 0.001 | U32

## Temporal Active Index in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36928 | 0x9040 | Info | 24 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36928 | 0x9040 | 2 | Ea + for day n-1 | Wh / 0.1 | U32
36930 | 0x9042 | 2 | Ea - for day n-1 | Wh / 0.1 | U32
36932 | 0x9044 | 2 | Ea + for day n | Wh / 0.1 | U32
36934 | 0x9046 | 2 | Ea - for day n | Wh / 0.1 | U32
36936 | 0x9048 | 2 | Ea + for Week n-1 | Wh / 0.1 | U32
36938 | 0x904A | 2 | Ea - for Week n-1 | Wh / 0.1 | U32
36940 | 0x904C | 2 | Ea + for Week n | Wh / 0.1 | U32
36942 | 0x904E | 2 | Ea - for Week n | Wh / 0.1 | U32
36944 | 0x9050 | 2 | Ea + for Month n-1 | Wh / 0.1 | U32
36946 | 0x9052 | 2 | Ea - for Month n-1 | Wh / 0.1 | U32
36948 | 0x9054 | 2 | Ea + for Month n | Wh / 0.1 | U32
36950 | 0x9056 | 2 | Ea - for Month n | Wh / 0.1 | U32

## Current without CT

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40576 | 0x9E80 | Info | 6 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40576 | 0x9E80 | 2 | Current: I1 | A / 1000 | U32
40578 | 0x9E82 | 2 | Current: I2 | A / 1000 | U32
40580 | 0x9E84 | 2 | Current: I3 | A / 1000 | U32

# Action

## Set Tariff

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40480 | 0x9E20 | Commands | 2 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40480 | 0x9E20 | 1 | Reserved | - | U8
40481 | 0x9E21 | 1 | N? Tariff to set | - | U8

## Partial Energies Reset

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40512 | 0x9E40 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40512 | 0x9E40 | 1 | Reserved | - | -

# Industrialization

## Indus Mode and MID status

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40544 | 0x9E60 | Info | 2 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40544 | 0x9E60 | 1 | Indus Mode (0: indus mode disabled, 1: indus mode enabled) | - | U8
40545 | 0x9E61 | 1 | MID status (0: non-MID product, 1: MID product | - | U8

## COM Board Product ID

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40608 | 0x9EA0 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40608 | 0x9EA0 | 1 | Product ID :0x01: E3x/E4x COM Board0x02: E63 COM Board | - | U8