# General

# Identification

## Product identification

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50000 | 0xC350 | Info | 69 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50000 | 0xC350 | 4 | "SOCO" | - | STRING_16
50004 | 0xC354 | 1 | Product order ID (Countis:100, Protection:200, Atys:300, Diris:400) | - | U16
50005 | 0xC355 | 1 | Product ID (EX: 1000 ATS3) | - | U16
50006 | 0xC356 | 1 | MODBUS Table Version | - | U16
50007 | 0xC357 | 1 | Product software version (EX: 100 Version 1.00) | - | U16
50008 | 0xC358 | 1 | Serial_AA_SS | - | U16_HEX
50009 | 0xC359 | 1 | Serial_SST_L | - | U16_HEX
50010 | 0xC35A | 1 | Serial_order | - | U16
50011 | 0xC35B | 2 | Serial_Reserve | - | U32
50013 | 0xC35D | 4 | See "Code table" tab for more details | - | U64_HEX
50017 | 0xC361 | 1 | Customization data loaded (True/False) | - | U8
50018 | 0xC362 | 1 | Product version (Major) | - | U16
50019 | 0xC363 | 1 | Product version (Minor) | - | U16
50020 | 0xC364 | 1 | Product version (Revision) | - | U16
50021 | 0xC365 | 1 | Product version (Build) | - | U16
50022 | 0xC366 | 3 | Product build date | - | DATETIME_3
50025 | 0xC369 | 1 | Software technical base version (Major) | - | U16
50026 | 0xC36A | 1 | Software technical base version (Minor) | - | U16
50027 | 0xC36B | 1 | Software technical base version (Revision) | - | U16
50028 | 0xC36C | 1 | Customization version (Major) | - | U16
50029 | 0xC36D | 1 | Customization version (Minor) | - | U16
50030 | 0xC36E | 4 | Product VLO (EX : "880100") | - | STRING_NORM
50034 | 0xC372 | 4 | Customization VLO (EX : "880700") | - | STRING_NORM
50038 | 0xC376 | 4 | Software technical base VLO (EX : "880600") | - | STRING_NORM
50042 | 0xC37A | 8 | Vendor name (EX : "SOCOMEC") | - | STRING_NORM
50050 | 0xC382 | 8 | Product name (EX : "PMD EE") | - | STRING_NORM
50058 | 0xC38A | 8 | Extended name | - | STRING_NORM
50066 | 0xC392 | 1 | Resource version (Build 2) | - | U16
50067 | 0xC393 | 2 | Net ID | - | U32_HEX

## Option Module identification

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49936 | 0xC310 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49936 | 0xC310 | 1 | Option module ID on slot 1: 0 : Com Option 1 : Log IO Option 2 : Analog IO Option 3 : Temp Option 4 : None | - | U8
49937 | 0xC311 | 1 | Option module ID on slot 2: 0 : Com Option 1 : Log IO Option 2 : Analog IO Option 3 : Tem Option 4 : None | - | U8
49938 | 0xC312 | 1 | Option module ID on slot 3: 0 : Com Option 1 : Log IO Option 2 : Analog IO Option 3 : Tem Option 4 : None | - | U8
49939 | 0xC313 | 1 | Option module ID on slot 4: 0 : Com Option 1 : Log IO Option 2 : Analog IO Option 3 : Tem Option 4 : None | - | U8

## RF identification

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49968 | 0xC330 | Info | 17 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49968 | 0xC330 | 16 | Serial number | - | STRING_NORM
49984 | 0xC340 | 1 | RF board connected 0 : Not connected 1 : Connected | - | U16

# Common settings

## Modbus settings

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57344 | 0xE000 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57344 | 0xE000 | 1 | Slave Address | - | U8

## RS485 settings

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57345 | 0xE001 | Settings | 3 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57345 | 0xE001 | 1 | Baudrate : 0 : 1200 1 : 2400 2 : 4800 3 : 9600 4 : 19200 5 : 38400 6 : 57600 7 : 115200 | - | U16
57346 | 0xE002 | 1 | Stop bit : 0 : 1 1 : 2 | - | U16
57347 | 0xE003 | 1 | Parity : 0 : None 1 : Odd 2 : Even | - | U16

## RF settings

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57360 | 0xE010 | Settings | 2 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57360 | 0xE010 | 1 | Channel selected | - | U16
57361 | 0xE011 | 1 | Sub network (0 : no subnet) : | - | U8

## Hour/Date setting ( Write 6 words in one time Function 16)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57600 | 0xE100 | Settings | 6 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57600 | 0xE100 | 1 | Day | - | U8
57601 | 0xE101 | 1 | Month | - | U8
57602 | 0xE102 | 1 | Year | - | U16
57603 | 0xE103 | 1 | Hour | - | U8
57604 | 0xE104 | 1 | Minute | - | U8
57605 | 0xE105 | 1 | Second | - | U8

# Actions

## Action system ( Write Function only )

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57856 | 0xE200 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57856 | 0xE200 | 1 | Action : 0xA1 : Save Product Configuration 0xB2 : Product reboot 0xE5 : Reset to factory settings | - | U8_HEX

## Identification by blinking LED

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57864 | 0xE208 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57864 | 0xE208 | 1 | Action 1 : Start blinking | - | U16

## USB function ( Write Function only )

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57872 | 0xE210 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57872 | 0xE210 | 1 | USB function : 0x01 : DFU 0x02 : PCL 0x03 : Mass storage 0x04 : Option slot 1 0x05 : Option slot 2 0x06 : Option slot 3 0x07 : Option slot 4 0x08 : RF module | - | U8_HEX

## Lock system

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
58112 | 0xE300 | Settings | 2 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
58112 | 0xE300 | 1 | Code to submit | - | U16
58113 | 0xE301 | 1 | Delocker ID | - | U16

# Maintenance

## Operating hours counters

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
512 | 0x0200 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
512 | 0x0200 | 2 | Total operating hours counter | s | U32
514 | 0x0202 | 2 | Partial operating hours counter | s | U32

## Partial operating hours counter reset

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
528 | 0x0210 | Commands | 1 | USER | NONE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
528 | 0x0210 | 1 | Reset command 0 : Reset | - | U16

## Events log

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
624 | 0x0270 | Command | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
624 | 0x0270 | 1 | Start record number (0 to 65534) or 65535 for last record | - | U16

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
640 | 0x0280 | Header | 3 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
640 | 0x0280 | 1 | Next record number | - | U16
641 | 0x0281 | 1 | Items count (max 3 per request) | - | U16
642 | 0x0282 | 1 | Item size (words) | - | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
643 | 0x0283 | Data | 8 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
643 | 0x0283 | 1 | Event ID | - | U16_HEX
644 | 0x0284 | 2 | Start Date | s | DATETIME
646 | 0x0286 | 1 | Cause | - | U16_HEX
647 | 0x0287 | 2 | Value 1 | - | S32
649 | 0x0289 | 2 | Value 2 | - | S32

## Reset histo

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
544 | 0x0220 | Commands | 1 | USER | NONE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
544 | 0x0220 | 1 | Action 0 : No action 1 : Reset alarms history 2 : Reset EN50160 / Inrush events history 4 : Reset system events 8 : Reset load curves 16 : Reset average trends | - | U16

# Application

# Wiring settings

# Network

##

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
12288 | 0x3000 | Settings | 9 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
12288 | 0x3000 | 1 | Network connection type 0 : Not defined 1 : 1P + N 2 : 2P 3 : 2P + N 4 : 3P 5 : 3P + N | - | U8
12289 | 0x3001 | 2 | Nominal Voltage | V | U32
12291 | 0x3003 | 1 | Nominal Frequency 0 : 50 Hz 1 : 60 Hz | - | U8
12292 | 0x3004 | 1 | Phase rotation 0 : V1 - V2 - V3 1 : V1 - V3 - V2 | - | U8
12293 | 0x3005 | 1 | Voltage transformer used 0 : No 1 : Yes | - | U8
12294 | 0x3006 | 2 | Voltage transformer rate : primary | - | U32
12296 | 0x3008 | 1 | Voltage transformer rate : secondary | - | U16

# Sensors

##

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
13568 | 0x3500 | Settings | 8 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
13568 | 0x3500 | 1 | Sensor 1 : Way 0 : Positive 1 : Negative | - | U8
13569 | 0x3501 | 1 | Sensor 1 : associated LineV 0 : LineV1 1 : LineV2 2 : LineV3 3 : LineVn 5 : LineVUndefined | - | U8
13570 | 0x3502 | 1 | Sensor 2 : Way 0 : Positive 1 : Negative | - | U8
13571 | 0x3503 | 1 | Sensor 2 : associated LineV 0 : LineV1 1 : LineV2 2 : LineV3 3 : LineVn 5 : LineVUndefined | - | U8
13572 | 0x3504 | 1 | Sensor 3 : Way 0 : Positive 1 : Negative | - | U8
13573 | 0x3505 | 1 | Sensor 3 : associated LineV 0 : LineV1 1 : LineV2 2 : LineV3 3 : LineVn 5 : LineVUndefined | - | U8
13574 | 0x3506 | 1 | Sensor 4 : Way 0 : Positive 1 : Negative | - | U8
13575 | 0x3507 | 1 | Sensor 4 : associated LineV 0 : LineV1 1 : LineV2 2 : LineV3 3 : LineVn 5 : LineVUndefined | - | U8

# Loads

## Load settings #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
13824 | 0x3600 | Settings | 14 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
13824 | 0x3600 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
13825 | 0x3601 | 1 | Type 0 : Undefined 1 : 1P+N-1CT 2 : 2P-1CT 3 : 2P+N-2CT 4 : 3P-1CT 5 : 3P-2CT 6 : 3P-3CT 7 : 3P+N-1CT 8 : 3P+N-3CT 9 : 3P+N-4CT | - | U8
13826 | 0x3602 | 1 | Inom | A | U16
13827 | 0x3603 | 1 | Reserved | - | -
13828 | 0x3604 | 8 | Reserved | - | -
13836 | 0x360C | 1 | Nature | - | U8
13837 | 0x360D | 1 | Usage | - | U8

## Load settings #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
13856 | 0x3620 | Settings | 14 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
13856 | 0x3620 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
13857 | 0x3621 | 1 | Type 0 : Undefined 1 : 1P+N-1CT 2 : 2P-1CT 3 : 2P+N-2CT 4 : 3P-1CT 5 : 3P-2CT 6 : 3P-3CT 7 : 3P+N-1CT 8 : 3P+N-3CT 9 : 3P+N-4CT | - | U8
13858 | 0x3622 | 1 | Inom | A | U16
13859 | 0x3623 | 1 | Reserved | - | -
13860 | 0x3624 | 8 | Reserved | - | -
13868 | 0x362C | 1 | Nature | - | U8
13869 | 0x362D | 1 | Usage | - | U8

## Load settings #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
13888 | 0x3640 | Settings | 14 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
13888 | 0x3640 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
13889 | 0x3641 | 1 | Type 0 : Undefined 1 : 1P+N-1CT 2 : 2P-1CT 3 : 2P+N-2CT 4 : 3P-1CT 5 : 3P-2CT 6 : 3P-3CT 7 : 3P+N-1CT 8 : 3P+N-3CT 9 : 3P+N-4CT | - | U8
13890 | 0x3642 | 1 | Inom | A | U16
13891 | 0x3643 | 1 | Reserved | - | -
13892 | 0x3644 | 8 | Reserved | - | -
13900 | 0x364C | 1 | Nature | - | U8
13901 | 0x364D | 1 | Usage | - | U8

## Load settings #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
13920 | 0x3660 | Settings | 14 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
13920 | 0x3660 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
13921 | 0x3661 | 1 | Type 0 : Undefined 1 : 1P+N-1CT 2 : 2P-1CT 3 : 2P+N-2CT 4 : 3P-1CT 5 : 3P-2CT 6 : 3P-3CT 7 : 3P+N-1CT 8 : 3P+N-3CT 9 : 3P+N-4CT | - | U8
13922 | 0x3662 | 1 | Inom | A | U16
13923 | 0x3663 | 1 | Reserved | - | -
13924 | 0x3664 | 8 | Reserved | - | -
13932 | 0x366C | 1 | Nature | - | U8
13933 | 0x366D | 1 | Usage | - | U8

# Measurement

## External top synchro

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
34896 | 0x8850 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
34896 | 0x8850 | 1 | Top synchro command 1 : Send top synchro | - | U16

## Load curves

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
34912 | 0x8860 | Command | 3 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
34912 | 0x8860 | 1 | Start record number (0 to 65534) or 65535 for last record | - | U16
34913 | 0x8861 | 1 | Load number: 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 | - | U16
34914 | 0x8862 | 1 | Power type: 0 : P_pos - Positive active power 1 : P_neg - Negative active power 2 : Q_pos - Positive reactive power 3 : Q_neg - Negative reactive power 4 : S - Apparent power | - | U16

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
34928 | 0x8870 | Header | 8 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
34928 | 0x8870 | 1 | Next record number | - | U16
34929 | 0x8871 | 1 | Items count (24 per record) | - | U16
34930 | 0x8872 | 1 | Item size | - | U16
34931 | 0x8873 | 1 | Load number: 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 | - | U16
34932 | 0x8874 | 1 | Power type: 0 : P_pos - Positive active power (W) 1 : P_neg - Negative active power (W) 2 : Q_pos - Positive reactive power (var) 3 : Q_neg - Negative reactive power (var) 4 : S - Apparent power (VA) | - | U16
34933 | 0x8875 | 1 | Integration period duration | s | U16
34934 | 0x8876 | 1 | Numerator rate | - | U16
34935 | 0x8877 | 1 | Denominator rate | - | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
34936 | 0x8878 | Data | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
34936 | 0x8878 | 2 | Date | s | DATETIME
34938 | 0x887A | 1 | Flags: 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
34939 | 0x887B | 1 | Point value | min | U16

## Load curves raw

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
35072 | 0x8900 | Command | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
35072 | 0x8900 | 1 | Start record number (0 to 65534) or 65535 for last record | - | U16

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
35088 | 0x8910 | Header | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
35088 | 0x8910 | 1 | Next record number | - | U16
35089 | 0x8911 | 1 | Items count (2 per record) | - | U16
35090 | 0x8912 | 1 | Item size | - | U16
35091 | 0x8913 | 1 | Integration period duration | s | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
35092 | 0x8914 | Data | 59 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
35092 | 0x8914 | 2 | Date | - | DATETIME
35094 | 0x8916 | 1 | Flags | - | U16
35095 | 0x8917 | 2 | Power item 1 | - | U32
35097 | 0x8919 | 2 | Power item 2 | - | U32
35099 | 0x891B | 2 | Power item 3 | - | U32
35101 | 0x891D | 2 | Power item 4 | - | U32
35103 | 0x891F | 2 | Power item 5 | - | U32
35105 | 0x8921 | 2 | Power item 6 | - | U32
35107 | 0x8923 | 2 | Power item 7 | - | U32
35109 | 0x8925 | 2 | Power item 8 | - | U32
35111 | 0x8927 | 2 | Power item 9 | - | U32
35113 | 0x8929 | 2 | Power item 10 | - | U32
35115 | 0x892B | 2 | Power item 11 | - | U32
35117 | 0x892D | 2 | Power item 12 | - | U32
35119 | 0x892F | 2 | Reserved | - | -
35121 | 0x8931 | 2 | Reserved | - | -
35123 | 0x8933 | 2 | Reserved | - | -
35125 | 0x8935 | 2 | Reserved | - | -
35127 | 0x8937 | 2 | Reserved | - | -
35129 | 0x8939 | 2 | Reserved | - | -
35131 | 0x893B | 2 | Reserved | - | -
35133 | 0x893D | 2 | Reserved | - | -
35135 | 0x893F | 2 | Reserved | - | -
35137 | 0x8941 | 2 | Reserved | - | -
35139 | 0x8943 | 2 | Reserved | - | -
35141 | 0x8945 | 2 | Reserved | - | -
35143 | 0x8947 | 2 | Reserved | - | -
35145 | 0x8949 | 2 | Reserved | - | -
35147 | 0x894B | 2 | Reserved | - | -
35149 | 0x894D | 2 | Reserved | - | -

## Set tariff number

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
35215 | 0x898F | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
35215 | 0x898F | 1 | Set tariff number 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16

# Loads

## Inst. measurement - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
18432 | 0x4800 | Info | 92 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
18432 | 0x4800 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
18433 | 0x4801 | 2 | Date of last instance | s | DATETIME
18435 | 0x4803 | 1 | Integration time | s / 5 | U16
18436 | 0x4804 | 2 | System Ph-N Voltage | V / 100 | U32
18438 | 0x4806 | 2 | System Ph-Ph Voltage | V / 100 | U32
18440 | 0x4808 | 2 | System Current | A / 1000 | U32
18442 | 0x480A | 2 | Frequency | Hz / 1000 | U32
18444 | 0x480C | 2 | Ph-N Voltage : V1 | V / 100 | U32
18446 | 0x480E | 2 | Ph-N Voltage : V2 | V / 100 | U32
18448 | 0x4810 | 2 | Ph-N Voltage : V3 | V / 100 | U32
18450 | 0x4812 | 2 | Ph-N Voltage : Vn | V / 100 | U32
18452 | 0x4814 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
18454 | 0x4816 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
18456 | 0x4818 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
18458 | 0x481A | 2 | Current : I1 | A / 1000 | U32
18460 | 0x481C | 2 | Current : I2 | A / 1000 | U32
18462 | 0x481E | 2 | Current : I3 | A / 1000 | U32
18464 | 0x4820 | 2 | Current : In | A / 1000 | U32
18466 | 0x4822 | 1 | Inba | % / 100 | U16
18467 | 0x4823 | 2 | Idir | A / 1000 | U32
18469 | 0x4825 | 2 | Iinv | A / 1000 | U32
18471 | 0x4827 | 2 | Ihom | A / 1000 | U32
18473 | 0x4829 | 1 | Inb | % / 100 | U16
18474 | 0x482A | 2 | Snom | VA | U32
18476 | 0x482C | 2 | Total active power | W | S32
18478 | 0x482E | 2 | Total reactive power | var | S32
18480 | 0x4830 | 2 | Total lagging reactive power | var | S32
18482 | 0x4832 | 2 | Total leading reactive power | var | S32
18484 | 0x4834 | 2 | Total apparent power | VA | U32
18486 | 0x4836 | 1 | Total power factor | - / 1000 | S16
18487 | 0x4837 | 1 | Total Power factor type : 0 : undefined 1 : leading 2 : lagging | - | U8
18488 | 0x4838 | 2 | Active power : P1 | W | S32
18490 | 0x483A | 2 | Active power : P2 | W | S32
18492 | 0x483C | 2 | Active power : P3 | W | S32
18494 | 0x483E | 2 | Reactive power : Q1 | var | S32
18496 | 0x4840 | 2 | Reactive power : Q2 | var | S32
18498 | 0x4842 | 2 | Reactive power : Q3 | var | S32
18500 | 0x4844 | 2 | Lagging reactive power : Q1_lagg | var | S32
18502 | 0x4846 | 2 | Lagging reactive power : Q2_lagg | var | S32
18504 | 0x4848 | 2 | Lagging reactive power : Q3_lagg | var | S32
18506 | 0x484A | 2 | Leading reactive power : Q1_lead | var | S32
18508 | 0x484C | 2 | Leading reactive power : Q2_lead | var | S32
18510 | 0x484E | 2 | Leading reactive power : Q3_lead | var | S32
18512 | 0x4850 | 2 | Apparent power : S1 | VA | U32
18514 | 0x4852 | 2 | Apparent power : S2 | VA | U32
18516 | 0x4854 | 2 | Apparent power : S3 | VA | U32
18518 | 0x4856 | 1 | Power factor : PF1 | - / 1000 | S16
18519 | 0x4857 | 1 | Power factor : PF2 | - / 1000 | S16
18520 | 0x4858 | 1 | Power factor : PF3 | - / 1000 | S16
18521 | 0x4859 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
18522 | 0x485A | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
18523 | 0x485B | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Inst. measurement - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20480 | 0x5000 | Info | 92 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20480 | 0x5000 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
20481 | 0x5001 | 2 | Date of last instance | s | DATETIME
20483 | 0x5003 | 1 | Integration time | s / 5 | U16
20484 | 0x5004 | 2 | System Ph-N Voltage | V / 100 | U32
20486 | 0x5006 | 2 | System Ph-Ph Voltage | V / 100 | U32
20488 | 0x5008 | 2 | System Current | A / 1000 | U32
20490 | 0x500A | 2 | Frequency | Hz / 1000 | U32
20492 | 0x500C | 2 | Ph-N Voltage : V1 | V / 100 | U32
20494 | 0x500E | 2 | Ph-N Voltage : V2 | V / 100 | U32
20496 | 0x5010 | 2 | Ph-N Voltage : V3 | V / 100 | U32
20498 | 0x5012 | 2 | Ph-N Voltage : Vn | V / 100 | U32
20500 | 0x5014 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
20502 | 0x5016 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
20504 | 0x5018 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
20506 | 0x501A | 2 | Current : I1 | A / 1000 | U32
20508 | 0x501C | 2 | Current : I2 | A / 1000 | U32
20510 | 0x501E | 2 | Current : I3 | A / 1000 | U32
20512 | 0x5020 | 2 | Current : In | A / 1000 | U32
20514 | 0x5022 | 1 | Inba | % / 100 | U16
20515 | 0x5023 | 2 | Idir | A / 1000 | U32
20517 | 0x5025 | 2 | Iinv | A / 1000 | U32
20519 | 0x5027 | 2 | Ihom | A / 1000 | U32
20521 | 0x5029 | 1 | Inb | % / 100 | U16
20522 | 0x502A | 2 | Snom | VA | U32
20524 | 0x502C | 2 | Total active power | W | S32
20526 | 0x502E | 2 | Total reactive power | var | S32
20528 | 0x5030 | 2 | Total lagging reactive power | var | S32
20530 | 0x5032 | 2 | Total leading reactive power | var | S32
20532 | 0x5034 | 2 | Total apparent power | VA | U32
20534 | 0x5036 | 1 | Total power factor | - / 1000 | S16
20535 | 0x5037 | 1 | Total Power factor type : 0 : undefined 1 : leading 2 : lagging | - | U8
20536 | 0x5038 | 2 | Active power : P1 | W | S32
20538 | 0x503A | 2 | Active power : P2 | W | S32
20540 | 0x503C | 2 | Active power : P3 | W | S32
20542 | 0x503E | 2 | Reactive power : Q1 | var | S32
20544 | 0x5040 | 2 | Reactive power : Q2 | var | S32
20546 | 0x5042 | 2 | Reactive power : Q3 | var | S32
20548 | 0x5044 | 2 | Lagging reactive power : Q1_lagg | var | S32
20550 | 0x5046 | 2 | Lagging reactive power : Q2_lagg | var | S32
20552 | 0x5048 | 2 | Lagging reactive power : Q3_lagg | var | S32
20554 | 0x504A | 2 | Leading reactive power : Q1_lead | var | S32
20556 | 0x504C | 2 | Leading reactive power : Q2_lead | var | S32
20558 | 0x504E | 2 | Leading reactive power : Q3_lead | var | S32
20560 | 0x5050 | 2 | Apparent power : S1 | VA | U32
20562 | 0x5052 | 2 | Apparent power : S2 | VA | U32
20564 | 0x5054 | 2 | Apparent power : S3 | VA | U32
20566 | 0x5056 | 1 | Power factor : PF1 | - / 1000 | S16
20567 | 0x5057 | 1 | Power factor : PF2 | - / 1000 | S16
20568 | 0x5058 | 1 | Power factor : PF3 | - / 1000 | S16
20569 | 0x5059 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
20570 | 0x505A | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
20571 | 0x505B | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Inst. measurement - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22528 | 0x5800 | Info | 92 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22528 | 0x5800 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
22529 | 0x5801 | 2 | Date of last instance | s | DATETIME
22531 | 0x5803 | 1 | Integration time | s / 5 | U16
22532 | 0x5804 | 2 | System Ph-N Voltage | V / 100 | U32
22534 | 0x5806 | 2 | System Ph-Ph Voltage | V / 100 | U32
22536 | 0x5808 | 2 | System Current | A / 1000 | U32
22538 | 0x580A | 2 | Frequency | Hz / 1000 | U32
22540 | 0x580C | 2 | Ph-N Voltage : V1 | V / 100 | U32
22542 | 0x580E | 2 | Ph-N Voltage : V2 | V / 100 | U32
22544 | 0x5810 | 2 | Ph-N Voltage : V3 | V / 100 | U32
22546 | 0x5812 | 2 | Ph-N Voltage : Vn | V / 100 | U32
22548 | 0x5814 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
22550 | 0x5816 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
22552 | 0x5818 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
22554 | 0x581A | 2 | Current : I1 | A / 1000 | U32
22556 | 0x581C | 2 | Current : I2 | A / 1000 | U32
22558 | 0x581E | 2 | Current : I3 | A / 1000 | U32
22560 | 0x5820 | 2 | Current : In | A / 1000 | U32
22562 | 0x5822 | 1 | Inba | % / 100 | U16
22563 | 0x5823 | 2 | Idir | A / 1000 | U32
22565 | 0x5825 | 2 | Iinv | A / 1000 | U32
22567 | 0x5827 | 2 | Ihom | A / 1000 | U32
22569 | 0x5829 | 1 | Inb | % / 100 | U16
22570 | 0x582A | 2 | Snom | VA | U32
22572 | 0x582C | 2 | Total active power | W | S32
22574 | 0x582E | 2 | Total reactive power | var | S32
22576 | 0x5830 | 2 | Total lagging reactive power | var | S32
22578 | 0x5832 | 2 | Total leading reactive power | var | S32
22580 | 0x5834 | 2 | Total apparent power | VA | U32
22582 | 0x5836 | 1 | Total power factor | - / 1000 | S16
22583 | 0x5837 | 1 | Total Power factor type : 0 : undefined 1 : leading 2 : lagging | - | U8
22584 | 0x5838 | 2 | Active power : P1 | W | S32
22586 | 0x583A | 2 | Active power : P2 | W | S32
22588 | 0x583C | 2 | Active power : P3 | W | S32
22590 | 0x583E | 2 | Reactive power : Q1 | var | S32
22592 | 0x5840 | 2 | Reactive power : Q2 | var | S32
22594 | 0x5842 | 2 | Reactive power : Q3 | var | S32
22596 | 0x5844 | 2 | Lagging reactive power : Q1_lagg | var | S32
22598 | 0x5846 | 2 | Lagging reactive power : Q2_lagg | var | S32
22600 | 0x5848 | 2 | Lagging reactive power : Q3_lagg | var | S32
22602 | 0x584A | 2 | Leading reactive power : Q1_lead | var | S32
22604 | 0x584C | 2 | Leading reactive power : Q2_lead | var | S32
22606 | 0x584E | 2 | Leading reactive power : Q3_lead | var | S32
22608 | 0x5850 | 2 | Apparent power : S1 | VA | U32
22610 | 0x5852 | 2 | Apparent power : S2 | VA | U32
22612 | 0x5854 | 2 | Apparent power : S3 | VA | U32
22614 | 0x5856 | 1 | Power factor : PF1 | - / 1000 | S16
22615 | 0x5857 | 1 | Power factor : PF2 | - / 1000 | S16
22616 | 0x5858 | 1 | Power factor : PF3 | - / 1000 | S16
22617 | 0x5859 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
22618 | 0x585A | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
22619 | 0x585B | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Inst. measurement - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24576 | 0x6000 | Info | 92 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24576 | 0x6000 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
24577 | 0x6001 | 2 | Date of last instance | s | DATETIME
24579 | 0x6003 | 1 | Integration time | s / 5 | U16
24580 | 0x6004 | 2 | System Ph-N Voltage | V / 100 | U32
24582 | 0x6006 | 2 | System Ph-Ph Voltage | V / 100 | U32
24584 | 0x6008 | 2 | System Current | A / 1000 | U32
24586 | 0x600A | 2 | Frequency | Hz / 1000 | U32
24588 | 0x600C | 2 | Ph-N Voltage : V1 | V / 100 | U32
24590 | 0x600E | 2 | Ph-N Voltage : V2 | V / 100 | U32
24592 | 0x6010 | 2 | Ph-N Voltage : V3 | V / 100 | U32
24594 | 0x6012 | 2 | Ph-N Voltage : Vn | V / 100 | U32
24596 | 0x6014 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
24598 | 0x6016 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
24600 | 0x6018 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
24602 | 0x601A | 2 | Current : I1 | A / 1000 | U32
24604 | 0x601C | 2 | Current : I2 | A / 1000 | U32
24606 | 0x601E | 2 | Current : I3 | A / 1000 | U32
24608 | 0x6020 | 2 | Current : In | A / 1000 | U32
24610 | 0x6022 | 1 | Inba | % / 100 | U16
24611 | 0x6023 | 2 | Idir | A / 1000 | U32
24613 | 0x6025 | 2 | Iinv | A / 1000 | U32
24615 | 0x6027 | 2 | Ihom | A / 1000 | U32
24617 | 0x6029 | 1 | Inb | % / 100 | U16
24618 | 0x602A | 2 | Snom | VA | U32
24620 | 0x602C | 2 | Total active power | W | S32
24622 | 0x602E | 2 | Total reactive power | var | S32
24624 | 0x6030 | 2 | Total lagging reactive power | var | S32
24626 | 0x6032 | 2 | Total leading reactive power | var | S32
24628 | 0x6034 | 2 | Total apparent power | VA | U32
24630 | 0x6036 | 1 | Total power factor | - / 1000 | S16
24631 | 0x6037 | 1 | Total Power factor type : 0 : undefined 1 : leading 2 : lagging | - | U8
24632 | 0x6038 | 2 | Active power : P1 | W | S32
24634 | 0x603A | 2 | Active power : P2 | W | S32
24636 | 0x603C | 2 | Active power : P3 | W | S32
24638 | 0x603E | 2 | Reactive power : Q1 | var | S32
24640 | 0x6040 | 2 | Reactive power : Q2 | var | S32
24642 | 0x6042 | 2 | Reactive power : Q3 | var | S32
24644 | 0x6044 | 2 | Lagging reactive power : Q1_lagg | var | S32
24646 | 0x6046 | 2 | Lagging reactive power : Q2_lagg | var | S32
24648 | 0x6048 | 2 | Lagging reactive power : Q3_lagg | var | S32
24650 | 0x604A | 2 | Leading reactive power : Q1_lead | var | S32
24652 | 0x604C | 2 | Leading reactive power : Q2_lead | var | S32
24654 | 0x604E | 2 | Leading reactive power : Q3_lead | var | S32
24656 | 0x6050 | 2 | Apparent power : S1 | VA | U32
24658 | 0x6052 | 2 | Apparent power : S2 | VA | U32
24660 | 0x6054 | 2 | Apparent power : S3 | VA | U32
24662 | 0x6056 | 1 | Power factor : PF1 | - / 1000 | S16
24663 | 0x6057 | 1 | Power factor : PF2 | - / 1000 | S16
24664 | 0x6058 | 1 | Power factor : PF3 | - / 1000 | S16
24665 | 0x6059 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
24666 | 0x605A | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
24667 | 0x605B | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Avg. measurement - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
18560 | 0x4880 | Info | 93 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
18560 | 0x4880 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
18561 | 0x4881 | 2 | Date of last instance | s | DATETIME
18563 | 0x4883 | 1 | Integration time | s | U16
18564 | 0x4884 | 2 | System Ph-N Voltage | V / 100 | U32
18566 | 0x4886 | 2 | System Ph-Ph Voltage | V / 100 | U32
18568 | 0x4888 | 2 | System Current | A / 1000 | U32
18570 | 0x488A | 2 | Frequency | Hz / 1000 | U32
18572 | 0x488C | 2 | Ph-N Voltage : V1 | V / 100 | U32
18574 | 0x488E | 2 | Ph-N Voltage : V2 | V / 100 | U32
18576 | 0x4890 | 2 | Ph-N Voltage : V3 | V / 100 | U32
18578 | 0x4892 | 2 | Ph-N Voltage : Vn | V / 100 | U32
18580 | 0x4894 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
18582 | 0x4896 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
18584 | 0x4898 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
18586 | 0x489A | 2 | Current : I1 | A / 1000 | U32
18588 | 0x489C | 2 | Current : I2 | A / 1000 | U32
18590 | 0x489E | 2 | Current : I3 | A / 1000 | U32
18592 | 0x48A0 | 2 | Current : In | A / 1000 | U32
18594 | 0x48A2 | 1 | Inba | % / 100 | U16
18595 | 0x48A3 | 2 | Idir | A / 1000 | U32
18597 | 0x48A5 | 2 | Iinv | A / 1000 | U32
18599 | 0x48A7 | 2 | Ihom | A / 1000 | U32
18601 | 0x48A9 | 1 | Inb | % / 100 | U16
18602 | 0x48AA | 2 | Snom | VA | U32
18604 | 0x48AC | 2 | Total active power | W | S32
18606 | 0x48AE | 2 | Total reactive power | var | S32
18608 | 0x48B0 | 2 | Total lagging reactive power | var | S32
18610 | 0x48B2 | 2 | Total leading reactive power | var | S32
18612 | 0x48B4 | 2 | Total apparent power | VA | U32
18614 | 0x48B6 | 1 | Total power factor | - / 1000 | S16
18615 | 0x48B7 | 1 | Total Power factor type : 0 : undefined 1 : leading 2 : lagging | - | U8
18616 | 0x48B8 | 2 | Active power : P1 | W | S32
18618 | 0x48BA | 2 | Active power : P2 | W | S32
18620 | 0x48BC | 2 | Active power : P3 | W | S32
18622 | 0x48BE | 2 | Reactive power : Q1 | var | S32
18624 | 0x48C0 | 2 | Reactive power : Q2 | var | S32
18626 | 0x48C2 | 2 | Reactive power : Q3 | var | S32
18628 | 0x48C4 | 2 | Lagging reactive power : Q1_lagg | var | S32
18630 | 0x48C6 | 2 | Lagging reactive power : Q2_lagg | var | S32
18632 | 0x48C8 | 2 | Lagging reactive power : Q3_lagg | var | S32
18634 | 0x48CA | 2 | Leading reactive power : Q1_lead | var | S32
18636 | 0x48CC | 2 | Leading reactive power : Q2_lead | var | S32
18638 | 0x48CE | 2 | Leading reactive power : Q3_lead | var | S32
18640 | 0x48D0 | 2 | Apparent power : S1 | VA | U32
18642 | 0x48D2 | 2 | Apparent power : S2 | VA | U32
18644 | 0x48D4 | 2 | Apparent power : S3 | VA | U32
18646 | 0x48D6 | 1 | Power factor : PF1 | - / 1000 | S16
18647 | 0x48D7 | 1 | Power factor : PF2 | - / 1000 | S16
18648 | 0x48D8 | 1 | Power factor : PF3 | - / 1000 | S16
18649 | 0x48D9 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
18650 | 0x48DA | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
18651 | 0x48DB | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Avg. measurement - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20608 | 0x5080 | Info | 93 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20608 | 0x5080 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
20609 | 0x5081 | 2 | Date of last instance | s | DATETIME
20611 | 0x5083 | 1 | Integration time | s | U16
20612 | 0x5084 | 2 | System Ph-N Voltage | V / 100 | U32
20614 | 0x5086 | 2 | System Ph-Ph Voltage | V / 100 | U32
20616 | 0x5088 | 2 | System Current | A / 1000 | U32
20618 | 0x508A | 2 | Frequency | Hz / 1000 | U32
20620 | 0x508C | 2 | Ph-N Voltage : V1 | V / 100 | U32
20622 | 0x508E | 2 | Ph-N Voltage : V2 | V / 100 | U32
20624 | 0x5090 | 2 | Ph-N Voltage : V3 | V / 100 | U32
20626 | 0x5092 | 2 | Ph-N Voltage : Vn | V / 100 | U32
20628 | 0x5094 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
20630 | 0x5096 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
20632 | 0x5098 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
20634 | 0x509A | 2 | Current : I1 | A / 1000 | U32
20636 | 0x509C | 2 | Current : I2 | A / 1000 | U32
20638 | 0x509E | 2 | Current : I3 | A / 1000 | U32
20640 | 0x50A0 | 2 | Current : In | A / 1000 | U32
20642 | 0x50A2 | 1 | Inba | % / 100 | U16
20643 | 0x50A3 | 2 | Idir | A / 1000 | U32
20645 | 0x50A5 | 2 | Iinv | A / 1000 | U32
20647 | 0x50A7 | 2 | Ihom | A / 1000 | U32
20649 | 0x50A9 | 1 | Inb | % / 100 | U16
20650 | 0x50AA | 2 | Snom | VA | U32
20652 | 0x50AC | 2 | Total active power | W | S32
20654 | 0x50AE | 2 | Total reactive power | var | S32
20656 | 0x50B0 | 2 | Total lagging reactive power | var | S32
20658 | 0x50B2 | 2 | Total leading reactive power | var | S32
20660 | 0x50B4 | 2 | Total apparent power | VA | U32
20662 | 0x50B6 | 1 | Total power factor | - / 1000 | S16
20663 | 0x50B7 | 1 | Total Power factor type : 0 : undefined 1 : leading 2 : lagging | - | U8
20664 | 0x50B8 | 2 | Active power : P1 | W | S32
20666 | 0x50BA | 2 | Active power : P2 | W | S32
20668 | 0x50BC | 2 | Active power : P3 | W | S32
20670 | 0x50BE | 2 | Reactive power : Q1 | var | S32
20672 | 0x50C0 | 2 | Reactive power : Q2 | var | S32
20674 | 0x50C2 | 2 | Reactive power : Q3 | var | S32
20676 | 0x50C4 | 2 | Lagging reactive power : Q1_lagg | var | S32
20678 | 0x50C6 | 2 | Lagging reactive power : Q2_lagg | var | S32
20680 | 0x50C8 | 2 | Lagging reactive power : Q3_lagg | var | S32
20682 | 0x50CA | 2 | Leading reactive power : Q1_lead | var | S32
20684 | 0x50CC | 2 | Leading reactive power : Q2_lead | var | S32
20686 | 0x50CE | 2 | Leading reactive power : Q3_lead | var | S32
20688 | 0x50D0 | 2 | Apparent power : S1 | VA | U32
20690 | 0x50D2 | 2 | Apparent power : S2 | VA | U32
20692 | 0x50D4 | 2 | Apparent power : S3 | VA | U32
20694 | 0x50D6 | 1 | Power factor : PF1 | - / 1000 | S16
20695 | 0x50D7 | 1 | Power factor : PF2 | - / 1000 | S16
20696 | 0x50D8 | 1 | Power factor : PF3 | - / 1000 | S16
20697 | 0x50D9 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
20698 | 0x50DA | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
20699 | 0x50DB | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Avg. measurement - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22656 | 0x5880 | Info | 93 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22656 | 0x5880 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
22657 | 0x5881 | 2 | Date of last instance | s | DATETIME
22659 | 0x5883 | 1 | Integration time | s | U16
22660 | 0x5884 | 2 | System Ph-N Voltage | V / 100 | U32
22662 | 0x5886 | 2 | System Ph-Ph Voltage | V / 100 | U32
22664 | 0x5888 | 2 | System Current | A / 1000 | U32
22666 | 0x588A | 2 | Frequency | Hz / 1000 | U32
22668 | 0x588C | 2 | Ph-N Voltage : V1 | V / 100 | U32
22670 | 0x588E | 2 | Ph-N Voltage : V2 | V / 100 | U32
22672 | 0x5890 | 2 | Ph-N Voltage : V3 | V / 100 | U32
22674 | 0x5892 | 2 | Ph-N Voltage : Vn | V / 100 | U32
22676 | 0x5894 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
22678 | 0x5896 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
22680 | 0x5898 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
22682 | 0x589A | 2 | Current : I1 | A / 1000 | U32
22684 | 0x589C | 2 | Current : I2 | A / 1000 | U32
22686 | 0x589E | 2 | Current : I3 | A / 1000 | U32
22688 | 0x58A0 | 2 | Current : In | A / 1000 | U32
22690 | 0x58A2 | 1 | Inba | % / 100 | U16
22691 | 0x58A3 | 2 | Idir | A / 1000 | U32
22693 | 0x58A5 | 2 | Iinv | A / 1000 | U32
22695 | 0x58A7 | 2 | Ihom | A / 1000 | U32
22697 | 0x58A9 | 1 | Inb | % / 100 | U16
22698 | 0x58AA | 2 | Snom | VA | U32
22700 | 0x58AC | 2 | Total active power | W | S32
22702 | 0x58AE | 2 | Total reactive power | var | S32
22704 | 0x58B0 | 2 | Total lagging reactive power | var | S32
22706 | 0x58B2 | 2 | Total leading reactive power | var | S32
22708 | 0x58B4 | 2 | Total apparent power | VA | U32
22710 | 0x58B6 | 1 | Total power factor | - / 1000 | S16
22711 | 0x58B7 | 1 | Total Power factor type : 0 : undefined 1 : leading 2 : lagging | - | U8
22712 | 0x58B8 | 2 | Active power : P1 | W | S32
22714 | 0x58BA | 2 | Active power : P2 | W | S32
22716 | 0x58BC | 2 | Active power : P3 | W | S32
22718 | 0x58BE | 2 | Reactive power : Q1 | var | S32
22720 | 0x58C0 | 2 | Reactive power : Q2 | var | S32
22722 | 0x58C2 | 2 | Reactive power : Q3 | var | S32
22724 | 0x58C4 | 2 | Lagging reactive power : Q1_lagg | var | S32
22726 | 0x58C6 | 2 | Lagging reactive power : Q2_lagg | var | S32
22728 | 0x58C8 | 2 | Lagging reactive power : Q3_lagg | var | S32
22730 | 0x58CA | 2 | Leading reactive power : Q1_lead | var | S32
22732 | 0x58CC | 2 | Leading reactive power : Q2_lead | var | S32
22734 | 0x58CE | 2 | Leading reactive power : Q3_lead | var | S32
22736 | 0x58D0 | 2 | Apparent power : S1 | VA | U32
22738 | 0x58D2 | 2 | Apparent power : S2 | VA | U32
22740 | 0x58D4 | 2 | Apparent power : S3 | VA | U32
22742 | 0x58D6 | 1 | Power factor : PF1 | - / 1000 | S16
22743 | 0x58D7 | 1 | Power factor : PF2 | - / 1000 | S16
22744 | 0x58D8 | 1 | Power factor : PF3 | - / 1000 | S16
22745 | 0x58D9 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
22746 | 0x58DA | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
22747 | 0x58DB | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Avg. measurement - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24704 | 0x6080 | Info | 93 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24704 | 0x6080 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
24705 | 0x6081 | 2 | Date of last instance | s | DATETIME
24707 | 0x6083 | 1 | Integration time | s | U16
24708 | 0x6084 | 2 | System Ph-N Voltage | V / 100 | U32
24710 | 0x6086 | 2 | System Ph-Ph Voltage | V / 100 | U32
24712 | 0x6088 | 2 | System Current | A / 1000 | U32
24714 | 0x608A | 2 | Frequency | Hz / 1000 | U32
24716 | 0x608C | 2 | Ph-N Voltage : V1 | V / 100 | U32
24718 | 0x608E | 2 | Ph-N Voltage : V2 | V / 100 | U32
24720 | 0x6090 | 2 | Ph-N Voltage : V3 | V / 100 | U32
24722 | 0x6092 | 2 | Ph-N Voltage : Vn | V / 100 | U32
24724 | 0x6094 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
24726 | 0x6096 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
24728 | 0x6098 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
24730 | 0x609A | 2 | Current : I1 | A / 1000 | U32
24732 | 0x609C | 2 | Current : I2 | A / 1000 | U32
24734 | 0x609E | 2 | Current : I3 | A / 1000 | U32
24736 | 0x60A0 | 2 | Current : In | A / 1000 | U32
24738 | 0x60A2 | 1 | Inba | % / 100 | U16
24739 | 0x60A3 | 2 | Idir | A / 1000 | U32
24741 | 0x60A5 | 2 | Iinv | A / 1000 | U32
24743 | 0x60A7 | 2 | Ihom | A / 1000 | U32
24745 | 0x60A9 | 1 | Inb | % / 100 | U16
24746 | 0x60AA | 2 | Snom | VA | U32
24748 | 0x60AC | 2 | Total active power | W | S32
24750 | 0x60AE | 2 | Total reactive power | var | S32
24752 | 0x60B0 | 2 | Total lagging reactive power | var | S32
24754 | 0x60B2 | 2 | Total leading reactive power | var | S32
24756 | 0x60B4 | 2 | Total apparent power | VA | U32
24758 | 0x60B6 | 1 | Total power factor | - / 1000 | S16
24759 | 0x60B7 | 1 | Total Power factor type : 0 : undefined 1 : leading 2 : lagging | - | U8
24760 | 0x60B8 | 2 | Active power : P1 | W | S32
24762 | 0x60BA | 2 | Active power : P2 | W | S32
24764 | 0x60BC | 2 | Active power : P3 | W | S32
24766 | 0x60BE | 2 | Reactive power : Q1 | var | S32
24768 | 0x60C0 | 2 | Reactive power : Q2 | var | S32
24770 | 0x60C2 | 2 | Reactive power : Q3 | var | S32
24772 | 0x60C4 | 2 | Lagging reactive power : Q1_lagg | var | S32
24774 | 0x60C6 | 2 | Lagging reactive power : Q2_lagg | var | S32
24776 | 0x60C8 | 2 | Lagging reactive power : Q3_lagg | var | S32
24778 | 0x60CA | 2 | Leading reactive power : Q1_lead | var | S32
24780 | 0x60CC | 2 | Leading reactive power : Q2_lead | var | S32
24782 | 0x60CE | 2 | Leading reactive power : Q3_lead | var | S32
24784 | 0x60D0 | 2 | Apparent power : S1 | VA | U32
24786 | 0x60D2 | 2 | Apparent power : S2 | VA | U32
24788 | 0x60D4 | 2 | Apparent power : S3 | VA | U32
24790 | 0x60D6 | 1 | Power factor : PF1 | - / 1000 | S16
24791 | 0x60D7 | 1 | Power factor : PF2 | - / 1000 | S16
24792 | 0x60D8 | 1 | Power factor : PF3 | - / 1000 | S16
24793 | 0x60D9 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
24794 | 0x60DA | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
24795 | 0x60DB | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Inst. fundamental measurement - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
18688 | 0x4900 | Info | 84 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
18688 | 0x4900 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
18689 | 0x4901 | 2 | Date of last instance | s | DATETIME
18691 | 0x4903 | 1 | Integration time | s / 5 | U16
18692 | 0x4904 | 2 | Ph-N voltage: V1h1 | V / 100 | U32
18694 | 0x4906 | 2 | Ph-N voltage: V2h1 | V / 100 | U32
18696 | 0x4908 | 2 | Ph-N voltage: V3h1 | V / 100 | U32
18698 | 0x490A | 2 | Ph-N voltage: Vnh1 | V / 100 | U32
18700 | 0x490C | 1 | Ph-N voltage phase: phV1h1 | ? / 10 | S16
18701 | 0x490D | 1 | Ph-N voltage phase: phV2h1 | ? / 10 | S16
18702 | 0x490E | 1 | Ph-N voltage phase: phV3h1 | ? / 10 | S16
18703 | 0x490F | 1 | Ph-N voltage phase: phVnh1 | ? / 10 | S16
18704 | 0x4910 | 2 | Ph-Ph voltage: U12h1 | V / 100 | U32
18706 | 0x4912 | 2 | Ph-Ph voltage: U23h1 | V / 100 | U32
18708 | 0x4914 | 2 | Ph-Ph voltage: U31h1 | V / 100 | U32
18710 | 0x4916 | 1 | Ph-Ph voltage phase: phU12h1 | ? / 10 | S16
18711 | 0x4917 | 1 | Ph-Ph voltage phase: phU23h1 | ? / 10 | S16
18712 | 0x4918 | 1 | Ph-Ph voltage phase: phU31h1 | ? / 10 | S16
18713 | 0x4919 | 2 | Current: I1h1 | A / 1000 | U32
18715 | 0x491B | 2 | Current: I2h1 | A / 1000 | U32
18717 | 0x491D | 2 | Current: I3h1 | A / 1000 | U32
18719 | 0x491F | 2 | Current: Inh1 | A / 1000 | U32
18721 | 0x4921 | 1 | Current phase: phI1h1 | ? / 10 | S16
18722 | 0x4922 | 1 | Current phase: phI2h1 | ? / 10 | S16
18723 | 0x4923 | 1 | Current phase: phI3h1 | ? / 10 | S16
18724 | 0x4924 | 1 | Current phase: phInh1 | ? / 10 | S16
18725 | 0x4925 | 1 | phi current voltage: phiI1h1V1h1 | ? / 10 | S16
18726 | 0x4926 | 1 | phi current voltage: phiI2h1V2h1 | ? / 10 | S16
18727 | 0x4927 | 1 | phi current voltage: phiI3h1V3h1 | ? / 10 | S16
18728 | 0x4928 | 1 | phi current voltage: phiInh1Vnh1 | ? / 10 | S16
18729 | 0x4929 | 2 | P1h1 | W | S32
18731 | 0x492B | 2 | P2h1 | W | S32
18733 | 0x492D | 2 | P3h1 | W | S32
18735 | 0x492F | 2 | Ptoth1 | W / 0.1 | S32
18737 | 0x4931 | 2 | Q1h1 | var | S32
18739 | 0x4933 | 2 | Q2h1 | var | S32
18741 | 0x4935 | 2 | Q3h1 | var | S32
18743 | 0x4937 | 2 | Qtoth1 | var / 0.1 | S32
18745 | 0x4939 | 1 | Cos(phi) : phiI1h1V1h1 | - / 1000 | S16
18746 | 0x493A | 1 | Cos(phi) : phiI2h1V2h1 | - / 1000 | S16
18747 | 0x493B | 1 | Cos(phi) : phiI3h1V3h1 | - / 1000 | S16
18748 | 0x493C | 1 | Tan(phi) : phiI1h1V1h1 | - / 1000 | S16
18749 | 0x493D | 1 | Tan(phi) : phiI2h1V2h1 | - / 1000 | S16
18750 | 0x493E | 1 | Tan(phi) : phiI3h1V3h1 | - / 1000 | S16
18751 | 0x493F | 1 | Ph-N Voltage total harmonic distortion : THD V1 | % / 100 | U16
18752 | 0x4940 | 1 | Ph-N Voltage total harmonic distortion : THD V2 | % / 100 | U16
18753 | 0x4941 | 1 | Ph-N Voltage total harmonic distortion : THD V3 | % / 100 | U16
18754 | 0x4942 | 1 | Ph-Ph Voltage total harmonic distortion : THD U12 | % / 100 | U16
18755 | 0x4943 | 1 | Ph-Ph Voltage total harmonic distortion : THD U23 | % / 100 | U16
18756 | 0x4944 | 1 | Ph-Ph Voltage total harmonic distortion : THD U31 | % / 100 | U16
18757 | 0x4945 | 1 | Current total harmonic distortion : THD I1 | % / 100 | U16
18758 | 0x4946 | 1 | Current total harmonic distortion : THD I2 | % / 100 | U16
18759 | 0x4947 | 1 | Current total harmonic distortion : THD I3 | % / 100 | U16
18760 | 0x4948 | 1 | Current total harmonic distortion : THD In | % / 100 | U16
18761 | 0x4949 | 1 | K-Factor I1 | - / 100 | U16
18762 | 0x494A | 1 | K-Factor I2 | - / 100 | U16
18763 | 0x494B | 1 | K-Factor I3 | - / 100 | U16
18764 | 0x494C | 1 | K-Factor In | - / 100 | U16
18765 | 0x494D | 1 | System THD V | % / 100 | U16
18766 | 0x494E | 1 | System THD U | % / 100 | U16
18767 | 0x494F | 1 | System THD I | % / 100 | U16
18768 | 0x4950 | 1 | Crest factor : I1 | - / 1000 | U16
18769 | 0x4951 | 1 | Crest factor : I2 | - / 1000 | U16
18770 | 0x4952 | 1 | Crest factor : I3 | - / 1000 | U16
18771 | 0x4953 | 1 | Crest factor : In | - / 1000 | U16

## Inst. fundamental measurement - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20736 | 0x5100 | Info | 84 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20736 | 0x5100 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
20737 | 0x5101 | 2 | Date of last instance | s | DATETIME
20739 | 0x5103 | 1 | Integration time | s / 5 | U16
20740 | 0x5104 | 2 | Ph-N voltage: V1h1 | V / 100 | U32
20742 | 0x5106 | 2 | Ph-N voltage: V2h1 | V / 100 | U32
20744 | 0x5108 | 2 | Ph-N voltage: V3h1 | V / 100 | U32
20746 | 0x510A | 2 | Ph-N voltage: Vnh1 | V / 100 | U32
20748 | 0x510C | 1 | Ph-N voltage phase: phV1h1 | ? / 10 | S16
20749 | 0x510D | 1 | Ph-N voltage phase: phV2h1 | ? / 10 | S16
20750 | 0x510E | 1 | Ph-N voltage phase: phV3h1 | ? / 10 | S16
20751 | 0x510F | 1 | Ph-N voltage phase: phVnh1 | ? / 10 | S16
20752 | 0x5110 | 2 | Ph-Ph voltage: U12h1 | V / 100 | U32
20754 | 0x5112 | 2 | Ph-Ph voltage: U23h1 | V / 100 | U32
20756 | 0x5114 | 2 | Ph-Ph voltage: U31h1 | V / 100 | U32
20758 | 0x5116 | 1 | Ph-Ph voltage phase: phU12h1 | ? / 10 | S16
20759 | 0x5117 | 1 | Ph-Ph voltage phase: phU23h1 | ? / 10 | S16
20760 | 0x5118 | 1 | Ph-Ph voltage phase: phU31h1 | ? / 10 | S16
20761 | 0x5119 | 2 | Current: I1h1 | A / 1000 | U32
20763 | 0x511B | 2 | Current: I2h1 | A / 1000 | U32
20765 | 0x511D | 2 | Current: I3h1 | A / 1000 | U32
20767 | 0x511F | 2 | Current: Inh1 | A / 1000 | U32
20769 | 0x5121 | 1 | Current phase: phI1h1 | ? / 10 | S16
20770 | 0x5122 | 1 | Current phase: phI2h1 | ? / 10 | S16
20771 | 0x5123 | 1 | Current phase: phI3h1 | ? / 10 | S16
20772 | 0x5124 | 1 | Current phase: phInh1 | ? / 10 | S16
20773 | 0x5125 | 1 | phi current voltage: phiI1h1V1h1 | ? / 10 | S16
20774 | 0x5126 | 1 | phi current voltage: phiI2h1V2h1 | ? / 10 | S16
20775 | 0x5127 | 1 | phi current voltage: phiI3h1V3h1 | ? / 10 | S16
20776 | 0x5128 | 1 | phi current voltage: phiInh1Vnh1 | ? / 10 | S16
20777 | 0x5129 | 2 | P1h1 | W | S32
20779 | 0x512B | 2 | P2h1 | W | S32
20781 | 0x512D | 2 | P3h1 | W | S32
20783 | 0x512F | 2 | Ptoth1 | W / 0.1 | S32
20785 | 0x5131 | 2 | Q1h1 | var | S32
20787 | 0x5133 | 2 | Q2h1 | var | S32
20789 | 0x5135 | 2 | Q3h1 | var | S32
20791 | 0x5137 | 2 | Qtoth1 | var / 0.1 | S32
20793 | 0x5139 | 1 | Cos(phi) : phiI1h1V1h1 | - / 1000 | S16
20794 | 0x513A | 1 | Cos(phi) : phiI2h1V2h1 | - / 1000 | S16
20795 | 0x513B | 1 | Cos(phi) : phiI3h1V3h1 | - / 1000 | S16
20796 | 0x513C | 1 | Tan(phi) : phiI1h1V1h1 | - / 1000 | S16
20797 | 0x513D | 1 | Tan(phi) : phiI2h1V2h1 | - / 1000 | S16
20798 | 0x513E | 1 | Tan(phi) : phiI3h1V3h1 | - / 1000 | S16
20799 | 0x513F | 1 | Ph-N Voltage total harmonic distortion : THD V1 | % / 100 | U16
20800 | 0x5140 | 1 | Ph-N Voltage total harmonic distortion : THD V2 | % / 100 | U16
20801 | 0x5141 | 1 | Ph-N Voltage total harmonic distortion : THD V3 | % / 100 | U16
20802 | 0x5142 | 1 | Ph-Ph Voltage total harmonic distortion : THD U12 | % / 100 | U16
20803 | 0x5143 | 1 | Ph-Ph Voltage total harmonic distortion : THD U23 | % / 100 | U16
20804 | 0x5144 | 1 | Ph-Ph Voltage total harmonic distortion : THD U31 | % / 100 | U16
20805 | 0x5145 | 1 | Current total harmonic distortion : THD I1 | % / 100 | U16
20806 | 0x5146 | 1 | Current total harmonic distortion : THD I2 | % / 100 | U16
20807 | 0x5147 | 1 | Current total harmonic distortion : THD I3 | % / 100 | U16
20808 | 0x5148 | 1 | Current total harmonic distortion : THD In | % / 100 | U16
20809 | 0x5149 | 1 | K-Factor I1 | - / 100 | U16
20810 | 0x514A | 1 | K-Factor I2 | - / 100 | U16
20811 | 0x514B | 1 | K-Factor I3 | - / 100 | U16
20812 | 0x514C | 1 | K-Factor In | - / 100 | U16
20813 | 0x514D | 1 | System THD V | % / 100 | U16
20814 | 0x514E | 1 | System THD U | % / 100 | U16
20815 | 0x514F | 1 | System THD I | % / 100 | U16
20816 | 0x5150 | 1 | Crest factor : I1 | - / 1000 | U16
20817 | 0x5151 | 1 | Crest factor : I2 | - / 1000 | U16
20818 | 0x5152 | 1 | Crest factor : I3 | - / 1000 | U16
20819 | 0x5153 | 1 | Crest factor : In | - / 1000 | U16

## Inst. fundamental measurement - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22784 | 0x5900 | Info | 84 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22784 | 0x5900 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
22785 | 0x5901 | 2 | Date of last instance | s | DATETIME
22787 | 0x5903 | 1 | Integration time | s / 5 | U16
22788 | 0x5904 | 2 | Ph-N voltage: V1h1 | V / 100 | U32
22790 | 0x5906 | 2 | Ph-N voltage: V2h1 | V / 100 | U32
22792 | 0x5908 | 2 | Ph-N voltage: V3h1 | V / 100 | U32
22794 | 0x590A | 2 | Ph-N voltage: Vnh1 | V / 100 | U32
22796 | 0x590C | 1 | Ph-N voltage phase: phV1h1 | ? / 10 | S16
22797 | 0x590D | 1 | Ph-N voltage phase: phV2h1 | ? / 10 | S16
22798 | 0x590E | 1 | Ph-N voltage phase: phV3h1 | ? / 10 | S16
22799 | 0x590F | 1 | Ph-N voltage phase: phVnh1 | ? / 10 | S16
22800 | 0x5910 | 2 | Ph-Ph voltage: U12h1 | V / 100 | U32
22802 | 0x5912 | 2 | Ph-Ph voltage: U23h1 | V / 100 | U32
22804 | 0x5914 | 2 | Ph-Ph voltage: U31h1 | V / 100 | U32
22806 | 0x5916 | 1 | Ph-Ph voltage phase: phU12h1 | ? / 10 | S16
22807 | 0x5917 | 1 | Ph-Ph voltage phase: phU23h1 | ? / 10 | S16
22808 | 0x5918 | 1 | Ph-Ph voltage phase: phU31h1 | ? / 10 | S16
22809 | 0x5919 | 2 | Current: I1h1 | A / 1000 | U32
22811 | 0x591B | 2 | Current: I2h1 | A / 1000 | U32
22813 | 0x591D | 2 | Current: I3h1 | A / 1000 | U32
22815 | 0x591F | 2 | Current: Inh1 | A / 1000 | U32
22817 | 0x5921 | 1 | Current phase: phI1h1 | ? / 10 | S16
22818 | 0x5922 | 1 | Current phase: phI2h1 | ? / 10 | S16
22819 | 0x5923 | 1 | Current phase: phI3h1 | ? / 10 | S16
22820 | 0x5924 | 1 | Current phase: phInh1 | ? / 10 | S16
22821 | 0x5925 | 1 | phi current voltage: phiI1h1V1h1 | ? / 10 | S16
22822 | 0x5926 | 1 | phi current voltage: phiI2h1V2h1 | ? / 10 | S16
22823 | 0x5927 | 1 | phi current voltage: phiI3h1V3h1 | ? / 10 | S16
22824 | 0x5928 | 1 | phi current voltage: phiInh1Vnh1 | ? / 10 | S16
22825 | 0x5929 | 2 | P1h1 | W | S32
22827 | 0x592B | 2 | P2h1 | W | S32
22829 | 0x592D | 2 | P3h1 | W | S32
22831 | 0x592F | 2 | Ptoth1 | W / 0.1 | S32
22833 | 0x5931 | 2 | Q1h1 | var | S32
22835 | 0x5933 | 2 | Q2h1 | var | S32
22837 | 0x5935 | 2 | Q3h1 | var | S32
22839 | 0x5937 | 2 | Qtoth1 | var / 0.1 | S32
22841 | 0x5939 | 1 | Cos(phi) : phiI1h1V1h1 | - / 1000 | S16
22842 | 0x593A | 1 | Cos(phi) : phiI2h1V2h1 | - / 1000 | S16
22843 | 0x593B | 1 | Cos(phi) : phiI3h1V3h1 | - / 1000 | S16
22844 | 0x593C | 1 | Tan(phi) : phiI1h1V1h1 | - / 1000 | S16
22845 | 0x593D | 1 | Tan(phi) : phiI2h1V2h1 | - / 1000 | S16
22846 | 0x593E | 1 | Tan(phi) : phiI3h1V3h1 | - / 1000 | S16
22847 | 0x593F | 1 | Ph-N Voltage total harmonic distortion : THD V1 | % / 100 | U16
22848 | 0x5940 | 1 | Ph-N Voltage total harmonic distortion : THD V2 | % / 100 | U16
22849 | 0x5941 | 1 | Ph-N Voltage total harmonic distortion : THD V3 | % / 100 | U16
22850 | 0x5942 | 1 | Ph-Ph Voltage total harmonic distortion : THD U12 | % / 100 | U16
22851 | 0x5943 | 1 | Ph-Ph Voltage total harmonic distortion : THD U23 | % / 100 | U16
22852 | 0x5944 | 1 | Ph-Ph Voltage total harmonic distortion : THD U31 | % / 100 | U16
22853 | 0x5945 | 1 | Current total harmonic distortion : THD I1 | % / 100 | U16
22854 | 0x5946 | 1 | Current total harmonic distortion : THD I2 | % / 100 | U16
22855 | 0x5947 | 1 | Current total harmonic distortion : THD I3 | % / 100 | U16
22856 | 0x5948 | 1 | Current total harmonic distortion : THD In | % / 100 | U16
22857 | 0x5949 | 1 | K-Factor I1 | - / 100 | U16
22858 | 0x594A | 1 | K-Factor I2 | - / 100 | U16
22859 | 0x594B | 1 | K-Factor I3 | - / 100 | U16
22860 | 0x594C | 1 | K-Factor In | - / 100 | U16
22861 | 0x594D | 1 | System THD V | % / 100 | U16
22862 | 0x594E | 1 | System THD U | % / 100 | U16
22863 | 0x594F | 1 | System THD I | % / 100 | U16
22864 | 0x5950 | 1 | Crest factor : I1 | - / 1000 | U16
22865 | 0x5951 | 1 | Crest factor : I2 | - / 1000 | U16
22866 | 0x5952 | 1 | Crest factor : I3 | - / 1000 | U16
22867 | 0x5953 | 1 | Crest factor : In | - / 1000 | U16

## Inst. fundamental measurement - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24832 | 0x6100 | Info | 84 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24832 | 0x6100 | 1 | Load status 0 : Disabled 1 : Enabled | - | U8
24833 | 0x6101 | 2 | Date of last instance | s | DATETIME
24835 | 0x6103 | 1 | Integration time | s / 5 | U16
24836 | 0x6104 | 2 | Ph-N voltage: V1h1 | V / 100 | U32
24838 | 0x6106 | 2 | Ph-N voltage: V2h1 | V / 100 | U32
24840 | 0x6108 | 2 | Ph-N voltage: V3h1 | V / 100 | U32
24842 | 0x610A | 2 | Ph-N voltage: Vnh1 | V / 100 | U32
24844 | 0x610C | 1 | Ph-N voltage phase: phV1h1 | ? / 10 | S16
24845 | 0x610D | 1 | Ph-N voltage phase: phV2h1 | ? / 10 | S16
24846 | 0x610E | 1 | Ph-N voltage phase: phV3h1 | ? / 10 | S16
24847 | 0x610F | 1 | Ph-N voltage phase: phVnh1 | ? / 10 | S16
24848 | 0x6110 | 2 | Ph-Ph voltage: U12h1 | V / 100 | U32
24850 | 0x6112 | 2 | Ph-Ph voltage: U23h1 | V / 100 | U32
24852 | 0x6114 | 2 | Ph-Ph voltage: U31h1 | V / 100 | U32
24854 | 0x6116 | 1 | Ph-Ph voltage phase: phU12h1 | ? / 10 | S16
24855 | 0x6117 | 1 | Ph-Ph voltage phase: phU23h1 | ? / 10 | S16
24856 | 0x6118 | 1 | Ph-Ph voltage phase: phU31h1 | ? / 10 | S16
24857 | 0x6119 | 2 | Current: I1h1 | A / 1000 | U32
24859 | 0x611B | 2 | Current: I2h1 | A / 1000 | U32
24861 | 0x611D | 2 | Current: I3h1 | A / 1000 | U32
24863 | 0x611F | 2 | Current: Inh1 | A / 1000 | U32
24865 | 0x6121 | 1 | Current phase: phI1h1 | ? / 10 | S16
24866 | 0x6122 | 1 | Current phase: phI2h1 | ? / 10 | S16
24867 | 0x6123 | 1 | Current phase: phI3h1 | ? / 10 | S16
24868 | 0x6124 | 1 | Current phase: phInh1 | ? / 10 | S16
24869 | 0x6125 | 1 | phi current voltage: phiI1h1V1h1 | ? / 10 | S16
24870 | 0x6126 | 1 | phi current voltage: phiI2h1V2h1 | ? / 10 | S16
24871 | 0x6127 | 1 | phi current voltage: phiI3h1V3h1 | ? / 10 | S16
24872 | 0x6128 | 1 | phi current voltage: phiInh1Vnh1 | ? / 10 | S16
24873 | 0x6129 | 2 | P1h1 | W | S32
24875 | 0x612B | 2 | P2h1 | W | S32
24877 | 0x612D | 2 | P3h1 | W | S32
24879 | 0x612F | 2 | Ptoth1 | W / 0.1 | S32
24881 | 0x6131 | 2 | Q1h1 | var | S32
24883 | 0x6133 | 2 | Q2h1 | var | S32
24885 | 0x6135 | 2 | Q3h1 | var | S32
24887 | 0x6137 | 2 | Qtoth1 | var / 0.1 | S32
24889 | 0x6139 | 1 | Cos(phi) : phiI1h1V1h1 | - / 1000 | S16
24890 | 0x613A | 1 | Cos(phi) : phiI2h1V2h1 | - / 1000 | S16
24891 | 0x613B | 1 | Cos(phi) : phiI3h1V3h1 | - / 1000 | S16
24892 | 0x613C | 1 | Tan(phi) : phiI1h1V1h1 | - / 1000 | S16
24893 | 0x613D | 1 | Tan(phi) : phiI2h1V2h1 | - / 1000 | S16
24894 | 0x613E | 1 | Tan(phi) : phiI3h1V3h1 | - / 1000 | S16
24895 | 0x613F | 1 | Ph-N Voltage total harmonic distortion : THD V1 | % / 100 | U16
24896 | 0x6140 | 1 | Ph-N Voltage total harmonic distortion : THD V2 | % / 100 | U16
24897 | 0x6141 | 1 | Ph-N Voltage total harmonic distortion : THD V3 | % / 100 | U16
24898 | 0x6142 | 1 | Ph-Ph Voltage total harmonic distortion : THD U12 | % / 100 | U16
24899 | 0x6143 | 1 | Ph-Ph Voltage total harmonic distortion : THD U23 | % / 100 | U16
24900 | 0x6144 | 1 | Ph-Ph Voltage total harmonic distortion : THD U31 | % / 100 | U16
24901 | 0x6145 | 1 | Current total harmonic distortion : THD I1 | % / 100 | U16
24902 | 0x6146 | 1 | Current total harmonic distortion : THD I2 | % / 100 | U16
24903 | 0x6147 | 1 | Current total harmonic distortion : THD I3 | % / 100 | U16
24904 | 0x6148 | 1 | Current total harmonic distortion : THD In | % / 100 | U16
24905 | 0x6149 | 1 | K-Factor I1 | - / 100 | U16
24906 | 0x614A | 1 | K-Factor I2 | - / 100 | U16
24907 | 0x614B | 1 | K-Factor I3 | - / 100 | U16
24908 | 0x614C | 1 | K-Factor In | - / 100 | U16
24909 | 0x614D | 1 | System THD V | % / 100 | U16
24910 | 0x614E | 1 | System THD U | % / 100 | U16
24911 | 0x614F | 1 | System THD I | % / 100 | U16
24912 | 0x6150 | 1 | Crest factor : I1 | - / 1000 | U16
24913 | 0x6151 | 1 | Crest factor : I2 | - / 1000 | U16
24914 | 0x6152 | 1 | Crest factor : I3 | - / 1000 | U16
24915 | 0x6153 | 1 | Crest factor : In | - / 1000 | U16

## Inst. measurement max - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
18816 | 0x4980 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
18816 | 0x4980 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
18817 | 0x4981 | 2 | Maximum Frequency | Hz / 1000 | U32
18819 | 0x4983 | 2 | Date of maximum F | - | DATETIME
18821 | 0x4985 | 2 | Maximum Ph-N Voltage : V1 | V / 100 | U32
18823 | 0x4987 | 2 | Date of maximum V1 | - | DATETIME
18825 | 0x4989 | 2 | Maximum Ph-N Voltage : V2 | V / 100 | U32
18827 | 0x498B | 2 | Date of maximum V2 | - | DATETIME
18829 | 0x498D | 2 | Maximum Ph-N Voltage : V3 | V / 100 | U32
18831 | 0x498F | 2 | Date of maximum V3 | - | DATETIME
18833 | 0x4991 | 2 | Maximum Ph-N Voltage : Vn | V / 100 | U32
18835 | 0x4993 | 2 | Date of maximum Vn | - | DATETIME
18837 | 0x4995 | 2 | Maximum Ph-Ph Voltage : U12 | V / 100 | U32
18839 | 0x4997 | 2 | Date of maximum U12 | - | DATETIME
18841 | 0x4999 | 2 | Maximum Ph-Ph Voltage : U23 | V / 100 | U32
18843 | 0x499B | 2 | Date of maximum U23 | - | DATETIME
18845 | 0x499D | 2 | Maximum Ph-Ph Voltage : U31 | V / 100 | U32
18847 | 0x499F | 2 | Date of maximum U31 | - | DATETIME
18849 | 0x49A1 | 2 | Maximum Current : I1 | A / 1000 | U32
18851 | 0x49A3 | 2 | Date of maximum I1 | - | DATETIME
18853 | 0x49A5 | 2 | Maximum Current : I2 | A / 1000 | U32
18855 | 0x49A7 | 2 | Date of maximum I2 | - | DATETIME
18857 | 0x49A9 | 2 | Maximum Current : I3 | A / 1000 | U32
18859 | 0x49AB | 2 | Date of maximum I3 | - | DATETIME
18861 | 0x49AD | 2 | Maximum Current : In | A / 1000 | U32
18863 | 0x49AF | 2 | Date of maximum In | - | DATETIME
18865 | 0x49B1 | 2 | Maximum Total active power | W | S32
18867 | 0x49B3 | 2 | Date of maximum Ptot | - | DATETIME
18869 | 0x49B5 | 2 | Maximum Total reactive power | var | S32
18871 | 0x49B7 | 2 | Date of maximum Qtot | - | DATETIME
18873 | 0x49B9 | 2 | Maximum Total apparent power | VA | U32
18875 | 0x49BB | 2 | Date of maximum Stot | - | DATETIME
18877 | 0x49BD | 1 | Maximum Total power factor | - / 1000 | S16
18878 | 0x49BE | 1 | Maximum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
18879 | 0x49BF | 2 | Date of maximum Total power factor | - | DATETIME
18881 | 0x49C1 | 2 | Maximum Active power : P1 | W | S32
18883 | 0x49C3 | 2 | Date of maximum P1 | - | DATETIME
18885 | 0x49C5 | 2 | Maximum Active power : P2 | W | S32
18887 | 0x49C7 | 2 | Date of maximum P2 | - | DATETIME
18889 | 0x49C9 | 2 | Maximum Active power : P3 | W | S32
18891 | 0x49CB | 2 | Date of maximum P3 | - | DATETIME
18893 | 0x49CD | 2 | Maximum Reactive power : Q1 | var | S32
18895 | 0x49CF | 2 | Date of maximum Q1 | - | DATETIME
18897 | 0x49D1 | 2 | Maximum Reactive power : Q2 | var | S32
18899 | 0x49D3 | 2 | Date of maximum Q2 | - | DATETIME
18901 | 0x49D5 | 2 | Maximum Reactive power : Q3 | var | S32
18903 | 0x49D7 | 2 | Date of maximum Q3 | - | DATETIME
18905 | 0x49D9 | 2 | Maximum Apparent power : S1 | VA | U32
18907 | 0x49DB | 2 | Date of maximum S1 | - | DATETIME
18909 | 0x49DD | 2 | Maximum Apparent power : S2 | VA | U32
18911 | 0x49DF | 2 | Date of maximum S2 | - | DATETIME
18913 | 0x49E1 | 2 | Maximum Apparent power : S3 | VA | U32
18915 | 0x49E3 | 2 | Date of maximum S3 | - | DATETIME
18917 | 0x49E5 | 1 | Maximum Power factor : PF1 | - / 1000 | S16
18918 | 0x49E6 | 1 | Maximum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
18919 | 0x49E7 | 2 | Date of maximum PF1 | - | DATETIME
18921 | 0x49E9 | 1 | Maximum Power factor : PF2 | - / 1000 | S16
18922 | 0x49EA | 1 | Maximum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
18923 | 0x49EB | 2 | Date of maximum PF2 | - | DATETIME
18925 | 0x49ED | 1 | Maximum Power factor : PF3 | - / 1000 | S16
18926 | 0x49EE | 1 | Maximum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
18927 | 0x49EF | 2 | Date of maximum PF3 | - | DATETIME

## Inst. measurement max - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20864 | 0x5180 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20864 | 0x5180 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
20865 | 0x5181 | 2 | Maximum Frequency | Hz / 1000 | U32
20867 | 0x5183 | 2 | Date of maximum F | - | DATETIME
20869 | 0x5185 | 2 | Maximum Ph-N Voltage : V1 | V / 100 | U32
20871 | 0x5187 | 2 | Date of maximum V1 | - | DATETIME
20873 | 0x5189 | 2 | Maximum Ph-N Voltage : V2 | V / 100 | U32
20875 | 0x518B | 2 | Date of maximum V2 | - | DATETIME
20877 | 0x518D | 2 | Maximum Ph-N Voltage : V3 | V / 100 | U32
20879 | 0x518F | 2 | Date of maximum V3 | - | DATETIME
20881 | 0x5191 | 2 | Maximum Ph-N Voltage : Vn | V / 100 | U32
20883 | 0x5193 | 2 | Date of maximum Vn | - | DATETIME
20885 | 0x5195 | 2 | Maximum Ph-Ph Voltage : U12 | V / 100 | U32
20887 | 0x5197 | 2 | Date of maximum U12 | - | DATETIME
20889 | 0x5199 | 2 | Maximum Ph-Ph Voltage : U23 | V / 100 | U32
20891 | 0x519B | 2 | Date of maximum U23 | - | DATETIME
20893 | 0x519D | 2 | Maximum Ph-Ph Voltage : U31 | V / 100 | U32
20895 | 0x519F | 2 | Date of maximum U31 | - | DATETIME
20897 | 0x51A1 | 2 | Maximum Current : I1 | A / 1000 | U32
20899 | 0x51A3 | 2 | Date of maximum I1 | - | DATETIME
20901 | 0x51A5 | 2 | Maximum Current : I2 | A / 1000 | U32
20903 | 0x51A7 | 2 | Date of maximum I2 | - | DATETIME
20905 | 0x51A9 | 2 | Maximum Current : I3 | A / 1000 | U32
20907 | 0x51AB | 2 | Date of maximum I3 | - | DATETIME
20909 | 0x51AD | 2 | Maximum Current : In | A / 1000 | U32
20911 | 0x51AF | 2 | Date of maximum In | - | DATETIME
20913 | 0x51B1 | 2 | Maximum Total active power | W | S32
20915 | 0x51B3 | 2 | Date of maximum Ptot | - | DATETIME
20917 | 0x51B5 | 2 | Maximum Total reactive power | var | S32
20919 | 0x51B7 | 2 | Date of maximum Qtot | - | DATETIME
20921 | 0x51B9 | 2 | Maximum Total apparent power | VA | U32
20923 | 0x51BB | 2 | Date of maximum Stot | - | DATETIME
20925 | 0x51BD | 1 | Maximum Total power factor | - / 1000 | S16
20926 | 0x51BE | 1 | Maximum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
20927 | 0x51BF | 2 | Date of maximum Total power factor | - | DATETIME
20929 | 0x51C1 | 2 | Maximum Active power : P1 | W | S32
20931 | 0x51C3 | 2 | Date of maximum P1 | - | DATETIME
20933 | 0x51C5 | 2 | Maximum Active power : P2 | W | S32
20935 | 0x51C7 | 2 | Date of maximum P2 | - | DATETIME
20937 | 0x51C9 | 2 | Maximum Active power : P3 | W | S32
20939 | 0x51CB | 2 | Date of maximum P3 | - | DATETIME
20941 | 0x51CD | 2 | Maximum Reactive power : Q1 | var | S32
20943 | 0x51CF | 2 | Date of maximum Q1 | - | DATETIME
20945 | 0x51D1 | 2 | Maximum Reactive power : Q2 | var | S32
20947 | 0x51D3 | 2 | Date of maximum Q2 | - | DATETIME
20949 | 0x51D5 | 2 | Maximum Reactive power : Q3 | var | S32
20951 | 0x51D7 | 2 | Date of maximum Q3 | - | DATETIME
20953 | 0x51D9 | 2 | Maximum Apparent power : S1 | VA | U32
20955 | 0x51DB | 2 | Date of maximum S1 | - | DATETIME
20957 | 0x51DD | 2 | Maximum Apparent power : S2 | VA | U32
20959 | 0x51DF | 2 | Date of maximum S2 | - | DATETIME
20961 | 0x51E1 | 2 | Maximum Apparent power : S3 | VA | U32
20963 | 0x51E3 | 2 | Date of maximum S3 | - | DATETIME
20965 | 0x51E5 | 1 | Maximum Power factor : PF1 | - / 1000 | S16
20966 | 0x51E6 | 1 | Maximum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
20967 | 0x51E7 | 2 | Date of maximum PF1 | - | DATETIME
20969 | 0x51E9 | 1 | Maximum Power factor : PF2 | - / 1000 | S16
20970 | 0x51EA | 1 | Maximum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
20971 | 0x51EB | 2 | Date of maximum PF2 | - | DATETIME
20973 | 0x51ED | 1 | Maximum Power factor : PF3 | - / 1000 | S16
20974 | 0x51EE | 1 | Maximum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
20975 | 0x51EF | 2 | Date of maximum PF3 | - | DATETIME

## Inst. measurement max - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22912 | 0x5980 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22912 | 0x5980 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
22913 | 0x5981 | 2 | Maximum Frequency | Hz / 1000 | U32
22915 | 0x5983 | 2 | Date of maximum F | - | DATETIME
22917 | 0x5985 | 2 | Maximum Ph-N Voltage : V1 | V / 100 | U32
22919 | 0x5987 | 2 | Date of maximum V1 | - | DATETIME
22921 | 0x5989 | 2 | Maximum Ph-N Voltage : V2 | V / 100 | U32
22923 | 0x598B | 2 | Date of maximum V2 | - | DATETIME
22925 | 0x598D | 2 | Maximum Ph-N Voltage : V3 | V / 100 | U32
22927 | 0x598F | 2 | Date of maximum V3 | - | DATETIME
22929 | 0x5991 | 2 | Maximum Ph-N Voltage : Vn | V / 100 | U32
22931 | 0x5993 | 2 | Date of maximum Vn | - | DATETIME
22933 | 0x5995 | 2 | Maximum Ph-Ph Voltage : U12 | V / 100 | U32
22935 | 0x5997 | 2 | Date of maximum U12 | - | DATETIME
22937 | 0x5999 | 2 | Maximum Ph-Ph Voltage : U23 | V / 100 | U32
22939 | 0x599B | 2 | Date of maximum U23 | - | DATETIME
22941 | 0x599D | 2 | Maximum Ph-Ph Voltage : U31 | V / 100 | U32
22943 | 0x599F | 2 | Date of maximum U31 | - | DATETIME
22945 | 0x59A1 | 2 | Maximum Current : I1 | A / 1000 | U32
22947 | 0x59A3 | 2 | Date of maximum I1 | - | DATETIME
22949 | 0x59A5 | 2 | Maximum Current : I2 | A / 1000 | U32
22951 | 0x59A7 | 2 | Date of maximum I2 | - | DATETIME
22953 | 0x59A9 | 2 | Maximum Current : I3 | A / 1000 | U32
22955 | 0x59AB | 2 | Date of maximum I3 | - | DATETIME
22957 | 0x59AD | 2 | Maximum Current : In | A / 1000 | U32
22959 | 0x59AF | 2 | Date of maximum In | - | DATETIME
22961 | 0x59B1 | 2 | Maximum Total active power | W | S32
22963 | 0x59B3 | 2 | Date of maximum Ptot | - | DATETIME
22965 | 0x59B5 | 2 | Maximum Total reactive power | var | S32
22967 | 0x59B7 | 2 | Date of maximum Qtot | - | DATETIME
22969 | 0x59B9 | 2 | Maximum Total apparent power | VA | U32
22971 | 0x59BB | 2 | Date of maximum Stot | - | DATETIME
22973 | 0x59BD | 1 | Maximum Total power factor | - / 1000 | S16
22974 | 0x59BE | 1 | Maximum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
22975 | 0x59BF | 2 | Date of maximum Total power factor | - | DATETIME
22977 | 0x59C1 | 2 | Maximum Active power : P1 | W | S32
22979 | 0x59C3 | 2 | Date of maximum P1 | - | DATETIME
22981 | 0x59C5 | 2 | Maximum Active power : P2 | W | S32
22983 | 0x59C7 | 2 | Date of maximum P2 | - | DATETIME
22985 | 0x59C9 | 2 | Maximum Active power : P3 | W | S32
22987 | 0x59CB | 2 | Date of maximum P3 | - | DATETIME
22989 | 0x59CD | 2 | Maximum Reactive power : Q1 | var | S32
22991 | 0x59CF | 2 | Date of maximum Q1 | - | DATETIME
22993 | 0x59D1 | 2 | Maximum Reactive power : Q2 | var | S32
22995 | 0x59D3 | 2 | Date of maximum Q2 | - | DATETIME
22997 | 0x59D5 | 2 | Maximum Reactive power : Q3 | var | S32
22999 | 0x59D7 | 2 | Date of maximum Q3 | - | DATETIME
23001 | 0x59D9 | 2 | Maximum Apparent power : S1 | VA | U32
23003 | 0x59DB | 2 | Date of maximum S1 | - | DATETIME
23005 | 0x59DD | 2 | Maximum Apparent power : S2 | VA | U32
23007 | 0x59DF | 2 | Date of maximum S2 | - | DATETIME
23009 | 0x59E1 | 2 | Maximum Apparent power : S3 | VA | U32
23011 | 0x59E3 | 2 | Date of maximum S3 | - | DATETIME
23013 | 0x59E5 | 1 | Maximum Power factor : PF1 | - / 1000 | S16
23014 | 0x59E6 | 1 | Maximum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
23015 | 0x59E7 | 2 | Date of maximum PF1 | - | DATETIME
23017 | 0x59E9 | 1 | Maximum Power factor : PF2 | - / 1000 | S16
23018 | 0x59EA | 1 | Maximum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
23019 | 0x59EB | 2 | Date of maximum PF2 | - | DATETIME
23021 | 0x59ED | 1 | Maximum Power factor : PF3 | - / 1000 | S16
23022 | 0x59EE | 1 | Maximum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
23023 | 0x59EF | 2 | Date of maximum PF3 | - | DATETIME

## Inst. measurement max - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24960 | 0x6180 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24960 | 0x6180 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
24961 | 0x6181 | 2 | Maximum Frequency | Hz / 1000 | U32
24963 | 0x6183 | 2 | Date of maximum F | - | DATETIME
24965 | 0x6185 | 2 | Maximum Ph-N Voltage : V1 | V / 100 | U32
24967 | 0x6187 | 2 | Date of maximum V1 | - | DATETIME
24969 | 0x6189 | 2 | Maximum Ph-N Voltage : V2 | V / 100 | U32
24971 | 0x618B | 2 | Date of maximum V2 | - | DATETIME
24973 | 0x618D | 2 | Maximum Ph-N Voltage : V3 | V / 100 | U32
24975 | 0x618F | 2 | Date of maximum V3 | - | DATETIME
24977 | 0x6191 | 2 | Maximum Ph-N Voltage : Vn | V / 100 | U32
24979 | 0x6193 | 2 | Date of maximum Vn | - | DATETIME
24981 | 0x6195 | 2 | Maximum Ph-Ph Voltage : U12 | V / 100 | U32
24983 | 0x6197 | 2 | Date of maximum U12 | - | DATETIME
24985 | 0x6199 | 2 | Maximum Ph-Ph Voltage : U23 | V / 100 | U32
24987 | 0x619B | 2 | Date of maximum U23 | - | DATETIME
24989 | 0x619D | 2 | Maximum Ph-Ph Voltage : U31 | V / 100 | U32
24991 | 0x619F | 2 | Date of maximum U31 | - | DATETIME
24993 | 0x61A1 | 2 | Maximum Current : I1 | A / 1000 | U32
24995 | 0x61A3 | 2 | Date of maximum I1 | - | DATETIME
24997 | 0x61A5 | 2 | Maximum Current : I2 | A / 1000 | U32
24999 | 0x61A7 | 2 | Date of maximum I2 | - | DATETIME
25001 | 0x61A9 | 2 | Maximum Current : I3 | A / 1000 | U32
25003 | 0x61AB | 2 | Date of maximum I3 | - | DATETIME
25005 | 0x61AD | 2 | Maximum Current : In | A / 1000 | U32
25007 | 0x61AF | 2 | Date of maximum In | - | DATETIME
25009 | 0x61B1 | 2 | Maximum Total active power | W | S32
25011 | 0x61B3 | 2 | Date of maximum Ptot | - | DATETIME
25013 | 0x61B5 | 2 | Maximum Total reactive power | var | S32
25015 | 0x61B7 | 2 | Date of maximum Qtot | - | DATETIME
25017 | 0x61B9 | 2 | Maximum Total apparent power | VA | U32
25019 | 0x61BB | 2 | Date of maximum Stot | - | DATETIME
25021 | 0x61BD | 1 | Maximum Total power factor | - / 1000 | S16
25022 | 0x61BE | 1 | Maximum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
25023 | 0x61BF | 2 | Date of maximum Total power factor | - | DATETIME
25025 | 0x61C1 | 2 | Maximum Active power : P1 | W | S32
25027 | 0x61C3 | 2 | Date of maximum P1 | - | DATETIME
25029 | 0x61C5 | 2 | Maximum Active power : P2 | W | S32
25031 | 0x61C7 | 2 | Date of maximum P2 | - | DATETIME
25033 | 0x61C9 | 2 | Maximum Active power : P3 | W | S32
25035 | 0x61CB | 2 | Date of maximum P3 | - | DATETIME
25037 | 0x61CD | 2 | Maximum Reactive power : Q1 | var | S32
25039 | 0x61CF | 2 | Date of maximum Q1 | - | DATETIME
25041 | 0x61D1 | 2 | Maximum Reactive power : Q2 | var | S32
25043 | 0x61D3 | 2 | Date of maximum Q2 | - | DATETIME
25045 | 0x61D5 | 2 | Maximum Reactive power : Q3 | var | S32
25047 | 0x61D7 | 2 | Date of maximum Q3 | - | DATETIME
25049 | 0x61D9 | 2 | Maximum Apparent power : S1 | VA | U32
25051 | 0x61DB | 2 | Date of maximum S1 | - | DATETIME
25053 | 0x61DD | 2 | Maximum Apparent power : S2 | VA | U32
25055 | 0x61DF | 2 | Date of maximum S2 | - | DATETIME
25057 | 0x61E1 | 2 | Maximum Apparent power : S3 | VA | U32
25059 | 0x61E3 | 2 | Date of maximum S3 | - | DATETIME
25061 | 0x61E5 | 1 | Maximum Power factor : PF1 | - / 1000 | S16
25062 | 0x61E6 | 1 | Maximum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
25063 | 0x61E7 | 2 | Date of maximum PF1 | - | DATETIME
25065 | 0x61E9 | 1 | Maximum Power factor : PF2 | - / 1000 | S16
25066 | 0x61EA | 1 | Maximum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
25067 | 0x61EB | 2 | Date of maximum PF2 | - | DATETIME
25069 | 0x61ED | 1 | Maximum Power factor : PF3 | - / 1000 | S16
25070 | 0x61EE | 1 | Maximum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
25071 | 0x61EF | 2 | Date of maximum PF3 | - | DATETIME

## Inst. measurement min - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
19072 | 0x4A80 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
19072 | 0x4A80 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
19073 | 0x4A81 | 2 | Minimum Frequency | Hz / 1000 | U32
19075 | 0x4A83 | 2 | Date of minimum F | - | DATETIME
19077 | 0x4A85 | 2 | Minimum Ph-N Voltage : V1 | V / 100 | U32
19079 | 0x4A87 | 2 | Date of minimum V1 | - | DATETIME
19081 | 0x4A89 | 2 | Minimum Ph-N Voltage : V2 | V / 100 | U32
19083 | 0x4A8B | 2 | Date of minimum V2 | - | DATETIME
19085 | 0x4A8D | 2 | Minimum Ph-N Voltage : V3 | V / 100 | U32
19087 | 0x4A8F | 2 | Date of minimum V3 | - | DATETIME
19089 | 0x4A91 | 2 | Minimum Ph-N Voltage : Vn | V / 100 | U32
19091 | 0x4A93 | 2 | Date of minimum Vn | - | DATETIME
19093 | 0x4A95 | 2 | Minimum Ph-Ph Voltage : U12 | V / 100 | U32
19095 | 0x4A97 | 2 | Date of minimum U12 | - | DATETIME
19097 | 0x4A99 | 2 | Minimum Ph-Ph Voltage : U23 | V / 100 | U32
19099 | 0x4A9B | 2 | Date of minimum U23 | - | DATETIME
19101 | 0x4A9D | 2 | Minimum Ph-Ph Voltage : U31 | V / 100 | U32
19103 | 0x4A9F | 2 | Date of minimum U31 | - | DATETIME
19105 | 0x4AA1 | 2 | Minimum Current : I1 | A / 1000 | U32
19107 | 0x4AA3 | 2 | Date of minimum I1 | - | DATETIME
19109 | 0x4AA5 | 2 | Minimum Current : I2 | A / 1000 | U32
19111 | 0x4AA7 | 2 | Date of minimum I2 | - | DATETIME
19113 | 0x4AA9 | 2 | Minimum Current : I3 | A / 1000 | U32
19115 | 0x4AAB | 2 | Date of minimum I3 | - | DATETIME
19117 | 0x4AAD | 2 | Minimum Current : In | A / 1000 | U32
19119 | 0x4AAF | 2 | Date of minimum In | - | DATETIME
19121 | 0x4AB1 | 2 | Minimum Total active power | W | S32
19123 | 0x4AB3 | 2 | Date of minimum Ptot | - | DATETIME
19125 | 0x4AB5 | 2 | Minimum Total reactive power | var | S32
19127 | 0x4AB7 | 2 | Date of minimum Qtot | - | DATETIME
19129 | 0x4AB9 | 2 | Minimum Total apparent power | VA | U32
19131 | 0x4ABB | 2 | Date of minimum Stot | - | DATETIME
19133 | 0x4ABD | 1 | Minimum Total power factor | - / 1000 | S16
19134 | 0x4ABE | 1 | Minimum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
19135 | 0x4ABF | 2 | Date of minimum Total power factor | - | DATETIME
19137 | 0x4AC1 | 2 | Minimum Active power : P1 | W | S32
19139 | 0x4AC3 | 2 | Date of minimum P1 | - | DATETIME
19141 | 0x4AC5 | 2 | Minimum Active power : P2 | W | S32
19143 | 0x4AC7 | 2 | Date of minimum P2 | - | DATETIME
19145 | 0x4AC9 | 2 | Minimum Active power : P3 | W | S32
19147 | 0x4ACB | 2 | Date of minimum P3 | - | DATETIME
19149 | 0x4ACD | 2 | Minimum Reactive power : Q1 | var | S32
19151 | 0x4ACF | 2 | Date of minimum Q1 | - | DATETIME
19153 | 0x4AD1 | 2 | Minimum Reactive power : Q2 | var | S32
19155 | 0x4AD3 | 2 | Date of minimum Q2 | - | DATETIME
19157 | 0x4AD5 | 2 | Minimum Reactive power : Q3 | var | S32
19159 | 0x4AD7 | 2 | Date of minimum Q3 | - | DATETIME
19161 | 0x4AD9 | 2 | Minimum Apparent power : S1 | VA | U32
19163 | 0x4ADB | 2 | Date of minimum S1 | - | DATETIME
19165 | 0x4ADD | 2 | Minimum Apparent power : S2 | VA | U32
19167 | 0x4ADF | 2 | Date of minimum S2 | - | DATETIME
19169 | 0x4AE1 | 2 | Minimum Apparent power : S3 | VA | U32
19171 | 0x4AE3 | 2 | Date of minimum S3 | - | DATETIME
19173 | 0x4AE5 | 1 | Minimum Power factor : PF1 | - / 1000 | S16
19174 | 0x4AE6 | 1 | Minimum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
19175 | 0x4AE7 | 2 | Date of minimum PF1 | - | DATETIME
19177 | 0x4AE9 | 1 | Minimum Power factor : PF2 | - / 1000 | S16
19178 | 0x4AEA | 1 | Minimum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
19179 | 0x4AEB | 2 | Date of minimum PF2 | - | DATETIME
19181 | 0x4AED | 1 | Minimum Power factor : PF3 | - / 1000 | S16
19182 | 0x4AEE | 1 | Minimum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
19183 | 0x4AEF | 2 | Date of minimum PF3 | - | DATETIME

## Inst. measurement min - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
21120 | 0x5280 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
21120 | 0x5280 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
21121 | 0x5281 | 2 | Minimum Frequency | Hz / 1000 | U32
21123 | 0x5283 | 2 | Date of minimum F | - | DATETIME
21125 | 0x5285 | 2 | Minimum Ph-N Voltage : V1 | V / 100 | U32
21127 | 0x5287 | 2 | Date of minimum V1 | - | DATETIME
21129 | 0x5289 | 2 | Minimum Ph-N Voltage : V2 | V / 100 | U32
21131 | 0x528B | 2 | Date of minimum V2 | - | DATETIME
21133 | 0x528D | 2 | Minimum Ph-N Voltage : V3 | V / 100 | U32
21135 | 0x528F | 2 | Date of minimum V3 | - | DATETIME
21137 | 0x5291 | 2 | Minimum Ph-N Voltage : Vn | V / 100 | U32
21139 | 0x5293 | 2 | Date of minimum Vn | - | DATETIME
21141 | 0x5295 | 2 | Minimum Ph-Ph Voltage : U12 | V / 100 | U32
21143 | 0x5297 | 2 | Date of minimum U12 | - | DATETIME
21145 | 0x5299 | 2 | Minimum Ph-Ph Voltage : U23 | V / 100 | U32
21147 | 0x529B | 2 | Date of minimum U23 | - | DATETIME
21149 | 0x529D | 2 | Minimum Ph-Ph Voltage : U31 | V / 100 | U32
21151 | 0x529F | 2 | Date of minimum U31 | - | DATETIME
21153 | 0x52A1 | 2 | Minimum Current : I1 | A / 1000 | U32
21155 | 0x52A3 | 2 | Date of minimum I1 | - | DATETIME
21157 | 0x52A5 | 2 | Minimum Current : I2 | A / 1000 | U32
21159 | 0x52A7 | 2 | Date of minimum I2 | - | DATETIME
21161 | 0x52A9 | 2 | Minimum Current : I3 | A / 1000 | U32
21163 | 0x52AB | 2 | Date of minimum I3 | - | DATETIME
21165 | 0x52AD | 2 | Minimum Current : In | A / 1000 | U32
21167 | 0x52AF | 2 | Date of minimum In | - | DATETIME
21169 | 0x52B1 | 2 | Minimum Total active power | W | S32
21171 | 0x52B3 | 2 | Date of minimum Ptot | - | DATETIME
21173 | 0x52B5 | 2 | Minimum Total reactive power | var | S32
21175 | 0x52B7 | 2 | Date of minimum Qtot | - | DATETIME
21177 | 0x52B9 | 2 | Minimum Total apparent power | VA | U32
21179 | 0x52BB | 2 | Date of minimum Stot | - | DATETIME
21181 | 0x52BD | 1 | Minimum Total power factor | - / 1000 | S16
21182 | 0x52BE | 1 | Minimum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
21183 | 0x52BF | 2 | Date of minimum Total power factor | - | DATETIME
21185 | 0x52C1 | 2 | Minimum Active power : P1 | W | S32
21187 | 0x52C3 | 2 | Date of minimum P1 | - | DATETIME
21189 | 0x52C5 | 2 | Minimum Active power : P2 | W | S32
21191 | 0x52C7 | 2 | Date of minimum P2 | - | DATETIME
21193 | 0x52C9 | 2 | Minimum Active power : P3 | W | S32
21195 | 0x52CB | 2 | Date of minimum P3 | - | DATETIME
21197 | 0x52CD | 2 | Minimum Reactive power : Q1 | var | S32
21199 | 0x52CF | 2 | Date of minimum Q1 | - | DATETIME
21201 | 0x52D1 | 2 | Minimum Reactive power : Q2 | var | S32
21203 | 0x52D3 | 2 | Date of minimum Q2 | - | DATETIME
21205 | 0x52D5 | 2 | Minimum Reactive power : Q3 | var | S32
21207 | 0x52D7 | 2 | Date of minimum Q3 | - | DATETIME
21209 | 0x52D9 | 2 | Minimum Apparent power : S1 | VA | U32
21211 | 0x52DB | 2 | Date of minimum S1 | - | DATETIME
21213 | 0x52DD | 2 | Minimum Apparent power : S2 | VA | U32
21215 | 0x52DF | 2 | Date of minimum S2 | - | DATETIME
21217 | 0x52E1 | 2 | Minimum Apparent power : S3 | VA | U32
21219 | 0x52E3 | 2 | Date of minimum S3 | - | DATETIME
21221 | 0x52E5 | 1 | Minimum Power factor : PF1 | - / 1000 | S16
21222 | 0x52E6 | 1 | Minimum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
21223 | 0x52E7 | 2 | Date of minimum PF1 | - | DATETIME
21225 | 0x52E9 | 1 | Minimum Power factor : PF2 | - / 1000 | S16
21226 | 0x52EA | 1 | Minimum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
21227 | 0x52EB | 2 | Date of minimum PF2 | - | DATETIME
21229 | 0x52ED | 1 | Minimum Power factor : PF3 | - / 1000 | S16
21230 | 0x52EE | 1 | Minimum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
21231 | 0x52EF | 2 | Date of minimum PF3 | - | DATETIME

## Inst. measurement min - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
23168 | 0x5A80 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
23168 | 0x5A80 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
23169 | 0x5A81 | 2 | Minimum Frequency | Hz / 1000 | U32
23171 | 0x5A83 | 2 | Date of minimum F | - | DATETIME
23173 | 0x5A85 | 2 | Minimum Ph-N Voltage : V1 | V / 100 | U32
23175 | 0x5A87 | 2 | Date of minimum V1 | - | DATETIME
23177 | 0x5A89 | 2 | Minimum Ph-N Voltage : V2 | V / 100 | U32
23179 | 0x5A8B | 2 | Date of minimum V2 | - | DATETIME
23181 | 0x5A8D | 2 | Minimum Ph-N Voltage : V3 | V / 100 | U32
23183 | 0x5A8F | 2 | Date of minimum V3 | - | DATETIME
23185 | 0x5A91 | 2 | Minimum Ph-N Voltage : Vn | V / 100 | U32
23187 | 0x5A93 | 2 | Date of minimum Vn | - | DATETIME
23189 | 0x5A95 | 2 | Minimum Ph-Ph Voltage : U12 | V / 100 | U32
23191 | 0x5A97 | 2 | Date of minimum U12 | - | DATETIME
23193 | 0x5A99 | 2 | Minimum Ph-Ph Voltage : U23 | V / 100 | U32
23195 | 0x5A9B | 2 | Date of minimum U23 | - | DATETIME
23197 | 0x5A9D | 2 | Minimum Ph-Ph Voltage : U31 | V / 100 | U32
23199 | 0x5A9F | 2 | Date of minimum U31 | - | DATETIME
23201 | 0x5AA1 | 2 | Minimum Current : I1 | A / 1000 | U32
23203 | 0x5AA3 | 2 | Date of minimum I1 | - | DATETIME
23205 | 0x5AA5 | 2 | Minimum Current : I2 | A / 1000 | U32
23207 | 0x5AA7 | 2 | Date of minimum I2 | - | DATETIME
23209 | 0x5AA9 | 2 | Minimum Current : I3 | A / 1000 | U32
23211 | 0x5AAB | 2 | Date of minimum I3 | - | DATETIME
23213 | 0x5AAD | 2 | Minimum Current : In | A / 1000 | U32
23215 | 0x5AAF | 2 | Date of minimum In | - | DATETIME
23217 | 0x5AB1 | 2 | Minimum Total active power | W | S32
23219 | 0x5AB3 | 2 | Date of minimum Ptot | - | DATETIME
23221 | 0x5AB5 | 2 | Minimum Total reactive power | var | S32
23223 | 0x5AB7 | 2 | Date of minimum Qtot | - | DATETIME
23225 | 0x5AB9 | 2 | Minimum Total apparent power | VA | U32
23227 | 0x5ABB | 2 | Date of minimum Stot | - | DATETIME
23229 | 0x5ABD | 1 | Minimum Total power factor | - / 1000 | S16
23230 | 0x5ABE | 1 | Minimum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
23231 | 0x5ABF | 2 | Date of minimum Total power factor | - | DATETIME
23233 | 0x5AC1 | 2 | Minimum Active power : P1 | W | S32
23235 | 0x5AC3 | 2 | Date of minimum P1 | - | DATETIME
23237 | 0x5AC5 | 2 | Minimum Active power : P2 | W | S32
23239 | 0x5AC7 | 2 | Date of minimum P2 | - | DATETIME
23241 | 0x5AC9 | 2 | Minimum Active power : P3 | W | S32
23243 | 0x5ACB | 2 | Date of minimum P3 | - | DATETIME
23245 | 0x5ACD | 2 | Minimum Reactive power : Q1 | var | S32
23247 | 0x5ACF | 2 | Date of minimum Q1 | - | DATETIME
23249 | 0x5AD1 | 2 | Minimum Reactive power : Q2 | var | S32
23251 | 0x5AD3 | 2 | Date of minimum Q2 | - | DATETIME
23253 | 0x5AD5 | 2 | Minimum Reactive power : Q3 | var | S32
23255 | 0x5AD7 | 2 | Date of minimum Q3 | - | DATETIME
23257 | 0x5AD9 | 2 | Minimum Apparent power : S1 | VA | U32
23259 | 0x5ADB | 2 | Date of minimum S1 | - | DATETIME
23261 | 0x5ADD | 2 | Minimum Apparent power : S2 | VA | U32
23263 | 0x5ADF | 2 | Date of minimum S2 | - | DATETIME
23265 | 0x5AE1 | 2 | Minimum Apparent power : S3 | VA | U32
23267 | 0x5AE3 | 2 | Date of minimum S3 | - | DATETIME
23269 | 0x5AE5 | 1 | Minimum Power factor : PF1 | - / 1000 | S16
23270 | 0x5AE6 | 1 | Minimum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
23271 | 0x5AE7 | 2 | Date of minimum PF1 | - | DATETIME
23273 | 0x5AE9 | 1 | Minimum Power factor : PF2 | - / 1000 | S16
23274 | 0x5AEA | 1 | Minimum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
23275 | 0x5AEB | 2 | Date of minimum PF2 | - | DATETIME
23277 | 0x5AED | 1 | Minimum Power factor : PF3 | - / 1000 | S16
23278 | 0x5AEE | 1 | Minimum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
23279 | 0x5AEF | 2 | Date of minimum PF3 | - | DATETIME

## Inst. measurement min - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
25216 | 0x6280 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
25216 | 0x6280 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
25217 | 0x6281 | 2 | Minimum Frequency | Hz / 1000 | U32
25219 | 0x6283 | 2 | Date of minimum F | - | DATETIME
25221 | 0x6285 | 2 | Minimum Ph-N Voltage : V1 | V / 100 | U32
25223 | 0x6287 | 2 | Date of minimum V1 | - | DATETIME
25225 | 0x6289 | 2 | Minimum Ph-N Voltage : V2 | V / 100 | U32
25227 | 0x628B | 2 | Date of minimum V2 | - | DATETIME
25229 | 0x628D | 2 | Minimum Ph-N Voltage : V3 | V / 100 | U32
25231 | 0x628F | 2 | Date of minimum V3 | - | DATETIME
25233 | 0x6291 | 2 | Minimum Ph-N Voltage : Vn | V / 100 | U32
25235 | 0x6293 | 2 | Date of minimum Vn | - | DATETIME
25237 | 0x6295 | 2 | Minimum Ph-Ph Voltage : U12 | V / 100 | U32
25239 | 0x6297 | 2 | Date of minimum U12 | - | DATETIME
25241 | 0x6299 | 2 | Minimum Ph-Ph Voltage : U23 | V / 100 | U32
25243 | 0x629B | 2 | Date of minimum U23 | - | DATETIME
25245 | 0x629D | 2 | Minimum Ph-Ph Voltage : U31 | V / 100 | U32
25247 | 0x629F | 2 | Date of minimum U31 | - | DATETIME
25249 | 0x62A1 | 2 | Minimum Current : I1 | A / 1000 | U32
25251 | 0x62A3 | 2 | Date of minimum I1 | - | DATETIME
25253 | 0x62A5 | 2 | Minimum Current : I2 | A / 1000 | U32
25255 | 0x62A7 | 2 | Date of minimum I2 | - | DATETIME
25257 | 0x62A9 | 2 | Minimum Current : I3 | A / 1000 | U32
25259 | 0x62AB | 2 | Date of minimum I3 | - | DATETIME
25261 | 0x62AD | 2 | Minimum Current : In | A / 1000 | U32
25263 | 0x62AF | 2 | Date of minimum In | - | DATETIME
25265 | 0x62B1 | 2 | Minimum Total active power | W | S32
25267 | 0x62B3 | 2 | Date of minimum Ptot | - | DATETIME
25269 | 0x62B5 | 2 | Minimum Total reactive power | var | S32
25271 | 0x62B7 | 2 | Date of minimum Qtot | - | DATETIME
25273 | 0x62B9 | 2 | Minimum Total apparent power | VA | U32
25275 | 0x62BB | 2 | Date of minimum Stot | - | DATETIME
25277 | 0x62BD | 1 | Minimum Total power factor | - / 1000 | S16
25278 | 0x62BE | 1 | Minimum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
25279 | 0x62BF | 2 | Date of minimum Total power factor | - | DATETIME
25281 | 0x62C1 | 2 | Minimum Active power : P1 | W | S32
25283 | 0x62C3 | 2 | Date of minimum P1 | - | DATETIME
25285 | 0x62C5 | 2 | Minimum Active power : P2 | W | S32
25287 | 0x62C7 | 2 | Date of minimum P2 | - | DATETIME
25289 | 0x62C9 | 2 | Minimum Active power : P3 | W | S32
25291 | 0x62CB | 2 | Date of minimum P3 | - | DATETIME
25293 | 0x62CD | 2 | Minimum Reactive power : Q1 | var | S32
25295 | 0x62CF | 2 | Date of minimum Q1 | - | DATETIME
25297 | 0x62D1 | 2 | Minimum Reactive power : Q2 | var | S32
25299 | 0x62D3 | 2 | Date of minimum Q2 | - | DATETIME
25301 | 0x62D5 | 2 | Minimum Reactive power : Q3 | var | S32
25303 | 0x62D7 | 2 | Date of minimum Q3 | - | DATETIME
25305 | 0x62D9 | 2 | Minimum Apparent power : S1 | VA | U32
25307 | 0x62DB | 2 | Date of minimum S1 | - | DATETIME
25309 | 0x62DD | 2 | Minimum Apparent power : S2 | VA | U32
25311 | 0x62DF | 2 | Date of minimum S2 | - | DATETIME
25313 | 0x62E1 | 2 | Minimum Apparent power : S3 | VA | U32
25315 | 0x62E3 | 2 | Date of minimum S3 | - | DATETIME
25317 | 0x62E5 | 1 | Minimum Power factor : PF1 | - / 1000 | S16
25318 | 0x62E6 | 1 | Minimum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
25319 | 0x62E7 | 2 | Date of minimum PF1 | - | DATETIME
25321 | 0x62E9 | 1 | Minimum Power factor : PF2 | - / 1000 | S16
25322 | 0x62EA | 1 | Minimum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
25323 | 0x62EB | 2 | Date of minimum PF2 | - | DATETIME
25325 | 0x62ED | 1 | Minimum Power factor : PF3 | - / 1000 | S16
25326 | 0x62EE | 1 | Minimum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
25327 | 0x62EF | 2 | Date of minimum PF3 | - | DATETIME

## Avg. measurement max - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
19328 | 0x4B80 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
19328 | 0x4B80 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
19329 | 0x4B81 | 2 | Maximum Frequency | Hz / 1000 | U32
19331 | 0x4B83 | 2 | Date of maximum F | - | DATETIME
19333 | 0x4B85 | 2 | Maximum Ph-N Voltage : V1 | V / 100 | U32
19335 | 0x4B87 | 2 | Date of maximum V1 | - | DATETIME
19337 | 0x4B89 | 2 | Maximum Ph-N Voltage : V2 | V / 100 | U32
19339 | 0x4B8B | 2 | Date of maximum V2 | - | DATETIME
19341 | 0x4B8D | 2 | Maximum Ph-N Voltage : V3 | V / 100 | U32
19343 | 0x4B8F | 2 | Date of maximum V3 | - | DATETIME
19345 | 0x4B91 | 2 | Maximum Ph-N Voltage : Vn | V / 100 | U32
19347 | 0x4B93 | 2 | Date of maximum Vn | - | DATETIME
19349 | 0x4B95 | 2 | Maximum Ph-Ph Voltage : U12 | V / 100 | U32
19351 | 0x4B97 | 2 | Date of maximum U12 | - | DATETIME
19353 | 0x4B99 | 2 | Maximum Ph-Ph Voltage : U23 | V / 100 | U32
19355 | 0x4B9B | 2 | Date of maximum U23 | - | DATETIME
19357 | 0x4B9D | 2 | Maximum Ph-Ph Voltage : U31 | V / 100 | U32
19359 | 0x4B9F | 2 | Date of maximum U31 | - | DATETIME
19361 | 0x4BA1 | 2 | Maximum Current : I1 | A / 1000 | U32
19363 | 0x4BA3 | 2 | Date of maximum I1 | - | DATETIME
19365 | 0x4BA5 | 2 | Maximum Current : I2 | A / 1000 | U32
19367 | 0x4BA7 | 2 | Date of maximum I2 | - | DATETIME
19369 | 0x4BA9 | 2 | Maximum Current : I3 | A / 1000 | U32
19371 | 0x4BAB | 2 | Date of maximum I3 | - | DATETIME
19373 | 0x4BAD | 2 | Maximum Current : In | A / 1000 | U32
19375 | 0x4BAF | 2 | Date of maximum In | - | DATETIME
19377 | 0x4BB1 | 2 | Maximum Total active power | W | S32
19379 | 0x4BB3 | 2 | Date of maximum Ptot | - | DATETIME
19381 | 0x4BB5 | 2 | Maximum Total reactive power | var | S32
19383 | 0x4BB7 | 2 | Date of maximum Qtot | - | DATETIME
19385 | 0x4BB9 | 2 | Maximum Total apparent power | VA | U32
19387 | 0x4BBB | 2 | Date of maximum Stot | - | DATETIME
19389 | 0x4BBD | 1 | Maximum Total power factor | - / 1000 | S16
19390 | 0x4BBE | 1 | Maximum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
19391 | 0x4BBF | 2 | Date of maximum Total power factor | - | DATETIME
19393 | 0x4BC1 | 2 | Maximum Active power : P1 | W | S32
19395 | 0x4BC3 | 2 | Date of maximum P1 | - | DATETIME
19397 | 0x4BC5 | 2 | Maximum Active power : P2 | W | S32
19399 | 0x4BC7 | 2 | Date of maximum P2 | - | DATETIME
19401 | 0x4BC9 | 2 | Maximum Active power : P3 | W | S32
19403 | 0x4BCB | 2 | Date of maximum P3 | - | DATETIME
19405 | 0x4BCD | 2 | Maximum Reactive power : Q1 | var | S32
19407 | 0x4BCF | 2 | Date of maximum Q1 | - | DATETIME
19409 | 0x4BD1 | 2 | Maximum Reactive power : Q2 | var | S32
19411 | 0x4BD3 | 2 | Date of maximum Q2 | - | DATETIME
19413 | 0x4BD5 | 2 | Maximum Reactive power : Q3 | var | S32
19415 | 0x4BD7 | 2 | Date of maximum Q3 | - | DATETIME
19417 | 0x4BD9 | 2 | Maximum Apparent power : S1 | VA | U32
19419 | 0x4BDB | 2 | Date of maximum S1 | - | DATETIME
19421 | 0x4BDD | 2 | Maximum Apparent power : S2 | VA | U32
19423 | 0x4BDF | 2 | Date of maximum S2 | - | DATETIME
19425 | 0x4BE1 | 2 | Maximum Apparent power : S3 | VA | U32
19427 | 0x4BE3 | 2 | Date of maximum S3 | - | DATETIME
19429 | 0x4BE5 | 1 | Maximum Power factor : PF1 | - / 1000 | S16
19430 | 0x4BE6 | 1 | Maximum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
19431 | 0x4BE7 | 2 | Date of maximum PF1 | - | DATETIME
19433 | 0x4BE9 | 1 | Maximum Power factor : PF2 | - / 1000 | S16
19434 | 0x4BEA | 1 | Maximum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
19435 | 0x4BEB | 2 | Date of maximum PF2 | - | DATETIME
19437 | 0x4BED | 1 | Maximum Power factor : PF3 | - / 1000 | S16
19438 | 0x4BEE | 1 | Maximum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
19439 | 0x4BEF | 2 | Date of maximum PF3 | - | DATETIME

## Avg. measurement max - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
21376 | 0x5380 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
21376 | 0x5380 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
21377 | 0x5381 | 2 | Maximum Frequency | Hz / 1000 | U32
21379 | 0x5383 | 2 | Date of maximum F | - | DATETIME
21381 | 0x5385 | 2 | Maximum Ph-N Voltage : V1 | V / 100 | U32
21383 | 0x5387 | 2 | Date of maximum V1 | - | DATETIME
21385 | 0x5389 | 2 | Maximum Ph-N Voltage : V2 | V / 100 | U32
21387 | 0x538B | 2 | Date of maximum V2 | - | DATETIME
21389 | 0x538D | 2 | Maximum Ph-N Voltage : V3 | V / 100 | U32
21391 | 0x538F | 2 | Date of maximum V3 | - | DATETIME
21393 | 0x5391 | 2 | Maximum Ph-N Voltage : Vn | V / 100 | U32
21395 | 0x5393 | 2 | Date of maximum Vn | - | DATETIME
21397 | 0x5395 | 2 | Maximum Ph-Ph Voltage : U12 | V / 100 | U32
21399 | 0x5397 | 2 | Date of maximum U12 | - | DATETIME
21401 | 0x5399 | 2 | Maximum Ph-Ph Voltage : U23 | V / 100 | U32
21403 | 0x539B | 2 | Date of maximum U23 | - | DATETIME
21405 | 0x539D | 2 | Maximum Ph-Ph Voltage : U31 | V / 100 | U32
21407 | 0x539F | 2 | Date of maximum U31 | - | DATETIME
21409 | 0x53A1 | 2 | Maximum Current : I1 | A / 1000 | U32
21411 | 0x53A3 | 2 | Date of maximum I1 | - | DATETIME
21413 | 0x53A5 | 2 | Maximum Current : I2 | A / 1000 | U32
21415 | 0x53A7 | 2 | Date of maximum I2 | - | DATETIME
21417 | 0x53A9 | 2 | Maximum Current : I3 | A / 1000 | U32
21419 | 0x53AB | 2 | Date of maximum I3 | - | DATETIME
21421 | 0x53AD | 2 | Maximum Current : In | A / 1000 | U32
21423 | 0x53AF | 2 | Date of maximum In | - | DATETIME
21425 | 0x53B1 | 2 | Maximum Total active power | W | S32
21427 | 0x53B3 | 2 | Date of maximum Ptot | - | DATETIME
21429 | 0x53B5 | 2 | Maximum Total reactive power | var | S32
21431 | 0x53B7 | 2 | Date of maximum Qtot | - | DATETIME
21433 | 0x53B9 | 2 | Maximum Total apparent power | VA | U32
21435 | 0x53BB | 2 | Date of maximum Stot | - | DATETIME
21437 | 0x53BD | 1 | Maximum Total power factor | - / 1000 | S16
21438 | 0x53BE | 1 | Maximum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
21439 | 0x53BF | 2 | Date of maximum Total power factor | - | DATETIME
21441 | 0x53C1 | 2 | Maximum Active power : P1 | W | S32
21443 | 0x53C3 | 2 | Date of maximum P1 | - | DATETIME
21445 | 0x53C5 | 2 | Maximum Active power : P2 | W | S32
21447 | 0x53C7 | 2 | Date of maximum P2 | - | DATETIME
21449 | 0x53C9 | 2 | Maximum Active power : P3 | W | S32
21451 | 0x53CB | 2 | Date of maximum P3 | - | DATETIME
21453 | 0x53CD | 2 | Maximum Reactive power : Q1 | var | S32
21455 | 0x53CF | 2 | Date of maximum Q1 | - | DATETIME
21457 | 0x53D1 | 2 | Maximum Reactive power : Q2 | var | S32
21459 | 0x53D3 | 2 | Date of maximum Q2 | - | DATETIME
21461 | 0x53D5 | 2 | Maximum Reactive power : Q3 | var | S32
21463 | 0x53D7 | 2 | Date of maximum Q3 | - | DATETIME
21465 | 0x53D9 | 2 | Maximum Apparent power : S1 | VA | U32
21467 | 0x53DB | 2 | Date of maximum S1 | - | DATETIME
21469 | 0x53DD | 2 | Maximum Apparent power : S2 | VA | U32
21471 | 0x53DF | 2 | Date of maximum S2 | - | DATETIME
21473 | 0x53E1 | 2 | Maximum Apparent power : S3 | VA | U32
21475 | 0x53E3 | 2 | Date of maximum S3 | - | DATETIME
21477 | 0x53E5 | 1 | Maximum Power factor : PF1 | - / 1000 | S16
21478 | 0x53E6 | 1 | Maximum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
21479 | 0x53E7 | 2 | Date of maximum PF1 | - | DATETIME
21481 | 0x53E9 | 1 | Maximum Power factor : PF2 | - / 1000 | S16
21482 | 0x53EA | 1 | Maximum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
21483 | 0x53EB | 2 | Date of maximum PF2 | - | DATETIME
21485 | 0x53ED | 1 | Maximum Power factor : PF3 | - / 1000 | S16
21486 | 0x53EE | 1 | Maximum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
21487 | 0x53EF | 2 | Date of maximum PF3 | - | DATETIME

## Avg. measurement max - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
23424 | 0x5B80 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
23424 | 0x5B80 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
23425 | 0x5B81 | 2 | Maximum Frequency | Hz / 1000 | U32
23427 | 0x5B83 | 2 | Date of maximum F | - | DATETIME
23429 | 0x5B85 | 2 | Maximum Ph-N Voltage : V1 | V / 100 | U32
23431 | 0x5B87 | 2 | Date of maximum V1 | - | DATETIME
23433 | 0x5B89 | 2 | Maximum Ph-N Voltage : V2 | V / 100 | U32
23435 | 0x5B8B | 2 | Date of maximum V2 | - | DATETIME
23437 | 0x5B8D | 2 | Maximum Ph-N Voltage : V3 | V / 100 | U32
23439 | 0x5B8F | 2 | Date of maximum V3 | - | DATETIME
23441 | 0x5B91 | 2 | Maximum Ph-N Voltage : Vn | V / 100 | U32
23443 | 0x5B93 | 2 | Date of maximum Vn | - | DATETIME
23445 | 0x5B95 | 2 | Maximum Ph-Ph Voltage : U12 | V / 100 | U32
23447 | 0x5B97 | 2 | Date of maximum U12 | - | DATETIME
23449 | 0x5B99 | 2 | Maximum Ph-Ph Voltage : U23 | V / 100 | U32
23451 | 0x5B9B | 2 | Date of maximum U23 | - | DATETIME
23453 | 0x5B9D | 2 | Maximum Ph-Ph Voltage : U31 | V / 100 | U32
23455 | 0x5B9F | 2 | Date of maximum U31 | - | DATETIME
23457 | 0x5BA1 | 2 | Maximum Current : I1 | A / 1000 | U32
23459 | 0x5BA3 | 2 | Date of maximum I1 | - | DATETIME
23461 | 0x5BA5 | 2 | Maximum Current : I2 | A / 1000 | U32
23463 | 0x5BA7 | 2 | Date of maximum I2 | - | DATETIME
23465 | 0x5BA9 | 2 | Maximum Current : I3 | A / 1000 | U32
23467 | 0x5BAB | 2 | Date of maximum I3 | - | DATETIME
23469 | 0x5BAD | 2 | Maximum Current : In | A / 1000 | U32
23471 | 0x5BAF | 2 | Date of maximum In | - | DATETIME
23473 | 0x5BB1 | 2 | Maximum Total active power | W | S32
23475 | 0x5BB3 | 2 | Date of maximum Ptot | - | DATETIME
23477 | 0x5BB5 | 2 | Maximum Total reactive power | var | S32
23479 | 0x5BB7 | 2 | Date of maximum Qtot | - | DATETIME
23481 | 0x5BB9 | 2 | Maximum Total apparent power | VA | U32
23483 | 0x5BBB | 2 | Date of maximum Stot | - | DATETIME
23485 | 0x5BBD | 1 | Maximum Total power factor | - / 1000 | S16
23486 | 0x5BBE | 1 | Maximum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
23487 | 0x5BBF | 2 | Date of maximum Total power factor | - | DATETIME
23489 | 0x5BC1 | 2 | Maximum Active power : P1 | W | S32
23491 | 0x5BC3 | 2 | Date of maximum P1 | - | DATETIME
23493 | 0x5BC5 | 2 | Maximum Active power : P2 | W | S32
23495 | 0x5BC7 | 2 | Date of maximum P2 | - | DATETIME
23497 | 0x5BC9 | 2 | Maximum Active power : P3 | W | S32
23499 | 0x5BCB | 2 | Date of maximum P3 | - | DATETIME
23501 | 0x5BCD | 2 | Maximum Reactive power : Q1 | var | S32
23503 | 0x5BCF | 2 | Date of maximum Q1 | - | DATETIME
23505 | 0x5BD1 | 2 | Maximum Reactive power : Q2 | var | S32
23507 | 0x5BD3 | 2 | Date of maximum Q2 | - | DATETIME
23509 | 0x5BD5 | 2 | Maximum Reactive power : Q3 | var | S32
23511 | 0x5BD7 | 2 | Date of maximum Q3 | - | DATETIME
23513 | 0x5BD9 | 2 | Maximum Apparent power : S1 | VA | U32
23515 | 0x5BDB | 2 | Date of maximum S1 | - | DATETIME
23517 | 0x5BDD | 2 | Maximum Apparent power : S2 | VA | U32
23519 | 0x5BDF | 2 | Date of maximum S2 | - | DATETIME
23521 | 0x5BE1 | 2 | Maximum Apparent power : S3 | VA | U32
23523 | 0x5BE3 | 2 | Date of maximum S3 | - | DATETIME
23525 | 0x5BE5 | 1 | Maximum Power factor : PF1 | - / 1000 | S16
23526 | 0x5BE6 | 1 | Maximum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
23527 | 0x5BE7 | 2 | Date of maximum PF1 | - | DATETIME
23529 | 0x5BE9 | 1 | Maximum Power factor : PF2 | - / 1000 | S16
23530 | 0x5BEA | 1 | Maximum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
23531 | 0x5BEB | 2 | Date of maximum PF2 | - | DATETIME
23533 | 0x5BED | 1 | Maximum Power factor : PF3 | - / 1000 | S16
23534 | 0x5BEE | 1 | Maximum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
23535 | 0x5BEF | 2 | Date of maximum PF3 | - | DATETIME

## Avg. measurement max - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
25472 | 0x6380 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
25472 | 0x6380 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
25473 | 0x6381 | 2 | Maximum Frequency | Hz / 1000 | U32
25475 | 0x6383 | 2 | Date of maximum F | - | DATETIME
25477 | 0x6385 | 2 | Maximum Ph-N Voltage : V1 | V / 100 | U32
25479 | 0x6387 | 2 | Date of maximum V1 | - | DATETIME
25481 | 0x6389 | 2 | Maximum Ph-N Voltage : V2 | V / 100 | U32
25483 | 0x638B | 2 | Date of maximum V2 | - | DATETIME
25485 | 0x638D | 2 | Maximum Ph-N Voltage : V3 | V / 100 | U32
25487 | 0x638F | 2 | Date of maximum V3 | - | DATETIME
25489 | 0x6391 | 2 | Maximum Ph-N Voltage : Vn | V / 100 | U32
25491 | 0x6393 | 2 | Date of maximum Vn | - | DATETIME
25493 | 0x6395 | 2 | Maximum Ph-Ph Voltage : U12 | V / 100 | U32
25495 | 0x6397 | 2 | Date of maximum U12 | - | DATETIME
25497 | 0x6399 | 2 | Maximum Ph-Ph Voltage : U23 | V / 100 | U32
25499 | 0x639B | 2 | Date of maximum U23 | - | DATETIME
25501 | 0x639D | 2 | Maximum Ph-Ph Voltage : U31 | V / 100 | U32
25503 | 0x639F | 2 | Date of maximum U31 | - | DATETIME
25505 | 0x63A1 | 2 | Maximum Current : I1 | A / 1000 | U32
25507 | 0x63A3 | 2 | Date of maximum I1 | - | DATETIME
25509 | 0x63A5 | 2 | Maximum Current : I2 | A / 1000 | U32
25511 | 0x63A7 | 2 | Date of maximum I2 | - | DATETIME
25513 | 0x63A9 | 2 | Maximum Current : I3 | A / 1000 | U32
25515 | 0x63AB | 2 | Date of maximum I3 | - | DATETIME
25517 | 0x63AD | 2 | Maximum Current : In | A / 1000 | U32
25519 | 0x63AF | 2 | Date of maximum In | - | DATETIME
25521 | 0x63B1 | 2 | Maximum Total active power | W | S32
25523 | 0x63B3 | 2 | Date of maximum Ptot | - | DATETIME
25525 | 0x63B5 | 2 | Maximum Total reactive power | var | S32
25527 | 0x63B7 | 2 | Date of maximum Qtot | - | DATETIME
25529 | 0x63B9 | 2 | Maximum Total apparent power | VA | U32
25531 | 0x63BB | 2 | Date of maximum Stot | - | DATETIME
25533 | 0x63BD | 1 | Maximum Total power factor | - / 1000 | S16
25534 | 0x63BE | 1 | Maximum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
25535 | 0x63BF | 2 | Date of maximum Total power factor | - | DATETIME
25537 | 0x63C1 | 2 | Maximum Active power : P1 | W | S32
25539 | 0x63C3 | 2 | Date of maximum P1 | - | DATETIME
25541 | 0x63C5 | 2 | Maximum Active power : P2 | W | S32
25543 | 0x63C7 | 2 | Date of maximum P2 | - | DATETIME
25545 | 0x63C9 | 2 | Maximum Active power : P3 | W | S32
25547 | 0x63CB | 2 | Date of maximum P3 | - | DATETIME
25549 | 0x63CD | 2 | Maximum Reactive power : Q1 | var | S32
25551 | 0x63CF | 2 | Date of maximum Q1 | - | DATETIME
25553 | 0x63D1 | 2 | Maximum Reactive power : Q2 | var | S32
25555 | 0x63D3 | 2 | Date of maximum Q2 | - | DATETIME
25557 | 0x63D5 | 2 | Maximum Reactive power : Q3 | var | S32
25559 | 0x63D7 | 2 | Date of maximum Q3 | - | DATETIME
25561 | 0x63D9 | 2 | Maximum Apparent power : S1 | VA | U32
25563 | 0x63DB | 2 | Date of maximum S1 | - | DATETIME
25565 | 0x63DD | 2 | Maximum Apparent power : S2 | VA | U32
25567 | 0x63DF | 2 | Date of maximum S2 | - | DATETIME
25569 | 0x63E1 | 2 | Maximum Apparent power : S3 | VA | U32
25571 | 0x63E3 | 2 | Date of maximum S3 | - | DATETIME
25573 | 0x63E5 | 1 | Maximum Power factor : PF1 | - / 1000 | S16
25574 | 0x63E6 | 1 | Maximum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
25575 | 0x63E7 | 2 | Date of maximum PF1 | - | DATETIME
25577 | 0x63E9 | 1 | Maximum Power factor : PF2 | - / 1000 | S16
25578 | 0x63EA | 1 | Maximum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
25579 | 0x63EB | 2 | Date of maximum PF2 | - | DATETIME
25581 | 0x63ED | 1 | Maximum Power factor : PF3 | - / 1000 | S16
25582 | 0x63EE | 1 | Maximum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
25583 | 0x63EF | 2 | Date of maximum PF3 | - | DATETIME

## Avg. measurement min - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
19456 | 0x4C00 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
19456 | 0x4C00 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
19457 | 0x4C01 | 2 | Minimum Frequency | Hz / 1000 | U32
19459 | 0x4C03 | 2 | Date of minimum F | - | DATETIME
19461 | 0x4C05 | 2 | Minimum Ph-N Voltage : V1 | V / 100 | U32
19463 | 0x4C07 | 2 | Date of minimum V1 | - | DATETIME
19465 | 0x4C09 | 2 | Minimum Ph-N Voltage : V2 | V / 100 | U32
19467 | 0x4C0B | 2 | Date of minimum V2 | - | DATETIME
19469 | 0x4C0D | 2 | Minimum Ph-N Voltage : V3 | V / 100 | U32
19471 | 0x4C0F | 2 | Date of minimum V3 | - | DATETIME
19473 | 0x4C11 | 2 | Minimum Ph-N Voltage : Vn | V / 100 | U32
19475 | 0x4C13 | 2 | Date of minimum Vn | - | DATETIME
19477 | 0x4C15 | 2 | Minimum Ph-Ph Voltage : U12 | V / 100 | U32
19479 | 0x4C17 | 2 | Date of minimum U12 | - | DATETIME
19481 | 0x4C19 | 2 | Minimum Ph-Ph Voltage : U23 | V / 100 | U32
19483 | 0x4C1B | 2 | Date of minimum U23 | - | DATETIME
19485 | 0x4C1D | 2 | Minimum Ph-Ph Voltage : U31 | V / 100 | U32
19487 | 0x4C1F | 2 | Date of minimum U31 | - | DATETIME
19489 | 0x4C21 | 2 | Minimum Current : I1 | A / 1000 | U32
19491 | 0x4C23 | 2 | Date of minimum I1 | - | DATETIME
19493 | 0x4C25 | 2 | Minimum Current : I2 | A / 1000 | U32
19495 | 0x4C27 | 2 | Date of minimum I2 | - | DATETIME
19497 | 0x4C29 | 2 | Minimum Current : I3 | A / 1000 | U32
19499 | 0x4C2B | 2 | Date of minimum I3 | - | DATETIME
19501 | 0x4C2D | 2 | Minimum Current : In | A / 1000 | U32
19503 | 0x4C2F | 2 | Date of minimum In | - | DATETIME
19505 | 0x4C31 | 2 | Minimum Total active power | W | S32
19507 | 0x4C33 | 2 | Date of minimum Ptot | - | DATETIME
19509 | 0x4C35 | 2 | Minimum Total reactive power | var | S32
19511 | 0x4C37 | 2 | Date of minimum Qtot | - | DATETIME
19513 | 0x4C39 | 2 | Minimum Total apparent power | VA | U32
19515 | 0x4C3B | 2 | Date of minimum Stot | - | DATETIME
19517 | 0x4C3D | 1 | Minimum Total power factor | - / 1000 | S16
19518 | 0x4C3E | 1 | Minimum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
19519 | 0x4C3F | 2 | Date of minimum Total power factor | - | DATETIME
19521 | 0x4C41 | 2 | Minimum Active power : P1 | W | S32
19523 | 0x4C43 | 2 | Date of minimum P1 | - | DATETIME
19525 | 0x4C45 | 2 | Minimum Active power : P2 | W | S32
19527 | 0x4C47 | 2 | Date of minimum P2 | - | DATETIME
19529 | 0x4C49 | 2 | Minimum Active power : P3 | W | S32
19531 | 0x4C4B | 2 | Date of minimum P3 | - | DATETIME
19533 | 0x4C4D | 2 | Minimum Reactive power : Q1 | var | S32
19535 | 0x4C4F | 2 | Date of minimum Q1 | - | DATETIME
19537 | 0x4C51 | 2 | Minimum Reactive power : Q2 | var | S32
19539 | 0x4C53 | 2 | Date of minimum Q2 | - | DATETIME
19541 | 0x4C55 | 2 | Minimum Reactive power : Q3 | var | S32
19543 | 0x4C57 | 2 | Date of minimum Q3 | - | DATETIME
19545 | 0x4C59 | 2 | Minimum Apparent power : S1 | VA | U32
19547 | 0x4C5B | 2 | Date of minimum S1 | - | DATETIME
19549 | 0x4C5D | 2 | Minimum Apparent power : S2 | VA | U32
19551 | 0x4C5F | 2 | Date of minimum S2 | - | DATETIME
19553 | 0x4C61 | 2 | Minimum Apparent power : S3 | VA | U32
19555 | 0x4C63 | 2 | Date of minimum S3 | - | DATETIME
19557 | 0x4C65 | 1 | Minimum Power factor : PF1 | - / 1000 | S16
19558 | 0x4C66 | 1 | Minimum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
19559 | 0x4C67 | 2 | Date of minimum PF1 | - | DATETIME
19561 | 0x4C69 | 1 | Minimum Power factor : PF2 | - / 1000 | S16
19562 | 0x4C6A | 1 | Minimum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
19563 | 0x4C6B | 2 | Date of minimum PF2 | - | DATETIME
19565 | 0x4C6D | 1 | Minimum Power factor : PF3 | - / 1000 | S16
19566 | 0x4C6E | 1 | Minimum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
19567 | 0x4C6F | 2 | Date of minimum PF3 | - | DATETIME

## Avg. measurement min - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
21504 | 0x5400 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
21504 | 0x5400 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
21505 | 0x5401 | 2 | Minimum Frequency | Hz / 1000 | U32
21507 | 0x5403 | 2 | Date of minimum F | - | DATETIME
21509 | 0x5405 | 2 | Minimum Ph-N Voltage : V1 | V / 100 | U32
21511 | 0x5407 | 2 | Date of minimum V1 | - | DATETIME
21513 | 0x5409 | 2 | Minimum Ph-N Voltage : V2 | V / 100 | U32
21515 | 0x540B | 2 | Date of minimum V2 | - | DATETIME
21517 | 0x540D | 2 | Minimum Ph-N Voltage : V3 | V / 100 | U32
21519 | 0x540F | 2 | Date of minimum V3 | - | DATETIME
21521 | 0x5411 | 2 | Minimum Ph-N Voltage : Vn | V / 100 | U32
21523 | 0x5413 | 2 | Date of minimum Vn | - | DATETIME
21525 | 0x5415 | 2 | Minimum Ph-Ph Voltage : U12 | V / 100 | U32
21527 | 0x5417 | 2 | Date of minimum U12 | - | DATETIME
21529 | 0x5419 | 2 | Minimum Ph-Ph Voltage : U23 | V / 100 | U32
21531 | 0x541B | 2 | Date of minimum U23 | - | DATETIME
21533 | 0x541D | 2 | Minimum Ph-Ph Voltage : U31 | V / 100 | U32
21535 | 0x541F | 2 | Date of minimum U31 | - | DATETIME
21537 | 0x5421 | 2 | Minimum Current : I1 | A / 1000 | U32
21539 | 0x5423 | 2 | Date of minimum I1 | - | DATETIME
21541 | 0x5425 | 2 | Minimum Current : I2 | A / 1000 | U32
21543 | 0x5427 | 2 | Date of minimum I2 | - | DATETIME
21545 | 0x5429 | 2 | Minimum Current : I3 | A / 1000 | U32
21547 | 0x542B | 2 | Date of minimum I3 | - | DATETIME
21549 | 0x542D | 2 | Minimum Current : In | A / 1000 | U32
21551 | 0x542F | 2 | Date of minimum In | - | DATETIME
21553 | 0x5431 | 2 | Minimum Total active power | W | S32
21555 | 0x5433 | 2 | Date of minimum Ptot | - | DATETIME
21557 | 0x5435 | 2 | Minimum Total reactive power | var | S32
21559 | 0x5437 | 2 | Date of minimum Qtot | - | DATETIME
21561 | 0x5439 | 2 | Minimum Total apparent power | VA | U32
21563 | 0x543B | 2 | Date of minimum Stot | - | DATETIME
21565 | 0x543D | 1 | Minimum Total power factor | - / 1000 | S16
21566 | 0x543E | 1 | Minimum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
21567 | 0x543F | 2 | Date of minimum Total power factor | - | DATETIME
21569 | 0x5441 | 2 | Minimum Active power : P1 | W | S32
21571 | 0x5443 | 2 | Date of minimum P1 | - | DATETIME
21573 | 0x5445 | 2 | Minimum Active power : P2 | W | S32
21575 | 0x5447 | 2 | Date of minimum P2 | - | DATETIME
21577 | 0x5449 | 2 | Minimum Active power : P3 | W | S32
21579 | 0x544B | 2 | Date of minimum P3 | - | DATETIME
21581 | 0x544D | 2 | Minimum Reactive power : Q1 | var | S32
21583 | 0x544F | 2 | Date of minimum Q1 | - | DATETIME
21585 | 0x5451 | 2 | Minimum Reactive power : Q2 | var | S32
21587 | 0x5453 | 2 | Date of minimum Q2 | - | DATETIME
21589 | 0x5455 | 2 | Minimum Reactive power : Q3 | var | S32
21591 | 0x5457 | 2 | Date of minimum Q3 | - | DATETIME
21593 | 0x5459 | 2 | Minimum Apparent power : S1 | VA | U32
21595 | 0x545B | 2 | Date of minimum S1 | - | DATETIME
21597 | 0x545D | 2 | Minimum Apparent power : S2 | VA | U32
21599 | 0x545F | 2 | Date of minimum S2 | - | DATETIME
21601 | 0x5461 | 2 | Minimum Apparent power : S3 | VA | U32
21603 | 0x5463 | 2 | Date of minimum S3 | - | DATETIME
21605 | 0x5465 | 1 | Minimum Power factor : PF1 | - / 1000 | S16
21606 | 0x5466 | 1 | Minimum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
21607 | 0x5467 | 2 | Date of minimum PF1 | - | DATETIME
21609 | 0x5469 | 1 | Minimum Power factor : PF2 | - / 1000 | S16
21610 | 0x546A | 1 | Minimum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
21611 | 0x546B | 2 | Date of minimum PF2 | - | DATETIME
21613 | 0x546D | 1 | Minimum Power factor : PF3 | - / 1000 | S16
21614 | 0x546E | 1 | Minimum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
21615 | 0x546F | 2 | Date of minimum PF3 | - | DATETIME

## Avg. measurement min - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
23552 | 0x5C00 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
23552 | 0x5C00 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
23553 | 0x5C01 | 2 | Minimum Frequency | Hz / 1000 | U32
23555 | 0x5C03 | 2 | Date of minimum F | - | DATETIME
23557 | 0x5C05 | 2 | Minimum Ph-N Voltage : V1 | V / 100 | U32
23559 | 0x5C07 | 2 | Date of minimum V1 | - | DATETIME
23561 | 0x5C09 | 2 | Minimum Ph-N Voltage : V2 | V / 100 | U32
23563 | 0x5C0B | 2 | Date of minimum V2 | - | DATETIME
23565 | 0x5C0D | 2 | Minimum Ph-N Voltage : V3 | V / 100 | U32
23567 | 0x5C0F | 2 | Date of minimum V3 | - | DATETIME
23569 | 0x5C11 | 2 | Minimum Ph-N Voltage : Vn | V / 100 | U32
23571 | 0x5C13 | 2 | Date of minimum Vn | - | DATETIME
23573 | 0x5C15 | 2 | Minimum Ph-Ph Voltage : U12 | V / 100 | U32
23575 | 0x5C17 | 2 | Date of minimum U12 | - | DATETIME
23577 | 0x5C19 | 2 | Minimum Ph-Ph Voltage : U23 | V / 100 | U32
23579 | 0x5C1B | 2 | Date of minimum U23 | - | DATETIME
23581 | 0x5C1D | 2 | Minimum Ph-Ph Voltage : U31 | V / 100 | U32
23583 | 0x5C1F | 2 | Date of minimum U31 | - | DATETIME
23585 | 0x5C21 | 2 | Minimum Current : I1 | A / 1000 | U32
23587 | 0x5C23 | 2 | Date of minimum I1 | - | DATETIME
23589 | 0x5C25 | 2 | Minimum Current : I2 | A / 1000 | U32
23591 | 0x5C27 | 2 | Date of minimum I2 | - | DATETIME
23593 | 0x5C29 | 2 | Minimum Current : I3 | A / 1000 | U32
23595 | 0x5C2B | 2 | Date of minimum I3 | - | DATETIME
23597 | 0x5C2D | 2 | Minimum Current : In | A / 1000 | U32
23599 | 0x5C2F | 2 | Date of minimum In | - | DATETIME
23601 | 0x5C31 | 2 | Minimum Total active power | W | S32
23603 | 0x5C33 | 2 | Date of minimum Ptot | - | DATETIME
23605 | 0x5C35 | 2 | Minimum Total reactive power | var | S32
23607 | 0x5C37 | 2 | Date of minimum Qtot | - | DATETIME
23609 | 0x5C39 | 2 | Minimum Total apparent power | VA | U32
23611 | 0x5C3B | 2 | Date of minimum Stot | - | DATETIME
23613 | 0x5C3D | 1 | Minimum Total power factor | - / 1000 | S16
23614 | 0x5C3E | 1 | Minimum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
23615 | 0x5C3F | 2 | Date of minimum Total power factor | - | DATETIME
23617 | 0x5C41 | 2 | Minimum Active power : P1 | W | S32
23619 | 0x5C43 | 2 | Date of minimum P1 | - | DATETIME
23621 | 0x5C45 | 2 | Minimum Active power : P2 | W | S32
23623 | 0x5C47 | 2 | Date of minimum P2 | - | DATETIME
23625 | 0x5C49 | 2 | Minimum Active power : P3 | W | S32
23627 | 0x5C4B | 2 | Date of minimum P3 | - | DATETIME
23629 | 0x5C4D | 2 | Minimum Reactive power : Q1 | var | S32
23631 | 0x5C4F | 2 | Date of minimum Q1 | - | DATETIME
23633 | 0x5C51 | 2 | Minimum Reactive power : Q2 | var | S32
23635 | 0x5C53 | 2 | Date of minimum Q2 | - | DATETIME
23637 | 0x5C55 | 2 | Minimum Reactive power : Q3 | var | S32
23639 | 0x5C57 | 2 | Date of minimum Q3 | - | DATETIME
23641 | 0x5C59 | 2 | Minimum Apparent power : S1 | VA | U32
23643 | 0x5C5B | 2 | Date of minimum S1 | - | DATETIME
23645 | 0x5C5D | 2 | Minimum Apparent power : S2 | VA | U32
23647 | 0x5C5F | 2 | Date of minimum S2 | - | DATETIME
23649 | 0x5C61 | 2 | Minimum Apparent power : S3 | VA | U32
23651 | 0x5C63 | 2 | Date of minimum S3 | - | DATETIME
23653 | 0x5C65 | 1 | Minimum Power factor : PF1 | - / 1000 | S16
23654 | 0x5C66 | 1 | Minimum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
23655 | 0x5C67 | 2 | Date of minimum PF1 | - | DATETIME
23657 | 0x5C69 | 1 | Minimum Power factor : PF2 | - / 1000 | S16
23658 | 0x5C6A | 1 | Minimum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
23659 | 0x5C6B | 2 | Date of minimum PF2 | - | DATETIME
23661 | 0x5C6D | 1 | Minimum Power factor : PF3 | - / 1000 | S16
23662 | 0x5C6E | 1 | Minimum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
23663 | 0x5C6F | 2 | Date of minimum PF3 | - | DATETIME

## Avg. measurement min - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
25600 | 0x6400 | Info | 113 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
25600 | 0x6400 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
25601 | 0x6401 | 2 | Minimum Frequency | Hz / 1000 | U32
25603 | 0x6403 | 2 | Date of minimum F | - | DATETIME
25605 | 0x6405 | 2 | Minimum Ph-N Voltage : V1 | V / 100 | U32
25607 | 0x6407 | 2 | Date of minimum V1 | - | DATETIME
25609 | 0x6409 | 2 | Minimum Ph-N Voltage : V2 | V / 100 | U32
25611 | 0x640B | 2 | Date of minimum V2 | - | DATETIME
25613 | 0x640D | 2 | Minimum Ph-N Voltage : V3 | V / 100 | U32
25615 | 0x640F | 2 | Date of minimum V3 | - | DATETIME
25617 | 0x6411 | 2 | Minimum Ph-N Voltage : Vn | V / 100 | U32
25619 | 0x6413 | 2 | Date of minimum Vn | - | DATETIME
25621 | 0x6415 | 2 | Minimum Ph-Ph Voltage : U12 | V / 100 | U32
25623 | 0x6417 | 2 | Date of minimum U12 | - | DATETIME
25625 | 0x6419 | 2 | Minimum Ph-Ph Voltage : U23 | V / 100 | U32
25627 | 0x641B | 2 | Date of minimum U23 | - | DATETIME
25629 | 0x641D | 2 | Minimum Ph-Ph Voltage : U31 | V / 100 | U32
25631 | 0x641F | 2 | Date of minimum U31 | - | DATETIME
25633 | 0x6421 | 2 | Minimum Current : I1 | A / 1000 | U32
25635 | 0x6423 | 2 | Date of minimum I1 | - | DATETIME
25637 | 0x6425 | 2 | Minimum Current : I2 | A / 1000 | U32
25639 | 0x6427 | 2 | Date of minimum I2 | - | DATETIME
25641 | 0x6429 | 2 | Minimum Current : I3 | A / 1000 | U32
25643 | 0x642B | 2 | Date of minimum I3 | - | DATETIME
25645 | 0x642D | 2 | Minimum Current : In | A / 1000 | U32
25647 | 0x642F | 2 | Date of minimum In | - | DATETIME
25649 | 0x6431 | 2 | Minimum Total active power | W | S32
25651 | 0x6433 | 2 | Date of minimum Ptot | - | DATETIME
25653 | 0x6435 | 2 | Minimum Total reactive power | var | S32
25655 | 0x6437 | 2 | Date of minimum Qtot | - | DATETIME
25657 | 0x6439 | 2 | Minimum Total apparent power | VA | U32
25659 | 0x643B | 2 | Date of minimum Stot | - | DATETIME
25661 | 0x643D | 1 | Minimum Total power factor | - / 1000 | S16
25662 | 0x643E | 1 | Minimum Total Power factor type 0 : undefined 1 : leading 2 : lagging | - | U8
25663 | 0x643F | 2 | Date of minimum Total power factor | - | DATETIME
25665 | 0x6441 | 2 | Minimum Active power : P1 | W | S32
25667 | 0x6443 | 2 | Date of minimum P1 | - | DATETIME
25669 | 0x6445 | 2 | Minimum Active power : P2 | W | S32
25671 | 0x6447 | 2 | Date of minimum P2 | - | DATETIME
25673 | 0x6449 | 2 | Minimum Active power : P3 | W | S32
25675 | 0x644B | 2 | Date of minimum P3 | - | DATETIME
25677 | 0x644D | 2 | Minimum Reactive power : Q1 | var | S32
25679 | 0x644F | 2 | Date of minimum Q1 | - | DATETIME
25681 | 0x6451 | 2 | Minimum Reactive power : Q2 | var | S32
25683 | 0x6453 | 2 | Date of minimum Q2 | - | DATETIME
25685 | 0x6455 | 2 | Minimum Reactive power : Q3 | var | S32
25687 | 0x6457 | 2 | Date of minimum Q3 | - | DATETIME
25689 | 0x6459 | 2 | Minimum Apparent power : S1 | VA | U32
25691 | 0x645B | 2 | Date of minimum S1 | - | DATETIME
25693 | 0x645D | 2 | Minimum Apparent power : S2 | VA | U32
25695 | 0x645F | 2 | Date of minimum S2 | - | DATETIME
25697 | 0x6461 | 2 | Minimum Apparent power : S3 | VA | U32
25699 | 0x6463 | 2 | Date of minimum S3 | - | DATETIME
25701 | 0x6465 | 1 | Minimum Power factor : PF1 | - / 1000 | S16
25702 | 0x6466 | 1 | Minimum Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
25703 | 0x6467 | 2 | Date of minimum PF1 | - | DATETIME
25705 | 0x6469 | 1 | Minimum Power factor : PF2 | - / 1000 | S16
25706 | 0x646A | 1 | Minimum Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
25707 | 0x646B | 2 | Date of minimum PF2 | - | DATETIME
25709 | 0x646D | 1 | Minimum Power factor : PF3 | - / 1000 | S16
25710 | 0x646E | 1 | Minimum Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8
25711 | 0x646F | 2 | Date of minimum PF3 | - | DATETIME

## Inst. quality min/max - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
19584 | 0x4C80 | Info | 91 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
19584 | 0x4C80 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
19585 | 0x4C81 | 1 | Maximum total harmonic distortion : THD I1 | % / 100 | U16
19586 | 0x4C82 | 2 | Date of last maximum THD I1 | - | DATETIME
19588 | 0x4C84 | 1 | Maximum total harmonic distortion : THD I2 | % / 100 | U16
19589 | 0x4C85 | 2 | Date of last maximum THD I2 | - | DATETIME
19591 | 0x4C87 | 1 | Maximum total harmonic distortion : THD I3 | % / 100 | U16
19592 | 0x4C88 | 2 | Date of last maximum THD I3 | - | DATETIME
19594 | 0x4C8A | 1 | Maximum total harmonic distortion : THD In | % / 100 | U16
19595 | 0x4C8B | 2 | Date of last maximum THD In | - | DATETIME
19597 | 0x4C8D | 1 | Maximum Inba | % / 100 | U16
19598 | 0x4C8E | 2 | Date of maximum Inba | - | DATETIME
19600 | 0x4C90 | 1 | Maximum Inb | % / 100 | U16
19601 | 0x4C91 | 2 | Date of maximum Inb | - | DATETIME
19603 | 0x4C93 | 1 | Maximum Phi I1 / V1 | ? / 100 | S16
19604 | 0x4C94 | 2 | Date of maximum Phi I1 / V1 | - | DATETIME
19606 | 0x4C96 | 1 | Maximum Phi I2 / V2 | ? / 100 | S16
19607 | 0x4C97 | 2 | Date of maximum Phi I2 / V2 | - | DATETIME
19609 | 0x4C99 | 1 | Maximum Phi I3 / V3 | ? / 100 | S16
19610 | 0x4C9A | 2 | Date of maximum Phi I3 / V3 | - | DATETIME
19612 | 0x4C9C | 1 | Maximum Phi In / Vn | - / 100 | S16
19613 | 0x4C9D | 2 | Date of maximum Phi In / Vn | - | DATETIME
19615 | 0x4C9F | 1 | Minimum total harmonic distortion : THD I1 | % / 100 | U16
19616 | 0x4CA0 | 2 | Date of last minimum THD I1 | - | DATETIME
19618 | 0x4CA2 | 1 | Minimum total harmonic distortion : THD I2 | % / 100 | U16
19619 | 0x4CA3 | 2 | Date of last minimum THD I2 | - | DATETIME
19621 | 0x4CA5 | 1 | Minimum total harmonic distortion : THD I3 | % / 100 | U16
19622 | 0x4CA6 | 2 | Date of last minimum THD I3 | - | DATETIME
19624 | 0x4CA8 | 1 | Minimum total harmonic distortion : THD In | % / 100 | U16
19625 | 0x4CA9 | 2 | Date of last minimum THD In | - | DATETIME
19627 | 0x4CAB | 1 | Minimum Inba | % / 100 | U16
19628 | 0x4CAC | 2 | Date of minimum Inba | - | DATETIME
19630 | 0x4CAE | 1 | Minimum Inb | % / 100 | U16
19631 | 0x4CAF | 2 | Date of minimum Inb | - | DATETIME
19633 | 0x4CB1 | 1 | Minimum Phi I1 / V1 | ? / 100 | S16
19634 | 0x4CB2 | 2 | Date of minimum Phi I1 / V1 | - | DATETIME
19636 | 0x4CB4 | 1 | Minimum Phi I2 / V2 | ? / 100 | S16
19637 | 0x4CB5 | 2 | Date of minimum Phi I2 / V2 | - | DATETIME
19639 | 0x4CB7 | 1 | Minimum Phi I3 / V3 | ? / 100 | S16
19640 | 0x4CB8 | 2 | Date of minimum Phi I3 / V3 | - | DATETIME
19642 | 0x4CBA | 1 | Minimum Phi In / Vn | - / 100 | S16
19643 | 0x4CBB | 2 | Date of minimum Phi In / Vn | - | DATETIME
19645 | 0x4CBD | 1 | Maximum total harmonic distortion : THD Isys | % / 100 | U16
19646 | 0x4CBE | 2 | Date of last maximum THD Isys | - | DATETIME
19648 | 0x4CC0 | 1 | Maximum crest factor I1 | - / 1000 | U16
19649 | 0x4CC1 | 2 | Date of maximum crest factor I1 | - | DATETIME
19651 | 0x4CC3 | 1 | Maximum crest factor I2 | - / 1000 | U16
19652 | 0x4CC4 | 2 | Date of maximum crest factor I2 | - | DATETIME
19654 | 0x4CC6 | 1 | Maximum crest factor I3 | - / 1000 | U16
19655 | 0x4CC7 | 2 | Date of maximum crest factor I3 | - | DATETIME
19657 | 0x4CC9 | 1 | Maximum crest factor In | - / 1000 | U16
19658 | 0x4CCA | 2 | Date of maximum crest factor In | - | DATETIME
19660 | 0x4CCC | 1 | Minimum crest factor I1 | - / 1000 | U16
19661 | 0x4CCD | 2 | Date of minimum crest factor I1 | - | DATETIME
19663 | 0x4CCF | 1 | Minimum crest factor I2 | - / 1000 | U16
19664 | 0x4CD0 | 2 | Date of minimum crest factor I2 | - | DATETIME
19666 | 0x4CD2 | 1 | Minimum crest factor I3 | - / 1000 | U16
19667 | 0x4CD3 | 2 | Date of minimum crest factor I3 | - | DATETIME
19669 | 0x4CD5 | 1 | Minimum crest factor In | - / 1000 | U16
19670 | 0x4CD6 | 2 | Date of minimum crest factor In | - | DATETIME
19672 | 0x4CD8 | 1 | Minimum total harmonic distortion : THD Isys | % / 100 | U16
19673 | 0x4CD9 | 2 | Date of last minimum THD Isys | - | DATETIME

## Inst. quality min/max - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
21632 | 0x5480 | Info | 91 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
21632 | 0x5480 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
21633 | 0x5481 | 1 | Maximum total harmonic distortion : THD I1 | % / 100 | U16
21634 | 0x5482 | 2 | Date of last maximum THD I1 | - | DATETIME
21636 | 0x5484 | 1 | Maximum total harmonic distortion : THD I2 | % / 100 | U16
21637 | 0x5485 | 2 | Date of last maximum THD I2 | - | DATETIME
21639 | 0x5487 | 1 | Maximum total harmonic distortion : THD I3 | % / 100 | U16
21640 | 0x5488 | 2 | Date of last maximum THD I3 | - | DATETIME
21642 | 0x548A | 1 | Maximum total harmonic distortion : THD In | % / 100 | U16
21643 | 0x548B | 2 | Date of last maximum THD In | - | DATETIME
21645 | 0x548D | 1 | Maximum Inba | % / 100 | U16
21646 | 0x548E | 2 | Date of maximum Inba | - | DATETIME
21648 | 0x5490 | 1 | Maximum Inb | % / 100 | U16
21649 | 0x5491 | 2 | Date of maximum Inb | - | DATETIME
21651 | 0x5493 | 1 | Maximum Phi I1 / V1 | ? / 100 | S16
21652 | 0x5494 | 2 | Date of maximum Phi I1 / V1 | - | DATETIME
21654 | 0x5496 | 1 | Maximum Phi I2 / V2 | ? / 100 | S16
21655 | 0x5497 | 2 | Date of maximum Phi I2 / V2 | - | DATETIME
21657 | 0x5499 | 1 | Maximum Phi I3 / V3 | ? / 100 | S16
21658 | 0x549A | 2 | Date of maximum Phi I3 / V3 | - | DATETIME
21660 | 0x549C | 1 | Maximum Phi In / Vn | - / 100 | S16
21661 | 0x549D | 2 | Date of maximum Phi In / Vn | - | DATETIME
21663 | 0x549F | 1 | Minimum total harmonic distortion : THD I1 | % / 100 | U16
21664 | 0x54A0 | 2 | Date of last minimum THD I1 | - | DATETIME
21666 | 0x54A2 | 1 | Minimum total harmonic distortion : THD I2 | % / 100 | U16
21667 | 0x54A3 | 2 | Date of last minimum THD I2 | - | DATETIME
21669 | 0x54A5 | 1 | Minimum total harmonic distortion : THD I3 | % / 100 | U16
21670 | 0x54A6 | 2 | Date of last minimum THD I3 | - | DATETIME
21672 | 0x54A8 | 1 | Minimum total harmonic distortion : THD In | % / 100 | U16
21673 | 0x54A9 | 2 | Date of last minimum THD In | - | DATETIME
21675 | 0x54AB | 1 | Minimum Inba | % / 100 | U16
21676 | 0x54AC | 2 | Date of minimum Inba | - | DATETIME
21678 | 0x54AE | 1 | Minimum Inb | % / 100 | U16
21679 | 0x54AF | 2 | Date of minimum Inb | - | DATETIME
21681 | 0x54B1 | 1 | Minimum Phi I1 / V1 | ? / 100 | S16
21682 | 0x54B2 | 2 | Date of minimum Phi I1 / V1 | - | DATETIME
21684 | 0x54B4 | 1 | Minimum Phi I2 / V2 | ? / 100 | S16
21685 | 0x54B5 | 2 | Date of minimum Phi I2 / V2 | - | DATETIME
21687 | 0x54B7 | 1 | Minimum Phi I3 / V3 | ? / 100 | S16
21688 | 0x54B8 | 2 | Date of minimum Phi I3 / V3 | - | DATETIME
21690 | 0x54BA | 1 | Minimum Phi In / Vn | - / 100 | S16
21691 | 0x54BB | 2 | Date of minimum Phi In / Vn | - | DATETIME
21693 | 0x54BD | 1 | Maximum total harmonic distortion : THD Isys | % / 100 | U16
21694 | 0x54BE | 2 | Date of last maximum THD Isys | - | DATETIME
21696 | 0x54C0 | 1 | Maximum crest factor I1 | - / 1000 | U16
21697 | 0x54C1 | 2 | Date of maximum crest factor I1 | - | DATETIME
21699 | 0x54C3 | 1 | Maximum crest factor I2 | - / 1000 | U16
21700 | 0x54C4 | 2 | Date of maximum crest factor I2 | - | DATETIME
21702 | 0x54C6 | 1 | Maximum crest factor I3 | - / 1000 | U16
21703 | 0x54C7 | 2 | Date of maximum crest factor I3 | - | DATETIME
21705 | 0x54C9 | 1 | Maximum crest factor In | - / 1000 | U16
21706 | 0x54CA | 2 | Date of maximum crest factor In | - | DATETIME
21708 | 0x54CC | 1 | Minimum crest factor I1 | - / 1000 | U16
21709 | 0x54CD | 2 | Date of minimum crest factor I1 | - | DATETIME
21711 | 0x54CF | 1 | Minimum crest factor I2 | - / 1000 | U16
21712 | 0x54D0 | 2 | Date of minimum crest factor I2 | - | DATETIME
21714 | 0x54D2 | 1 | Minimum crest factor I3 | - / 1000 | U16
21715 | 0x54D3 | 2 | Date of minimum crest factor I3 | - | DATETIME
21717 | 0x54D5 | 1 | Minimum crest factor In | - / 1000 | U16
21718 | 0x54D6 | 2 | Date of minimum crest factor In | - | DATETIME
21720 | 0x54D8 | 1 | Minimum total harmonic distortion : THD Isys | % / 100 | U16
21721 | 0x54D9 | 2 | Date of last minimum THD Isys | - | DATETIME

## Inst. quality min/max - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
23680 | 0x5C80 | Info | 91 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
23680 | 0x5C80 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
23681 | 0x5C81 | 1 | Maximum total harmonic distortion : THD I1 | % / 100 | U16
23682 | 0x5C82 | 2 | Date of last maximum THD I1 | - | DATETIME
23684 | 0x5C84 | 1 | Maximum total harmonic distortion : THD I2 | % / 100 | U16
23685 | 0x5C85 | 2 | Date of last maximum THD I2 | - | DATETIME
23687 | 0x5C87 | 1 | Maximum total harmonic distortion : THD I3 | % / 100 | U16
23688 | 0x5C88 | 2 | Date of last maximum THD I3 | - | DATETIME
23690 | 0x5C8A | 1 | Maximum total harmonic distortion : THD In | % / 100 | U16
23691 | 0x5C8B | 2 | Date of last maximum THD In | - | DATETIME
23693 | 0x5C8D | 1 | Maximum Inba | % / 100 | U16
23694 | 0x5C8E | 2 | Date of maximum Inba | - | DATETIME
23696 | 0x5C90 | 1 | Maximum Inb | % / 100 | U16
23697 | 0x5C91 | 2 | Date of maximum Inb | - | DATETIME
23699 | 0x5C93 | 1 | Maximum Phi I1 / V1 | ? / 100 | S16
23700 | 0x5C94 | 2 | Date of maximum Phi I1 / V1 | - | DATETIME
23702 | 0x5C96 | 1 | Maximum Phi I2 / V2 | ? / 100 | S16
23703 | 0x5C97 | 2 | Date of maximum Phi I2 / V2 | - | DATETIME
23705 | 0x5C99 | 1 | Maximum Phi I3 / V3 | ? / 100 | S16
23706 | 0x5C9A | 2 | Date of maximum Phi I3 / V3 | - | DATETIME
23708 | 0x5C9C | 1 | Maximum Phi In / Vn | - / 100 | S16
23709 | 0x5C9D | 2 | Date of maximum Phi In / Vn | - | DATETIME
23711 | 0x5C9F | 1 | Minimum total harmonic distortion : THD I1 | % / 100 | U16
23712 | 0x5CA0 | 2 | Date of last minimum THD I1 | - | DATETIME
23714 | 0x5CA2 | 1 | Minimum total harmonic distortion : THD I2 | % / 100 | U16
23715 | 0x5CA3 | 2 | Date of last minimum THD I2 | - | DATETIME
23717 | 0x5CA5 | 1 | Minimum total harmonic distortion : THD I3 | % / 100 | U16
23718 | 0x5CA6 | 2 | Date of last minimum THD I3 | - | DATETIME
23720 | 0x5CA8 | 1 | Minimum total harmonic distortion : THD In | % / 100 | U16
23721 | 0x5CA9 | 2 | Date of last minimum THD In | - | DATETIME
23723 | 0x5CAB | 1 | Minimum Inba | % / 100 | U16
23724 | 0x5CAC | 2 | Date of minimum Inba | - | DATETIME
23726 | 0x5CAE | 1 | Minimum Inb | % / 100 | U16
23727 | 0x5CAF | 2 | Date of minimum Inb | - | DATETIME
23729 | 0x5CB1 | 1 | Minimum Phi I1 / V1 | ? / 100 | S16
23730 | 0x5CB2 | 2 | Date of minimum Phi I1 / V1 | - | DATETIME
23732 | 0x5CB4 | 1 | Minimum Phi I2 / V2 | ? / 100 | S16
23733 | 0x5CB5 | 2 | Date of minimum Phi I2 / V2 | - | DATETIME
23735 | 0x5CB7 | 1 | Minimum Phi I3 / V3 | ? / 100 | S16
23736 | 0x5CB8 | 2 | Date of minimum Phi I3 / V3 | - | DATETIME
23738 | 0x5CBA | 1 | Minimum Phi In / Vn | - / 100 | S16
23739 | 0x5CBB | 2 | Date of minimum Phi In / Vn | - | DATETIME
23741 | 0x5CBD | 1 | Maximum total harmonic distortion : THD Isys | % / 100 | U16
23742 | 0x5CBE | 2 | Date of last maximum THD Isys | - | DATETIME
23744 | 0x5CC0 | 1 | Maximum crest factor I1 | - / 1000 | U16
23745 | 0x5CC1 | 2 | Date of maximum crest factor I1 | - | DATETIME
23747 | 0x5CC3 | 1 | Maximum crest factor I2 | - / 1000 | U16
23748 | 0x5CC4 | 2 | Date of maximum crest factor I2 | - | DATETIME
23750 | 0x5CC6 | 1 | Maximum crest factor I3 | - / 1000 | U16
23751 | 0x5CC7 | 2 | Date of maximum crest factor I3 | - | DATETIME
23753 | 0x5CC9 | 1 | Maximum crest factor In | - / 1000 | U16
23754 | 0x5CCA | 2 | Date of maximum crest factor In | - | DATETIME
23756 | 0x5CCC | 1 | Minimum crest factor I1 | - / 1000 | U16
23757 | 0x5CCD | 2 | Date of minimum crest factor I1 | - | DATETIME
23759 | 0x5CCF | 1 | Minimum crest factor I2 | - / 1000 | U16
23760 | 0x5CD0 | 2 | Date of minimum crest factor I2 | - | DATETIME
23762 | 0x5CD2 | 1 | Minimum crest factor I3 | - / 1000 | U16
23763 | 0x5CD3 | 2 | Date of minimum crest factor I3 | - | DATETIME
23765 | 0x5CD5 | 1 | Minimum crest factor In | - / 1000 | U16
23766 | 0x5CD6 | 2 | Date of minimum crest factor In | - | DATETIME
23768 | 0x5CD8 | 1 | Minimum total harmonic distortion : THD Isys | % / 100 | U16
23769 | 0x5CD9 | 2 | Date of last minimum THD Isys | - | DATETIME

## Inst. quality min/max - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
25728 | 0x6480 | Info | 91 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
25728 | 0x6480 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
25729 | 0x6481 | 1 | Maximum total harmonic distortion : THD I1 | % / 100 | U16
25730 | 0x6482 | 2 | Date of last maximum THD I1 | - | DATETIME
25732 | 0x6484 | 1 | Maximum total harmonic distortion : THD I2 | % / 100 | U16
25733 | 0x6485 | 2 | Date of last maximum THD I2 | - | DATETIME
25735 | 0x6487 | 1 | Maximum total harmonic distortion : THD I3 | % / 100 | U16
25736 | 0x6488 | 2 | Date of last maximum THD I3 | - | DATETIME
25738 | 0x648A | 1 | Maximum total harmonic distortion : THD In | % / 100 | U16
25739 | 0x648B | 2 | Date of last maximum THD In | - | DATETIME
25741 | 0x648D | 1 | Maximum Inba | % / 100 | U16
25742 | 0x648E | 2 | Date of maximum Inba | - | DATETIME
25744 | 0x6490 | 1 | Maximum Inb | % / 100 | U16
25745 | 0x6491 | 2 | Date of maximum Inb | - | DATETIME
25747 | 0x6493 | 1 | Maximum Phi I1 / V1 | ? / 100 | S16
25748 | 0x6494 | 2 | Date of maximum Phi I1 / V1 | - | DATETIME
25750 | 0x6496 | 1 | Maximum Phi I2 / V2 | ? / 100 | S16
25751 | 0x6497 | 2 | Date of maximum Phi I2 / V2 | - | DATETIME
25753 | 0x6499 | 1 | Maximum Phi I3 / V3 | ? / 100 | S16
25754 | 0x649A | 2 | Date of maximum Phi I3 / V3 | - | DATETIME
25756 | 0x649C | 1 | Maximum Phi In / Vn | - / 100 | S16
25757 | 0x649D | 2 | Date of maximum Phi In / Vn | - | DATETIME
25759 | 0x649F | 1 | Minimum total harmonic distortion : THD I1 | % / 100 | U16
25760 | 0x64A0 | 2 | Date of last minimum THD I1 | - | DATETIME
25762 | 0x64A2 | 1 | Minimum total harmonic distortion : THD I2 | % / 100 | U16
25763 | 0x64A3 | 2 | Date of last minimum THD I2 | - | DATETIME
25765 | 0x64A5 | 1 | Minimum total harmonic distortion : THD I3 | % / 100 | U16
25766 | 0x64A6 | 2 | Date of last minimum THD I3 | - | DATETIME
25768 | 0x64A8 | 1 | Minimum total harmonic distortion : THD In | % / 100 | U16
25769 | 0x64A9 | 2 | Date of last minimum THD In | - | DATETIME
25771 | 0x64AB | 1 | Minimum Inba | % / 100 | U16
25772 | 0x64AC | 2 | Date of minimum Inba | - | DATETIME
25774 | 0x64AE | 1 | Minimum Inb | % / 100 | U16
25775 | 0x64AF | 2 | Date of minimum Inb | - | DATETIME
25777 | 0x64B1 | 1 | Minimum Phi I1 / V1 | ? / 100 | S16
25778 | 0x64B2 | 2 | Date of minimum Phi I1 / V1 | - | DATETIME
25780 | 0x64B4 | 1 | Minimum Phi I2 / V2 | ? / 100 | S16
25781 | 0x64B5 | 2 | Date of minimum Phi I2 / V2 | - | DATETIME
25783 | 0x64B7 | 1 | Minimum Phi I3 / V3 | ? / 100 | S16
25784 | 0x64B8 | 2 | Date of minimum Phi I3 / V3 | - | DATETIME
25786 | 0x64BA | 1 | Minimum Phi In / Vn | - / 100 | S16
25787 | 0x64BB | 2 | Date of minimum Phi In / Vn | - | DATETIME
25789 | 0x64BD | 1 | Maximum total harmonic distortion : THD Isys | % / 100 | U16
25790 | 0x64BE | 2 | Date of last maximum THD Isys | - | DATETIME
25792 | 0x64C0 | 1 | Maximum crest factor I1 | - / 1000 | U16
25793 | 0x64C1 | 2 | Date of maximum crest factor I1 | - | DATETIME
25795 | 0x64C3 | 1 | Maximum crest factor I2 | - / 1000 | U16
25796 | 0x64C4 | 2 | Date of maximum crest factor I2 | - | DATETIME
25798 | 0x64C6 | 1 | Maximum crest factor I3 | - / 1000 | U16
25799 | 0x64C7 | 2 | Date of maximum crest factor I3 | - | DATETIME
25801 | 0x64C9 | 1 | Maximum crest factor In | - / 1000 | U16
25802 | 0x64CA | 2 | Date of maximum crest factor In | - | DATETIME
25804 | 0x64CC | 1 | Minimum crest factor I1 | - / 1000 | U16
25805 | 0x64CD | 2 | Date of minimum crest factor I1 | - | DATETIME
25807 | 0x64CF | 1 | Minimum crest factor I2 | - / 1000 | U16
25808 | 0x64D0 | 2 | Date of minimum crest factor I2 | - | DATETIME
25810 | 0x64D2 | 1 | Minimum crest factor I3 | - / 1000 | U16
25811 | 0x64D3 | 2 | Date of minimum crest factor I3 | - | DATETIME
25813 | 0x64D5 | 1 | Minimum crest factor In | - / 1000 | U16
25814 | 0x64D6 | 2 | Date of minimum crest factor In | - | DATETIME
25816 | 0x64D8 | 1 | Minimum total harmonic distortion : THD Isys | % / 100 | U16
25817 | 0x64D9 | 2 | Date of last minimum THD Isys | - | DATETIME

## Inst. I harmonics - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
19712 | 0x4D00 | Info | 109 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
19712 | 0x4D00 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
19713 | 0x4D01 | 1 | harmonic I1 row 2 | % / 100 | U16
19714 | 0x4D02 | 1 | harmonic I2 row 2 | % / 100 | U16
19715 | 0x4D03 | 1 | harmonic I3 row 2 | % / 100 | U16
19716 | 0x4D04 | 1 | harmonic In row 2 | % / 100 | U16
19717 | 0x4D05 | 1 | harmonic I1 row 3 | % / 100 | U16
19718 | 0x4D06 | 1 | harmonic I2 row 3 | % / 100 | U16
19719 | 0x4D07 | 1 | harmonic I3 row 3 | % / 100 | U16
19720 | 0x4D08 | 1 | harmonic In row 3 | % / 100 | U16
19721 | 0x4D09 | 1 | harmonic I1 row 4 | % / 100 | U16
19722 | 0x4D0A | 1 | harmonic I2 row 4 | % / 100 | U16
19723 | 0x4D0B | 1 | harmonic I3 row 4 | % / 100 | U16
19724 | 0x4D0C | 1 | harmonic In row 4 | % / 100 | U16
19725 | 0x4D0D | 1 | harmonic I1 row 5 | % / 100 | U16
19726 | 0x4D0E | 1 | harmonic I2 row 5 | % / 100 | U16
19727 | 0x4D0F | 1 | harmonic I3 row 5 | % / 100 | U16
19728 | 0x4D10 | 1 | harmonic In row 5 | % / 100 | U16
19729 | 0x4D11 | 1 | harmonic I1 row 6 | % / 100 | U16
19730 | 0x4D12 | 1 | harmonic I2 row 6 | % / 100 | U16
19731 | 0x4D13 | 1 | harmonic I3 row 6 | % / 100 | U16
19732 | 0x4D14 | 1 | harmonic In row 6 | % / 100 | U16
19733 | 0x4D15 | 1 | harmonic I1 row 7 | % / 100 | U16
19734 | 0x4D16 | 1 | harmonic I2 row 7 | % / 100 | U16
19735 | 0x4D17 | 1 | harmonic I3 row 7 | % / 100 | U16
19736 | 0x4D18 | 1 | harmonic In row 7 | % / 100 | U16
19737 | 0x4D19 | 1 | harmonic I1 row 8 | % / 100 | U16
19738 | 0x4D1A | 1 | harmonic I2 row 8 | % / 100 | U16
19739 | 0x4D1B | 1 | harmonic I3 row 8 | % / 100 | U16
19740 | 0x4D1C | 1 | harmonic In row 8 | % / 100 | U16
19741 | 0x4D1D | 1 | harmonic I1 row 9 | % / 100 | U16
19742 | 0x4D1E | 1 | harmonic I2 row 9 | % / 100 | U16
19743 | 0x4D1F | 1 | harmonic I3 row 9 | % / 100 | U16
19744 | 0x4D20 | 1 | harmonic In row 9 | % / 100 | U16
19745 | 0x4D21 | 1 | harmonic I1 row 10 | % / 100 | U16
19746 | 0x4D22 | 1 | harmonic I2 row 10 | % / 100 | U16
19747 | 0x4D23 | 1 | harmonic I3 row 10 | % / 100 | U16
19748 | 0x4D24 | 1 | harmonic In row 10 | % / 100 | U16
19749 | 0x4D25 | 1 | harmonic I1 row 11 | % / 100 | U16
19750 | 0x4D26 | 1 | harmonic I2 row 11 | % / 100 | U16
19751 | 0x4D27 | 1 | harmonic I3 row 11 | % / 100 | U16
19752 | 0x4D28 | 1 | harmonic In row 11 | % / 100 | U16
19753 | 0x4D29 | 1 | harmonic I1 row 12 | % / 100 | U16
19754 | 0x4D2A | 1 | harmonic I2 row 12 | % / 100 | U16
19755 | 0x4D2B | 1 | harmonic I3 row 12 | % / 100 | U16
19756 | 0x4D2C | 1 | harmonic In row 12 | % / 100 | U16
19757 | 0x4D2D | 1 | harmonic I1 row 13 | % / 100 | U16
19758 | 0x4D2E | 1 | harmonic I2 row 13 | % / 100 | U16
19759 | 0x4D2F | 1 | harmonic I3 row 13 | % / 100 | U16
19760 | 0x4D30 | 1 | harmonic In row 13 | % / 100 | U16
19761 | 0x4D31 | 1 | harmonic I1 row 14 | % / 100 | U16
19762 | 0x4D32 | 1 | harmonic I2 row 14 | % / 100 | U16
19763 | 0x4D33 | 1 | harmonic I3 row 14 | % / 100 | U16
19764 | 0x4D34 | 1 | harmonic In row 14 | % / 100 | U16
19765 | 0x4D35 | 1 | harmonic I1 row 15 | % / 100 | U16
19766 | 0x4D36 | 1 | harmonic I2 row 15 | % / 100 | U16
19767 | 0x4D37 | 1 | harmonic I3 row 15 | % / 100 | U16
19768 | 0x4D38 | 1 | harmonic In row 15 | % / 100 | U16
19769 | 0x4D39 | 1 | harmonic I1 row 16 | % / 100 | U16
19770 | 0x4D3A | 1 | harmonic I2 row 16 | % / 100 | U16
19771 | 0x4D3B | 1 | harmonic I3 row 16 | % / 100 | U16
19772 | 0x4D3C | 1 | harmonic In row 16 | % / 100 | U16
19773 | 0x4D3D | 1 | harmonic I1 row 17 | % / 100 | U16
19774 | 0x4D3E | 1 | harmonic I2 row 17 | % / 100 | U16
19775 | 0x4D3F | 1 | harmonic I3 row 17 | % / 100 | U16
19776 | 0x4D40 | 1 | harmonic In row 17 | % / 100 | U16
19777 | 0x4D41 | 1 | harmonic I1 row 18 | % / 100 | U16
19778 | 0x4D42 | 1 | harmonic I2 row 18 | % / 100 | U16
19779 | 0x4D43 | 1 | harmonic I3 row 18 | % / 100 | U16
19780 | 0x4D44 | 1 | harmonic In row 18 | % / 100 | U16
19781 | 0x4D45 | 1 | harmonic I1 row 19 | % / 100 | U16
19782 | 0x4D46 | 1 | harmonic I2 row 19 | % / 100 | U16
19783 | 0x4D47 | 1 | harmonic I3 row 19 | % / 100 | U16
19784 | 0x4D48 | 1 | harmonic In row 19 | % / 100 | U16
19785 | 0x4D49 | 1 | harmonic I1 row 20 | % / 100 | U16
19786 | 0x4D4A | 1 | harmonic I2 row 20 | % / 100 | U16
19787 | 0x4D4B | 1 | harmonic I3 row 20 | % / 100 | U16
19788 | 0x4D4C | 1 | harmonic In row 20 | % / 100 | U16
19789 | 0x4D4D | 1 | harmonic I1 row 21 | % / 100 | U16
19790 | 0x4D4E | 1 | harmonic I2 row 21 | % / 100 | U16
19791 | 0x4D4F | 1 | harmonic I3 row 21 | % / 100 | U16
19792 | 0x4D50 | 1 | harmonic In row 21 | % / 100 | U16
19793 | 0x4D51 | 1 | harmonic I1 row 22 | % / 100 | U16
19794 | 0x4D52 | 1 | harmonic I2 row 22 | % / 100 | U16
19795 | 0x4D53 | 1 | harmonic I3 row 22 | % / 100 | U16
19796 | 0x4D54 | 1 | harmonic In row 22 | % / 100 | U16
19797 | 0x4D55 | 1 | harmonic I1 row 23 | % / 100 | U16
19798 | 0x4D56 | 1 | harmonic I2 row 23 | % / 100 | U16
19799 | 0x4D57 | 1 | harmonic I3 row 23 | % / 100 | U16
19800 | 0x4D58 | 1 | harmonic In row 23 | % / 100 | U16
19801 | 0x4D59 | 1 | harmonic I1 row 24 | % / 100 | U16
19802 | 0x4D5A | 1 | harmonic I2 row 24 | % / 100 | U16
19803 | 0x4D5B | 1 | harmonic I3 row 24 | % / 100 | U16
19804 | 0x4D5C | 1 | harmonic In row 24 | % / 100 | U16
19805 | 0x4D5D | 1 | harmonic I1 row 25 | % / 100 | U16
19806 | 0x4D5E | 1 | harmonic I2 row 25 | % / 100 | U16
19807 | 0x4D5F | 1 | harmonic I3 row 25 | % / 100 | U16
19808 | 0x4D60 | 1 | harmonic In row 25 | % / 100 | U16
19809 | 0x4D61 | 1 | harmonic I1 row 26 to 34 | % / 100 | U16
19810 | 0x4D62 | 1 | harmonic I2 row 26 to 34 | % / 100 | U16
19811 | 0x4D63 | 1 | harmonic I3 row 26 to 34 | % / 100 | U16
19812 | 0x4D64 | 1 | harmonic In row 26 to 34 | % / 100 | U16
19813 | 0x4D65 | 1 | harmonic I1 row 35 to 50 | % / 100 | U16
19814 | 0x4D66 | 1 | harmonic I2 row 35 to 50 | % / 100 | U16
19815 | 0x4D67 | 1 | harmonic I3 row 35 to 50 | % / 100 | U16
19816 | 0x4D68 | 1 | harmonic In row 35 to 50 | % / 100 | U16
19817 | 0x4D69 | 1 | harmonic I1 row 51 to 63 | % / 100 | U16
19818 | 0x4D6A | 1 | harmonic I2 row 51 to 63 | % / 100 | U16
19819 | 0x4D6B | 1 | harmonic I3 row 51 to 63 | % / 100 | U16
19820 | 0x4D6C | 1 | harmonic In row 51 to 63 | % / 100 | U16

## Inst. I harmonics - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
21760 | 0x5500 | Info | 109 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
21760 | 0x5500 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
21761 | 0x5501 | 1 | harmonic I1 row 2 | % / 100 | U16
21762 | 0x5502 | 1 | harmonic I2 row 2 | % / 100 | U16
21763 | 0x5503 | 1 | harmonic I3 row 2 | % / 100 | U16
21764 | 0x5504 | 1 | harmonic In row 2 | % / 100 | U16
21765 | 0x5505 | 1 | harmonic I1 row 3 | % / 100 | U16
21766 | 0x5506 | 1 | harmonic I2 row 3 | % / 100 | U16
21767 | 0x5507 | 1 | harmonic I3 row 3 | % / 100 | U16
21768 | 0x5508 | 1 | harmonic In row 3 | % / 100 | U16
21769 | 0x5509 | 1 | harmonic I1 row 4 | % / 100 | U16
21770 | 0x550A | 1 | harmonic I2 row 4 | % / 100 | U16
21771 | 0x550B | 1 | harmonic I3 row 4 | % / 100 | U16
21772 | 0x550C | 1 | harmonic In row 4 | % / 100 | U16
21773 | 0x550D | 1 | harmonic I1 row 5 | % / 100 | U16
21774 | 0x550E | 1 | harmonic I2 row 5 | % / 100 | U16
21775 | 0x550F | 1 | harmonic I3 row 5 | % / 100 | U16
21776 | 0x5510 | 1 | harmonic In row 5 | % / 100 | U16
21777 | 0x5511 | 1 | harmonic I1 row 6 | % / 100 | U16
21778 | 0x5512 | 1 | harmonic I2 row 6 | % / 100 | U16
21779 | 0x5513 | 1 | harmonic I3 row 6 | % / 100 | U16
21780 | 0x5514 | 1 | harmonic In row 6 | % / 100 | U16
21781 | 0x5515 | 1 | harmonic I1 row 7 | % / 100 | U16
21782 | 0x5516 | 1 | harmonic I2 row 7 | % / 100 | U16
21783 | 0x5517 | 1 | harmonic I3 row 7 | % / 100 | U16
21784 | 0x5518 | 1 | harmonic In row 7 | % / 100 | U16
21785 | 0x5519 | 1 | harmonic I1 row 8 | % / 100 | U16
21786 | 0x551A | 1 | harmonic I2 row 8 | % / 100 | U16
21787 | 0x551B | 1 | harmonic I3 row 8 | % / 100 | U16
21788 | 0x551C | 1 | harmonic In row 8 | % / 100 | U16
21789 | 0x551D | 1 | harmonic I1 row 9 | % / 100 | U16
21790 | 0x551E | 1 | harmonic I2 row 9 | % / 100 | U16
21791 | 0x551F | 1 | harmonic I3 row 9 | % / 100 | U16
21792 | 0x5520 | 1 | harmonic In row 9 | % / 100 | U16
21793 | 0x5521 | 1 | harmonic I1 row 10 | % / 100 | U16
21794 | 0x5522 | 1 | harmonic I2 row 10 | % / 100 | U16
21795 | 0x5523 | 1 | harmonic I3 row 10 | % / 100 | U16
21796 | 0x5524 | 1 | harmonic In row 10 | % / 100 | U16
21797 | 0x5525 | 1 | harmonic I1 row 11 | % / 100 | U16
21798 | 0x5526 | 1 | harmonic I2 row 11 | % / 100 | U16
21799 | 0x5527 | 1 | harmonic I3 row 11 | % / 100 | U16
21800 | 0x5528 | 1 | harmonic In row 11 | % / 100 | U16
21801 | 0x5529 | 1 | harmonic I1 row 12 | % / 100 | U16
21802 | 0x552A | 1 | harmonic I2 row 12 | % / 100 | U16
21803 | 0x552B | 1 | harmonic I3 row 12 | % / 100 | U16
21804 | 0x552C | 1 | harmonic In row 12 | % / 100 | U16
21805 | 0x552D | 1 | harmonic I1 row 13 | % / 100 | U16
21806 | 0x552E | 1 | harmonic I2 row 13 | % / 100 | U16
21807 | 0x552F | 1 | harmonic I3 row 13 | % / 100 | U16
21808 | 0x5530 | 1 | harmonic In row 13 | % / 100 | U16
21809 | 0x5531 | 1 | harmonic I1 row 14 | % / 100 | U16
21810 | 0x5532 | 1 | harmonic I2 row 14 | % / 100 | U16
21811 | 0x5533 | 1 | harmonic I3 row 14 | % / 100 | U16
21812 | 0x5534 | 1 | harmonic In row 14 | % / 100 | U16
21813 | 0x5535 | 1 | harmonic I1 row 15 | % / 100 | U16
21814 | 0x5536 | 1 | harmonic I2 row 15 | % / 100 | U16
21815 | 0x5537 | 1 | harmonic I3 row 15 | % / 100 | U16
21816 | 0x5538 | 1 | harmonic In row 15 | % / 100 | U16
21817 | 0x5539 | 1 | harmonic I1 row 16 | % / 100 | U16
21818 | 0x553A | 1 | harmonic I2 row 16 | % / 100 | U16
21819 | 0x553B | 1 | harmonic I3 row 16 | % / 100 | U16
21820 | 0x553C | 1 | harmonic In row 16 | % / 100 | U16
21821 | 0x553D | 1 | harmonic I1 row 17 | % / 100 | U16
21822 | 0x553E | 1 | harmonic I2 row 17 | % / 100 | U16
21823 | 0x553F | 1 | harmonic I3 row 17 | % / 100 | U16
21824 | 0x5540 | 1 | harmonic In row 17 | % / 100 | U16
21825 | 0x5541 | 1 | harmonic I1 row 18 | % / 100 | U16
21826 | 0x5542 | 1 | harmonic I2 row 18 | % / 100 | U16
21827 | 0x5543 | 1 | harmonic I3 row 18 | % / 100 | U16
21828 | 0x5544 | 1 | harmonic In row 18 | % / 100 | U16
21829 | 0x5545 | 1 | harmonic I1 row 19 | % / 100 | U16
21830 | 0x5546 | 1 | harmonic I2 row 19 | % / 100 | U16
21831 | 0x5547 | 1 | harmonic I3 row 19 | % / 100 | U16
21832 | 0x5548 | 1 | harmonic In row 19 | % / 100 | U16
21833 | 0x5549 | 1 | harmonic I1 row 20 | % / 100 | U16
21834 | 0x554A | 1 | harmonic I2 row 20 | % / 100 | U16
21835 | 0x554B | 1 | harmonic I3 row 20 | % / 100 | U16
21836 | 0x554C | 1 | harmonic In row 20 | % / 100 | U16
21837 | 0x554D | 1 | harmonic I1 row 21 | % / 100 | U16
21838 | 0x554E | 1 | harmonic I2 row 21 | % / 100 | U16
21839 | 0x554F | 1 | harmonic I3 row 21 | % / 100 | U16
21840 | 0x5550 | 1 | harmonic In row 21 | % / 100 | U16
21841 | 0x5551 | 1 | harmonic I1 row 22 | % / 100 | U16
21842 | 0x5552 | 1 | harmonic I2 row 22 | % / 100 | U16
21843 | 0x5553 | 1 | harmonic I3 row 22 | % / 100 | U16
21844 | 0x5554 | 1 | harmonic In row 22 | % / 100 | U16
21845 | 0x5555 | 1 | harmonic I1 row 23 | % / 100 | U16
21846 | 0x5556 | 1 | harmonic I2 row 23 | % / 100 | U16
21847 | 0x5557 | 1 | harmonic I3 row 23 | % / 100 | U16
21848 | 0x5558 | 1 | harmonic In row 23 | % / 100 | U16
21849 | 0x5559 | 1 | harmonic I1 row 24 | % / 100 | U16
21850 | 0x555A | 1 | harmonic I2 row 24 | % / 100 | U16
21851 | 0x555B | 1 | harmonic I3 row 24 | % / 100 | U16
21852 | 0x555C | 1 | harmonic In row 24 | % / 100 | U16
21853 | 0x555D | 1 | harmonic I1 row 25 | % / 100 | U16
21854 | 0x555E | 1 | harmonic I2 row 25 | % / 100 | U16
21855 | 0x555F | 1 | harmonic I3 row 25 | % / 100 | U16
21856 | 0x5560 | 1 | harmonic In row 25 | % / 100 | U16
21857 | 0x5561 | 1 | harmonic I1 row 26 to 34 | % / 100 | U16
21858 | 0x5562 | 1 | harmonic I2 row 26 to 34 | % / 100 | U16
21859 | 0x5563 | 1 | harmonic I3 row 26 to 34 | % / 100 | U16
21860 | 0x5564 | 1 | harmonic In row 26 to 34 | % / 100 | U16
21861 | 0x5565 | 1 | harmonic I1 row 35 to 50 | % / 100 | U16
21862 | 0x5566 | 1 | harmonic I2 row 35 to 50 | % / 100 | U16
21863 | 0x5567 | 1 | harmonic I3 row 35 to 50 | % / 100 | U16
21864 | 0x5568 | 1 | harmonic In row 35 to 50 | % / 100 | U16
21865 | 0x5569 | 1 | harmonic I1 row 51 to 63 | % / 100 | U16
21866 | 0x556A | 1 | harmonic I2 row 51 to 63 | % / 100 | U16
21867 | 0x556B | 1 | harmonic I3 row 51 to 63 | % / 100 | U16
21868 | 0x556C | 1 | harmonic In row 51 to 63 | % / 100 | U16

## Inst. I harmonics - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
23808 | 0x5D00 | Info | 109 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
23808 | 0x5D00 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
23809 | 0x5D01 | 1 | harmonic I1 row 2 | % / 100 | U16
23810 | 0x5D02 | 1 | harmonic I2 row 2 | % / 100 | U16
23811 | 0x5D03 | 1 | harmonic I3 row 2 | % / 100 | U16
23812 | 0x5D04 | 1 | harmonic In row 2 | % / 100 | U16
23813 | 0x5D05 | 1 | harmonic I1 row 3 | % / 100 | U16
23814 | 0x5D06 | 1 | harmonic I2 row 3 | % / 100 | U16
23815 | 0x5D07 | 1 | harmonic I3 row 3 | % / 100 | U16
23816 | 0x5D08 | 1 | harmonic In row 3 | % / 100 | U16
23817 | 0x5D09 | 1 | harmonic I1 row 4 | % / 100 | U16
23818 | 0x5D0A | 1 | harmonic I2 row 4 | % / 100 | U16
23819 | 0x5D0B | 1 | harmonic I3 row 4 | % / 100 | U16
23820 | 0x5D0C | 1 | harmonic In row 4 | % / 100 | U16
23821 | 0x5D0D | 1 | harmonic I1 row 5 | % / 100 | U16
23822 | 0x5D0E | 1 | harmonic I2 row 5 | % / 100 | U16
23823 | 0x5D0F | 1 | harmonic I3 row 5 | % / 100 | U16
23824 | 0x5D10 | 1 | harmonic In row 5 | % / 100 | U16
23825 | 0x5D11 | 1 | harmonic I1 row 6 | % / 100 | U16
23826 | 0x5D12 | 1 | harmonic I2 row 6 | % / 100 | U16
23827 | 0x5D13 | 1 | harmonic I3 row 6 | % / 100 | U16
23828 | 0x5D14 | 1 | harmonic In row 6 | % / 100 | U16
23829 | 0x5D15 | 1 | harmonic I1 row 7 | % / 100 | U16
23830 | 0x5D16 | 1 | harmonic I2 row 7 | % / 100 | U16
23831 | 0x5D17 | 1 | harmonic I3 row 7 | % / 100 | U16
23832 | 0x5D18 | 1 | harmonic In row 7 | % / 100 | U16
23833 | 0x5D19 | 1 | harmonic I1 row 8 | % / 100 | U16
23834 | 0x5D1A | 1 | harmonic I2 row 8 | % / 100 | U16
23835 | 0x5D1B | 1 | harmonic I3 row 8 | % / 100 | U16
23836 | 0x5D1C | 1 | harmonic In row 8 | % / 100 | U16
23837 | 0x5D1D | 1 | harmonic I1 row 9 | % / 100 | U16
23838 | 0x5D1E | 1 | harmonic I2 row 9 | % / 100 | U16
23839 | 0x5D1F | 1 | harmonic I3 row 9 | % / 100 | U16
23840 | 0x5D20 | 1 | harmonic In row 9 | % / 100 | U16
23841 | 0x5D21 | 1 | harmonic I1 row 10 | % / 100 | U16
23842 | 0x5D22 | 1 | harmonic I2 row 10 | % / 100 | U16
23843 | 0x5D23 | 1 | harmonic I3 row 10 | % / 100 | U16
23844 | 0x5D24 | 1 | harmonic In row 10 | % / 100 | U16
23845 | 0x5D25 | 1 | harmonic I1 row 11 | % / 100 | U16
23846 | 0x5D26 | 1 | harmonic I2 row 11 | % / 100 | U16
23847 | 0x5D27 | 1 | harmonic I3 row 11 | % / 100 | U16
23848 | 0x5D28 | 1 | harmonic In row 11 | % / 100 | U16
23849 | 0x5D29 | 1 | harmonic I1 row 12 | % / 100 | U16
23850 | 0x5D2A | 1 | harmonic I2 row 12 | % / 100 | U16
23851 | 0x5D2B | 1 | harmonic I3 row 12 | % / 100 | U16
23852 | 0x5D2C | 1 | harmonic In row 12 | % / 100 | U16
23853 | 0x5D2D | 1 | harmonic I1 row 13 | % / 100 | U16
23854 | 0x5D2E | 1 | harmonic I2 row 13 | % / 100 | U16
23855 | 0x5D2F | 1 | harmonic I3 row 13 | % / 100 | U16
23856 | 0x5D30 | 1 | harmonic In row 13 | % / 100 | U16
23857 | 0x5D31 | 1 | harmonic I1 row 14 | % / 100 | U16
23858 | 0x5D32 | 1 | harmonic I2 row 14 | % / 100 | U16
23859 | 0x5D33 | 1 | harmonic I3 row 14 | % / 100 | U16
23860 | 0x5D34 | 1 | harmonic In row 14 | % / 100 | U16
23861 | 0x5D35 | 1 | harmonic I1 row 15 | % / 100 | U16
23862 | 0x5D36 | 1 | harmonic I2 row 15 | % / 100 | U16
23863 | 0x5D37 | 1 | harmonic I3 row 15 | % / 100 | U16
23864 | 0x5D38 | 1 | harmonic In row 15 | % / 100 | U16
23865 | 0x5D39 | 1 | harmonic I1 row 16 | % / 100 | U16
23866 | 0x5D3A | 1 | harmonic I2 row 16 | % / 100 | U16
23867 | 0x5D3B | 1 | harmonic I3 row 16 | % / 100 | U16
23868 | 0x5D3C | 1 | harmonic In row 16 | % / 100 | U16
23869 | 0x5D3D | 1 | harmonic I1 row 17 | % / 100 | U16
23870 | 0x5D3E | 1 | harmonic I2 row 17 | % / 100 | U16
23871 | 0x5D3F | 1 | harmonic I3 row 17 | % / 100 | U16
23872 | 0x5D40 | 1 | harmonic In row 17 | % / 100 | U16
23873 | 0x5D41 | 1 | harmonic I1 row 18 | % / 100 | U16
23874 | 0x5D42 | 1 | harmonic I2 row 18 | % / 100 | U16
23875 | 0x5D43 | 1 | harmonic I3 row 18 | % / 100 | U16
23876 | 0x5D44 | 1 | harmonic In row 18 | % / 100 | U16
23877 | 0x5D45 | 1 | harmonic I1 row 19 | % / 100 | U16
23878 | 0x5D46 | 1 | harmonic I2 row 19 | % / 100 | U16
23879 | 0x5D47 | 1 | harmonic I3 row 19 | % / 100 | U16
23880 | 0x5D48 | 1 | harmonic In row 19 | % / 100 | U16
23881 | 0x5D49 | 1 | harmonic I1 row 20 | % / 100 | U16
23882 | 0x5D4A | 1 | harmonic I2 row 20 | % / 100 | U16
23883 | 0x5D4B | 1 | harmonic I3 row 20 | % / 100 | U16
23884 | 0x5D4C | 1 | harmonic In row 20 | % / 100 | U16
23885 | 0x5D4D | 1 | harmonic I1 row 21 | % / 100 | U16
23886 | 0x5D4E | 1 | harmonic I2 row 21 | % / 100 | U16
23887 | 0x5D4F | 1 | harmonic I3 row 21 | % / 100 | U16
23888 | 0x5D50 | 1 | harmonic In row 21 | % / 100 | U16
23889 | 0x5D51 | 1 | harmonic I1 row 22 | % / 100 | U16
23890 | 0x5D52 | 1 | harmonic I2 row 22 | % / 100 | U16
23891 | 0x5D53 | 1 | harmonic I3 row 22 | % / 100 | U16
23892 | 0x5D54 | 1 | harmonic In row 22 | % / 100 | U16
23893 | 0x5D55 | 1 | harmonic I1 row 23 | % / 100 | U16
23894 | 0x5D56 | 1 | harmonic I2 row 23 | % / 100 | U16
23895 | 0x5D57 | 1 | harmonic I3 row 23 | % / 100 | U16
23896 | 0x5D58 | 1 | harmonic In row 23 | % / 100 | U16
23897 | 0x5D59 | 1 | harmonic I1 row 24 | % / 100 | U16
23898 | 0x5D5A | 1 | harmonic I2 row 24 | % / 100 | U16
23899 | 0x5D5B | 1 | harmonic I3 row 24 | % / 100 | U16
23900 | 0x5D5C | 1 | harmonic In row 24 | % / 100 | U16
23901 | 0x5D5D | 1 | harmonic I1 row 25 | % / 100 | U16
23902 | 0x5D5E | 1 | harmonic I2 row 25 | % / 100 | U16
23903 | 0x5D5F | 1 | harmonic I3 row 25 | % / 100 | U16
23904 | 0x5D60 | 1 | harmonic In row 25 | % / 100 | U16
23905 | 0x5D61 | 1 | harmonic I1 row 26 to 34 | % / 100 | U16
23906 | 0x5D62 | 1 | harmonic I2 row 26 to 34 | % / 100 | U16
23907 | 0x5D63 | 1 | harmonic I3 row 26 to 34 | % / 100 | U16
23908 | 0x5D64 | 1 | harmonic In row 26 to 34 | % / 100 | U16
23909 | 0x5D65 | 1 | harmonic I1 row 35 to 50 | % / 100 | U16
23910 | 0x5D66 | 1 | harmonic I2 row 35 to 50 | % / 100 | U16
23911 | 0x5D67 | 1 | harmonic I3 row 35 to 50 | % / 100 | U16
23912 | 0x5D68 | 1 | harmonic In row 35 to 50 | % / 100 | U16
23913 | 0x5D69 | 1 | harmonic I1 row 51 to 63 | % / 100 | U16
23914 | 0x5D6A | 1 | harmonic I2 row 51 to 63 | % / 100 | U16
23915 | 0x5D6B | 1 | harmonic I3 row 51 to 63 | % / 100 | U16
23916 | 0x5D6C | 1 | harmonic In row 51 to 63 | % / 100 | U16

## Inst. I harmonics - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
25856 | 0x6500 | Info | 109 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
25856 | 0x6500 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
25857 | 0x6501 | 1 | harmonic I1 row 2 | % / 100 | U16
25858 | 0x6502 | 1 | harmonic I2 row 2 | % / 100 | U16
25859 | 0x6503 | 1 | harmonic I3 row 2 | % / 100 | U16
25860 | 0x6504 | 1 | harmonic In row 2 | % / 100 | U16
25861 | 0x6505 | 1 | harmonic I1 row 3 | % / 100 | U16
25862 | 0x6506 | 1 | harmonic I2 row 3 | % / 100 | U16
25863 | 0x6507 | 1 | harmonic I3 row 3 | % / 100 | U16
25864 | 0x6508 | 1 | harmonic In row 3 | % / 100 | U16
25865 | 0x6509 | 1 | harmonic I1 row 4 | % / 100 | U16
25866 | 0x650A | 1 | harmonic I2 row 4 | % / 100 | U16
25867 | 0x650B | 1 | harmonic I3 row 4 | % / 100 | U16
25868 | 0x650C | 1 | harmonic In row 4 | % / 100 | U16
25869 | 0x650D | 1 | harmonic I1 row 5 | % / 100 | U16
25870 | 0x650E | 1 | harmonic I2 row 5 | % / 100 | U16
25871 | 0x650F | 1 | harmonic I3 row 5 | % / 100 | U16
25872 | 0x6510 | 1 | harmonic In row 5 | % / 100 | U16
25873 | 0x6511 | 1 | harmonic I1 row 6 | % / 100 | U16
25874 | 0x6512 | 1 | harmonic I2 row 6 | % / 100 | U16
25875 | 0x6513 | 1 | harmonic I3 row 6 | % / 100 | U16
25876 | 0x6514 | 1 | harmonic In row 6 | % / 100 | U16
25877 | 0x6515 | 1 | harmonic I1 row 7 | % / 100 | U16
25878 | 0x6516 | 1 | harmonic I2 row 7 | % / 100 | U16
25879 | 0x6517 | 1 | harmonic I3 row 7 | % / 100 | U16
25880 | 0x6518 | 1 | harmonic In row 7 | % / 100 | U16
25881 | 0x6519 | 1 | harmonic I1 row 8 | % / 100 | U16
25882 | 0x651A | 1 | harmonic I2 row 8 | % / 100 | U16
25883 | 0x651B | 1 | harmonic I3 row 8 | % / 100 | U16
25884 | 0x651C | 1 | harmonic In row 8 | % / 100 | U16
25885 | 0x651D | 1 | harmonic I1 row 9 | % / 100 | U16
25886 | 0x651E | 1 | harmonic I2 row 9 | % / 100 | U16
25887 | 0x651F | 1 | harmonic I3 row 9 | % / 100 | U16
25888 | 0x6520 | 1 | harmonic In row 9 | % / 100 | U16
25889 | 0x6521 | 1 | harmonic I1 row 10 | % / 100 | U16
25890 | 0x6522 | 1 | harmonic I2 row 10 | % / 100 | U16
25891 | 0x6523 | 1 | harmonic I3 row 10 | % / 100 | U16
25892 | 0x6524 | 1 | harmonic In row 10 | % / 100 | U16
25893 | 0x6525 | 1 | harmonic I1 row 11 | % / 100 | U16
25894 | 0x6526 | 1 | harmonic I2 row 11 | % / 100 | U16
25895 | 0x6527 | 1 | harmonic I3 row 11 | % / 100 | U16
25896 | 0x6528 | 1 | harmonic In row 11 | % / 100 | U16
25897 | 0x6529 | 1 | harmonic I1 row 12 | % / 100 | U16
25898 | 0x652A | 1 | harmonic I2 row 12 | % / 100 | U16
25899 | 0x652B | 1 | harmonic I3 row 12 | % / 100 | U16
25900 | 0x652C | 1 | harmonic In row 12 | % / 100 | U16
25901 | 0x652D | 1 | harmonic I1 row 13 | % / 100 | U16
25902 | 0x652E | 1 | harmonic I2 row 13 | % / 100 | U16
25903 | 0x652F | 1 | harmonic I3 row 13 | % / 100 | U16
25904 | 0x6530 | 1 | harmonic In row 13 | % / 100 | U16
25905 | 0x6531 | 1 | harmonic I1 row 14 | % / 100 | U16
25906 | 0x6532 | 1 | harmonic I2 row 14 | % / 100 | U16
25907 | 0x6533 | 1 | harmonic I3 row 14 | % / 100 | U16
25908 | 0x6534 | 1 | harmonic In row 14 | % / 100 | U16
25909 | 0x6535 | 1 | harmonic I1 row 15 | % / 100 | U16
25910 | 0x6536 | 1 | harmonic I2 row 15 | % / 100 | U16
25911 | 0x6537 | 1 | harmonic I3 row 15 | % / 100 | U16
25912 | 0x6538 | 1 | harmonic In row 15 | % / 100 | U16
25913 | 0x6539 | 1 | harmonic I1 row 16 | % / 100 | U16
25914 | 0x653A | 1 | harmonic I2 row 16 | % / 100 | U16
25915 | 0x653B | 1 | harmonic I3 row 16 | % / 100 | U16
25916 | 0x653C | 1 | harmonic In row 16 | % / 100 | U16
25917 | 0x653D | 1 | harmonic I1 row 17 | % / 100 | U16
25918 | 0x653E | 1 | harmonic I2 row 17 | % / 100 | U16
25919 | 0x653F | 1 | harmonic I3 row 17 | % / 100 | U16
25920 | 0x6540 | 1 | harmonic In row 17 | % / 100 | U16
25921 | 0x6541 | 1 | harmonic I1 row 18 | % / 100 | U16
25922 | 0x6542 | 1 | harmonic I2 row 18 | % / 100 | U16
25923 | 0x6543 | 1 | harmonic I3 row 18 | % / 100 | U16
25924 | 0x6544 | 1 | harmonic In row 18 | % / 100 | U16
25925 | 0x6545 | 1 | harmonic I1 row 19 | % / 100 | U16
25926 | 0x6546 | 1 | harmonic I2 row 19 | % / 100 | U16
25927 | 0x6547 | 1 | harmonic I3 row 19 | % / 100 | U16
25928 | 0x6548 | 1 | harmonic In row 19 | % / 100 | U16
25929 | 0x6549 | 1 | harmonic I1 row 20 | % / 100 | U16
25930 | 0x654A | 1 | harmonic I2 row 20 | % / 100 | U16
25931 | 0x654B | 1 | harmonic I3 row 20 | % / 100 | U16
25932 | 0x654C | 1 | harmonic In row 20 | % / 100 | U16
25933 | 0x654D | 1 | harmonic I1 row 21 | % / 100 | U16
25934 | 0x654E | 1 | harmonic I2 row 21 | % / 100 | U16
25935 | 0x654F | 1 | harmonic I3 row 21 | % / 100 | U16
25936 | 0x6550 | 1 | harmonic In row 21 | % / 100 | U16
25937 | 0x6551 | 1 | harmonic I1 row 22 | % / 100 | U16
25938 | 0x6552 | 1 | harmonic I2 row 22 | % / 100 | U16
25939 | 0x6553 | 1 | harmonic I3 row 22 | % / 100 | U16
25940 | 0x6554 | 1 | harmonic In row 22 | % / 100 | U16
25941 | 0x6555 | 1 | harmonic I1 row 23 | % / 100 | U16
25942 | 0x6556 | 1 | harmonic I2 row 23 | % / 100 | U16
25943 | 0x6557 | 1 | harmonic I3 row 23 | % / 100 | U16
25944 | 0x6558 | 1 | harmonic In row 23 | % / 100 | U16
25945 | 0x6559 | 1 | harmonic I1 row 24 | % / 100 | U16
25946 | 0x655A | 1 | harmonic I2 row 24 | % / 100 | U16
25947 | 0x655B | 1 | harmonic I3 row 24 | % / 100 | U16
25948 | 0x655C | 1 | harmonic In row 24 | % / 100 | U16
25949 | 0x655D | 1 | harmonic I1 row 25 | % / 100 | U16
25950 | 0x655E | 1 | harmonic I2 row 25 | % / 100 | U16
25951 | 0x655F | 1 | harmonic I3 row 25 | % / 100 | U16
25952 | 0x6560 | 1 | harmonic In row 25 | % / 100 | U16
25953 | 0x6561 | 1 | harmonic I1 row 26 to 34 | % / 100 | U16
25954 | 0x6562 | 1 | harmonic I2 row 26 to 34 | % / 100 | U16
25955 | 0x6563 | 1 | harmonic I3 row 26 to 34 | % / 100 | U16
25956 | 0x6564 | 1 | harmonic In row 26 to 34 | % / 100 | U16
25957 | 0x6565 | 1 | harmonic I1 row 35 to 50 | % / 100 | U16
25958 | 0x6566 | 1 | harmonic I2 row 35 to 50 | % / 100 | U16
25959 | 0x6567 | 1 | harmonic I3 row 35 to 50 | % / 100 | U16
25960 | 0x6568 | 1 | harmonic In row 35 to 50 | % / 100 | U16
25961 | 0x6569 | 1 | harmonic I1 row 51 to 63 | % / 100 | U16
25962 | 0x656A | 1 | harmonic I2 row 51 to 63 | % / 100 | U16
25963 | 0x656B | 1 | harmonic I3 row 51 to 63 | % / 100 | U16
25964 | 0x656C | 1 | harmonic In row 51 to 63 | % / 100 | U16

## Energy measurement - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
19840 | 0x4D80 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
19840 | 0x4D80 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
19841 | 0x4D81 | 2 | Total Hour meter | s | U32
19843 | 0x4D83 | 2 | Total Positive active Energy : Ea+ | Wh / 0.001 | U32
19845 | 0x4D85 | 1 | Total Residual positive active Energy : rEa+ | Wh / 10 | U16
19846 | 0x4D86 | 2 | Total Negative active Energy : Ea- | Wh / 0.001 | U32
19848 | 0x4D88 | 1 | Total Residual negative active Energy : rEa- | Wh / 10 | U16
19849 | 0x4D89 | 2 | Total Positive reactive Energy : Er+ | varh / 0.001 | U32
19851 | 0x4D8B | 1 | Total Residual positive reactive Energy : rEr+ | varh / 10 | U16
19852 | 0x4D8C | 2 | Total Negative reactive Energy : Er- | varh / 0.001 | U32
19854 | 0x4D8E | 1 | Total Residual negative reactive Energy : rEr- | varh / 10 | U16
19855 | 0x4D8F | 2 | Total Apparent Energy : Eap | VAh / 0.001 | U32
19857 | 0x4D91 | 1 | Total Residual apparent Energy : rEap | VAh / 10 | U16
19858 | 0x4D92 | 2 | Total positive lagging reactive Energy : Er+ (lagging) | varh / 0.001 | U32
19860 | 0x4D94 | 1 | Total residual positive lagging reactive Energy : rEr+ (lagging) | varh / 10 | U16
19861 | 0x4D95 | 2 | Total negative lagging reactive Energy : Er- (lagging) | varh / 0.001 | U32
19863 | 0x4D97 | 1 | Total residual negative lagging reactive Energy : rEr- (lagging) | varh / 10 | U16
19864 | 0x4D98 | 2 | Total positive leading reactive Energy : Er+ (leading) | varh / 0.001 | U32
19866 | 0x4D9A | 1 | Total residual positive leading reactive Energy : rEr+ (leading) | varh / 10 | U16
19867 | 0x4D9B | 2 | Total negative leading reactive Energy : Er- (leading) | varh / 0.001 | U32
19869 | 0x4D9D | 1 | Total residual negative leading reactive Energy : rEr- (leading) | varh / 10 | U16
19870 | 0x4D9E | 2 | Partial Hour meter | s | U32
19872 | 0x4DA0 | 2 | Partial positive active Energy : Ea+ | Wh / 0.001 | U32
19874 | 0x4DA2 | 1 | Partial residual positive active Energy : rEa+ | Wh / 10 | U16
19875 | 0x4DA3 | 2 | Partial negative active Energy : Ea- | Wh / 0.001 | U32
19877 | 0x4DA5 | 1 | Partial residual negative active Energy : rEa- | Wh / 10 | U16
19878 | 0x4DA6 | 2 | Partial positive reactive Energy : Er+ | varh / 0.001 | U32
19880 | 0x4DA8 | 1 | Partial residual positive reactive Energy : rEr+ | varh / 10 | U16
19881 | 0x4DA9 | 2 | Partial negative reactive Energy : Er- | varh / 0.001 | U32
19883 | 0x4DAB | 1 | Partial residual negative reactive Energy : rEr- | varh / 10 | U16
19884 | 0x4DAC | 2 | Partial Apparent Energy : Eap | VAh / 0.001 | U32
19886 | 0x4DAE | 1 | Partial residual apparent Energy : rEap | VAh / 10 | U16
19887 | 0x4DAF | 2 | Last Partial Reset date | - | DATETIME
19889 | 0x4DB1 | 2 | Last Partial Hour meter | s | U32
19891 | 0x4DB3 | 2 | Last Partial positive active Energy : Ea+ | Wh / 0.001 | U32
19893 | 0x4DB5 | 1 | Last Partial residual positive active Energy : rEa+ | Wh / 10 | U16
19894 | 0x4DB6 | 2 | Last Partial negative active Energy : Ea- | Wh / 0.001 | U32
19896 | 0x4DB8 | 1 | Last Partial residual negative active Energy : rEa- | Wh / 10 | U16
19897 | 0x4DB9 | 2 | Last Partial positive reactive Energy : Er+ | varh / 0.001 | U32
19899 | 0x4DBB | 1 | Last Partial residual positive reactive Energy : rEr+ | varh / 10 | U16
19900 | 0x4DBC | 2 | Last Partial negative reactive Energy : Er- | varh / 0.001 | U32
19902 | 0x4DBE | 1 | Last Partial residual negative reactive Energy : rEr- | varh / 10 | U16
19903 | 0x4DBF | 2 | Last Partial Apparent Energy : Eap | VAh / 0.001 | U32
19905 | 0x4DC1 | 1 | Last Partial residual apparent Energy : rEap | VAh / 10 | U16

## Energy measurement - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
21888 | 0x5580 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
21888 | 0x5580 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
21889 | 0x5581 | 2 | Total Hour meter | s | U32
21891 | 0x5583 | 2 | Total Positive active Energy : Ea+ | Wh / 0.001 | U32
21893 | 0x5585 | 1 | Total Residual positive active Energy : rEa+ | Wh / 10 | U16
21894 | 0x5586 | 2 | Total Negative active Energy : Ea- | Wh / 0.001 | U32
21896 | 0x5588 | 1 | Total Residual negative active Energy : rEa- | Wh / 10 | U16
21897 | 0x5589 | 2 | Total Positive reactive Energy : Er+ | varh / 0.001 | U32
21899 | 0x558B | 1 | Total Residual positive reactive Energy : rEr+ | varh / 10 | U16
21900 | 0x558C | 2 | Total Negative reactive Energy : Er- | varh / 0.001 | U32
21902 | 0x558E | 1 | Total Residual negative reactive Energy : rEr- | varh / 10 | U16
21903 | 0x558F | 2 | Total Apparent Energy : Eap | VAh / 0.001 | U32
21905 | 0x5591 | 1 | Total Residual apparent Energy : rEap | VAh / 10 | U16
21906 | 0x5592 | 2 | Total positive lagging reactive Energy : Er+ (lagging) | varh / 0.001 | U32
21908 | 0x5594 | 1 | Total residual positive lagging reactive Energy : rEr+ (lagging) | varh / 10 | U16
21909 | 0x5595 | 2 | Total negative lagging reactive Energy : Er- (lagging) | varh / 0.001 | U32
21911 | 0x5597 | 1 | Total residual negative lagging reactive Energy : rEr- (lagging) | varh / 10 | U16
21912 | 0x5598 | 2 | Total positive leading reactive Energy : Er+ (leading) | varh / 0.001 | U32
21914 | 0x559A | 1 | Total residual positive leading reactive Energy : rEr+ (leading) | varh / 10 | U16
21915 | 0x559B | 2 | Total negative leading reactive Energy : Er- (leading) | varh / 0.001 | U32
21917 | 0x559D | 1 | Total residual negative leading reactive Energy : rEr- (leading) | varh / 10 | U16
21918 | 0x559E | 2 | Partial Hour meter | s | U32
21920 | 0x55A0 | 2 | Partial positive active Energy : Ea+ | Wh / 0.001 | U32
21922 | 0x55A2 | 1 | Partial residual positive active Energy : rEa+ | Wh / 10 | U16
21923 | 0x55A3 | 2 | Partial negative active Energy : Ea- | Wh / 0.001 | U32
21925 | 0x55A5 | 1 | Partial residual negative active Energy : rEa- | Wh / 10 | U16
21926 | 0x55A6 | 2 | Partial positive reactive Energy : Er+ | varh / 0.001 | U32
21928 | 0x55A8 | 1 | Partial residual positive reactive Energy : rEr+ | varh / 10 | U16
21929 | 0x55A9 | 2 | Partial negative reactive Energy : Er- | varh / 0.001 | U32
21931 | 0x55AB | 1 | Partial residual negative reactive Energy : rEr- | varh / 10 | U16
21932 | 0x55AC | 2 | Partial Apparent Energy : Eap | VAh / 0.001 | U32
21934 | 0x55AE | 1 | Partial residual apparent Energy : rEap | VAh / 10 | U16
21935 | 0x55AF | 2 | Last Partial Reset date | - | DATETIME
21937 | 0x55B1 | 2 | Last Partial Hour meter | s | U32
21939 | 0x55B3 | 2 | Last Partial positive active Energy : Ea+ | Wh / 0.001 | U32
21941 | 0x55B5 | 1 | Last Partial residual positive active Energy : rEa+ | Wh / 10 | U16
21942 | 0x55B6 | 2 | Last Partial negative active Energy : Ea- | Wh / 0.001 | U32
21944 | 0x55B8 | 1 | Last Partial residual negative active Energy : rEa- | Wh / 10 | U16
21945 | 0x55B9 | 2 | Last Partial positive reactive Energy : Er+ | varh / 0.001 | U32
21947 | 0x55BB | 1 | Last Partial residual positive reactive Energy : rEr+ | varh / 10 | U16
21948 | 0x55BC | 2 | Last Partial negative reactive Energy : Er- | varh / 0.001 | U32
21950 | 0x55BE | 1 | Last Partial residual negative reactive Energy : rEr- | varh / 10 | U16
21951 | 0x55BF | 2 | Last Partial Apparent Energy : Eap | VAh / 0.001 | U32
21953 | 0x55C1 | 1 | Last Partial residual apparent Energy : rEap | VAh / 10 | U16

## Energy measurement - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
23936 | 0x5D80 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
23936 | 0x5D80 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
23937 | 0x5D81 | 2 | Total Hour meter | s | U32
23939 | 0x5D83 | 2 | Total Positive active Energy : Ea+ | Wh / 0.001 | U32
23941 | 0x5D85 | 1 | Total Residual positive active Energy : rEa+ | Wh / 10 | U16
23942 | 0x5D86 | 2 | Total Negative active Energy : Ea- | Wh / 0.001 | U32
23944 | 0x5D88 | 1 | Total Residual negative active Energy : rEa- | Wh / 10 | U16
23945 | 0x5D89 | 2 | Total Positive reactive Energy : Er+ | varh / 0.001 | U32
23947 | 0x5D8B | 1 | Total Residual positive reactive Energy : rEr+ | varh / 10 | U16
23948 | 0x5D8C | 2 | Total Negative reactive Energy : Er- | varh / 0.001 | U32
23950 | 0x5D8E | 1 | Total Residual negative reactive Energy : rEr- | varh / 10 | U16
23951 | 0x5D8F | 2 | Total Apparent Energy : Eap | VAh / 0.001 | U32
23953 | 0x5D91 | 1 | Total Residual apparent Energy : rEap | VAh / 10 | U16
23954 | 0x5D92 | 2 | Total positive lagging reactive Energy : Er+ (lagging) | varh / 0.001 | U32
23956 | 0x5D94 | 1 | Total residual positive lagging reactive Energy : rEr+ (lagging) | varh / 10 | U16
23957 | 0x5D95 | 2 | Total negative lagging reactive Energy : Er- (lagging) | varh / 0.001 | U32
23959 | 0x5D97 | 1 | Total residual negative lagging reactive Energy : rEr- (lagging) | varh / 10 | U16
23960 | 0x5D98 | 2 | Total positive leading reactive Energy : Er+ (leading) | varh / 0.001 | U32
23962 | 0x5D9A | 1 | Total residual positive leading reactive Energy : rEr+ (leading) | varh / 10 | U16
23963 | 0x5D9B | 2 | Total negative leading reactive Energy : Er- (leading) | varh / 0.001 | U32
23965 | 0x5D9D | 1 | Total residual negative leading reactive Energy : rEr- (leading) | varh / 10 | U16
23966 | 0x5D9E | 2 | Partial Hour meter | s | U32
23968 | 0x5DA0 | 2 | Partial positive active Energy : Ea+ | Wh / 0.001 | U32
23970 | 0x5DA2 | 1 | Partial residual positive active Energy : rEa+ | Wh / 10 | U16
23971 | 0x5DA3 | 2 | Partial negative active Energy : Ea- | Wh / 0.001 | U32
23973 | 0x5DA5 | 1 | Partial residual negative active Energy : rEa- | Wh / 10 | U16
23974 | 0x5DA6 | 2 | Partial positive reactive Energy : Er+ | varh / 0.001 | U32
23976 | 0x5DA8 | 1 | Partial residual positive reactive Energy : rEr+ | varh / 10 | U16
23977 | 0x5DA9 | 2 | Partial negative reactive Energy : Er- | varh / 0.001 | U32
23979 | 0x5DAB | 1 | Partial residual negative reactive Energy : rEr- | varh / 10 | U16
23980 | 0x5DAC | 2 | Partial Apparent Energy : Eap | VAh / 0.001 | U32
23982 | 0x5DAE | 1 | Partial residual apparent Energy : rEap | VAh / 10 | U16
23983 | 0x5DAF | 2 | Last Partial Reset date | - | DATETIME
23985 | 0x5DB1 | 2 | Last Partial Hour meter | s | U32
23987 | 0x5DB3 | 2 | Last Partial positive active Energy : Ea+ | Wh / 0.001 | U32
23989 | 0x5DB5 | 1 | Last Partial residual positive active Energy : rEa+ | Wh / 10 | U16
23990 | 0x5DB6 | 2 | Last Partial negative active Energy : Ea- | Wh / 0.001 | U32
23992 | 0x5DB8 | 1 | Last Partial residual negative active Energy : rEa- | Wh / 10 | U16
23993 | 0x5DB9 | 2 | Last Partial positive reactive Energy : Er+ | varh / 0.001 | U32
23995 | 0x5DBB | 1 | Last Partial residual positive reactive Energy : rEr+ | varh / 10 | U16
23996 | 0x5DBC | 2 | Last Partial negative reactive Energy : Er- | varh / 0.001 | U32
23998 | 0x5DBE | 1 | Last Partial residual negative reactive Energy : rEr- | varh / 10 | U16
23999 | 0x5DBF | 2 | Last Partial Apparent Energy : Eap | VAh / 0.001 | U32
24001 | 0x5DC1 | 1 | Last Partial residual apparent Energy : rEap | VAh / 10 | U16

## Energy measurement - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
25984 | 0x6580 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
25984 | 0x6580 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
25985 | 0x6581 | 2 | Total Hour meter | s | U32
25987 | 0x6583 | 2 | Total Positive active Energy : Ea+ | Wh / 0.001 | U32
25989 | 0x6585 | 1 | Total Residual positive active Energy : rEa+ | Wh / 10 | U16
25990 | 0x6586 | 2 | Total Negative active Energy : Ea- | Wh / 0.001 | U32
25992 | 0x6588 | 1 | Total Residual negative active Energy : rEa- | Wh / 10 | U16
25993 | 0x6589 | 2 | Total Positive reactive Energy : Er+ | varh / 0.001 | U32
25995 | 0x658B | 1 | Total Residual positive reactive Energy : rEr+ | varh / 10 | U16
25996 | 0x658C | 2 | Total Negative reactive Energy : Er- | varh / 0.001 | U32
25998 | 0x658E | 1 | Total Residual negative reactive Energy : rEr- | varh / 10 | U16
25999 | 0x658F | 2 | Total Apparent Energy : Eap | VAh / 0.001 | U32
26001 | 0x6591 | 1 | Total Residual apparent Energy : rEap | VAh / 10 | U16
26002 | 0x6592 | 2 | Total positive lagging reactive Energy : Er+ (lagging) | varh / 0.001 | U32
26004 | 0x6594 | 1 | Total residual positive lagging reactive Energy : rEr+ (lagging) | varh / 10 | U16
26005 | 0x6595 | 2 | Total negative lagging reactive Energy : Er- (lagging) | varh / 0.001 | U32
26007 | 0x6597 | 1 | Total residual negative lagging reactive Energy : rEr- (lagging) | varh / 10 | U16
26008 | 0x6598 | 2 | Total positive leading reactive Energy : Er+ (leading) | varh / 0.001 | U32
26010 | 0x659A | 1 | Total residual positive leading reactive Energy : rEr+ (leading) | varh / 10 | U16
26011 | 0x659B | 2 | Total negative leading reactive Energy : Er- (leading) | varh / 0.001 | U32
26013 | 0x659D | 1 | Total residual negative leading reactive Energy : rEr- (leading) | varh / 10 | U16
26014 | 0x659E | 2 | Partial Hour meter | s | U32
26016 | 0x65A0 | 2 | Partial positive active Energy : Ea+ | Wh / 0.001 | U32
26018 | 0x65A2 | 1 | Partial residual positive active Energy : rEa+ | Wh / 10 | U16
26019 | 0x65A3 | 2 | Partial negative active Energy : Ea- | Wh / 0.001 | U32
26021 | 0x65A5 | 1 | Partial residual negative active Energy : rEa- | Wh / 10 | U16
26022 | 0x65A6 | 2 | Partial positive reactive Energy : Er+ | varh / 0.001 | U32
26024 | 0x65A8 | 1 | Partial residual positive reactive Energy : rEr+ | varh / 10 | U16
26025 | 0x65A9 | 2 | Partial negative reactive Energy : Er- | varh / 0.001 | U32
26027 | 0x65AB | 1 | Partial residual negative reactive Energy : rEr- | varh / 10 | U16
26028 | 0x65AC | 2 | Partial Apparent Energy : Eap | VAh / 0.001 | U32
26030 | 0x65AE | 1 | Partial residual apparent Energy : rEap | VAh / 10 | U16
26031 | 0x65AF | 2 | Last Partial Reset date | - | DATETIME
26033 | 0x65B1 | 2 | Last Partial Hour meter | s | U32
26035 | 0x65B3 | 2 | Last Partial positive active Energy : Ea+ | Wh / 0.001 | U32
26037 | 0x65B5 | 1 | Last Partial residual positive active Energy : rEa+ | Wh / 10 | U16
26038 | 0x65B6 | 2 | Last Partial negative active Energy : Ea- | Wh / 0.001 | U32
26040 | 0x65B8 | 1 | Last Partial residual negative active Energy : rEa- | Wh / 10 | U16
26041 | 0x65B9 | 2 | Last Partial positive reactive Energy : Er+ | varh / 0.001 | U32
26043 | 0x65BB | 1 | Last Partial residual positive reactive Energy : rEr+ | varh / 10 | U16
26044 | 0x65BC | 2 | Last Partial negative reactive Energy : Er- | varh / 0.001 | U32
26046 | 0x65BE | 1 | Last Partial residual negative reactive Energy : rEr- | varh / 10 | U16
26047 | 0x65BF | 2 | Last Partial Apparent Energy : Eap | VAh / 0.001 | U32
26049 | 0x65C1 | 1 | Last Partial residual apparent Energy : rEap | VAh / 10 | U16

## Energy measurement historical - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
19968 | 0x4E00 | Info | 79 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
19968 | 0x4E00 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
19969 | 0x4E01 | 2 | Predictive positive active Power : pP+ | W | U32
19971 | 0x4E03 | 2 | Predictive negative active Power : pP- | W | U32
19973 | 0x4E05 | 2 | Predictive positive reactive Power : pQ+ | var | U32
19975 | 0x4E07 | 2 | Predictive negative reactive Power : pQ- | var | U32
19977 | 0x4E09 | 2 | Predictive apparent Power : pS | VA | U32
19979 | 0x4E0B | 1 | Predictive power trend: 0 : Up 1 : Stable 2 : Down | - | U16
19980 | 0x4E0C | 2 | Predictive power countdown | s | U32
19982 | 0x4E0E | 2 | Load curve previous : Date (n-1) | - | DATETIME
19984 | 0x4E10 | 1 | Load curve previous : Flag (n-1) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
19985 | 0x4E11 | 2 | Load curve previous : P+ (n-1) | W | U32
19987 | 0x4E13 | 2 | Load curve previous : P- (n-1) | W | U32
19989 | 0x4E15 | 2 | Load curve previous : Q+ (n-1) | var | U32
19991 | 0x4E17 | 2 | Load curve previous : Q- (n-1) | var | U32
19993 | 0x4E19 | 2 | Load curve previous : S (n-1) | VA | U32
19995 | 0x4E1B | 2 | Load curve previous : Date (n-2) | - | DATETIME
19997 | 0x4E1D | 1 | Load curve previous : Flag (n-2) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
19998 | 0x4E1E | 2 | Load curve previous : P+ (n-2) | W | U32
20000 | 0x4E20 | 2 | Load curve previous : P- (n-2) | W | U32
20002 | 0x4E22 | 2 | Load curve previous : Q+ (n-2) | var | U32
20004 | 0x4E24 | 2 | Load curve previous : Q- (n-2) | var | U32
20006 | 0x4E26 | 2 | Load curve previous : S (n-2) | VA | U32
20008 | 0x4E28 | 2 | Load curve previous : Date (n-3) | - | DATETIME
20010 | 0x4E2A | 1 | Load curve previous : Flag (n-3) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
20011 | 0x4E2B | 2 | Load curve previous : P+ (n-3) | W | U32
20013 | 0x4E2D | 2 | Load curve previous : P- (n-3) | W | U32
20015 | 0x4E2F | 2 | Load curve previous : Q+ (n-3) | var | U32
20017 | 0x4E31 | 2 | Load curve previous : Q- (n-3) | var | U32
20019 | 0x4E33 | 2 | Load curve previous : S (n-3) | VA | U32
20021 | 0x4E35 | 2 | Load curve previous : Date (n-4) | - | DATETIME
20023 | 0x4E37 | 1 | Load curve previous : Flag (n-4) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
20024 | 0x4E38 | 2 | Load curve previous : P+ (n-4) | W | U32
20026 | 0x4E3A | 2 | Load curve previous : P- (n-4) | W | U32
20028 | 0x4E3C | 2 | Load curve previous : Q+ (n-4) | var | U32
20030 | 0x4E3E | 2 | Load curve previous : Q- (n-4) | var | U32
20032 | 0x4E40 | 2 | Load curve previous : S (n-4) | VA | U32
20034 | 0x4E42 | 2 | Load curve previous : Date (n-5) | - | DATETIME
20036 | 0x4E44 | 1 | Load curve previous : Flag (n-5) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
20037 | 0x4E45 | 2 | Load curve previous : P+ (n-5) | W | U32
20039 | 0x4E47 | 2 | Load curve previous : P- (n-5) | W | U32
20041 | 0x4E49 | 2 | Load curve previous : Q+ (n-5) | var | U32
20043 | 0x4E4B | 2 | Load curve previous : Q- (n-5) | var | U32
20045 | 0x4E4D | 2 | Load curve previous : S (n-5) | VA | U32

## Energy measurement historical - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22016 | 0x5600 | Info | 79 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22016 | 0x5600 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
22017 | 0x5601 | 2 | Predictive positive active Power : pP+ | W | U32
22019 | 0x5603 | 2 | Predictive negative active Power : pP- | W | U32
22021 | 0x5605 | 2 | Predictive positive reactive Power : pQ+ | var | U32
22023 | 0x5607 | 2 | Predictive negative reactive Power : pQ- | var | U32
22025 | 0x5609 | 2 | Predictive apparent Power : pS | VA | U32
22027 | 0x560B | 1 | Predictive power trend: 0 : Up 1 : Stable 2 : Down | - | U16
22028 | 0x560C | 2 | Predictive power countdown | s | U32
22030 | 0x560E | 2 | Load curve previous : Date (n-1) | - | DATETIME
22032 | 0x5610 | 1 | Load curve previous : Flag (n-1) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
22033 | 0x5611 | 2 | Load curve previous : P+ (n-1) | W | U32
22035 | 0x5613 | 2 | Load curve previous : P- (n-1) | W | U32
22037 | 0x5615 | 2 | Load curve previous : Q+ (n-1) | var | U32
22039 | 0x5617 | 2 | Load curve previous : Q- (n-1) | var | U32
22041 | 0x5619 | 2 | Load curve previous : S (n-1) | VA | U32
22043 | 0x561B | 2 | Load curve previous : Date (n-2) | - | DATETIME
22045 | 0x561D | 1 | Load curve previous : Flag (n-2) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
22046 | 0x561E | 2 | Load curve previous : P+ (n-2) | W | U32
22048 | 0x5620 | 2 | Load curve previous : P- (n-2) | W | U32
22050 | 0x5622 | 2 | Load curve previous : Q+ (n-2) | var | U32
22052 | 0x5624 | 2 | Load curve previous : Q- (n-2) | var | U32
22054 | 0x5626 | 2 | Load curve previous : S (n-2) | VA | U32
22056 | 0x5628 | 2 | Load curve previous : Date (n-3) | - | DATETIME
22058 | 0x562A | 1 | Load curve previous : Flag (n-3) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
22059 | 0x562B | 2 | Load curve previous : P+ (n-3) | W | U32
22061 | 0x562D | 2 | Load curve previous : P- (n-3) | W | U32
22063 | 0x562F | 2 | Load curve previous : Q+ (n-3) | var | U32
22065 | 0x5631 | 2 | Load curve previous : Q- (n-3) | var | U32
22067 | 0x5633 | 2 | Load curve previous : S (n-3) | VA | U32
22069 | 0x5635 | 2 | Load curve previous : Date (n-4) | - | DATETIME
22071 | 0x5637 | 1 | Load curve previous : Flag (n-4) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
22072 | 0x5638 | 2 | Load curve previous : P+ (n-4) | W | U32
22074 | 0x563A | 2 | Load curve previous : P- (n-4) | W | U32
22076 | 0x563C | 2 | Load curve previous : Q+ (n-4) | var | U32
22078 | 0x563E | 2 | Load curve previous : Q- (n-4) | var | U32
22080 | 0x5640 | 2 | Load curve previous : S (n-4) | VA | U32
22082 | 0x5642 | 2 | Load curve previous : Date (n-5) | - | DATETIME
22084 | 0x5644 | 1 | Load curve previous : Flag (n-5) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
22085 | 0x5645 | 2 | Load curve previous : P+ (n-5) | W | U32
22087 | 0x5647 | 2 | Load curve previous : P- (n-5) | W | U32
22089 | 0x5649 | 2 | Load curve previous : Q+ (n-5) | var | U32
22091 | 0x564B | 2 | Load curve previous : Q- (n-5) | var | U32
22093 | 0x564D | 2 | Load curve previous : S (n-5) | VA | U32

## Energy measurement historical - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24064 | 0x5E00 | Info | 79 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24064 | 0x5E00 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
24065 | 0x5E01 | 2 | Predictive positive active Power : pP+ | W | U32
24067 | 0x5E03 | 2 | Predictive negative active Power : pP- | W | U32
24069 | 0x5E05 | 2 | Predictive positive reactive Power : pQ+ | var | U32
24071 | 0x5E07 | 2 | Predictive negative reactive Power : pQ- | var | U32
24073 | 0x5E09 | 2 | Predictive apparent Power : pS | VA | U32
24075 | 0x5E0B | 1 | Predictive power trend: 0 : Up 1 : Stable 2 : Down | - | U16
24076 | 0x5E0C | 2 | Predictive power countdown | s | U32
24078 | 0x5E0E | 2 | Load curve previous : Date (n-1) | - | DATETIME
24080 | 0x5E10 | 1 | Load curve previous : Flag (n-1) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
24081 | 0x5E11 | 2 | Load curve previous : P+ (n-1) | W | U32
24083 | 0x5E13 | 2 | Load curve previous : P- (n-1) | W | U32
24085 | 0x5E15 | 2 | Load curve previous : Q+ (n-1) | var | U32
24087 | 0x5E17 | 2 | Load curve previous : Q- (n-1) | var | U32
24089 | 0x5E19 | 2 | Load curve previous : S (n-1) | VA | U32
24091 | 0x5E1B | 2 | Load curve previous : Date (n-2) | - | DATETIME
24093 | 0x5E1D | 1 | Load curve previous : Flag (n-2) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
24094 | 0x5E1E | 2 | Load curve previous : P+ (n-2) | W | U32
24096 | 0x5E20 | 2 | Load curve previous : P- (n-2) | W | U32
24098 | 0x5E22 | 2 | Load curve previous : Q+ (n-2) | var | U32
24100 | 0x5E24 | 2 | Load curve previous : Q- (n-2) | var | U32
24102 | 0x5E26 | 2 | Load curve previous : S (n-2) | VA | U32
24104 | 0x5E28 | 2 | Load curve previous : Date (n-3) | - | DATETIME
24106 | 0x5E2A | 1 | Load curve previous : Flag (n-3) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
24107 | 0x5E2B | 2 | Load curve previous : P+ (n-3) | W | U32
24109 | 0x5E2D | 2 | Load curve previous : P- (n-3) | W | U32
24111 | 0x5E2F | 2 | Load curve previous : Q+ (n-3) | var | U32
24113 | 0x5E31 | 2 | Load curve previous : Q- (n-3) | var | U32
24115 | 0x5E33 | 2 | Load curve previous : S (n-3) | VA | U32
24117 | 0x5E35 | 2 | Load curve previous : Date (n-4) | - | DATETIME
24119 | 0x5E37 | 1 | Load curve previous : Flag (n-4) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
24120 | 0x5E38 | 2 | Load curve previous : P+ (n-4) | W | U32
24122 | 0x5E3A | 2 | Load curve previous : P- (n-4) | W | U32
24124 | 0x5E3C | 2 | Load curve previous : Q+ (n-4) | var | U32
24126 | 0x5E3E | 2 | Load curve previous : Q- (n-4) | var | U32
24128 | 0x5E40 | 2 | Load curve previous : S (n-4) | VA | U32
24130 | 0x5E42 | 2 | Load curve previous : Date (n-5) | - | DATETIME
24132 | 0x5E44 | 1 | Load curve previous : Flag (n-5) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
24133 | 0x5E45 | 2 | Load curve previous : P+ (n-5) | W | U32
24135 | 0x5E47 | 2 | Load curve previous : P- (n-5) | W | U32
24137 | 0x5E49 | 2 | Load curve previous : Q+ (n-5) | var | U32
24139 | 0x5E4B | 2 | Load curve previous : Q- (n-5) | var | U32
24141 | 0x5E4D | 2 | Load curve previous : S (n-5) | VA | U32

## Energy measurement historical - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26112 | 0x6600 | Info | 79 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26112 | 0x6600 | 1 | Load status : 0 : Disabled 1 : Enabled | - | U8
26113 | 0x6601 | 2 | Predictive positive active Power : pP+ | W | U32
26115 | 0x6603 | 2 | Predictive negative active Power : pP- | W | U32
26117 | 0x6605 | 2 | Predictive positive reactive Power : pQ+ | var | U32
26119 | 0x6607 | 2 | Predictive negative reactive Power : pQ- | var | U32
26121 | 0x6609 | 2 | Predictive apparent Power : pS | VA | U32
26123 | 0x660B | 1 | Predictive power trend: 0 : Up 1 : Stable 2 : Down | - | U16
26124 | 0x660C | 2 | Predictive power countdown | s | U32
26126 | 0x660E | 2 | Load curve previous : Date (n-1) | - | DATETIME
26128 | 0x6610 | 1 | Load curve previous : Flag (n-1) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
26129 | 0x6611 | 2 | Load curve previous : P+ (n-1) | W | U32
26131 | 0x6613 | 2 | Load curve previous : P- (n-1) | W | U32
26133 | 0x6615 | 2 | Load curve previous : Q+ (n-1) | var | U32
26135 | 0x6617 | 2 | Load curve previous : Q- (n-1) | var | U32
26137 | 0x6619 | 2 | Load curve previous : S (n-1) | VA | U32
26139 | 0x661B | 2 | Load curve previous : Date (n-2) | - | DATETIME
26141 | 0x661D | 1 | Load curve previous : Flag (n-2) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
26142 | 0x661E | 2 | Load curve previous : P+ (n-2) | W | U32
26144 | 0x6620 | 2 | Load curve previous : P- (n-2) | W | U32
26146 | 0x6622 | 2 | Load curve previous : Q+ (n-2) | var | U32
26148 | 0x6624 | 2 | Load curve previous : Q- (n-2) | var | U32
26150 | 0x6626 | 2 | Load curve previous : S (n-2) | VA | U32
26152 | 0x6628 | 2 | Load curve previous : Date (n-3) | - | DATETIME
26154 | 0x662A | 1 | Load curve previous : Flag (n-3) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
26155 | 0x662B | 2 | Load curve previous : P+ (n-3) | W | U32
26157 | 0x662D | 2 | Load curve previous : P- (n-3) | W | U32
26159 | 0x662F | 2 | Load curve previous : Q+ (n-3) | var | U32
26161 | 0x6631 | 2 | Load curve previous : Q- (n-3) | var | U32
26163 | 0x6633 | 2 | Load curve previous : S (n-3) | VA | U32
26165 | 0x6635 | 2 | Load curve previous : Date (n-4) | - | DATETIME
26167 | 0x6637 | 1 | Load curve previous : Flag (n-4) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
26168 | 0x6638 | 2 | Load curve previous : P+ (n-4) | W | U32
26170 | 0x663A | 2 | Load curve previous : P- (n-4) | W | U32
26172 | 0x663C | 2 | Load curve previous : Q+ (n-4) | var | U32
26174 | 0x663E | 2 | Load curve previous : Q- (n-4) | var | U32
26176 | 0x6640 | 2 | Load curve previous : S (n-4) | VA | U32
26178 | 0x6642 | 2 | Load curve previous : Date (n-5) | - | DATETIME
26180 | 0x6644 | 1 | Load curve previous : Flag (n-5) 0 : full integration period and date/time set 1 : incomplete integration period and date/time set 2 : full integration period and date/time not set 3 : incomplete integration period and date/time not set | - | U16
26181 | 0x6645 | 2 | Load curve previous : P+ (n-5) | W | U32
26183 | 0x6647 | 2 | Load curve previous : P- (n-5) | W | U32
26185 | 0x6649 | 2 | Load curve previous : Q+ (n-5) | var | U32
26187 | 0x664B | 2 | Load curve previous : Q- (n-5) | var | U32
26189 | 0x664D | 2 | Load curve previous : S (n-5) | VA | U32

## Partial energies meters reset - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20096 | 0x4E80 | Commands | 1 | USER | NONE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20096 | 0x4E80 | 1 | Partial meters reset 0x003F : All | - | U16_HEX

## Partial energies meters reset - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22144 | 0x5680 | Commands | 1 | USER | NONE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22144 | 0x5680 | 1 | Partial meters reset 0x003F : All | - | U16_HEX

## Partial energies meters reset - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24192 | 0x5E80 | Commands | 1 | USER | NONE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24192 | 0x5E80 | 1 | Partial meters reset 0x003F : All | - | U16_HEX

## Partial energies meters reset - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26240 | 0x6680 | Commands | 1 | USER | NONE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26240 | 0x6680 | 1 | Partial meters reset 0x003F : All | - | U16_HEX

## Min/max reset - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20097 | 0x4E81 | Commands | 2 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20097 | 0x4E81 | 1 | Erase (1) : These values could be combine all 0x0001 : AVG Min/Max 4V 0x0002 : AVG Min/Max 3U 0x0004 : AVG Min/Max 4I 0x0008 : AVG Min/Max F 0x0030 : AVG Min/Max P 0x00C0 : AVG Min/Max Q 0x0100 : AVG Min/Max S 0x0200 : AVG Min/Max PF 0xFFFF : AVG Min/Max ALL | - | U16_HEX
20098 | 0x4E82 | 1 | Erase (2) : These values could be combine all 0x0001 : Instantaneous Min/Max 4V 0x0002 : Instantaneous Min/Max 3U 0x0004 : Instantaneous Min/Max 4I 0x0008 : Instantaneous Min/Max F 0x0030 : Instantaneous Min/Max P 0x00C0 : Instantaneous Min/Max Q 0x0100 : Instantaneous Min/Max S 0x0200 : Instantaneous Min/Max PF and Phi I/V 0x1000 : Instantaneous Min/Max THD I 0x8000 : Instantaneous Min/Max Crest Fact. I 0xFFFF : Instantaneous Min/Max ALL | - | U16_HEX

## Min/max reset - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22145 | 0x5681 | Commands | 2 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22145 | 0x5681 | 1 | Erase (1) : These values could be combine all 0x0001 : AVG Min/Max 4V 0x0002 : AVG Min/Max 3U 0x0004 : AVG Min/Max 4I 0x0008 : AVG Min/Max F 0x0030 : AVG Min/Max P 0x00C0 : AVG Min/Max Q 0x0100 : AVG Min/Max S 0x0200 : AVG Min/Max PF 0xFFFF : AVG Min/Max ALL | - | U16_HEX
22146 | 0x5682 | 1 | Erase (2) : These values could be combine all 0x0001 : Instantaneous Min/Max 4V 0x0002 : Instantaneous Min/Max 3U 0x0004 : Instantaneous Min/Max 4I 0x0008 : Instantaneous Min/Max F 0x0030 : Instantaneous Min/Max P 0x00C0 : Instantaneous Min/Max Q 0x0100 : Instantaneous Min/Max S 0x0200 : Instantaneous Min/Max PF and Phi I/V 0x1000 : Instantaneous Min/Max THD I 0x8000 : Instantaneous Min/Max Crest Fact. I 0xFFFF : Instantaneous Min/Max ALL | - | U16_HEX

## Min/max reset - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24193 | 0x5E81 | Commands | 2 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24193 | 0x5E81 | 1 | Erase (1) : These values could be combine all 0x0001 : AVG Min/Max 4V 0x0002 : AVG Min/Max 3U 0x0004 : AVG Min/Max 4I 0x0008 : AVG Min/Max F 0x0030 : AVG Min/Max P 0x00C0 : AVG Min/Max Q 0x0100 : AVG Min/Max S 0x0200 : AVG Min/Max PF 0xFFFF : AVG Min/Max ALL | - | U16_HEX
24194 | 0x5E82 | 1 | Erase (2) : These values could be combine all 0x0001 : Instantaneous Min/Max 4V 0x0002 : Instantaneous Min/Max 3U 0x0004 : Instantaneous Min/Max 4I 0x0008 : Instantaneous Min/Max F 0x0030 : Instantaneous Min/Max P 0x00C0 : Instantaneous Min/Max Q 0x0100 : Instantaneous Min/Max S 0x0200 : Instantaneous Min/Max PF and Phi I/V 0x1000 : Instantaneous Min/Max THD I 0x8000 : Instantaneous Min/Max Crest Fact. I 0xFFFF : Instantaneous Min/Max ALL | - | U16_HEX

## Min/max reset - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26241 | 0x6681 | Commands | 2 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26241 | 0x6681 | 1 | Erase (1) : These values could be combine all 0x0001 : AVG Min/Max 4V 0x0002 : AVG Min/Max 3U 0x0004 : AVG Min/Max 4I 0x0008 : AVG Min/Max F 0x0030 : AVG Min/Max P 0x00C0 : AVG Min/Max Q 0x0100 : AVG Min/Max S 0x0200 : AVG Min/Max PF 0xFFFF : AVG Min/Max ALL | - | U16_HEX
26242 | 0x6682 | 1 | Erase (2) : These values could be combine all 0x0001 : Instantaneous Min/Max 4V 0x0002 : Instantaneous Min/Max 3U 0x0004 : Instantaneous Min/Max 4I 0x0008 : Instantaneous Min/Max F 0x0030 : Instantaneous Min/Max P 0x00C0 : Instantaneous Min/Max Q 0x0100 : Instantaneous Min/Max S 0x0200 : Instantaneous Min/Max PF and Phi I/V 0x1000 : Instantaneous Min/Max THD I 0x8000 : Instantaneous Min/Max Crest Fact. I 0xFFFF : Instantaneous Min/Max ALL | - | U16_HEX

## Partial tariff meters reset - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20099 | 0x4E83 | Commands | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20099 | 0x4E83 | 1 | Partial tariff meters reset 0x003F : All | - | U16_HEX

## Partial tariff meters reset - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22147 | 0x5683 | Commands | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22147 | 0x5683 | 1 | Partial tariff meters reset 0x003F : All | - | U16_HEX

## Partial tariff meters reset - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24195 | 0x5E83 | Commands | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24195 | 0x5E83 | 1 | Partial tariff meters reset 0x003F : All | - | U16_HEX

## Partial tariff meters reset - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26243 | 0x6683 | Commands | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26243 | 0x6683 | 1 | Partial tariff meters reset 0x003F : All | - | U16_HEX

## Tariff meter (total) - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20224 | 0x4F00 | Info | 97 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20224 | 0x4F00 | 1 | Tariff number in progress 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16
20225 | 0x4F01 | 2 | T1 - Ea+ | Wh / 0.001 | U32
20227 | 0x4F03 | 2 | T2 - Ea+ | Wh / 0.001 | U32
20229 | 0x4F05 | 2 | T3 - Ea+ | Wh / 0.001 | U32
20231 | 0x4F07 | 2 | T4 - Ea+ | Wh / 0.001 | U32
20233 | 0x4F09 | 2 | T5 - Ea+ | Wh / 0.001 | U32
20235 | 0x4F0B | 2 | T6 - Ea+ | Wh / 0.001 | U32
20237 | 0x4F0D | 2 | T7 - Ea+ | Wh / 0.001 | U32
20239 | 0x4F0F | 2 | T8 - Ea+ | Wh / 0.001 | U32
20241 | 0x4F11 | 2 | T1 - Ea- | Wh / 0.001 | U32
20243 | 0x4F13 | 2 | T2 - Ea- | Wh / 0.001 | U32
20245 | 0x4F15 | 2 | T3 - Ea- | Wh / 0.001 | U32
20247 | 0x4F17 | 2 | T4 - Ea- | Wh / 0.001 | U32
20249 | 0x4F19 | 2 | T5 - Ea- | Wh / 0.001 | U32
20251 | 0x4F1B | 2 | T6 - Ea- | Wh / 0.001 | U32
20253 | 0x4F1D | 2 | T7 - Ea- | Wh / 0.001 | U32
20255 | 0x4F1F | 2 | T8 - Ea- | Wh / 0.001 | U32
20257 | 0x4F21 | 2 | T1 - Er+ (lagging) | varh / 0.001 | U32
20259 | 0x4F23 | 2 | T2 - Er+ (lagging) | varh / 0.001 | U32
20261 | 0x4F25 | 2 | T3 - Er+ (lagging) | varh / 0.001 | U32
20263 | 0x4F27 | 2 | T4 - Er+ (lagging) | varh / 0.001 | U32
20265 | 0x4F29 | 2 | T5 - Er+ (lagging) | varh / 0.001 | U32
20267 | 0x4F2B | 2 | T6 - Er+ (lagging) | varh / 0.001 | U32
20269 | 0x4F2D | 2 | T7 - Er+ (lagging) | varh / 0.001 | U32
20271 | 0x4F2F | 2 | T8 - Er+ (lagging) | varh / 0.001 | U32
20273 | 0x4F31 | 2 | T1 - Er+ (leading) | varh / 0.001 | U32
20275 | 0x4F33 | 2 | T2 - Er+ (leading) | varh / 0.001 | U32
20277 | 0x4F35 | 2 | T3 - Er+ (leading) | varh / 0.001 | U32
20279 | 0x4F37 | 2 | T4 - Er+ (leading) | varh / 0.001 | U32
20281 | 0x4F39 | 2 | T5 - Er+ (leading) | varh / 0.001 | U32
20283 | 0x4F3B | 2 | T6 - Er+ (leading) | varh / 0.001 | U32
20285 | 0x4F3D | 2 | T7 - Er+ (leading) | varh / 0.001 | U32
20287 | 0x4F3F | 2 | T8 - Er+ (leading) | varh / 0.001 | U32
20289 | 0x4F41 | 2 | T1 - Er- | varh / 0.001 | U32
20291 | 0x4F43 | 2 | T2 - Er- | varh / 0.001 | U32
20293 | 0x4F45 | 2 | T3 - Er- | varh / 0.001 | U32
20295 | 0x4F47 | 2 | T4 - Er- | varh / 0.001 | U32
20297 | 0x4F49 | 2 | T5 - Er- | varh / 0.001 | U32
20299 | 0x4F4B | 2 | T6 - Er- | varh / 0.001 | U32
20301 | 0x4F4D | 2 | T7 - Er- | varh / 0.001 | U32
20303 | 0x4F4F | 2 | T8 - Er- | varh / 0.001 | U32
20305 | 0x4F51 | 2 | T1 - Eap | VAh / 0.001 | U32
20307 | 0x4F53 | 2 | T2 - Eap | VAh / 0.001 | U32
20309 | 0x4F55 | 2 | T3 - Eap | VAh / 0.001 | U32
20311 | 0x4F57 | 2 | T4 - Eap | VAh / 0.001 | U32
20313 | 0x4F59 | 2 | T5 - Eap | VAh / 0.001 | U32
20315 | 0x4F5B | 2 | T6 - Eap | VAh / 0.001 | U32
20317 | 0x4F5D | 2 | T7 - Eap | VAh / 0.001 | U32
20319 | 0x4F5F | 2 | T8 - Eap | VAh / 0.001 | U32

## Tariff meter (total) - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22272 | 0x5700 | Info | 97 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22272 | 0x5700 | 1 | Tariff number in progress 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16
22273 | 0x5701 | 2 | T1 - Ea+ | Wh / 0.001 | U32
22275 | 0x5703 | 2 | T2 - Ea+ | Wh / 0.001 | U32
22277 | 0x5705 | 2 | T3 - Ea+ | Wh / 0.001 | U32
22279 | 0x5707 | 2 | T4 - Ea+ | Wh / 0.001 | U32
22281 | 0x5709 | 2 | T5 - Ea+ | Wh / 0.001 | U32
22283 | 0x570B | 2 | T6 - Ea+ | Wh / 0.001 | U32
22285 | 0x570D | 2 | T7 - Ea+ | Wh / 0.001 | U32
22287 | 0x570F | 2 | T8 - Ea+ | Wh / 0.001 | U32
22289 | 0x5711 | 2 | T1 - Ea- | Wh / 0.001 | U32
22291 | 0x5713 | 2 | T2 - Ea- | Wh / 0.001 | U32
22293 | 0x5715 | 2 | T3 - Ea- | Wh / 0.001 | U32
22295 | 0x5717 | 2 | T4 - Ea- | Wh / 0.001 | U32
22297 | 0x5719 | 2 | T5 - Ea- | Wh / 0.001 | U32
22299 | 0x571B | 2 | T6 - Ea- | Wh / 0.001 | U32
22301 | 0x571D | 2 | T7 - Ea- | Wh / 0.001 | U32
22303 | 0x571F | 2 | T8 - Ea- | Wh / 0.001 | U32
22305 | 0x5721 | 2 | T1 - Er+ (lagging) | varh / 0.001 | U32
22307 | 0x5723 | 2 | T2 - Er+ (lagging) | varh / 0.001 | U32
22309 | 0x5725 | 2 | T3 - Er+ (lagging) | varh / 0.001 | U32
22311 | 0x5727 | 2 | T4 - Er+ (lagging) | varh / 0.001 | U32
22313 | 0x5729 | 2 | T5 - Er+ (lagging) | varh / 0.001 | U32
22315 | 0x572B | 2 | T6 - Er+ (lagging) | varh / 0.001 | U32
22317 | 0x572D | 2 | T7 - Er+ (lagging) | varh / 0.001 | U32
22319 | 0x572F | 2 | T8 - Er+ (lagging) | varh / 0.001 | U32
22321 | 0x5731 | 2 | T1 - Er+ (leading) | varh / 0.001 | U32
22323 | 0x5733 | 2 | T2 - Er+ (leading) | varh / 0.001 | U32
22325 | 0x5735 | 2 | T3 - Er+ (leading) | varh / 0.001 | U32
22327 | 0x5737 | 2 | T4 - Er+ (leading) | varh / 0.001 | U32
22329 | 0x5739 | 2 | T5 - Er+ (leading) | varh / 0.001 | U32
22331 | 0x573B | 2 | T6 - Er+ (leading) | varh / 0.001 | U32
22333 | 0x573D | 2 | T7 - Er+ (leading) | varh / 0.001 | U32
22335 | 0x573F | 2 | T8 - Er+ (leading) | varh / 0.001 | U32
22337 | 0x5741 | 2 | T1 - Er- | varh / 0.001 | U32
22339 | 0x5743 | 2 | T2 - Er- | varh / 0.001 | U32
22341 | 0x5745 | 2 | T3 - Er- | varh / 0.001 | U32
22343 | 0x5747 | 2 | T4 - Er- | varh / 0.001 | U32
22345 | 0x5749 | 2 | T5 - Er- | varh / 0.001 | U32
22347 | 0x574B | 2 | T6 - Er- | varh / 0.001 | U32
22349 | 0x574D | 2 | T7 - Er- | varh / 0.001 | U32
22351 | 0x574F | 2 | T8 - Er- | varh / 0.001 | U32
22353 | 0x5751 | 2 | T1 - Eap | VAh / 0.001 | U32
22355 | 0x5753 | 2 | T2 - Eap | VAh / 0.001 | U32
22357 | 0x5755 | 2 | T3 - Eap | VAh / 0.001 | U32
22359 | 0x5757 | 2 | T4 - Eap | VAh / 0.001 | U32
22361 | 0x5759 | 2 | T5 - Eap | VAh / 0.001 | U32
22363 | 0x575B | 2 | T6 - Eap | VAh / 0.001 | U32
22365 | 0x575D | 2 | T7 - Eap | VAh / 0.001 | U32
22367 | 0x575F | 2 | T8 - Eap | VAh / 0.001 | U32

## Tariff meter (total) - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24320 | 0x5F00 | Info | 97 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24320 | 0x5F00 | 1 | Tariff number in progress 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16
24321 | 0x5F01 | 2 | T1 - Ea+ | Wh / 0.001 | U32
24323 | 0x5F03 | 2 | T2 - Ea+ | Wh / 0.001 | U32
24325 | 0x5F05 | 2 | T3 - Ea+ | Wh / 0.001 | U32
24327 | 0x5F07 | 2 | T4 - Ea+ | Wh / 0.001 | U32
24329 | 0x5F09 | 2 | T5 - Ea+ | Wh / 0.001 | U32
24331 | 0x5F0B | 2 | T6 - Ea+ | Wh / 0.001 | U32
24333 | 0x5F0D | 2 | T7 - Ea+ | Wh / 0.001 | U32
24335 | 0x5F0F | 2 | T8 - Ea+ | Wh / 0.001 | U32
24337 | 0x5F11 | 2 | T1 - Ea- | Wh / 0.001 | U32
24339 | 0x5F13 | 2 | T2 - Ea- | Wh / 0.001 | U32
24341 | 0x5F15 | 2 | T3 - Ea- | Wh / 0.001 | U32
24343 | 0x5F17 | 2 | T4 - Ea- | Wh / 0.001 | U32
24345 | 0x5F19 | 2 | T5 - Ea- | Wh / 0.001 | U32
24347 | 0x5F1B | 2 | T6 - Ea- | Wh / 0.001 | U32
24349 | 0x5F1D | 2 | T7 - Ea- | Wh / 0.001 | U32
24351 | 0x5F1F | 2 | T8 - Ea- | Wh / 0.001 | U32
24353 | 0x5F21 | 2 | T1 - Er+ (lagging) | varh / 0.001 | U32
24355 | 0x5F23 | 2 | T2 - Er+ (lagging) | varh / 0.001 | U32
24357 | 0x5F25 | 2 | T3 - Er+ (lagging) | varh / 0.001 | U32
24359 | 0x5F27 | 2 | T4 - Er+ (lagging) | varh / 0.001 | U32
24361 | 0x5F29 | 2 | T5 - Er+ (lagging) | varh / 0.001 | U32
24363 | 0x5F2B | 2 | T6 - Er+ (lagging) | varh / 0.001 | U32
24365 | 0x5F2D | 2 | T7 - Er+ (lagging) | varh / 0.001 | U32
24367 | 0x5F2F | 2 | T8 - Er+ (lagging) | varh / 0.001 | U32
24369 | 0x5F31 | 2 | T1 - Er+ (leading) | varh / 0.001 | U32
24371 | 0x5F33 | 2 | T2 - Er+ (leading) | varh / 0.001 | U32
24373 | 0x5F35 | 2 | T3 - Er+ (leading) | varh / 0.001 | U32
24375 | 0x5F37 | 2 | T4 - Er+ (leading) | varh / 0.001 | U32
24377 | 0x5F39 | 2 | T5 - Er+ (leading) | varh / 0.001 | U32
24379 | 0x5F3B | 2 | T6 - Er+ (leading) | varh / 0.001 | U32
24381 | 0x5F3D | 2 | T7 - Er+ (leading) | varh / 0.001 | U32
24383 | 0x5F3F | 2 | T8 - Er+ (leading) | varh / 0.001 | U32
24385 | 0x5F41 | 2 | T1 - Er- | varh / 0.001 | U32
24387 | 0x5F43 | 2 | T2 - Er- | varh / 0.001 | U32
24389 | 0x5F45 | 2 | T3 - Er- | varh / 0.001 | U32
24391 | 0x5F47 | 2 | T4 - Er- | varh / 0.001 | U32
24393 | 0x5F49 | 2 | T5 - Er- | varh / 0.001 | U32
24395 | 0x5F4B | 2 | T6 - Er- | varh / 0.001 | U32
24397 | 0x5F4D | 2 | T7 - Er- | varh / 0.001 | U32
24399 | 0x5F4F | 2 | T8 - Er- | varh / 0.001 | U32
24401 | 0x5F51 | 2 | T1 - Eap | VAh / 0.001 | U32
24403 | 0x5F53 | 2 | T2 - Eap | VAh / 0.001 | U32
24405 | 0x5F55 | 2 | T3 - Eap | VAh / 0.001 | U32
24407 | 0x5F57 | 2 | T4 - Eap | VAh / 0.001 | U32
24409 | 0x5F59 | 2 | T5 - Eap | VAh / 0.001 | U32
24411 | 0x5F5B | 2 | T6 - Eap | VAh / 0.001 | U32
24413 | 0x5F5D | 2 | T7 - Eap | VAh / 0.001 | U32
24415 | 0x5F5F | 2 | T8 - Eap | VAh / 0.001 | U32

## Tariff meter (total) - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26368 | 0x6700 | Info | 97 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26368 | 0x6700 | 1 | Tariff number in progress 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16
26369 | 0x6701 | 2 | T1 - Ea+ | Wh / 0.001 | U32
26371 | 0x6703 | 2 | T2 - Ea+ | Wh / 0.001 | U32
26373 | 0x6705 | 2 | T3 - Ea+ | Wh / 0.001 | U32
26375 | 0x6707 | 2 | T4 - Ea+ | Wh / 0.001 | U32
26377 | 0x6709 | 2 | T5 - Ea+ | Wh / 0.001 | U32
26379 | 0x670B | 2 | T6 - Ea+ | Wh / 0.001 | U32
26381 | 0x670D | 2 | T7 - Ea+ | Wh / 0.001 | U32
26383 | 0x670F | 2 | T8 - Ea+ | Wh / 0.001 | U32
26385 | 0x6711 | 2 | T1 - Ea- | Wh / 0.001 | U32
26387 | 0x6713 | 2 | T2 - Ea- | Wh / 0.001 | U32
26389 | 0x6715 | 2 | T3 - Ea- | Wh / 0.001 | U32
26391 | 0x6717 | 2 | T4 - Ea- | Wh / 0.001 | U32
26393 | 0x6719 | 2 | T5 - Ea- | Wh / 0.001 | U32
26395 | 0x671B | 2 | T6 - Ea- | Wh / 0.001 | U32
26397 | 0x671D | 2 | T7 - Ea- | Wh / 0.001 | U32
26399 | 0x671F | 2 | T8 - Ea- | Wh / 0.001 | U32
26401 | 0x6721 | 2 | T1 - Er+ (lagging) | varh / 0.001 | U32
26403 | 0x6723 | 2 | T2 - Er+ (lagging) | varh / 0.001 | U32
26405 | 0x6725 | 2 | T3 - Er+ (lagging) | varh / 0.001 | U32
26407 | 0x6727 | 2 | T4 - Er+ (lagging) | varh / 0.001 | U32
26409 | 0x6729 | 2 | T5 - Er+ (lagging) | varh / 0.001 | U32
26411 | 0x672B | 2 | T6 - Er+ (lagging) | varh / 0.001 | U32
26413 | 0x672D | 2 | T7 - Er+ (lagging) | varh / 0.001 | U32
26415 | 0x672F | 2 | T8 - Er+ (lagging) | varh / 0.001 | U32
26417 | 0x6731 | 2 | T1 - Er+ (leading) | varh / 0.001 | U32
26419 | 0x6733 | 2 | T2 - Er+ (leading) | varh / 0.001 | U32
26421 | 0x6735 | 2 | T3 - Er+ (leading) | varh / 0.001 | U32
26423 | 0x6737 | 2 | T4 - Er+ (leading) | varh / 0.001 | U32
26425 | 0x6739 | 2 | T5 - Er+ (leading) | varh / 0.001 | U32
26427 | 0x673B | 2 | T6 - Er+ (leading) | varh / 0.001 | U32
26429 | 0x673D | 2 | T7 - Er+ (leading) | varh / 0.001 | U32
26431 | 0x673F | 2 | T8 - Er+ (leading) | varh / 0.001 | U32
26433 | 0x6741 | 2 | T1 - Er- | varh / 0.001 | U32
26435 | 0x6743 | 2 | T2 - Er- | varh / 0.001 | U32
26437 | 0x6745 | 2 | T3 - Er- | varh / 0.001 | U32
26439 | 0x6747 | 2 | T4 - Er- | varh / 0.001 | U32
26441 | 0x6749 | 2 | T5 - Er- | varh / 0.001 | U32
26443 | 0x674B | 2 | T6 - Er- | varh / 0.001 | U32
26445 | 0x674D | 2 | T7 - Er- | varh / 0.001 | U32
26447 | 0x674F | 2 | T8 - Er- | varh / 0.001 | U32
26449 | 0x6751 | 2 | T1 - Eap | VAh / 0.001 | U32
26451 | 0x6753 | 2 | T2 - Eap | VAh / 0.001 | U32
26453 | 0x6755 | 2 | T3 - Eap | VAh / 0.001 | U32
26455 | 0x6757 | 2 | T4 - Eap | VAh / 0.001 | U32
26457 | 0x6759 | 2 | T5 - Eap | VAh / 0.001 | U32
26459 | 0x675B | 2 | T6 - Eap | VAh / 0.001 | U32
26461 | 0x675D | 2 | T7 - Eap | VAh / 0.001 | U32
26463 | 0x675F | 2 | T8 - Eap | VAh / 0.001 | U32

## Tariff meter (partial) - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20352 | 0x4F80 | Info | 97 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20352 | 0x4F80 | 1 | Tariff number in progress 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16
20353 | 0x4F81 | 2 | T1 - Ea+ | Wh / 0.001 | U32
20355 | 0x4F83 | 2 | T2 - Ea+ | Wh / 0.001 | U32
20357 | 0x4F85 | 2 | T3 - Ea+ | Wh / 0.001 | U32
20359 | 0x4F87 | 2 | T4 - Ea+ | Wh / 0.001 | U32
20361 | 0x4F89 | 2 | T5 - Ea+ | Wh / 0.001 | U32
20363 | 0x4F8B | 2 | T6 - Ea+ | Wh / 0.001 | U32
20365 | 0x4F8D | 2 | T7 - Ea+ | Wh / 0.001 | U32
20367 | 0x4F8F | 2 | T8 - Ea+ | Wh / 0.001 | U32
20369 | 0x4F91 | 2 | T1 - Ea- | Wh / 0.001 | U32
20371 | 0x4F93 | 2 | T2 - Ea- | Wh / 0.001 | U32
20373 | 0x4F95 | 2 | T3 - Ea- | Wh / 0.001 | U32
20375 | 0x4F97 | 2 | T4 - Ea- | Wh / 0.001 | U32
20377 | 0x4F99 | 2 | T5 - Ea- | Wh / 0.001 | U32
20379 | 0x4F9B | 2 | T6 - Ea- | Wh / 0.001 | U32
20381 | 0x4F9D | 2 | T7 - Ea- | Wh / 0.001 | U32
20383 | 0x4F9F | 2 | T8 - Ea- | Wh / 0.001 | U32
20385 | 0x4FA1 | 2 | T1 - Er+ (lagging) | varh / 0.001 | U32
20387 | 0x4FA3 | 2 | T2 - Er+ (lagging) | varh / 0.001 | U32
20389 | 0x4FA5 | 2 | T3 - Er+ (lagging) | varh / 0.001 | U32
20391 | 0x4FA7 | 2 | T4 - Er+ (lagging) | varh / 0.001 | U32
20393 | 0x4FA9 | 2 | T5 - Er+ (lagging) | varh / 0.001 | U32
20395 | 0x4FAB | 2 | T6 - Er+ (lagging) | varh / 0.001 | U32
20397 | 0x4FAD | 2 | T7 - Er+ (lagging) | varh / 0.001 | U32
20399 | 0x4FAF | 2 | T8 - Er+ (lagging) | varh / 0.001 | U32
20401 | 0x4FB1 | 2 | T1 - Er+ (leading) | varh / 0.001 | U32
20403 | 0x4FB3 | 2 | T2 - Er+ (leading) | varh / 0.001 | U32
20405 | 0x4FB5 | 2 | T3 - Er+ (leading) | varh / 0.001 | U32
20407 | 0x4FB7 | 2 | T4 - Er+ (leading) | varh / 0.001 | U32
20409 | 0x4FB9 | 2 | T5 - Er+ (leading) | varh / 0.001 | U32
20411 | 0x4FBB | 2 | T6 - Er+ (leading) | varh / 0.001 | U32
20413 | 0x4FBD | 2 | T7 - Er+ (leading) | varh / 0.001 | U32
20415 | 0x4FBF | 2 | T8 - Er+ (leading) | varh / 0.001 | U32
20417 | 0x4FC1 | 2 | T1 - Er- | varh / 0.001 | U32
20419 | 0x4FC3 | 2 | T2 - Er- | varh / 0.001 | U32
20421 | 0x4FC5 | 2 | T3 - Er- | varh / 0.001 | U32
20423 | 0x4FC7 | 2 | T4 - Er- | varh / 0.001 | U32
20425 | 0x4FC9 | 2 | T5 - Er- | varh / 0.001 | U32
20427 | 0x4FCB | 2 | T6 - Er- | varh / 0.001 | U32
20429 | 0x4FCD | 2 | T7 - Er- | varh / 0.001 | U32
20431 | 0x4FCF | 2 | T8 - Er- | varh / 0.001 | U32
20433 | 0x4FD1 | 2 | T1 - Eap | VAh / 0.001 | U32
20435 | 0x4FD3 | 2 | T2 - Eap | VAh / 0.001 | U32
20437 | 0x4FD5 | 2 | T3 - Eap | VAh / 0.001 | U32
20439 | 0x4FD7 | 2 | T4 - Eap | VAh / 0.001 | U32
20441 | 0x4FD9 | 2 | T5 - Eap | VAh / 0.001 | U32
20443 | 0x4FDB | 2 | T6 - Eap | VAh / 0.001 | U32
20445 | 0x4FDD | 2 | T7 - Eap | VAh / 0.001 | U32
20447 | 0x4FDF | 2 | T8 - Eap | VAh / 0.001 | U32

## Tariff meter (partial) - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22400 | 0x5780 | Info | 97 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22400 | 0x5780 | 1 | Tariff number in progress 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16
22401 | 0x5781 | 2 | T1 - Ea+ | Wh / 0.001 | U32
22403 | 0x5783 | 2 | T2 - Ea+ | Wh / 0.001 | U32
22405 | 0x5785 | 2 | T3 - Ea+ | Wh / 0.001 | U32
22407 | 0x5787 | 2 | T4 - Ea+ | Wh / 0.001 | U32
22409 | 0x5789 | 2 | T5 - Ea+ | Wh / 0.001 | U32
22411 | 0x578B | 2 | T6 - Ea+ | Wh / 0.001 | U32
22413 | 0x578D | 2 | T7 - Ea+ | Wh / 0.001 | U32
22415 | 0x578F | 2 | T8 - Ea+ | Wh / 0.001 | U32
22417 | 0x5791 | 2 | T1 - Ea- | Wh / 0.001 | U32
22419 | 0x5793 | 2 | T2 - Ea- | Wh / 0.001 | U32
22421 | 0x5795 | 2 | T3 - Ea- | Wh / 0.001 | U32
22423 | 0x5797 | 2 | T4 - Ea- | Wh / 0.001 | U32
22425 | 0x5799 | 2 | T5 - Ea- | Wh / 0.001 | U32
22427 | 0x579B | 2 | T6 - Ea- | Wh / 0.001 | U32
22429 | 0x579D | 2 | T7 - Ea- | Wh / 0.001 | U32
22431 | 0x579F | 2 | T8 - Ea- | Wh / 0.001 | U32
22433 | 0x57A1 | 2 | T1 - Er+ (lagging) | varh / 0.001 | U32
22435 | 0x57A3 | 2 | T2 - Er+ (lagging) | varh / 0.001 | U32
22437 | 0x57A5 | 2 | T3 - Er+ (lagging) | varh / 0.001 | U32
22439 | 0x57A7 | 2 | T4 - Er+ (lagging) | varh / 0.001 | U32
22441 | 0x57A9 | 2 | T5 - Er+ (lagging) | varh / 0.001 | U32
22443 | 0x57AB | 2 | T6 - Er+ (lagging) | varh / 0.001 | U32
22445 | 0x57AD | 2 | T7 - Er+ (lagging) | varh / 0.001 | U32
22447 | 0x57AF | 2 | T8 - Er+ (lagging) | varh / 0.001 | U32
22449 | 0x57B1 | 2 | T1 - Er+ (leading) | varh / 0.001 | U32
22451 | 0x57B3 | 2 | T2 - Er+ (leading) | varh / 0.001 | U32
22453 | 0x57B5 | 2 | T3 - Er+ (leading) | varh / 0.001 | U32
22455 | 0x57B7 | 2 | T4 - Er+ (leading) | varh / 0.001 | U32
22457 | 0x57B9 | 2 | T5 - Er+ (leading) | varh / 0.001 | U32
22459 | 0x57BB | 2 | T6 - Er+ (leading) | varh / 0.001 | U32
22461 | 0x57BD | 2 | T7 - Er+ (leading) | varh / 0.001 | U32
22463 | 0x57BF | 2 | T8 - Er+ (leading) | varh / 0.001 | U32
22465 | 0x57C1 | 2 | T1 - Er- | varh / 0.001 | U32
22467 | 0x57C3 | 2 | T2 - Er- | varh / 0.001 | U32
22469 | 0x57C5 | 2 | T3 - Er- | varh / 0.001 | U32
22471 | 0x57C7 | 2 | T4 - Er- | varh / 0.001 | U32
22473 | 0x57C9 | 2 | T5 - Er- | varh / 0.001 | U32
22475 | 0x57CB | 2 | T6 - Er- | varh / 0.001 | U32
22477 | 0x57CD | 2 | T7 - Er- | varh / 0.001 | U32
22479 | 0x57CF | 2 | T8 - Er- | varh / 0.001 | U32
22481 | 0x57D1 | 2 | T1 - Eap | VAh / 0.001 | U32
22483 | 0x57D3 | 2 | T2 - Eap | VAh / 0.001 | U32
22485 | 0x57D5 | 2 | T3 - Eap | VAh / 0.001 | U32
22487 | 0x57D7 | 2 | T4 - Eap | VAh / 0.001 | U32
22489 | 0x57D9 | 2 | T5 - Eap | VAh / 0.001 | U32
22491 | 0x57DB | 2 | T6 - Eap | VAh / 0.001 | U32
22493 | 0x57DD | 2 | T7 - Eap | VAh / 0.001 | U32
22495 | 0x57DF | 2 | T8 - Eap | VAh / 0.001 | U32

## Tariff meter (partial) - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24448 | 0x5F80 | Info | 97 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24448 | 0x5F80 | 1 | Tariff number in progress 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16
24449 | 0x5F81 | 2 | T1 - Ea+ | Wh / 0.001 | U32
24451 | 0x5F83 | 2 | T2 - Ea+ | Wh / 0.001 | U32
24453 | 0x5F85 | 2 | T3 - Ea+ | Wh / 0.001 | U32
24455 | 0x5F87 | 2 | T4 - Ea+ | Wh / 0.001 | U32
24457 | 0x5F89 | 2 | T5 - Ea+ | Wh / 0.001 | U32
24459 | 0x5F8B | 2 | T6 - Ea+ | Wh / 0.001 | U32
24461 | 0x5F8D | 2 | T7 - Ea+ | Wh / 0.001 | U32
24463 | 0x5F8F | 2 | T8 - Ea+ | Wh / 0.001 | U32
24465 | 0x5F91 | 2 | T1 - Ea- | Wh / 0.001 | U32
24467 | 0x5F93 | 2 | T2 - Ea- | Wh / 0.001 | U32
24469 | 0x5F95 | 2 | T3 - Ea- | Wh / 0.001 | U32
24471 | 0x5F97 | 2 | T4 - Ea- | Wh / 0.001 | U32
24473 | 0x5F99 | 2 | T5 - Ea- | Wh / 0.001 | U32
24475 | 0x5F9B | 2 | T6 - Ea- | Wh / 0.001 | U32
24477 | 0x5F9D | 2 | T7 - Ea- | Wh / 0.001 | U32
24479 | 0x5F9F | 2 | T8 - Ea- | Wh / 0.001 | U32
24481 | 0x5FA1 | 2 | T1 - Er+ (lagging) | varh / 0.001 | U32
24483 | 0x5FA3 | 2 | T2 - Er+ (lagging) | varh / 0.001 | U32
24485 | 0x5FA5 | 2 | T3 - Er+ (lagging) | varh / 0.001 | U32
24487 | 0x5FA7 | 2 | T4 - Er+ (lagging) | varh / 0.001 | U32
24489 | 0x5FA9 | 2 | T5 - Er+ (lagging) | varh / 0.001 | U32
24491 | 0x5FAB | 2 | T6 - Er+ (lagging) | varh / 0.001 | U32
24493 | 0x5FAD | 2 | T7 - Er+ (lagging) | varh / 0.001 | U32
24495 | 0x5FAF | 2 | T8 - Er+ (lagging) | varh / 0.001 | U32
24497 | 0x5FB1 | 2 | T1 - Er+ (leading) | varh / 0.001 | U32
24499 | 0x5FB3 | 2 | T2 - Er+ (leading) | varh / 0.001 | U32
24501 | 0x5FB5 | 2 | T3 - Er+ (leading) | varh / 0.001 | U32
24503 | 0x5FB7 | 2 | T4 - Er+ (leading) | varh / 0.001 | U32
24505 | 0x5FB9 | 2 | T5 - Er+ (leading) | varh / 0.001 | U32
24507 | 0x5FBB | 2 | T6 - Er+ (leading) | varh / 0.001 | U32
24509 | 0x5FBD | 2 | T7 - Er+ (leading) | varh / 0.001 | U32
24511 | 0x5FBF | 2 | T8 - Er+ (leading) | varh / 0.001 | U32
24513 | 0x5FC1 | 2 | T1 - Er- | varh / 0.001 | U32
24515 | 0x5FC3 | 2 | T2 - Er- | varh / 0.001 | U32
24517 | 0x5FC5 | 2 | T3 - Er- | varh / 0.001 | U32
24519 | 0x5FC7 | 2 | T4 - Er- | varh / 0.001 | U32
24521 | 0x5FC9 | 2 | T5 - Er- | varh / 0.001 | U32
24523 | 0x5FCB | 2 | T6 - Er- | varh / 0.001 | U32
24525 | 0x5FCD | 2 | T7 - Er- | varh / 0.001 | U32
24527 | 0x5FCF | 2 | T8 - Er- | varh / 0.001 | U32
24529 | 0x5FD1 | 2 | T1 - Eap | VAh / 0.001 | U32
24531 | 0x5FD3 | 2 | T2 - Eap | VAh / 0.001 | U32
24533 | 0x5FD5 | 2 | T3 - Eap | VAh / 0.001 | U32
24535 | 0x5FD7 | 2 | T4 - Eap | VAh / 0.001 | U32
24537 | 0x5FD9 | 2 | T5 - Eap | VAh / 0.001 | U32
24539 | 0x5FDB | 2 | T6 - Eap | VAh / 0.001 | U32
24541 | 0x5FDD | 2 | T7 - Eap | VAh / 0.001 | U32
24543 | 0x5FDF | 2 | T8 - Eap | VAh / 0.001 | U32

## Tariff meter (partial) - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26496 | 0x6780 | Info | 97 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26496 | 0x6780 | 1 | Tariff number in progress 0 : Tariff 1 1 : Tariff 2 2 : Tariff 3 3 : Tariff 4 4 : Tariff 5 5 : Tariff 6 6 : Tariff 7 7 : Tariff 8 | - | U16
26497 | 0x6781 | 2 | T1 - Ea+ | Wh / 0.001 | U32
26499 | 0x6783 | 2 | T2 - Ea+ | Wh / 0.001 | U32
26501 | 0x6785 | 2 | T3 - Ea+ | Wh / 0.001 | U32
26503 | 0x6787 | 2 | T4 - Ea+ | Wh / 0.001 | U32
26505 | 0x6789 | 2 | T5 - Ea+ | Wh / 0.001 | U32
26507 | 0x678B | 2 | T6 - Ea+ | Wh / 0.001 | U32
26509 | 0x678D | 2 | T7 - Ea+ | Wh / 0.001 | U32
26511 | 0x678F | 2 | T8 - Ea+ | Wh / 0.001 | U32
26513 | 0x6791 | 2 | T1 - Ea- | Wh / 0.001 | U32
26515 | 0x6793 | 2 | T2 - Ea- | Wh / 0.001 | U32
26517 | 0x6795 | 2 | T3 - Ea- | Wh / 0.001 | U32
26519 | 0x6797 | 2 | T4 - Ea- | Wh / 0.001 | U32
26521 | 0x6799 | 2 | T5 - Ea- | Wh / 0.001 | U32
26523 | 0x679B | 2 | T6 - Ea- | Wh / 0.001 | U32
26525 | 0x679D | 2 | T7 - Ea- | Wh / 0.001 | U32
26527 | 0x679F | 2 | T8 - Ea- | Wh / 0.001 | U32
26529 | 0x67A1 | 2 | T1 - Er+ (lagging) | varh / 0.001 | U32
26531 | 0x67A3 | 2 | T2 - Er+ (lagging) | varh / 0.001 | U32
26533 | 0x67A5 | 2 | T3 - Er+ (lagging) | varh / 0.001 | U32
26535 | 0x67A7 | 2 | T4 - Er+ (lagging) | varh / 0.001 | U32
26537 | 0x67A9 | 2 | T5 - Er+ (lagging) | varh / 0.001 | U32
26539 | 0x67AB | 2 | T6 - Er+ (lagging) | varh / 0.001 | U32
26541 | 0x67AD | 2 | T7 - Er+ (lagging) | varh / 0.001 | U32
26543 | 0x67AF | 2 | T8 - Er+ (lagging) | varh / 0.001 | U32
26545 | 0x67B1 | 2 | T1 - Er+ (leading) | varh / 0.001 | U32
26547 | 0x67B3 | 2 | T2 - Er+ (leading) | varh / 0.001 | U32
26549 | 0x67B5 | 2 | T3 - Er+ (leading) | varh / 0.001 | U32
26551 | 0x67B7 | 2 | T4 - Er+ (leading) | varh / 0.001 | U32
26553 | 0x67B9 | 2 | T5 - Er+ (leading) | varh / 0.001 | U32
26555 | 0x67BB | 2 | T6 - Er+ (leading) | varh / 0.001 | U32
26557 | 0x67BD | 2 | T7 - Er+ (leading) | varh / 0.001 | U32
26559 | 0x67BF | 2 | T8 - Er+ (leading) | varh / 0.001 | U32
26561 | 0x67C1 | 2 | T1 - Er- | varh / 0.001 | U32
26563 | 0x67C3 | 2 | T2 - Er- | varh / 0.001 | U32
26565 | 0x67C5 | 2 | T3 - Er- | varh / 0.001 | U32
26567 | 0x67C7 | 2 | T4 - Er- | varh / 0.001 | U32
26569 | 0x67C9 | 2 | T5 - Er- | varh / 0.001 | U32
26571 | 0x67CB | 2 | T6 - Er- | varh / 0.001 | U32
26573 | 0x67CD | 2 | T7 - Er- | varh / 0.001 | U32
26575 | 0x67CF | 2 | T8 - Er- | varh / 0.001 | U32
26577 | 0x67D1 | 2 | T1 - Eap | VAh / 0.001 | U32
26579 | 0x67D3 | 2 | T2 - Eap | VAh / 0.001 | U32
26581 | 0x67D5 | 2 | T3 - Eap | VAh / 0.001 | U32
26583 | 0x67D7 | 2 | T4 - Eap | VAh / 0.001 | U32
26585 | 0x67D9 | 2 | T5 - Eap | VAh / 0.001 | U32
26587 | 0x67DB | 2 | T6 - Eap | VAh / 0.001 | U32
26589 | 0x67DD | 2 | T7 - Eap | VAh / 0.001 | U32
26591 | 0x67DF | 2 | T8 - Eap | VAh / 0.001 | U32

# Network

## Inst. measurement - Network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36864 | 0x9000 | Info | 37 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36864 | 0x9000 | 2 | Date of last instance | s | DATETIME
36866 | 0x9002 | 1 | Integration time | s / 5 | U16
36867 | 0x9003 | 2 | System Ph-N Voltage | V / 100 | U32
36869 | 0x9005 | 2 | System Ph-Ph Voltage | V / 100 | U32
36871 | 0x9007 | 2 | Frequency | Hz / 1000 | U32
36873 | 0x9009 | 2 | Ph-N Voltage : V1 | V / 100 | U32
36875 | 0x900B | 2 | Ph-N Voltage : V2 | V / 100 | U32
36877 | 0x900D | 2 | Ph-N Voltage : V3 | V / 100 | U32
36879 | 0x900F | 2 | Ph-N Voltage : Vn | V / 100 | U32
36881 | 0x9011 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
36883 | 0x9013 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
36885 | 0x9015 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
36887 | 0x9017 | 2 | Vdir | V / 100 | U32
36889 | 0x9019 | 2 | Vinv | V / 100 | U32
36891 | 0x901B | 2 | Vhom | V / 100 | U32
36893 | 0x901D | 1 | Vnb | % / 100 | U16
36894 | 0x901E | 2 | Udir | V / 100 | U32
36896 | 0x9020 | 2 | Uinv | V / 100 | U32
36898 | 0x9022 | 1 | Unb | % / 100 | U16
36899 | 0x9023 | 1 | Vnba | % / 100 | U16
36900 | 0x9024 | 1 | Unba | % / 100 | U16

## Avg. measurement - Network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36992 | 0x9080 | Info | 37 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36992 | 0x9080 | 2 | Date of last instance | s | DATETIME
36994 | 0x9082 | 1 | Integration time | s | U16
36995 | 0x9083 | 2 | System Ph-N Voltage | V / 100 | U32
36997 | 0x9085 | 2 | System Ph-Ph Voltage | V / 100 | U32
36999 | 0x9087 | 2 | Frequency | Hz / 1000 | U32
37001 | 0x9089 | 2 | Ph-N Voltage : V1 | V / 100 | U32
37003 | 0x908B | 2 | Ph-N Voltage : V2 | V / 100 | U32
37005 | 0x908D | 2 | Ph-N Voltage : V3 | V / 100 | U32
37007 | 0x908F | 2 | Ph-N Voltage : Vn | V / 100 | U32
37009 | 0x9091 | 2 | Ph-Ph Voltage : U12 | V / 100 | U32
37011 | 0x9093 | 2 | Ph-Ph Voltage : U23 | V / 100 | U32
37013 | 0x9095 | 2 | Ph-Ph Voltage : U31 | V / 100 | U32
37015 | 0x9097 | 2 | Vdir | V / 100 | U32
37017 | 0x9099 | 2 | Vinv | V / 100 | U32
37019 | 0x909B | 2 | Vhom | V / 100 | U32
37021 | 0x909D | 1 | Vnb | % / 100 | U16
37022 | 0x909E | 2 | Udir | V / 100 | U32
37024 | 0x90A0 | 2 | Uinv | V / 100 | U32
37026 | 0x90A2 | 1 | Unb | % / 100 | U16
37027 | 0x90A3 | 1 | Vnba | % / 100 | U16
37028 | 0x90A4 | 1 | Unba | % / 100 | U16

## Inst. fundamental measurement - Network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37120 | 0x9100 | Info | 38 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37120 | 0x9100 | 2 | Date of last instance | s | DATETIME
37122 | 0x9102 | 1 | Integration time | s / 5 | U16
37123 | 0x9103 | 2 | Ph-N voltage: V1h1 | V / 100 | U32
37125 | 0x9105 | 2 | Ph-N voltage: V2h1 | V / 100 | U32
37127 | 0x9107 | 2 | Ph-N voltage: V3h1 | V / 100 | U32
37129 | 0x9109 | 2 | Ph-N voltage: Vnh1 | V / 100 | U32
37131 | 0x910B | 1 | Ph-N voltage phase: phV1h1 | ? / 10 | S16
37132 | 0x910C | 1 | Ph-N voltage phase: phV2h1 | ? / 10 | S16
37133 | 0x910D | 1 | Ph-N voltage phase: phV3h1 | ? / 10 | S16
37134 | 0x910E | 1 | Ph-N voltage phase: phVnh1 | ? / 10 | S16
37135 | 0x910F | 2 | Ph-Ph voltage: U12h1 | V / 100 | U32
37137 | 0x9111 | 2 | Ph-Ph voltage: U23h1 | V / 100 | U32
37139 | 0x9113 | 2 | Ph-Ph voltage: U31h1 | V / 100 | U32
37141 | 0x9115 | 1 | Ph-Ph voltage phase: phU12h1 | ? / 10 | S16
37142 | 0x9116 | 1 | Ph-Ph voltage phase: phU23h1 | ? / 10 | S16
37143 | 0x9117 | 1 | Ph-Ph voltage phase: phU31h1 | ? / 10 | S16
37144 | 0x9118 | 1 | Ph-N Voltage total harmonic distortion : THD V1 | % / 100 | U16
37145 | 0x9119 | 1 | Ph-N Voltage total harmonic distortion : THD V2 | % / 100 | U16
37146 | 0x911A | 1 | Ph-N Voltage total harmonic distortion : THD V3 | % / 100 | U16
37147 | 0x911B | 1 | Ph-Ph Voltage total harmonic distortion : THD U12 | % / 100 | U16
37148 | 0x911C | 1 | Ph-Ph Voltage total harmonic distortion : THD U23 | % / 100 | U16
37149 | 0x911D | 1 | Ph-Ph Voltage total harmonic distortion : THD U31 | % / 100 | U16
37150 | 0x911E | 1 | System THD V | % / 100 | U16
37151 | 0x911F | 1 | System THD U | % / 100 | U16
37152 | 0x9120 | 1 | Crest factor : V1 | - / 1000 | U16
37153 | 0x9121 | 1 | Crest factor : V2 | - / 1000 | U16
37154 | 0x9122 | 1 | Crest factor : V3 | - / 1000 | U16
37155 | 0x9123 | 1 | Crest factor : U12 | - / 1000 | U16
37156 | 0x9124 | 1 | Crest factor : U23 | - / 1000 | U16
37157 | 0x9125 | 1 | Crest factor : U31 | - / 1000 | U16

## Inst. quality min/max - Network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37248 | 0x9180 | Info | 108 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37248 | 0x9180 | 1 | Maximum Vnb | % / 100 | U16
37249 | 0x9181 | 2 | Date of maximum Vnb | - | DATETIME
37251 | 0x9183 | 1 | Maximum Vnba | % / 100 | U16
37252 | 0x9184 | 2 | Date of maximum Vnba | - | DATETIME
37254 | 0x9186 | 1 | Maximum Unb | % / 100 | U16
37255 | 0x9187 | 2 | Date of maximum Unb | - | DATETIME
37257 | 0x9189 | 1 | Maximum Unba | % / 100 | U16
37258 | 0x918A | 2 | Date of maximum Unba | - | DATETIME
37260 | 0x918C | 1 | Maximum THD V1 | % / 100 | U16
37261 | 0x918D | 2 | Date of maximum THD V1 | - | DATETIME
37263 | 0x918F | 1 | Maximum THD V2 | % / 100 | U16
37264 | 0x9190 | 2 | Date of maximum THD V2 | - | DATETIME
37266 | 0x9192 | 1 | Maximum THD V3 | % / 100 | U16
37267 | 0x9193 | 2 | Date of maximum THD V3 | - | DATETIME
37269 | 0x9195 | 1 | Maximum THD U12 | % / 100 | U16
37270 | 0x9196 | 2 | Date of maximum THD U12 | - | DATETIME
37272 | 0x9198 | 1 | Maximum THD U23 | % / 100 | U16
37273 | 0x9199 | 2 | Date of maximum THD U23 | - | DATETIME
37275 | 0x919B | 1 | Maximum THD U31 | % / 100 | U16
37276 | 0x919C | 2 | Date of maximum THD U31 | - | DATETIME
37278 | 0x919E | 1 | Minimum Vnb | % / 100 | U16
37279 | 0x919F | 2 | Date of minimum Vnb | - | DATETIME
37281 | 0x91A1 | 1 | Minimum Vnba | % / 100 | U16
37282 | 0x91A2 | 2 | Date of minimum Vnba | - | DATETIME
37284 | 0x91A4 | 1 | Minimum Unb | % / 100 | U16
37285 | 0x91A5 | 2 | Date of minimum Unb | - | DATETIME
37287 | 0x91A7 | 1 | Minimum Unba | % / 100 | U16
37288 | 0x91A8 | 2 | Date of minimum Unba | - | DATETIME
37290 | 0x91AA | 1 | Minimum THD V1 | % / 100 | U16
37291 | 0x91AB | 2 | Date of minimum THD V1 | - | DATETIME
37293 | 0x91AD | 1 | Minimum THD V2 | % / 100 | U16
37294 | 0x91AE | 2 | Date of minimum THD V2 | - | DATETIME
37296 | 0x91B0 | 1 | Minimum THD V3 | % / 100 | U16
37297 | 0x91B1 | 2 | Date of minimum THD V3 | - | DATETIME
37299 | 0x91B3 | 1 | Minimum THD U12 | % / 100 | U16
37300 | 0x91B4 | 2 | Date of minimum THD U12 | - | DATETIME
37302 | 0x91B6 | 1 | Minimum THD U23 | % / 100 | U16
37303 | 0x91B7 | 2 | Date of minimum THD U23 | - | DATETIME
37305 | 0x91B9 | 1 | Minimum THD U31 | % / 100 | U16
37306 | 0x91BA | 2 | Date of minimum THD U31 | - | DATETIME
37308 | 0x91BC | 1 | Maximum THD Vsys | % / 100 | U16
37309 | 0x91BD | 2 | Date of maximum THD Vsys | - | DATETIME
37311 | 0x91BF | 1 | Maximum THD Usys | % / 100 | U16
37312 | 0x91C0 | 2 | Date of maximum THD Usys | - | DATETIME
37314 | 0x91C2 | 1 | Maximum crest factor V1 | - / 1000 | U16
37315 | 0x91C3 | 2 | Date of maximum crest factor V1 | - | DATETIME
37317 | 0x91C5 | 1 | Maximum crest factor V2 | - / 1000 | U16
37318 | 0x91C6 | 2 | Date of maximum crest factor V2 | - | DATETIME
37320 | 0x91C8 | 1 | Maximum crest factor V3 | - / 1000 | U16
37321 | 0x91C9 | 2 | Date of maximum crest factor V3 | - | DATETIME
37323 | 0x91CB | 1 | Maximum crest factor U12 | - / 1000 | U16
37324 | 0x91CC | 2 | Date of maximum crest factor U12 | - | DATETIME
37326 | 0x91CE | 1 | Maximum crest factor U23 | - / 1000 | U16
37327 | 0x91CF | 2 | Date of maximum crest factor U23 | - | DATETIME
37329 | 0x91D1 | 1 | Maximum crest factor U31 | - / 1000 | U16
37330 | 0x91D2 | 2 | Date of maximum crest factor U31 | - | DATETIME
37332 | 0x91D4 | 1 | Minimum crest factor V1 | - / 1000 | U16
37333 | 0x91D5 | 2 | Date of minimum crest factor V1 | - | DATETIME
37335 | 0x91D7 | 1 | Minimum crest factor V2 | - / 1000 | U16
37336 | 0x91D8 | 2 | Date of minimum crest factor V2 | - | DATETIME
37338 | 0x91DA | 1 | Minimum crest factor V3 | - / 1000 | U16
37339 | 0x91DB | 2 | Date of minimum crest factor V3 | - | DATETIME
37341 | 0x91DD | 1 | Minimum crest factor U12 | - / 1000 | U16
37342 | 0x91DE | 2 | Date of minimum crest factor U12 | - | DATETIME
37344 | 0x91E0 | 1 | Minimum crest factor U23 | - / 1000 | U16
37345 | 0x91E1 | 2 | Date of minimum crest factor U23 | - | DATETIME
37347 | 0x91E3 | 1 | Minimum crest factor U31 | - / 1000 | U16
37348 | 0x91E4 | 2 | Date of minimum crest factor U31 | - | DATETIME
37350 | 0x91E6 | 1 | Minimum THD Vsys | % / 100 | U16
37351 | 0x91E7 | 2 | Date of minimum THD Vsys | - | DATETIME
37353 | 0x91E9 | 1 | Minimum THD Usys | % / 100 | U16
37354 | 0x91EA | 2 | Date of minimum THD Usys | - | DATETIME

## Inst. V harmonics - Network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37504 | 0x9280 | Info | 81 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37504 | 0x9280 | 1 | harmonic V1 row 2 | % / 100 | U16
37505 | 0x9281 | 1 | harmonic V2 row 2 | % / 100 | U16
37506 | 0x9282 | 1 | harmonic V3 row 2 | % / 100 | U16
37507 | 0x9283 | 1 | harmonic V1 row 3 | % / 100 | U16
37508 | 0x9284 | 1 | harmonic V2 row 3 | % / 100 | U16
37509 | 0x9285 | 1 | harmonic V3 row 3 | % / 100 | U16
37510 | 0x9286 | 1 | harmonic V1 row 4 | % / 100 | U16
37511 | 0x9287 | 1 | harmonic V2 row 4 | % / 100 | U16
37512 | 0x9288 | 1 | harmonic V3 row 4 | % / 100 | U16
37513 | 0x9289 | 1 | harmonic V1 row 5 | % / 100 | U16
37514 | 0x928A | 1 | harmonic V2 row 5 | % / 100 | U16
37515 | 0x928B | 1 | harmonic V3 row 5 | % / 100 | U16
37516 | 0x928C | 1 | harmonic V1 row 6 | % / 100 | U16
37517 | 0x928D | 1 | harmonic V2 row 6 | % / 100 | U16
37518 | 0x928E | 1 | harmonic V3 row 6 | % / 100 | U16
37519 | 0x928F | 1 | harmonic V1 row 7 | % / 100 | U16
37520 | 0x9290 | 1 | harmonic V2 row 7 | % / 100 | U16
37521 | 0x9291 | 1 | harmonic V3 row 7 | % / 100 | U16
37522 | 0x9292 | 1 | harmonic V1 row 8 | % / 100 | U16
37523 | 0x9293 | 1 | harmonic V2 row 8 | % / 100 | U16
37524 | 0x9294 | 1 | harmonic V3 row 8 | % / 100 | U16
37525 | 0x9295 | 1 | harmonic V1 row 9 | % / 100 | U16
37526 | 0x9296 | 1 | harmonic V2 row 9 | % / 100 | U16
37527 | 0x9297 | 1 | harmonic V3 row 9 | % / 100 | U16
37528 | 0x9298 | 1 | harmonic V1 row 10 | % / 100 | U16
37529 | 0x9299 | 1 | harmonic V2 row 10 | % / 100 | U16
37530 | 0x929A | 1 | harmonic V3 row 10 | % / 100 | U16
37531 | 0x929B | 1 | harmonic V1 row 11 | % / 100 | U16
37532 | 0x929C | 1 | harmonic V2 row 11 | % / 100 | U16
37533 | 0x929D | 1 | harmonic V3 row 11 | % / 100 | U16
37534 | 0x929E | 1 | harmonic V1 row 12 | % / 100 | U16
37535 | 0x929F | 1 | harmonic V2 row 12 | % / 100 | U16
37536 | 0x92A0 | 1 | harmonic V3 row 12 | % / 100 | U16
37537 | 0x92A1 | 1 | harmonic V1 row 13 | % / 100 | U16
37538 | 0x92A2 | 1 | harmonic V2 row 13 | % / 100 | U16
37539 | 0x92A3 | 1 | harmonic V3 row 13 | % / 100 | U16
37540 | 0x92A4 | 1 | harmonic V1 row 14 | % / 100 | U16
37541 | 0x92A5 | 1 | harmonic V2 row 14 | % / 100 | U16
37542 | 0x92A6 | 1 | harmonic V3 row 14 | % / 100 | U16
37543 | 0x92A7 | 1 | harmonic V1 row 15 | % / 100 | U16
37544 | 0x92A8 | 1 | harmonic V2 row 15 | % / 100 | U16
37545 | 0x92A9 | 1 | harmonic V3 row 15 | % / 100 | U16
37546 | 0x92AA | 1 | harmonic V1 row 16 | % / 100 | U16
37547 | 0x92AB | 1 | harmonic V2 row 16 | % / 100 | U16
37548 | 0x92AC | 1 | harmonic V3 row 16 | % / 100 | U16
37549 | 0x92AD | 1 | harmonic V1 row 17 | % / 100 | U16
37550 | 0x92AE | 1 | harmonic V2 row 17 | % / 100 | U16
37551 | 0x92AF | 1 | harmonic V3 row 17 | % / 100 | U16
37552 | 0x92B0 | 1 | harmonic V1 row 18 | % / 100 | U16
37553 | 0x92B1 | 1 | harmonic V2 row 18 | % / 100 | U16
37554 | 0x92B2 | 1 | harmonic V3 row 18 | % / 100 | U16
37555 | 0x92B3 | 1 | harmonic V1 row 19 | % / 100 | U16
37556 | 0x92B4 | 1 | harmonic V2 row 19 | % / 100 | U16
37557 | 0x92B5 | 1 | harmonic V3 row 19 | % / 100 | U16
37558 | 0x92B6 | 1 | harmonic V1 row 20 | % / 100 | U16
37559 | 0x92B7 | 1 | harmonic V2 row 20 | % / 100 | U16
37560 | 0x92B8 | 1 | harmonic V3 row 20 | % / 100 | U16
37561 | 0x92B9 | 1 | harmonic V1 row 21 | % / 100 | U16
37562 | 0x92BA | 1 | harmonic V2 row 21 | % / 100 | U16
37563 | 0x92BB | 1 | harmonic V3 row 21 | % / 100 | U16
37564 | 0x92BC | 1 | harmonic V1 row 22 | % / 100 | U16
37565 | 0x92BD | 1 | harmonic V2 row 22 | % / 100 | U16
37566 | 0x92BE | 1 | harmonic V3 row 22 | % / 100 | U16
37567 | 0x92BF | 1 | harmonic V1 row 23 | % / 100 | U16
37568 | 0x92C0 | 1 | harmonic V2 row 23 | % / 100 | U16
37569 | 0x92C1 | 1 | harmonic V3 row 23 | % / 100 | U16
37570 | 0x92C2 | 1 | harmonic V1 row 24 | % / 100 | U16
37571 | 0x92C3 | 1 | harmonic V2 row 24 | % / 100 | U16
37572 | 0x92C4 | 1 | harmonic V3 row 24 | % / 100 | U16
37573 | 0x92C5 | 1 | harmonic V1 row 25 | % / 100 | U16
37574 | 0x92C6 | 1 | harmonic V2 row 25 | % / 100 | U16
37575 | 0x92C7 | 1 | harmonic V3 row 25 | % / 100 | U16
37576 | 0x92C8 | 1 | harmonic V1 row 26 to 34 | % / 100 | U16
37577 | 0x92C9 | 1 | harmonic V2 row 26 to 34 | % / 100 | U16
37578 | 0x92CA | 1 | harmonic V3 row 26 to 34 | % / 100 | U16
37579 | 0x92CB | 1 | harmonic V1 row 35 to 50 | % / 100 | U16
37580 | 0x92CC | 1 | harmonic V2 row 35 to 50 | % / 100 | U16
37581 | 0x92CD | 1 | harmonic V3 row 35 to 50 | % / 100 | U16
37582 | 0x92CE | 1 | harmonic V1 row 51 to 63 | % / 100 | U16
37583 | 0x92CF | 1 | harmonic V2 row 51 to 63 | % / 100 | U16
37584 | 0x92D0 | 1 | harmonic V3 row 51 to 63 | % / 100 | U16

## Inst. U harmonics - Network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37632 | 0x9300 | Info | 81 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37632 | 0x9300 | 1 | harmonic U12 row 2 | % / 100 | U16
37633 | 0x9301 | 1 | harmonic U23 row 2 | % / 100 | U16
37634 | 0x9302 | 1 | harmonic U31 row 2 | % / 100 | U16
37635 | 0x9303 | 1 | harmonic U12 row 3 | % / 100 | U16
37636 | 0x9304 | 1 | harmonic U23 row 3 | % / 100 | U16
37637 | 0x9305 | 1 | harmonic U31 row 3 | % / 100 | U16
37638 | 0x9306 | 1 | harmonic U12 row 4 | % / 100 | U16
37639 | 0x9307 | 1 | harmonic U23 row 4 | % / 100 | U16
37640 | 0x9308 | 1 | harmonic U31 row 4 | % / 100 | U16
37641 | 0x9309 | 1 | harmonic U12 row 5 | % / 100 | U16
37642 | 0x930A | 1 | harmonic U23 row 5 | % / 100 | U16
37643 | 0x930B | 1 | harmonic U31 row 5 | % / 100 | U16
37644 | 0x930C | 1 | harmonic U12 row 6 | % / 100 | U16
37645 | 0x930D | 1 | harmonic U23 row 6 | % / 100 | U16
37646 | 0x930E | 1 | harmonic U31 row 6 | % / 100 | U16
37647 | 0x930F | 1 | harmonic U12 row 7 | % / 100 | U16
37648 | 0x9310 | 1 | harmonic U23 row 7 | % / 100 | U16
37649 | 0x9311 | 1 | harmonic U31 row 7 | % / 100 | U16
37650 | 0x9312 | 1 | harmonic U12 row 8 | % / 100 | U16
37651 | 0x9313 | 1 | harmonic U23 row 8 | % / 100 | U16
37652 | 0x9314 | 1 | harmonic U31 row 8 | % / 100 | U16
37653 | 0x9315 | 1 | harmonic U12 row 9 | % / 100 | U16
37654 | 0x9316 | 1 | harmonic U23 row 9 | % / 100 | U16
37655 | 0x9317 | 1 | harmonic U31 row 9 | % / 100 | U16
37656 | 0x9318 | 1 | harmonic U12 row 10 | % / 100 | U16
37657 | 0x9319 | 1 | harmonic U23 row 10 | % / 100 | U16
37658 | 0x931A | 1 | harmonic U31 row 10 | % / 100 | U16
37659 | 0x931B | 1 | harmonic U12 row 11 | % / 100 | U16
37660 | 0x931C | 1 | harmonic U23 row 11 | % / 100 | U16
37661 | 0x931D | 1 | harmonic U31 row 11 | % / 100 | U16
37662 | 0x931E | 1 | harmonic U12 row 12 | % / 100 | U16
37663 | 0x931F | 1 | harmonic U23 row 12 | % / 100 | U16
37664 | 0x9320 | 1 | harmonic U31 row 12 | % / 100 | U16
37665 | 0x9321 | 1 | harmonic U12 row 13 | % / 100 | U16
37666 | 0x9322 | 1 | harmonic U23 row 13 | % / 100 | U16
37667 | 0x9323 | 1 | harmonic U31 row 13 | % / 100 | U16
37668 | 0x9324 | 1 | harmonic U12 row 14 | % / 100 | U16
37669 | 0x9325 | 1 | harmonic U23 row 14 | % / 100 | U16
37670 | 0x9326 | 1 | harmonic U31 row 14 | % / 100 | U16
37671 | 0x9327 | 1 | harmonic U12 row 15 | % / 100 | U16
37672 | 0x9328 | 1 | harmonic U23 row 15 | % / 100 | U16
37673 | 0x9329 | 1 | harmonic U31 row 15 | % / 100 | U16
37674 | 0x932A | 1 | harmonic U12 row 16 | % / 100 | U16
37675 | 0x932B | 1 | harmonic U23 row 16 | % / 100 | U16
37676 | 0x932C | 1 | harmonic U31 row 16 | % / 100 | U16
37677 | 0x932D | 1 | harmonic U12 row 17 | % / 100 | U16
37678 | 0x932E | 1 | harmonic U23 row 17 | % / 100 | U16
37679 | 0x932F | 1 | harmonic U31 row 17 | % / 100 | U16
37680 | 0x9330 | 1 | harmonic U12 row 18 | % / 100 | U16
37681 | 0x9331 | 1 | harmonic U23 row 18 | % / 100 | U16
37682 | 0x9332 | 1 | harmonic U31 row 18 | % / 100 | U16
37683 | 0x9333 | 1 | harmonic U12 row 19 | % / 100 | U16
37684 | 0x9334 | 1 | harmonic U23 row 19 | % / 100 | U16
37685 | 0x9335 | 1 | harmonic U31 row 19 | % / 100 | U16
37686 | 0x9336 | 1 | harmonic U12 row 20 | % / 100 | U16
37687 | 0x9337 | 1 | harmonic U23 row 20 | % / 100 | U16
37688 | 0x9338 | 1 | harmonic U31 row 20 | % / 100 | U16
37689 | 0x9339 | 1 | harmonic U12 row 21 | % / 100 | U16
37690 | 0x933A | 1 | harmonic U23 row 21 | % / 100 | U16
37691 | 0x933B | 1 | harmonic U31 row 21 | % / 100 | U16
37692 | 0x933C | 1 | harmonic U12 row 22 | % / 100 | U16
37693 | 0x933D | 1 | harmonic U23 row 22 | % / 100 | U16
37694 | 0x933E | 1 | harmonic U31 row 22 | % / 100 | U16
37695 | 0x933F | 1 | harmonic U12 row 23 | % / 100 | U16
37696 | 0x9340 | 1 | harmonic U23 row 23 | % / 100 | U16
37697 | 0x9341 | 1 | harmonic U31 row 23 | % / 100 | U16
37698 | 0x9342 | 1 | harmonic U12 row 24 | % / 100 | U16
37699 | 0x9343 | 1 | harmonic U23 row 24 | % / 100 | U16
37700 | 0x9344 | 1 | harmonic U31 row 24 | % / 100 | U16
37701 | 0x9345 | 1 | harmonic U12 row 25 | % / 100 | U16
37702 | 0x9346 | 1 | harmonic U23 row 25 | % / 100 | U16
37703 | 0x9347 | 1 | harmonic U31 row 25 | % / 100 | U16
37704 | 0x9348 | 1 | harmonic U12 row 26 to 34 | % / 100 | U16
37705 | 0x9349 | 1 | harmonic U23 row 26 to 34 | % / 100 | U16
37706 | 0x934A | 1 | harmonic U31 row 26 to 34 | % / 100 | U16
37707 | 0x934B | 1 | harmonic U12 row 35 to 50 | % / 100 | U16
37708 | 0x934C | 1 | harmonic U23 row 35 to 50 | % / 100 | U16
37709 | 0x934D | 1 | harmonic U31 row 35 to 50 | % / 100 | U16
37710 | 0x934E | 1 | harmonic U12 row 51 to 63 | % / 100 | U16
37711 | 0x934F | 1 | harmonic U23 row 51 to 63 | % / 100 | U16
37712 | 0x9350 | 1 | harmonic U31 row 51 to 63 | % / 100 | U16

## Reset min/max - Network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37744 | 0x9370 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37744 | 0x9370 | 1 | Erase : These values could be combine all 0x0001 : Instantaneous Min/Max V unb 0x0002 : Instantaneous Min/Max U unb 0x0400 : Instantaneous Min/Max THD V 0x0800 : Instantaneous Min/Max THD U 0x2000 : Instantaneous Min/Max Crest Fact. V 0x4000 : Instantaneous Min/Max Crest Fact. U 0xFFFF : Instantaneous Min/Max ALL | - | U16_HEX

# Settings

## Power measurement settings

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
34816 | 0x8800 | Settings | 7 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
34816 | 0x8800 | 1 | Integration time for instantaneous | s / 5 | U16
34817 | 0x8801 | 1 | Integration time for average | min | U16
34818 | 0x8802 | 1 | Compute method for reactive and apparent powers : 0 : Arithmetic 1 : Vector | - | U16
34819 | 0x8803 | 1 | THD type : 0 : THD (fundamental) 1 : thd (RMS) | - | U16
34820 | 0x8804 | 1 | THD method : 0 : Total 1 : Spectrum | - | U16
34821 | 0x8805 | 1 | THD spectrum limit : 0 : Rank 40 1 : Rank 63 | - | U16
34822 | 0x8806 | 1 | Phase to neutral voltage lowest level | V | U16
34823 | 0x8807 | 1 | PF convention 0 : IEC 1 : IEEE | - | U16

## Energy measurement settings

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
34832 | 0x8810 | Settings | 28 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
34832 | 0x8810 | 1 | Integration time for load curve | min | U16
34833 | 0x8811 | 1 | Load curve top synchro source : 0 : Internal RTC 1 : External input 2 : External communication | - | U16
34834 | 0x8812 | 1 | Load selected for metrological LED: 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 254 : Sum of all loads | - | U16
34835 | 0x8813 | 1 | Energy associated to metrological LED: 0 : Positive active energy 1 : Negative active energy 2 : Positive reactive energy 3 : Negative reactive energy 4 : Apparent energy | - | U16
34836 | 0x8814 | 1 | Load curve point data 1 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34837 | 0x8815 | 1 | Load curve point data 1 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34838 | 0x8816 | 1 | Load curve point data 2 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34839 | 0x8817 | 1 | Load curve point data 2 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34840 | 0x8818 | 1 | Load curve point data 3 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34841 | 0x8819 | 1 | Load curve point data 3 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34842 | 0x881A | 1 | Load curve point data 4 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34843 | 0x881B | 1 | Load curve point data 4 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34844 | 0x881C | 1 | Load curve point data 5 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34845 | 0x881D | 1 | Load curve point data 5 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34846 | 0x881E | 1 | Load curve point data 6 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34847 | 0x881F | 1 | Load curve point data 6 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34848 | 0x8820 | 1 | Load curve point data 7 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34849 | 0x8821 | 1 | Load curve point data 7 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34850 | 0x8822 | 1 | Load curve point data 8 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34851 | 0x8823 | 1 | Load curve point data 8 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34852 | 0x8824 | 1 | Load curve point data 9 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34853 | 0x8825 | 1 | Load curve point data 9 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34854 | 0x8826 | 1 | Load curve point data 10 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34855 | 0x8827 | 1 | Load curve point data 10 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34856 | 0x8828 | 1 | Load curve point data 11 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34857 | 0x8829 | 1 | Load curve point data 11 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16
34858 | 0x882A | 1 | Load curve point data 12 associated load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Undefined | - | U16
34859 | 0x882B | 1 | Load curve point data 12 associated power 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S 5 : Unused | - | U16

## Tariff settings

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
35216 | 0x8990 | Settings | 10 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
35216 | 0x8990 | 1 | Number of tariff used (0 to 8) | - | U16
35217 | 0x8991 | 1 | Source 0 : Not used 1 : COM 2 : Inputs | - | U16
35218 | 0x8992 | 1 | Reserved | - | -
35219 | 0x8993 | 1 | Reserved | - | -
35220 | 0x8994 | 1 | Reserved | - | -
35221 | 0x8995 | 1 | Reserved | - | -
35222 | 0x8996 | 1 | Reserved | - | -
35223 | 0x8997 | 1 | Reserved | - | -
35224 | 0x8998 | 1 | Reserved | - | -
35225 | 0x8999 | 1 | Reserved | - | -

# Extensions

# Multi-fluid

## Settings of Multi-fluid #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10560 | 0x2940 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10560 | 0x2940 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10561 | 0x2941 | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10562 | 0x2942 | 8 | Reserved | - | -
10570 | 0x294A | 1 | Nature | - | U8
10571 | 0x294B | 1 | Usage | - | U8

## Settings of Multi-fluid #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10581 | 0x2955 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10581 | 0x2955 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10582 | 0x2956 | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10583 | 0x2957 | 8 | Reserved | - | -
10591 | 0x295F | 1 | Nature | - | U8
10592 | 0x2960 | 1 | Usage | - | U8

## Settings of Multi-fluid #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10602 | 0x296A | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10602 | 0x296A | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10603 | 0x296B | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10604 | 0x296C | 8 | Reserved | - | -
10612 | 0x2974 | 1 | Nature | - | U8
10613 | 0x2975 | 1 | Usage | - | U8

## Settings of Multi-fluid #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10623 | 0x297F | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10623 | 0x297F | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10624 | 0x2980 | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10625 | 0x2981 | 8 | Reserved | - | -
10633 | 0x2989 | 1 | Nature | - | U8
10634 | 0x298A | 1 | Usage | - | U8

## Settings of Multi-fluid #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10644 | 0x2994 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10644 | 0x2994 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10645 | 0x2995 | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10646 | 0x2996 | 8 | Reserved | - | -
10654 | 0x299E | 1 | Nature | - | U8
10655 | 0x299F | 1 | Usage | - | U8

## Settings of Multi-fluid #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10665 | 0x29A9 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10665 | 0x29A9 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10666 | 0x29AA | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10667 | 0x29AB | 8 | Reserved | - | -
10675 | 0x29B3 | 1 | Nature | - | U8
10676 | 0x29B4 | 1 | Usage | - | U8

## Settings of Multi-fluid #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10686 | 0x29BE | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10686 | 0x29BE | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10687 | 0x29BF | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10688 | 0x29C0 | 8 | Reserved | - | -
10696 | 0x29C8 | 1 | Nature | - | U8
10697 | 0x29C9 | 1 | Usage | - | U8

## Settings of Multi-fluid #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10707 | 0x29D3 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10707 | 0x29D3 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10708 | 0x29D4 | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10709 | 0x29D5 | 8 | Reserved | - | -
10717 | 0x29DD | 1 | Nature | - | U8
10718 | 0x29DE | 1 | Usage | - | U8

## Settings of Multi-fluid #9

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10728 | 0x29E8 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10728 | 0x29E8 | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10729 | 0x29E9 | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10730 | 0x29EA | 8 | Reserved | - | -
10738 | 0x29F2 | 1 | Nature | - | U8
10739 | 0x29F3 | 1 | Usage | - | U8

## Settings of Multi-fluid #10

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10749 | 0x29FD | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10749 | 0x29FD | 1 | Enabled 0 : Disabled 1 : Enabled | - | U8
10750 | 0x29FE | 1 | SrcIdx 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
10751 | 0x29FF | 8 | Reserved | - | -
10759 | 0x2A07 | 1 | Nature | - | U8
10760 | 0x2A08 | 1 | Usage | - | U8

## Multi-fluid feeder #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10240 | 0x2800 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10240 | 0x2800 | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10241 | 0x2801 | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10242 | 0x2802 | 8 | Reserved | - | -
10250 | 0x280A | 1 | Nature | - | U8
10251 | 0x280B | 1 | Usage | - | U8
10252 | 0x280C | 4 | Partial | - | S64
10256 | 0x2810 | 4 | Total | - | S64
10260 | 0x2814 | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10261 | 0x2815 | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10271 | 0x281F | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10271 | 0x281F | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10272 | 0x2820 | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10273 | 0x2821 | 8 | Reserved | - | -
10281 | 0x2829 | 1 | Nature | - | U8
10282 | 0x282A | 1 | Usage | - | U8
10283 | 0x282B | 4 | Partial | - | S64
10287 | 0x282F | 4 | Total | - | S64
10291 | 0x2833 | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10292 | 0x2834 | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10302 | 0x283E | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10302 | 0x283E | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10303 | 0x283F | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10304 | 0x2840 | 8 | Reserved | - | -
10312 | 0x2848 | 1 | Nature | - | U8
10313 | 0x2849 | 1 | Usage | - | U8
10314 | 0x284A | 4 | Partial | - | S64
10318 | 0x284E | 4 | Total | - | S64
10322 | 0x2852 | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10323 | 0x2853 | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10333 | 0x285D | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10333 | 0x285D | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10334 | 0x285E | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10335 | 0x285F | 8 | Reserved | - | -
10343 | 0x2867 | 1 | Nature | - | U8
10344 | 0x2868 | 1 | Usage | - | U8
10345 | 0x2869 | 4 | Partial | - | S64
10349 | 0x286D | 4 | Total | - | S64
10353 | 0x2871 | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10354 | 0x2872 | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10364 | 0x287C | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10364 | 0x287C | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10365 | 0x287D | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10366 | 0x287E | 8 | Reserved | - | -
10374 | 0x2886 | 1 | Nature | - | U8
10375 | 0x2887 | 1 | Usage | - | U8
10376 | 0x2888 | 4 | Partial | - | S64
10380 | 0x288C | 4 | Total | - | S64
10384 | 0x2890 | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10385 | 0x2891 | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10395 | 0x289B | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10395 | 0x289B | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10396 | 0x289C | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10397 | 0x289D | 8 | Reserved | - | -
10405 | 0x28A5 | 1 | Nature | - | U8
10406 | 0x28A6 | 1 | Usage | - | U8
10407 | 0x28A7 | 4 | Partial | - | S64
10411 | 0x28AB | 4 | Total | - | S64
10415 | 0x28AF | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10416 | 0x28B0 | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10426 | 0x28BA | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10426 | 0x28BA | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10427 | 0x28BB | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10428 | 0x28BC | 8 | Reserved | - | -
10436 | 0x28C4 | 1 | Nature | - | U8
10437 | 0x28C5 | 1 | Usage | - | U8
10438 | 0x28C6 | 4 | Partial | - | S64
10442 | 0x28CA | 4 | Total | - | S64
10446 | 0x28CE | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10447 | 0x28CF | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10457 | 0x28D9 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10457 | 0x28D9 | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10458 | 0x28DA | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10459 | 0x28DB | 8 | Reserved | - | -
10467 | 0x28E3 | 1 | Nature | - | U8
10468 | 0x28E4 | 1 | Usage | - | U8
10469 | 0x28E5 | 4 | Partial | - | S64
10473 | 0x28E9 | 4 | Total | - | S64
10477 | 0x28ED | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10478 | 0x28EE | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #9

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10488 | 0x28F8 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10488 | 0x28F8 | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10489 | 0x28F9 | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10490 | 0x28FA | 8 | Reserved | - | -
10498 | 0x2902 | 1 | Nature | - | U8
10499 | 0x2903 | 1 | Usage | - | U8
10500 | 0x2904 | 4 | Partial | - | S64
10504 | 0x2908 | 4 | Total | - | S64
10508 | 0x290C | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10509 | 0x290D | 2 | Weight | - / 100 | S32

## Multi-fluid feeder #10

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
10519 | 0x2917 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
10519 | 0x2917 | 1 | Enable 0 : Disabled 1 : Enabled | - | U8
10520 | 0x2918 | 1 | Status 0 : eMffSrcNotAvailable 1 : eMffSrcAvailable 2 : eMffSrcUnknown | - | U8
10521 | 0x2919 | 8 | Reserved | - | -
10529 | 0x2921 | 1 | Nature | - | U8
10530 | 0x2922 | 1 | Usage | - | U8
10531 | 0x2923 | 4 | Partial | - | S64
10535 | 0x2927 | 4 | Total | - | S64
10539 | 0x292B | 1 | Unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
10540 | 0x292C | 2 | Weight | - / 100 | S32

# I/O

# Logical I/O

## Settings of logical input - #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11008 | 0x2B00 | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11008 | 0x2B00 | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11009 | 0x2B01 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11010 | 0x2B02 | 2 | Pulse meter weight | - / 100 | S32
11012 | 0x2B04 | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11013 | 0x2B05 | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11015 | 0x2B07 | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11015 | 0x2B07 | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11016 | 0x2B08 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11017 | 0x2B09 | 2 | Pulse meter weight | - / 100 | S32
11019 | 0x2B0B | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11020 | 0x2B0C | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11022 | 0x2B0E | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11022 | 0x2B0E | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11023 | 0x2B0F | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11024 | 0x2B10 | 2 | Pulse meter weight | - / 100 | S32
11026 | 0x2B12 | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11027 | 0x2B13 | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11029 | 0x2B15 | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11029 | 0x2B15 | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11030 | 0x2B16 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11031 | 0x2B17 | 2 | Pulse meter weight | - / 100 | S32
11033 | 0x2B19 | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11034 | 0x2B1A | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11036 | 0x2B1C | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11036 | 0x2B1C | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11037 | 0x2B1D | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11038 | 0x2B1E | 2 | Pulse meter weight | - / 100 | S32
11040 | 0x2B20 | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11041 | 0x2B21 | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11043 | 0x2B23 | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11043 | 0x2B23 | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11044 | 0x2B24 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11045 | 0x2B25 | 2 | Pulse meter weight | - / 100 | S32
11047 | 0x2B27 | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11048 | 0x2B28 | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11050 | 0x2B2A | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11050 | 0x2B2A | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11051 | 0x2B2B | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11052 | 0x2B2C | 2 | Pulse meter weight | - / 100 | S32
11054 | 0x2B2E | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11055 | 0x2B2F | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11057 | 0x2B31 | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11057 | 0x2B31 | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11058 | 0x2B32 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11059 | 0x2B33 | 2 | Pulse meter weight | - / 100 | S32
11061 | 0x2B35 | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11062 | 0x2B36 | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #9

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11064 | 0x2B38 | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11064 | 0x2B38 | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11065 | 0x2B39 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11066 | 0x2B3A | 2 | Pulse meter weight | - / 100 | S32
11068 | 0x2B3C | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11069 | 0x2B3D | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical input - #10

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11071 | 0x2B3F | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11071 | 0x2B3F | 1 | Mode 0 : Bin State and Pulse meter 1 : Top synchro (only for input 1) 2 : Trip breaker (only for inputs 1 & 2) 3 : Tariff (1-2) 4 : Tariff (3-4) 5 : Tariff (5-8) | - | U8
11072 | 0x2B40 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8
11073 | 0x2B41 | 2 | Pulse meter weight | - / 100 | S32
11075 | 0x2B43 | 1 | Pulse meter unit 0 : Wh 1 : varh 2 : VAh 3 : m3 4 : Nm3 5 : J 6 : Imp 7 : L 8 : Custom Unit 10 : kWh 11 : kvarh 12 : kVAh 13 : km3 14 : kNm3 15 : kJ 16 : kImp 17 : kL 18 : kCustom Unit 20 : MWh 21 : Mvarh 22 : MVAh 23 : Mm3 24 : MNm3 25 : MJ 26 : MImp 27 : ML 28 : MCustom Unit 30 : GWh 31 : Gvarh 32 : GVAh 33 : Gm3 34 : GNm3 35 : GJ 36 : GImp 37 : GL 38 : GCustom Unit | - | U8
11076 | 0x2B44 | 1 | Time OnOff (only for Pulse Meter) | s / 100 | U8

## Settings of logical output - #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11104 | 0x2B60 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11104 | 0x2B60 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8

## Settings of logical output - #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11105 | 0x2B61 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11105 | 0x2B61 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8

## Settings of logical output - #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11106 | 0x2B62 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11106 | 0x2B62 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8

## Settings of logical output - #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11107 | 0x2B63 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11107 | 0x2B63 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8

## Settings of logical output - #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11108 | 0x2B64 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11108 | 0x2B64 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8

## Settings of logical output - #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11109 | 0x2B65 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11109 | 0x2B65 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8

## Settings of logical output - #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11110 | 0x2B66 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11110 | 0x2B66 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8

## Settings of logical output - #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11111 | 0x2B67 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11111 | 0x2B67 | 1 | Type 0 : Normally opened 1 : Normally closed | - | U8

## Logical Input

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11248 | 0x2BF0 | Info | 14 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11248 | 0x2BF0 | 1 | Inputs number | - | U16
11249 | 0x2BF1 | 1 | Bit x : Input x Available (1)/Not available (0) | - | U16_HEX
11250 | 0x2BF2 | 1 | Bit x : Input x Activated (1)/Deactivated (0) | - | U16_HEX
11251 | 0x2BF3 | 1 | Bit x : Input x NC (1)/NO (0) | - | U16_HEX
11252 | 0x2BF4 | 1 | Input 1 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11253 | 0x2BF5 | 1 | Input 2 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11254 | 0x2BF6 | 1 | Input 3 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11255 | 0x2BF7 | 1 | Input 4 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11256 | 0x2BF8 | 1 | Input 5 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11257 | 0x2BF9 | 1 | Input 6 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11258 | 0x2BFA | 1 | Input 7 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11259 | 0x2BFB | 1 | Input 8 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11260 | 0x2BFC | 1 | Input 9 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16
11261 | 0x2BFD | 1 | Input 10 function 0 : eFctNone 1 : eFctAlmAck 2 : eFctAlmIn 4 : eFctMff 6 : eFctTopSynchro 7 : eFctTrip 8 : eFctTariff 255 : eFctMutiple | - | U16

## Logical Output

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11280 | 0x2C10 | Settings | 14 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11280 | 0x2C10 | 1 | Outputs number | - | U16
11281 | 0x2C11 | 1 | Bit x : Output x Available (1)/Not available (0) | - | U16_HEX
11282 | 0x2C12 | 1 | Bit x : Output x Activated (1)/Deactivated (0) | - | U16_HEX
11283 | 0x2C13 | 1 | Bit x : Output x NC (1)/NO (0) | - | U16_HEX
11284 | 0x2C14 | 1 | Bit x : Output x Cmd Deactivate Yes (1)/No (0) | - | U16_HEX
11285 | 0x2C15 | 1 | Bit x : Output x Cmd Activate Yes (1)/No (0) | - | U16_HEX
11286 | 0x2C16 | 1 | Output 1 function 0 : eFctNone 3 : eFctAlmReport 5 : eFctLoadShedding 255 : eFctMutiple | - | U16
11287 | 0x2C17 | 1 | Output 2 function 0 : eFctNone 3 : eFctAlmReport 5 : eFctLoadShedding 255 : eFctMutiple | - | U16
11288 | 0x2C18 | 1 | Output 3 function 0 : eFctNone 3 : eFctAlmReport 5 : eFctLoadShedding 255 : eFctMutiple | - | U16
11289 | 0x2C19 | 1 | Output 4 function 0 : eFctNone 3 : eFctAlmReport 5 : eFctLoadShedding 255 : eFctMutiple | - | U16
11290 | 0x2C1A | 1 | Output 5 function 0 : eFctNone 3 : eFctAlmReport 5 : eFctLoadShedding 255 : eFctMutiple | - | U16
11291 | 0x2C1B | 1 | Output 6 function 0 : eFctNone 3 : eFctAlmReport 5 : eFctLoadShedding 255 : eFctMutiple | - | U16
11292 | 0x2C1C | 1 | Output 7 function 0 : eFctNone 3 : eFctAlmReport 5 : eFctLoadShedding 255 : eFctMutiple | - | U16
11293 | 0x2C1D | 1 | Output 8 function 0 : eFctNone 3 : eFctAlmReport 5 : eFctLoadShedding 255 : eFctMutiple | - | U16

## Circuit breaker / Trip unit state

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11312 | 0x2C30 | Info | 6 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11312 | 0x2C30 | 1 | Breaker state 0 : Opened 1 : Closed | - | U8
11313 | 0x2C31 | 1 | Trip state 0 : No trip 1 : Trip | - | U8
11314 | 0x2C32 | 2 | Trip count | - | U32
11316 | 0x2C34 | 2 | Last trip date | - | DATETIME

## Input Pulse Meters Reset

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11318 | 0x2C36 | Commands | 2 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11318 | 0x2C36 | 1 | Erase pulse: These values could be combine all 0x0001 : Input pulse counter 1 0x0002 : Input pulse counter 2 0x0004 : Input pulse counter 3 0x0008 : Input pulse counter 4 0x0010 : Input pulse counter 5 0x0020 : Input pulse counter 6 0x0040 : Input pulse counter 7 0x0080 : Input pulse counter 8 0x0100 : Input pulse counter 9 0x0200 : Input pulse counter 10 0x03FF : Input pulse counter ALL | - | U16_HEX
11319 | 0x2C37 | 1 | Erase Trip count 0 : No erase 1 : Erase count | - | U8

# Analog I/O

## Settings of analog input #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11328 | 0x2C40 | Settings | 13 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11328 | 0x2C40 | 5 | Reserved | - | -
11333 | 0x2C45 | 1 | Input Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11334 | 0x2C46 | 1 | Input Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : custom unit 13 : - | - | U8
11335 | 0x2C47 | 1 | Input X_Pt1 | A / 1000 | U8
11336 | 0x2C48 | 2 | Input Y_Pt1 | - | S32
11338 | 0x2C4A | 1 | Input X_Pt2 | A / 1000 | U8
11339 | 0x2C4B | 2 | Input Y_Pt2 | - | S32

## Settings of analog input #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11341 | 0x2C4D | Settings | 13 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11341 | 0x2C4D | 5 | Reserved | - | -
11346 | 0x2C52 | 1 | Input Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11347 | 0x2C53 | 1 | Input Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : custom unit 13 : - | - | U8
11348 | 0x2C54 | 1 | Input X_Pt1 | A / 1000 | U8
11349 | 0x2C55 | 2 | Input Y_Pt1 | - | S32
11351 | 0x2C57 | 1 | Input X_Pt2 | A / 1000 | U8
11352 | 0x2C58 | 2 | Input Y_Pt2 | - | S32

## Settings of analog input #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11354 | 0x2C5A | Settings | 13 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11354 | 0x2C5A | 5 | Reserved | - | -
11359 | 0x2C5F | 1 | Input Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11360 | 0x2C60 | 1 | Input Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : custom unit 13 : - | - | U8
11361 | 0x2C61 | 1 | Input X_Pt1 | A / 1000 | U8
11362 | 0x2C62 | 2 | Input Y_Pt1 | - | S32
11364 | 0x2C64 | 1 | Input X_Pt2 | A / 1000 | U8
11365 | 0x2C65 | 2 | Input Y_Pt2 | - | S32

## Settings of analog input #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11367 | 0x2C67 | Settings | 13 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11367 | 0x2C67 | 5 | Reserved | - | -
11372 | 0x2C6C | 1 | Input Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11373 | 0x2C6D | 1 | Input Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : custom unit 13 : - | - | U8
11374 | 0x2C6E | 1 | Input X_Pt1 | A / 1000 | U8
11375 | 0x2C6F | 2 | Input Y_Pt1 | - | S32
11377 | 0x2C71 | 1 | Input X_Pt2 | A / 1000 | U8
11378 | 0x2C72 | 2 | Input Y_Pt2 | - | S32

## Settings of analog input #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11380 | 0x2C74 | Settings | 13 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11380 | 0x2C74 | 5 | Reserved | - | -
11385 | 0x2C79 | 1 | Input Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11386 | 0x2C7A | 1 | Input Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : custom unit 13 : - | - | U8
11387 | 0x2C7B | 1 | Input X_Pt1 | A / 1000 | U8
11388 | 0x2C7C | 2 | Input Y_Pt1 | - | S32
11390 | 0x2C7E | 1 | Input X_Pt2 | A / 1000 | U8
11391 | 0x2C7F | 2 | Input Y_Pt2 | - | S32

## Settings of analog input #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11393 | 0x2C81 | Settings | 13 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11393 | 0x2C81 | 5 | Reserved | - | -
11398 | 0x2C86 | 1 | Input Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11399 | 0x2C87 | 1 | Input Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : custom unit 13 : - | - | U8
11400 | 0x2C88 | 1 | Input X_Pt1 | A / 1000 | U8
11401 | 0x2C89 | 2 | Input Y_Pt1 | - | S32
11403 | 0x2C8B | 1 | Input X_Pt2 | A / 1000 | U8
11404 | 0x2C8C | 2 | Input Y_Pt2 | - | S32

## Settings of analog input #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11406 | 0x2C8E | Settings | 13 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11406 | 0x2C8E | 5 | Reserved | - | -
11411 | 0x2C93 | 1 | Input Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11412 | 0x2C94 | 1 | Input Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : custom unit 13 : - | - | U8
11413 | 0x2C95 | 1 | Input X_Pt1 | A / 1000 | U8
11414 | 0x2C96 | 2 | Input Y_Pt1 | - | S32
11416 | 0x2C98 | 1 | Input X_Pt2 | A / 1000 | U8
11417 | 0x2C99 | 2 | Input Y_Pt2 | - | S32

## Settings of analog input #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11419 | 0x2C9B | Settings | 13 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11419 | 0x2C9B | 5 | Reserved | - | -
11424 | 0x2CA0 | 1 | Input Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11425 | 0x2CA1 | 1 | Input Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : custom unit 13 : - | - | U8
11426 | 0x2CA2 | 1 | Input X_Pt1 | A / 1000 | U8
11427 | 0x2CA3 | 2 | Input Y_Pt1 | - | S32
11429 | 0x2CA5 | 1 | Input X_Pt2 | A / 1000 | U8
11430 | 0x2CA6 | 2 | Input Y_Pt2 | - | S32

## Settings of analog output #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11440 | 0x2CB0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11440 | 0x2CB0 | 5 | Reserved | - | -
11445 | 0x2CB5 | 1 | Output Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11446 | 0x2CB6 | 1 | Output Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : Custom unit 13 : - | - | U8
11447 | 0x2CB7 | 1 | Output X_Pt1 | A / 1000 | U8
11448 | 0x2CB8 | 2 | Output Y_Pt1 | - | S32
11450 | 0x2CBA | 1 | Output X_Pt2 | A / 1000 | U8
11451 | 0x2CBB | 2 | Output Y_Pt2 | - | S32
11453 | 0x2CBD | 2 | Output Variable ServiceID | - | U32
11455 | 0x2CBF | 1 | Output Variable Instance | - | U16

## Settings of analog output #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11456 | 0x2CC0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11456 | 0x2CC0 | 5 | Reserved | - | -
11461 | 0x2CC5 | 1 | Output Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11462 | 0x2CC6 | 1 | Output Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : Custom unit 13 : - | - | U8
11463 | 0x2CC7 | 1 | Output X_Pt1 | A / 1000 | U8
11464 | 0x2CC8 | 2 | Output Y_Pt1 | - | S32
11466 | 0x2CCA | 1 | Output X_Pt2 | A / 1000 | U8
11467 | 0x2CCB | 2 | Output Y_Pt2 | - | S32
11469 | 0x2CCD | 2 | Output Variable ServiceID | - | U32
11471 | 0x2CCF | 1 | Output Variable Instance | - | U16

## Settings of analog output #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11472 | 0x2CD0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11472 | 0x2CD0 | 5 | Reserved | - | -
11477 | 0x2CD5 | 1 | Output Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11478 | 0x2CD6 | 1 | Output Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : Custom unit 13 : - | - | U8
11479 | 0x2CD7 | 1 | Output X_Pt1 | A / 1000 | U8
11480 | 0x2CD8 | 2 | Output Y_Pt1 | - | S32
11482 | 0x2CDA | 1 | Output X_Pt2 | A / 1000 | U8
11483 | 0x2CDB | 2 | Output Y_Pt2 | - | S32
11485 | 0x2CDD | 2 | Output Variable ServiceID | - | U32
11487 | 0x2CDF | 1 | Output Variable Instance | - | U16

## Settings of analog output #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11488 | 0x2CE0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11488 | 0x2CE0 | 5 | Reserved | - | -
11493 | 0x2CE5 | 1 | Output Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11494 | 0x2CE6 | 1 | Output Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : Custom unit 13 : - | - | U8
11495 | 0x2CE7 | 1 | Output X_Pt1 | A / 1000 | U8
11496 | 0x2CE8 | 2 | Output Y_Pt1 | - | S32
11498 | 0x2CEA | 1 | Output X_Pt2 | A / 1000 | U8
11499 | 0x2CEB | 2 | Output Y_Pt2 | - | S32
11501 | 0x2CED | 2 | Output Variable ServiceID | - | U32
11503 | 0x2CEF | 1 | Output Variable Instance | - | U16

## Settings of analog output #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11504 | 0x2CF0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11504 | 0x2CF0 | 5 | Reserved | - | -
11509 | 0x2CF5 | 1 | Output Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11510 | 0x2CF6 | 1 | Output Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : Custom unit 13 : - | - | U8
11511 | 0x2CF7 | 1 | Output X_Pt1 | A / 1000 | U8
11512 | 0x2CF8 | 2 | Output Y_Pt1 | - | S32
11514 | 0x2CFA | 1 | Output X_Pt2 | A / 1000 | U8
11515 | 0x2CFB | 2 | Output Y_Pt2 | - | S32
11517 | 0x2CFD | 2 | Output Variable ServiceID | - | U32
11519 | 0x2CFF | 1 | Output Variable Instance | - | U16

## Settings of analog output #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11520 | 0x2D00 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11520 | 0x2D00 | 5 | Reserved | - | -
11525 | 0x2D05 | 1 | Output Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11526 | 0x2D06 | 1 | Output Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : Custom unit 13 : - | - | U8
11527 | 0x2D07 | 1 | Output X_Pt1 | A / 1000 | U8
11528 | 0x2D08 | 2 | Output Y_Pt1 | - | S32
11530 | 0x2D0A | 1 | Output X_Pt2 | A / 1000 | U8
11531 | 0x2D0B | 2 | Output Y_Pt2 | - | S32
11533 | 0x2D0D | 2 | Output Variable ServiceID | - | U32
11535 | 0x2D0F | 1 | Output Variable Instance | - | U16

## Settings of analog output #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11536 | 0x2D10 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11536 | 0x2D10 | 5 | Reserved | - | -
11541 | 0x2D15 | 1 | Output Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11542 | 0x2D16 | 1 | Output Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : Custom unit 13 : - | - | U8
11543 | 0x2D17 | 1 | Output X_Pt1 | A / 1000 | U8
11544 | 0x2D18 | 2 | Output Y_Pt1 | - | S32
11546 | 0x2D1A | 1 | Output X_Pt2 | A / 1000 | U8
11547 | 0x2D1B | 2 | Output Y_Pt2 | - | S32
11549 | 0x2D1D | 2 | Output Variable ServiceID | - | U32
11551 | 0x2D1F | 1 | Output Variable Instance | - | U16

## Settings of analog output #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11552 | 0x2D20 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11552 | 0x2D20 | 5 | Reserved | - | -
11557 | 0x2D25 | 1 | Output Type 0 : 0 - 20 mA 1 : 4 - 20 mA | - | U8
11558 | 0x2D26 | 1 | Output Unit 0 : A 1 : V 2 : W 3 : kW 4 : var 5 : kvar 6 : VA 7 : kVA 8 : ?C 9 : ?F 10 : mbar 11 : bar 12 : Custom unit 13 : - | - | U8
11559 | 0x2D27 | 1 | Output X_Pt1 | A / 1000 | U8
11560 | 0x2D28 | 2 | Output Y_Pt1 | - | S32
11562 | 0x2D2A | 1 | Output X_Pt2 | A / 1000 | U8
11563 | 0x2D2B | 2 | Output Y_Pt2 | - | S32
11565 | 0x2D2D | 2 | Output Variable ServiceID | - | U32
11567 | 0x2D2F | 1 | Output Variable Instance | - | U16

## Analog Input #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11584 | 0x2D40 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11584 | 0x2D40 | 2 | Inst. value | - | S32
11586 | 0x2D42 | 2 | Avg. value | - | S32

## Analog Input #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11588 | 0x2D44 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11588 | 0x2D44 | 2 | Inst. value | - | S32
11590 | 0x2D46 | 2 | Avg. value | - | S32

## Analog Input #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11592 | 0x2D48 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11592 | 0x2D48 | 2 | Inst. value | - | S32
11594 | 0x2D4A | 2 | Avg. value | - | S32

## Analog Input #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11596 | 0x2D4C | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11596 | 0x2D4C | 2 | Inst. value | - | S32
11598 | 0x2D4E | 2 | Avg. value | - | S32

## Analog Input #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11600 | 0x2D50 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11600 | 0x2D50 | 2 | Inst. value | - | S32
11602 | 0x2D52 | 2 | Avg. value | - | S32

## Analog Input #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11604 | 0x2D54 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11604 | 0x2D54 | 2 | Inst. value | - | S32
11606 | 0x2D56 | 2 | Avg. value | - | S32

## Analog Input #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11608 | 0x2D58 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11608 | 0x2D58 | 2 | Inst. value | - | S32
11610 | 0x2D5A | 2 | Avg. value | - | S32

## Analog Input #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11612 | 0x2D5C | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11612 | 0x2D5C | 2 | Inst. value | - | S32
11614 | 0x2D5E | 2 | Avg. value | - | S32

## Analog Output #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11616 | 0x2D60 | Settings | 3 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11616 | 0x2D60 | 1 | Reserved | - | -
11617 | 0x2D61 | 2 | Value command (when output not linked to var.) | - | S32

## Analog Output #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11619 | 0x2D63 | Settings | 3 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11619 | 0x2D63 | 1 | Reserved | - | -
11620 | 0x2D64 | 2 | Value command (when output not linked to var.) | - | S32

## Analog Output #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11622 | 0x2D66 | Settings | 3 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11622 | 0x2D66 | 1 | Reserved | - | -
11623 | 0x2D67 | 2 | Value command (when output not linked to var.) | - | S32

## Analog Output #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11625 | 0x2D69 | Settings | 3 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11625 | 0x2D69 | 1 | Reserved | - | -
11626 | 0x2D6A | 2 | Value command (when output not linked to var.) | - | S32

## Analog Output #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11628 | 0x2D6C | Settings | 3 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11628 | 0x2D6C | 1 | Reserved | - | -
11629 | 0x2D6D | 2 | Value command (when output not linked to var.) | - | S32

## Analog Output #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11631 | 0x2D6F | Settings | 3 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11631 | 0x2D6F | 1 | Reserved | - | -
11632 | 0x2D70 | 2 | Value command (when output not linked to var.) | - | S32

## Analog Output #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11634 | 0x2D72 | Settings | 3 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11634 | 0x2D72 | 1 | Reserved | - | -
11635 | 0x2D73 | 2 | Value command (when output not linked to var.) | - | S32

## Analog Output #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11637 | 0x2D75 | Settings | 3 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11637 | 0x2D75 | 1 | Reserved | - | -
11638 | 0x2D76 | 2 | Value command (when output not linked to var.) | - | S32

## Analog I/O availability

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11648 | 0x2D80 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11648 | 0x2D80 | 1 | Inputs number | - | U16
11649 | 0x2D81 | 1 | Bit x : Input x Available (1)/Not available (0) | - | U16_HEX
11650 | 0x2D82 | 1 | Outputs number | - | U16
11651 | 0x2D83 | 1 | Bit x : Output x Available (1)/Not available (0) | - | U16_HEX

# Temperature

## Avg. Temperature #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11680 | 0x2DA0 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11680 | 0x2DA0 | 1 | Avg.Temperature | ?C / 100 | S16

## Avg. Temperature #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11681 | 0x2DA1 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11681 | 0x2DA1 | 1 | Avg.Temperature | ?C / 100 | S16

## Avg. Temperature #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11682 | 0x2DA2 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11682 | 0x2DA2 | 1 | Avg.Temperature | ?C / 100 | S16

## Avg. Temperature #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11683 | 0x2DA3 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11683 | 0x2DA3 | 1 | Avg.Temperature | ?C / 100 | S16

## Inst. Temperature #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11696 | 0x2DB0 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11696 | 0x2DB0 | 1 | Inst.Temperature | ?C / 100 | S16

## Inst. Temperature #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11697 | 0x2DB1 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11697 | 0x2DB1 | 1 | Inst.Temperature | ?C / 100 | S16

## Inst. Temperature #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11698 | 0x2DB2 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11698 | 0x2DB2 | 1 | Inst.Temperature | ?C / 100 | S16

## Inst. Temperature #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11699 | 0x2DB3 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11699 | 0x2DB3 | 1 | Inst.Temperature | ?C / 100 | S16

## Temperature availability

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
11712 | 0x2DC0 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
11712 | 0x2DC0 | 1 | Internal temperature number | - | U16
11713 | 0x2DC1 | 1 | Bit x : Internal Temp. x Available (1)/Not available (0) | - | U16_HEX
11714 | 0x2DC2 | 1 | External temperature number | - | U16
11715 | 0x2DC3 | 1 | Bit x : External Temp. x Available (1)/Not available (0) | - | U16_HEX

# Fieldbus

# Monitoring

# Alarms

## Analog alarm settings #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38912 | 0x9800 | Settings | 21 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38912 | 0x9800 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38913 | 0x9801 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38914 | 0x9802 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38915 | 0x9803 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38916 | 0x9804 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38917 | 0x9805 | 2 | Analog variable (ServiceID) | - | U32
38919 | 0x9807 | 1 | Analog variable (Instance index) | - | U16
38920 | 0x9808 | 1 | Analog variable (Instance type) | - | U16
38921 | 0x9809 | 1 | Variable data access : 0 : Single 1 : Triple (logical AND) 2 : Triple (logical OR) | - | U16
38922 | 0x980A | 4 | High threshold | - | S64
38926 | 0x980E | 4 | Low threshold | - | S64
38930 | 0x9812 | 1 | Hysteresis | % / 10 | U16
38931 | 0x9813 | 1 | Startup delay | s / 2 | U16
38932 | 0x9814 | 1 | Dropout delay | s / 2 | U16

## Analog alarm settings #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38935 | 0x9817 | Settings | 21 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38935 | 0x9817 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38936 | 0x9818 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38937 | 0x9819 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38938 | 0x981A | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38939 | 0x981B | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38940 | 0x981C | 2 | Analog variable (ServiceID) | - | U32
38942 | 0x981E | 1 | Analog variable (Instance index) | - | U16
38943 | 0x981F | 1 | Analog variable (Instance type) | - | U16
38944 | 0x9820 | 1 | Variable data access : 0 : Single 1 : Triple (logical AND) 2 : Triple (logical OR) | - | U16
38945 | 0x9821 | 4 | High threshold | - | S64
38949 | 0x9825 | 4 | Low threshold | - | S64
38953 | 0x9829 | 1 | Hysteresis | % / 10 | U16
38954 | 0x982A | 1 | Startup delay | s / 2 | U16
38955 | 0x982B | 1 | Dropout delay | s / 2 | U16

## Analog alarm settings #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38958 | 0x982E | Settings | 21 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38958 | 0x982E | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38959 | 0x982F | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38960 | 0x9830 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38961 | 0x9831 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38962 | 0x9832 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38963 | 0x9833 | 2 | Analog variable (ServiceID) | - | U32
38965 | 0x9835 | 1 | Analog variable (Instance index) | - | U16
38966 | 0x9836 | 1 | Analog variable (Instance type) | - | U16
38967 | 0x9837 | 1 | Variable data access : 0 : Single 1 : Triple (logical AND) 2 : Triple (logical OR) | - | U16
38968 | 0x9838 | 4 | High threshold | - | S64
38972 | 0x983C | 4 | Low threshold | - | S64
38976 | 0x9840 | 1 | Hysteresis | % / 10 | U16
38977 | 0x9841 | 1 | Startup delay | s / 2 | U16
38978 | 0x9842 | 1 | Dropout delay | s / 2 | U16

## Analog alarm settings #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38981 | 0x9845 | Settings | 21 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38981 | 0x9845 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38982 | 0x9846 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38983 | 0x9847 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38984 | 0x9848 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38985 | 0x9849 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38986 | 0x984A | 2 | Analog variable (ServiceID) | - | U32
38988 | 0x984C | 1 | Analog variable (Instance index) | - | U16
38989 | 0x984D | 1 | Analog variable (Instance type) | - | U16
38990 | 0x984E | 1 | Variable data access : 0 : Single 1 : Triple (logical AND) 2 : Triple (logical OR) | - | U16
38991 | 0x984F | 4 | High threshold | - | S64
38995 | 0x9853 | 4 | Low threshold | - | S64
38999 | 0x9857 | 1 | Hysteresis | % / 10 | U16
39000 | 0x9858 | 1 | Startup delay | s / 2 | U16
39001 | 0x9859 | 1 | Dropout delay | s / 2 | U16

## Analog alarm settings #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39004 | 0x985C | Settings | 21 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39004 | 0x985C | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39005 | 0x985D | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39006 | 0x985E | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39007 | 0x985F | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39008 | 0x9860 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39009 | 0x9861 | 2 | Analog variable (ServiceID) | - | U32
39011 | 0x9863 | 1 | Analog variable (Instance index) | - | U16
39012 | 0x9864 | 1 | Analog variable (Instance type) | - | U16
39013 | 0x9865 | 1 | Variable data access : 0 : Single 1 : Triple (logical AND) 2 : Triple (logical OR) | - | U16
39014 | 0x9866 | 4 | High threshold | - | S64
39018 | 0x986A | 4 | Low threshold | - | S64
39022 | 0x986E | 1 | Hysteresis | % / 10 | U16
39023 | 0x986F | 1 | Startup delay | s / 2 | U16
39024 | 0x9870 | 1 | Dropout delay | s / 2 | U16

## Analog alarm settings #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39027 | 0x9873 | Settings | 21 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39027 | 0x9873 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39028 | 0x9874 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39029 | 0x9875 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39030 | 0x9876 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39031 | 0x9877 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39032 | 0x9878 | 2 | Analog variable (ServiceID) | - | U32
39034 | 0x987A | 1 | Analog variable (Instance index) | - | U16
39035 | 0x987B | 1 | Analog variable (Instance type) | - | U16
39036 | 0x987C | 1 | Variable data access : 0 : Single 1 : Triple (logical AND) 2 : Triple (logical OR) | - | U16
39037 | 0x987D | 4 | High threshold | - | S64
39041 | 0x9881 | 4 | Low threshold | - | S64
39045 | 0x9885 | 1 | Hysteresis | % / 10 | U16
39046 | 0x9886 | 1 | Startup delay | s / 2 | U16
39047 | 0x9887 | 1 | Dropout delay | s / 2 | U16

## Analog alarm settings #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39050 | 0x988A | Settings | 21 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39050 | 0x988A | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39051 | 0x988B | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39052 | 0x988C | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39053 | 0x988D | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39054 | 0x988E | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39055 | 0x988F | 2 | Analog variable (ServiceID) | - | U32
39057 | 0x9891 | 1 | Analog variable (Instance index) | - | U16
39058 | 0x9892 | 1 | Analog variable (Instance type) | - | U16
39059 | 0x9893 | 1 | Variable data access : 0 : Single 1 : Triple (logical AND) 2 : Triple (logical OR) | - | U16
39060 | 0x9894 | 4 | High threshold | - | S64
39064 | 0x9898 | 4 | Low threshold | - | S64
39068 | 0x989C | 1 | Hysteresis | % / 10 | U16
39069 | 0x989D | 1 | Startup delay | s / 2 | U16
39070 | 0x989E | 1 | Dropout delay | s / 2 | U16

## Analog alarm settings #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39073 | 0x98A1 | Settings | 21 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39073 | 0x98A1 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39074 | 0x98A2 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39075 | 0x98A3 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39076 | 0x98A4 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39077 | 0x98A5 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39078 | 0x98A6 | 2 | Analog variable (ServiceID) | - | U32
39080 | 0x98A8 | 1 | Analog variable (Instance index) | - | U16
39081 | 0x98A9 | 1 | Analog variable (Instance type) | - | U16
39082 | 0x98AA | 1 | Variable data access : 0 : Single 1 : Triple (logical AND) 2 : Triple (logical OR) | - | U16
39083 | 0x98AB | 4 | High threshold | - | S64
39087 | 0x98AF | 4 | Low threshold | - | S64
39091 | 0x98B3 | 1 | Hysteresis | % / 10 | U16
39092 | 0x98B4 | 1 | Startup delay | s / 2 | U16
39093 | 0x98B5 | 1 | Dropout delay | s / 2 | U16

## Logical alarm settings #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39104 | 0x98C0 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39104 | 0x98C0 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39105 | 0x98C1 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39106 | 0x98C2 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39107 | 0x98C3 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39108 | 0x98C4 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39109 | 0x98C5 | 1 | Logical input 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39110 | 0x98C6 | 1 | Startup delay | s / 2 | U16
39111 | 0x98C7 | 1 | Dropout delay | s / 2 | U16

## Logical alarm settings #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39114 | 0x98CA | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39114 | 0x98CA | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39115 | 0x98CB | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39116 | 0x98CC | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39117 | 0x98CD | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39118 | 0x98CE | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39119 | 0x98CF | 1 | Logical input 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39120 | 0x98D0 | 1 | Startup delay | s / 2 | U16
39121 | 0x98D1 | 1 | Dropout delay | s / 2 | U16

## Logical alarm settings #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39124 | 0x98D4 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39124 | 0x98D4 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39125 | 0x98D5 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39126 | 0x98D6 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39127 | 0x98D7 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39128 | 0x98D8 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39129 | 0x98D9 | 1 | Logical input 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39130 | 0x98DA | 1 | Startup delay | s / 2 | U16
39131 | 0x98DB | 1 | Dropout delay | s / 2 | U16

## Logical alarm settings #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39134 | 0x98DE | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39134 | 0x98DE | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39135 | 0x98DF | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39136 | 0x98E0 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39137 | 0x98E1 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39138 | 0x98E2 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39139 | 0x98E3 | 1 | Logical input 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39140 | 0x98E4 | 1 | Startup delay | s / 2 | U16
39141 | 0x98E5 | 1 | Dropout delay | s / 2 | U16

## Combination alarm settings #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39152 | 0x98F0 | Settings | 10 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39152 | 0x98F0 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39153 | 0x98F1 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39154 | 0x98F2 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39155 | 0x98F3 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39156 | 0x98F4 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39157 | 0x98F5 | 1 | Alarm 1 (type) 0 : Analog 1 : Logical 2 : Combi 3 : EN50160 4 : Inrush | - | U16
39158 | 0x98F6 | 1 | Alarm 1 (index) | - | U16
39159 | 0x98F7 | 1 | Alarm 2 (type) 0 : Analog 1 : Logical 2 : Combi 3 : EN50160 4 : Inrush | - | U16
39160 | 0x98F8 | 1 | Alarm 2 (index) | - | U16
39161 | 0x98F9 | 1 | Operation : 0 : AND 1 : OR | - | U16

## Combination alarm settings #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39164 | 0x98FC | Settings | 10 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39164 | 0x98FC | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39165 | 0x98FD | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39166 | 0x98FE | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39167 | 0x98FF | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39168 | 0x9900 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39169 | 0x9901 | 1 | Alarm 1 (type) 0 : Analog 1 : Logical 2 : Combi 3 : EN50160 4 : Inrush | - | U16
39170 | 0x9902 | 1 | Alarm 1 (index) | - | U16
39171 | 0x9903 | 1 | Alarm 2 (type) 0 : Analog 1 : Logical 2 : Combi 3 : EN50160 4 : Inrush | - | U16
39172 | 0x9904 | 1 | Alarm 2 (index) | - | U16
39173 | 0x9905 | 1 | Operation : 0 : AND 1 : OR | - | U16

## Combination alarm settings #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39176 | 0x9908 | Settings | 10 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39176 | 0x9908 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39177 | 0x9909 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39178 | 0x990A | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39179 | 0x990B | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39180 | 0x990C | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39181 | 0x990D | 1 | Alarm 1 (type) 0 : Analog 1 : Logical 2 : Combi 3 : EN50160 4 : Inrush | - | U16
39182 | 0x990E | 1 | Alarm 1 (index) | - | U16
39183 | 0x990F | 1 | Alarm 2 (type) 0 : Analog 1 : Logical 2 : Combi 3 : EN50160 4 : Inrush | - | U16
39184 | 0x9910 | 1 | Alarm 2 (index) | - | U16
39185 | 0x9911 | 1 | Operation : 0 : AND 1 : OR | - | U16

## Combination alarm settings #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39188 | 0x9914 | Settings | 10 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39188 | 0x9914 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
39189 | 0x9915 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39190 | 0x9916 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
39191 | 0x9917 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39192 | 0x9918 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
39193 | 0x9919 | 1 | Alarm 1 (type) 0 : Analog 1 : Logical 2 : Combi 3 : EN50160 4 : Inrush | - | U16
39194 | 0x991A | 1 | Alarm 1 (index) | - | U16
39195 | 0x991B | 1 | Alarm 2 (type) 0 : Analog 1 : Logical 2 : Combi 3 : EN50160 4 : Inrush | - | U16
39196 | 0x991C | 1 | Alarm 2 (index) | - | U16
39197 | 0x991D | 1 | Operation : 0 : AND 1 : OR | - | U16

## Inrush alarm settings #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38420 | 0x9614 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38420 | 0x9614 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38421 | 0x9615 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38422 | 0x9616 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38423 | 0x9617 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38424 | 0x9618 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38425 | 0x9619 | 1 | Load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Unknown | - | U16
38426 | 0x961A | 1 | Startup delay | s / 2 | U16
38427 | 0x961B | 1 | Dropout delay | s / 2 | U16

## Inrush alarm settings #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38430 | 0x961E | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38430 | 0x961E | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38431 | 0x961F | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38432 | 0x9620 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38433 | 0x9621 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38434 | 0x9622 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38435 | 0x9623 | 1 | Load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Unknown | - | U16
38436 | 0x9624 | 1 | Startup delay | s / 2 | U16
38437 | 0x9625 | 1 | Dropout delay | s / 2 | U16

## Inrush alarm settings #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38440 | 0x9628 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38440 | 0x9628 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38441 | 0x9629 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38442 | 0x962A | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38443 | 0x962B | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38444 | 0x962C | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38445 | 0x962D | 1 | Load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Unknown | - | U16
38446 | 0x962E | 1 | Startup delay | s / 2 | U16
38447 | 0x962F | 1 | Dropout delay | s / 2 | U16

## Inrush alarm settings #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38450 | 0x9632 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38450 | 0x9632 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38451 | 0x9633 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38452 | 0x9634 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38453 | 0x9635 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38454 | 0x9636 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38455 | 0x9637 | 1 | Load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Unknown | - | U16
38456 | 0x9638 | 1 | Startup delay | s / 2 | U16
38457 | 0x9639 | 1 | Dropout delay | s / 2 | U16

## EN50160 alarm settings #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38460 | 0x963C | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38460 | 0x963C | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38461 | 0x963D | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38462 | 0x963E | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38463 | 0x963F | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38464 | 0x9640 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38465 | 0x9641 | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Inter | - | U16
38466 | 0x9642 | 1 | Startup delay | s / 2 | U16
38467 | 0x9643 | 1 | Dropout delay | s / 2 | U16

## EN50160 alarm settings #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38470 | 0x9646 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38470 | 0x9646 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38471 | 0x9647 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38472 | 0x9648 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38473 | 0x9649 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38474 | 0x964A | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38475 | 0x964B | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Inter | - | U16
38476 | 0x964C | 1 | Startup delay | s / 2 | U16
38477 | 0x964D | 1 | Dropout delay | s / 2 | U16

## EN50160 alarm settings #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38480 | 0x9650 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38480 | 0x9650 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38481 | 0x9651 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38482 | 0x9652 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38483 | 0x9653 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38484 | 0x9654 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38485 | 0x9655 | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Inter | - | U16
38486 | 0x9656 | 1 | Startup delay | s / 2 | U16
38487 | 0x9657 | 1 | Dropout delay | s / 2 | U16

## System alarm settings #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38144 | 0x9500 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38144 | 0x9500 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38145 | 0x9501 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38146 | 0x9502 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38147 | 0x9503 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38148 | 0x9504 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38149 | 0x9505 | 1 | Alarm Type 0 : None 1 : Net rotation 2 : V/I association 3 : CT disconnected 10 : Bad CT prim | - | U16
38150 | 0x9506 | 1 | Startup delay | s / 2 | U16
38151 | 0x9507 | 1 | Dropout delay | s / 2 | U16

## System alarm settings #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38154 | 0x950A | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38154 | 0x950A | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38155 | 0x950B | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38156 | 0x950C | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38157 | 0x950D | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38158 | 0x950E | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38159 | 0x950F | 1 | Alarm Type 0 : None 1 : Net rotation 2 : V/I association 3 : CT disconnected 10 : Bad CT prim | - | U16
38160 | 0x9510 | 1 | Startup delay | s / 2 | U16
38161 | 0x9511 | 1 | Dropout delay | s / 2 | U16

## System alarm settings #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38164 | 0x9514 | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38164 | 0x9514 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38165 | 0x9515 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38166 | 0x9516 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38167 | 0x9517 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38168 | 0x9518 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38169 | 0x9519 | 1 | Alarm Type 0 : None 1 : Net rotation 2 : V/I association 3 : CT disconnected 10 : Bad CT prim | - | U16
38170 | 0x951A | 1 | Startup delay | s / 2 | U16
38171 | 0x951B | 1 | Dropout delay | s / 2 | U16

## System alarm settings #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38174 | 0x951E | Settings | 8 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38174 | 0x951E | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
38175 | 0x951F | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38176 | 0x9520 | 1 | Acknowledgement method : 0 : None 1 : MODBUS only 2 : Logical input | - | U16
38177 | 0x9521 | 1 | Input for ack 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
38178 | 0x9522 | 1 | Output for report 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
38179 | 0x9523 | 1 | Alarm Type 0 : None 1 : Net rotation 2 : V/I association 3 : CT disconnected 10 : Bad CT prim | - | U16
38180 | 0x9524 | 1 | Startup delay | s / 2 | U16
38181 | 0x9525 | 1 | Dropout delay | s / 2 | U16

## Analog alarm current status #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39248 | 0x9950 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39248 | 0x9950 | 1 | Ack ID | - | U16
39249 | 0x9951 | 1 | Status 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39250 | 0x9952 | 1 | Alarm cause : 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or | - | U16
39251 | 0x9953 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39252 | 0x9954 | 2 | Start date | - | DATETIME
39254 | 0x9956 | 2 | Duration | - | U32
39256 | 0x9958 | 2 | Analog variable (ServiceID) | - | U32
39258 | 0x995A | 1 | Analog variable (Instance index) | - | U16
39259 | 0x995B | 1 | Analog variable (Instance type) | - | U16
39260 | 0x995C | 1 | Startup delay | s / 2 | U16
39261 | 0x995D | 1 | Dropout delay | s / 2 | U16
39262 | 0x995E | 1 | Hysteresis | % / 10 | U16
39263 | 0x995F | 4 | Threshold | - | S64
39267 | 0x9963 | 4 | Min/Max | - | S64

## Analog alarm current status #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39272 | 0x9968 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39272 | 0x9968 | 1 | Ack ID | - | U16
39273 | 0x9969 | 1 | Status 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39274 | 0x996A | 1 | Alarm cause : 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or | - | U16
39275 | 0x996B | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39276 | 0x996C | 2 | Start date | - | DATETIME
39278 | 0x996E | 2 | Duration | - | U32
39280 | 0x9970 | 2 | Analog variable (ServiceID) | - | U32
39282 | 0x9972 | 1 | Analog variable (Instance index) | - | U16
39283 | 0x9973 | 1 | Analog variable (Instance type) | - | U16
39284 | 0x9974 | 1 | Startup delay | s / 2 | U16
39285 | 0x9975 | 1 | Dropout delay | s / 2 | U16
39286 | 0x9976 | 1 | Hysteresis | % / 10 | U16
39287 | 0x9977 | 4 | Threshold | - | S64
39291 | 0x997B | 4 | Min/Max | - | S64

## Analog alarm current status #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39296 | 0x9980 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39296 | 0x9980 | 1 | Ack ID | - | U16
39297 | 0x9981 | 1 | Status 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39298 | 0x9982 | 1 | Alarm cause : 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or | - | U16
39299 | 0x9983 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39300 | 0x9984 | 2 | Start date | - | DATETIME
39302 | 0x9986 | 2 | Duration | - | U32
39304 | 0x9988 | 2 | Analog variable (ServiceID) | - | U32
39306 | 0x998A | 1 | Analog variable (Instance index) | - | U16
39307 | 0x998B | 1 | Analog variable (Instance type) | - | U16
39308 | 0x998C | 1 | Startup delay | s / 2 | U16
39309 | 0x998D | 1 | Dropout delay | s / 2 | U16
39310 | 0x998E | 1 | Hysteresis | % / 10 | U16
39311 | 0x998F | 4 | Threshold | - | S64
39315 | 0x9993 | 4 | Min/Max | - | S64

## Analog alarm current status #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39320 | 0x9998 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39320 | 0x9998 | 1 | Ack ID | - | U16
39321 | 0x9999 | 1 | Status 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39322 | 0x999A | 1 | Alarm cause : 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or | - | U16
39323 | 0x999B | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39324 | 0x999C | 2 | Start date | - | DATETIME
39326 | 0x999E | 2 | Duration | - | U32
39328 | 0x99A0 | 2 | Analog variable (ServiceID) | - | U32
39330 | 0x99A2 | 1 | Analog variable (Instance index) | - | U16
39331 | 0x99A3 | 1 | Analog variable (Instance type) | - | U16
39332 | 0x99A4 | 1 | Startup delay | s / 2 | U16
39333 | 0x99A5 | 1 | Dropout delay | s / 2 | U16
39334 | 0x99A6 | 1 | Hysteresis | % / 10 | U16
39335 | 0x99A7 | 4 | Threshold | - | S64
39339 | 0x99AB | 4 | Min/Max | - | S64

## Analog alarm current status #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39344 | 0x99B0 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39344 | 0x99B0 | 1 | Ack ID | - | U16
39345 | 0x99B1 | 1 | Status 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39346 | 0x99B2 | 1 | Alarm cause : 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or | - | U16
39347 | 0x99B3 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39348 | 0x99B4 | 2 | Start date | - | DATETIME
39350 | 0x99B6 | 2 | Duration | - | U32
39352 | 0x99B8 | 2 | Analog variable (ServiceID) | - | U32
39354 | 0x99BA | 1 | Analog variable (Instance index) | - | U16
39355 | 0x99BB | 1 | Analog variable (Instance type) | - | U16
39356 | 0x99BC | 1 | Startup delay | s / 2 | U16
39357 | 0x99BD | 1 | Dropout delay | s / 2 | U16
39358 | 0x99BE | 1 | Hysteresis | % / 10 | U16
39359 | 0x99BF | 4 | Threshold | - | S64
39363 | 0x99C3 | 4 | Min/Max | - | S64

## Analog alarm current status #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39368 | 0x99C8 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39368 | 0x99C8 | 1 | Ack ID | - | U16
39369 | 0x99C9 | 1 | Status 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39370 | 0x99CA | 1 | Alarm cause : 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or | - | U16
39371 | 0x99CB | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39372 | 0x99CC | 2 | Start date | - | DATETIME
39374 | 0x99CE | 2 | Duration | - | U32
39376 | 0x99D0 | 2 | Analog variable (ServiceID) | - | U32
39378 | 0x99D2 | 1 | Analog variable (Instance index) | - | U16
39379 | 0x99D3 | 1 | Analog variable (Instance type) | - | U16
39380 | 0x99D4 | 1 | Startup delay | s / 2 | U16
39381 | 0x99D5 | 1 | Dropout delay | s / 2 | U16
39382 | 0x99D6 | 1 | Hysteresis | % / 10 | U16
39383 | 0x99D7 | 4 | Threshold | - | S64
39387 | 0x99DB | 4 | Min/Max | - | S64

## Analog alarm current status #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39392 | 0x99E0 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39392 | 0x99E0 | 1 | Ack ID | - | U16
39393 | 0x99E1 | 1 | Status 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39394 | 0x99E2 | 1 | Alarm cause : 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or | - | U16
39395 | 0x99E3 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39396 | 0x99E4 | 2 | Start date | - | DATETIME
39398 | 0x99E6 | 2 | Duration | - | U32
39400 | 0x99E8 | 2 | Analog variable (ServiceID) | - | U32
39402 | 0x99EA | 1 | Analog variable (Instance index) | - | U16
39403 | 0x99EB | 1 | Analog variable (Instance type) | - | U16
39404 | 0x99EC | 1 | Startup delay | s / 2 | U16
39405 | 0x99ED | 1 | Dropout delay | s / 2 | U16
39406 | 0x99EE | 1 | Hysteresis | % / 10 | U16
39407 | 0x99EF | 4 | Threshold | - | S64
39411 | 0x99F3 | 4 | Min/Max | - | S64

## Analog alarm current status #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39416 | 0x99F8 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39416 | 0x99F8 | 1 | Ack ID | - | U16
39417 | 0x99F9 | 1 | Status 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39418 | 0x99FA | 1 | Alarm cause : 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or | - | U16
39419 | 0x99FB | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39420 | 0x99FC | 2 | Start date | - | DATETIME
39422 | 0x99FE | 2 | Duration | - | U32
39424 | 0x9A00 | 2 | Analog variable (ServiceID) | - | U32
39426 | 0x9A02 | 1 | Analog variable (Instance index) | - | U16
39427 | 0x9A03 | 1 | Analog variable (Instance type) | - | U16
39428 | 0x9A04 | 1 | Startup delay | s / 2 | U16
39429 | 0x9A05 | 1 | Dropout delay | s / 2 | U16
39430 | 0x9A06 | 1 | Hysteresis | % / 10 | U16
39431 | 0x9A07 | 4 | Threshold | - | S64
39435 | 0x9A0B | 4 | Min/Max | - | S64

## Logical alarm current status #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39456 | 0x9A20 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39456 | 0x9A20 | 1 | Ack ID | - | U16
39457 | 0x9A21 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39458 | 0x9A22 | 1 | Alarm cause : 0 : Cause Unknown 7 : Logical Active | - | U16
39459 | 0x9A23 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39460 | 0x9A24 | 2 | Start date | - | DATETIME
39462 | 0x9A26 | 2 | Duration | - | U32
39464 | 0x9A28 | 1 | Logical input 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39465 | 0x9A29 | 1 | Startup delay | s / 2 | U16
39466 | 0x9A2A | 1 | Dropout delay | s / 2 | U16

## Logical alarm current status #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39472 | 0x9A30 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39472 | 0x9A30 | 1 | Ack ID | - | U16
39473 | 0x9A31 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39474 | 0x9A32 | 1 | Alarm cause : 0 : Cause Unknown 7 : Logical Active | - | U16
39475 | 0x9A33 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39476 | 0x9A34 | 2 | Start date | - | DATETIME
39478 | 0x9A36 | 2 | Duration | - | U32
39480 | 0x9A38 | 1 | Logical input 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39481 | 0x9A39 | 1 | Startup delay | s / 2 | U16
39482 | 0x9A3A | 1 | Dropout delay | s / 2 | U16

## Logical alarm current status #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39488 | 0x9A40 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39488 | 0x9A40 | 1 | Ack ID | - | U16
39489 | 0x9A41 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39490 | 0x9A42 | 1 | Alarm cause : 0 : Cause Unknown 7 : Logical Active | - | U16
39491 | 0x9A43 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39492 | 0x9A44 | 2 | Start date | - | DATETIME
39494 | 0x9A46 | 2 | Duration | - | U32
39496 | 0x9A48 | 1 | Logical input 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39497 | 0x9A49 | 1 | Startup delay | s / 2 | U16
39498 | 0x9A4A | 1 | Dropout delay | s / 2 | U16

## Logical alarm current status #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39504 | 0x9A50 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39504 | 0x9A50 | 1 | Ack ID | - | U16
39505 | 0x9A51 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39506 | 0x9A52 | 1 | Alarm cause : 0 : Cause Unknown 7 : Logical Active | - | U16
39507 | 0x9A53 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39508 | 0x9A54 | 2 | Start date | - | DATETIME
39510 | 0x9A56 | 2 | Duration | - | U32
39512 | 0x9A58 | 1 | Logical input 0 : Input 1 1 : Input 2 2 : Input 3 3 : Input 4 4 : Input 5 5 : Input 6 6 : Input 7 7 : Input 8 8 : Input 9 9 : Input 10 255 : Not used | - | U16
39513 | 0x9A59 | 1 | Startup delay | s / 2 | U16
39514 | 0x9A5A | 1 | Dropout delay | s / 2 | U16

## Combination alarm current status #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39536 | 0x9A70 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39536 | 0x9A70 | 1 | Ack ID | - | U16
39537 | 0x9A71 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39538 | 0x9A72 | 1 | Alarm cause : 0 : Cause Unknown 8 : Combi. And 9 : Combi. Or | - | U16
39539 | 0x9A73 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39540 | 0x9A74 | 2 | Start date | - | DATETIME
39542 | 0x9A76 | 2 | Duration | - | U32
39544 | 0x9A78 | 1 | Alarm 1 | - | U16_HEX
39545 | 0x9A79 | 1 | Alarm 2 | - | U16_HEX
39546 | 0x9A7A | 1 | Alarm src 0 : AND 1 : OR (Alarm 1) 2 : OR (Alarm 2) | - | U16

## Combination alarm current status #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39552 | 0x9A80 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39552 | 0x9A80 | 1 | Ack ID | - | U16
39553 | 0x9A81 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39554 | 0x9A82 | 1 | Alarm cause : 0 : Cause Unknown 8 : Combi. And 9 : Combi. Or | - | U16
39555 | 0x9A83 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39556 | 0x9A84 | 2 | Start date | - | DATETIME
39558 | 0x9A86 | 2 | Duration | - | U32
39560 | 0x9A88 | 1 | Alarm 1 | - | U16_HEX
39561 | 0x9A89 | 1 | Alarm 2 | - | U16_HEX
39562 | 0x9A8A | 1 | Alarm src 0 : AND 1 : OR (Alarm 1) 2 : OR (Alarm 2) | - | U16

## Combination alarm current status #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39568 | 0x9A90 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39568 | 0x9A90 | 1 | Ack ID | - | U16
39569 | 0x9A91 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39570 | 0x9A92 | 1 | Alarm cause : 0 : Cause Unknown 8 : Combi. And 9 : Combi. Or | - | U16
39571 | 0x9A93 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39572 | 0x9A94 | 2 | Start date | - | DATETIME
39574 | 0x9A96 | 2 | Duration | - | U32
39576 | 0x9A98 | 1 | Alarm 1 | - | U16_HEX
39577 | 0x9A99 | 1 | Alarm 2 | - | U16_HEX
39578 | 0x9A9A | 1 | Alarm src 0 : AND 1 : OR (Alarm 1) 2 : OR (Alarm 2) | - | U16

## Combination alarm current status #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39584 | 0x9AA0 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39584 | 0x9AA0 | 1 | Ack ID | - | U16
39585 | 0x9AA1 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
39586 | 0x9AA2 | 1 | Alarm cause : 0 : Cause Unknown 8 : Combi. And 9 : Combi. Or | - | U16
39587 | 0x9AA3 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
39588 | 0x9AA4 | 2 | Start date | - | DATETIME
39590 | 0x9AA6 | 2 | Duration | - | U32
39592 | 0x9AA8 | 1 | Alarm 1 | - | U16_HEX
39593 | 0x9AA9 | 1 | Alarm 2 | - | U16_HEX
39594 | 0x9AAA | 1 | Alarm src 0 : AND 1 : OR (Alarm 1) 2 : OR (Alarm 2) | - | U16

## Inrush alarm current status #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38688 | 0x9720 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38688 | 0x9720 | 1 | Ack ID | - | U16
38689 | 0x9721 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38690 | 0x9722 | 1 | Alarm cause : 0 : Cause Unknown 11 : Inrush Active | - | U16
38691 | 0x9723 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38692 | 0x9724 | 2 | Start date | - | DATETIME
38694 | 0x9726 | 2 | Duration | - | U32
38696 | 0x9728 | 1 | Load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Unknown | - | U16
38697 | 0x9729 | 1 | Startup delay | s / 2 | U16
38698 | 0x972A | 1 | Dropout delay | s / 2 | U16

## Inrush alarm current status #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38704 | 0x9730 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38704 | 0x9730 | 1 | Ack ID | - | U16
38705 | 0x9731 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38706 | 0x9732 | 1 | Alarm cause : 0 : Cause Unknown 11 : Inrush Active | - | U16
38707 | 0x9733 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38708 | 0x9734 | 2 | Start date | - | DATETIME
38710 | 0x9736 | 2 | Duration | - | U32
38712 | 0x9738 | 1 | Load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Unknown | - | U16
38713 | 0x9739 | 1 | Startup delay | s / 2 | U16
38714 | 0x973A | 1 | Dropout delay | s / 2 | U16

## Inrush alarm current status #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38720 | 0x9740 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38720 | 0x9740 | 1 | Ack ID | - | U16
38721 | 0x9741 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38722 | 0x9742 | 1 | Alarm cause : 0 : Cause Unknown 11 : Inrush Active | - | U16
38723 | 0x9743 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38724 | 0x9744 | 2 | Start date | - | DATETIME
38726 | 0x9746 | 2 | Duration | - | U32
38728 | 0x9748 | 1 | Load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Unknown | - | U16
38729 | 0x9749 | 1 | Startup delay | s / 2 | U16
38730 | 0x974A | 1 | Dropout delay | s / 2 | U16

## Inrush alarm current status #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38736 | 0x9750 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38736 | 0x9750 | 1 | Ack ID | - | U16
38737 | 0x9751 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38738 | 0x9752 | 1 | Alarm cause : 0 : Cause Unknown 11 : Inrush Active | - | U16
38739 | 0x9753 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38740 | 0x9754 | 2 | Start date | - | DATETIME
38742 | 0x9756 | 2 | Duration | - | U32
38744 | 0x9758 | 1 | Load 0 : Load 1 1 : Load 2 2 : Load 3 3 : Load 4 255 : Unknown | - | U16
38745 | 0x9759 | 1 | Startup delay | s / 2 | U16
38746 | 0x975A | 1 | Dropout delay | s / 2 | U16

## EN50160 alarm current status #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38752 | 0x9760 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38752 | 0x9760 | 1 | Ack ID | - | U16
38753 | 0x9761 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38754 | 0x9762 | 1 | Alarm cause : 0 : Cause Unknown 10 : EN50160 Active | - | U16
38755 | 0x9763 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38756 | 0x9764 | 2 | Start date | - | DATETIME
38758 | 0x9766 | 2 | Duration | - | U32
38760 | 0x9768 | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Inter | - | U16
38761 | 0x9769 | 1 | Startup delay | s / 2 | U16
38762 | 0x976A | 1 | Dropout delay | s / 2 | U16

## EN50160 alarm current status #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38768 | 0x9770 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38768 | 0x9770 | 1 | Ack ID | - | U16
38769 | 0x9771 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38770 | 0x9772 | 1 | Alarm cause : 0 : Cause Unknown 10 : EN50160 Active | - | U16
38771 | 0x9773 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38772 | 0x9774 | 2 | Start date | - | DATETIME
38774 | 0x9776 | 2 | Duration | - | U32
38776 | 0x9778 | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Inter | - | U16
38777 | 0x9779 | 1 | Startup delay | s / 2 | U16
38778 | 0x977A | 1 | Dropout delay | s / 2 | U16

## EN50160 alarm current status #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38784 | 0x9780 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38784 | 0x9780 | 1 | Ack ID | - | U16
38785 | 0x9781 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38786 | 0x9782 | 1 | Alarm cause : 0 : Cause Unknown 10 : EN50160 Active | - | U16
38787 | 0x9783 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38788 | 0x9784 | 2 | Start date | - | DATETIME
38790 | 0x9786 | 2 | Duration | - | U32
38792 | 0x9788 | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Inter | - | U16
38793 | 0x9789 | 1 | Startup delay | s / 2 | U16
38794 | 0x978A | 1 | Dropout delay | s / 2 | U16

## System alarm current status #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38496 | 0x9660 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38496 | 0x9660 | 1 | Ack ID | - | U16
38497 | 0x9661 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38498 | 0x9662 | 1 | Alarm Type 0 : None 1 : Net rotation 2 : V/I association 3 : CT disconnected 10 : Bad CT prim | - | U16
38499 | 0x9663 | 1 | Alarm cause : 0 : Cause Unknown 12 : System Active | - | U16
38500 | 0x9664 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38501 | 0x9665 | 2 | Start date | - | DATETIME
38503 | 0x9667 | 2 | Duration | - | U32
38505 | 0x9669 | 1 | Startup delay | s / 2 | U16
38506 | 0x966A | 1 | Dropout delay | s / 2 | U16
38507 | 0x966B | 2 | Reserved | - | -
38509 | 0x966D | 1 | Line I 0 : eMspLineI1 1 : eMspLineI2 2 : eMspLineI3 3 : eMspLineI4 255 : eMspLineIUndefined | - | U16
38510 | 0x966E | 1 | Reserved | - | -
38511 | 0x966F | 4 | Reserved | - | -
38515 | 0x9673 | 4 | Reserved | - | -

## System alarm current status #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38520 | 0x9678 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38520 | 0x9678 | 1 | Ack ID | - | U16
38521 | 0x9679 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38522 | 0x967A | 1 | Alarm Type 0 : None 1 : Net rotation 2 : V/I association 3 : CT disconnected 10 : Bad CT prim | - | U16
38523 | 0x967B | 1 | Alarm cause : 0 : Cause Unknown 12 : System Active | - | U16
38524 | 0x967C | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38525 | 0x967D | 2 | Start date | - | DATETIME
38527 | 0x967F | 2 | Duration | - | U32
38529 | 0x9681 | 1 | Startup delay | s / 2 | U16
38530 | 0x9682 | 1 | Dropout delay | s / 2 | U16
38531 | 0x9683 | 2 | Reserved | - | -
38533 | 0x9685 | 1 | Line I 0 : eMspLineI1 1 : eMspLineI2 2 : eMspLineI3 3 : eMspLineI4 255 : eMspLineIUndefined | - | U16
38534 | 0x9686 | 1 | Reserved | - | -
38535 | 0x9687 | 4 | Reserved | - | -
38539 | 0x968B | 4 | Reserved | - | -

## System alarm current status #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38544 | 0x9690 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38544 | 0x9690 | 1 | Ack ID | - | U16
38545 | 0x9691 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38546 | 0x9692 | 1 | Alarm Type 0 : None 1 : Net rotation 2 : V/I association 3 : CT disconnected 10 : Bad CT prim | - | U16
38547 | 0x9693 | 1 | Alarm cause : 0 : Cause Unknown 12 : System Active | - | U16
38548 | 0x9694 | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38549 | 0x9695 | 2 | Start date | - | DATETIME
38551 | 0x9697 | 2 | Duration | - | U32
38553 | 0x9699 | 1 | Startup delay | s / 2 | U16
38554 | 0x969A | 1 | Dropout delay | s / 2 | U16
38555 | 0x969B | 2 | Reserved | - | -
38557 | 0x969D | 1 | Line I 0 : eMspLineI1 1 : eMspLineI2 2 : eMspLineI3 3 : eMspLineI4 255 : eMspLineIUndefined | - | U16
38558 | 0x969E | 1 | Reserved | - | -
38559 | 0x969F | 4 | Reserved | - | -
38563 | 0x96A3 | 4 | Reserved | - | -

## System alarm current status #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38568 | 0x96A8 | Info | 23 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38568 | 0x96A8 | 1 | Ack ID | - | U16
38569 | 0x96A9 | 1 | Status : 0 : Inactive 1 : Active 2 : Finished 3 : FinishedAndAck | - | U16
38570 | 0x96AA | 1 | Alarm Type 0 : None 1 : Net rotation 2 : V/I association 3 : CT disconnected 10 : Bad CT prim | - | U16
38571 | 0x96AB | 1 | Alarm cause : 0 : Cause Unknown 12 : System Active | - | U16
38572 | 0x96AC | 1 | Criticality : 0 : Information 1 : Not critical 2 : Critical | - | U16
38573 | 0x96AD | 2 | Start date | - | DATETIME
38575 | 0x96AF | 2 | Duration | - | U32
38577 | 0x96B1 | 1 | Startup delay | s / 2 | U16
38578 | 0x96B2 | 1 | Dropout delay | s / 2 | U16
38579 | 0x96B3 | 2 | Reserved | - | -
38581 | 0x96B5 | 1 | Line I 0 : eMspLineI1 1 : eMspLineI2 2 : eMspLineI3 3 : eMspLineI4 255 : eMspLineIUndefined | - | U16
38582 | 0x96B6 | 1 | Reserved | - | -
38583 | 0x96B7 | 4 | Reserved | - | -
38587 | 0x96BB | 4 | Reserved | - | -

## Acknowledgment of alarms

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39616 | 0x9AC0 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39616 | 0x9AC0 | 1 | Ack ID | - | U16

## Alarm log

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39632 | 0x9AD0 | Command | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39632 | 0x9AD0 | 1 | Start record number (0 to 65534) or 65535 for last record | - | U16

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39648 | 0x9AE0 | Header | 3 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39648 | 0x9AE0 | 1 | Next record number | - | U16
39649 | 0x9AE1 | 1 | Items count (max 7 per request) | - | U16
39650 | 0x9AE2 | 1 | Item size (words) | - | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
39651 | 0x9AE3 | Data | 21 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
39651 | 0x9AE3 | 1 | Alarm cause 0 : Cause Unknown 1 : Analog. High Th. Single 2 : Analog. High Th. Tri. And 3 : Analog. High Th. Tri. Or 4 : Analog. Low Th Single 5 : Analog. Low Th. Tri. And 6 : Analog. Low Th. Tri. Or 7 : Logical Active 8 : Combi. And 9 : Combi. Or 10 : EN50160 Active 11 : Inrush Active 12 : System Active | - | U16
39652 | 0x9AE4 | 1 | Criticality : 0 : Information 1 : Not Critical 2 : Critical | - | U16
39653 | 0x9AE5 | 2 | Start date | - | DATETIME
39655 | 0x9AE7 | 2 | Duration | - | U32
39657 | 0x9AE9 | 2 | Specific data 1 (depend on alarm type) | - | U32
39659 | 0x9AEB | 1 | Specific data 2 (depend on alarm type) | - | U16
39660 | 0x9AEC | 1 | Specific data 3 (depend on alarm type) | - | U16
39661 | 0x9AED | 1 | Specific data 4 (depend on alarm type) | - | U16
39662 | 0x9AEE | 1 | Specific data 5 (depend on alarm type) | - | U16
39663 | 0x9AEF | 1 | Specific data 6 (depend on alarm type) | - | U16
39664 | 0x9AF0 | 4 | Specific data 7 (depend on alarm type) | - | S64
39668 | 0x9AF4 | 4 | Specific data 8 (depend on alarm type) | - | S64

# Trend

## Trend settings

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
41872 | 0xA390 | Settings | 36 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
41872 | 0xA390 | 2 | ServiceID item 1 | - | U32
41874 | 0xA392 | 1 | Occurrence item 1: | - | U8
41875 | 0xA393 | 2 | ServiceID item 2 | - | U32
41877 | 0xA395 | 1 | Occurrence item 2: | - | U8
41878 | 0xA396 | 2 | ServiceID item 3 | - | U32
41880 | 0xA398 | 1 | Occurrence item 3: | - | U8
41881 | 0xA399 | 2 | ServiceID item 4 | - | U32
41883 | 0xA39B | 1 | Occurrence item 4: | - | U8
41884 | 0xA39C | 2 | ServiceID item 5 | - | U32
41886 | 0xA39E | 1 | Occurrence item 5: | - | U8
41887 | 0xA39F | 2 | ServiceID item 6 | - | U32
41889 | 0xA3A1 | 1 | Occurrence item 6: | - | U8
41890 | 0xA3A2 | 2 | ServiceID item 7 | - | U32
41892 | 0xA3A4 | 1 | Occurrence item 7: | - | U8
41893 | 0xA3A5 | 2 | ServiceID item 8 | - | U32
41895 | 0xA3A7 | 1 | Occurrence item 8: | - | U8
41896 | 0xA3A8 | 2 | ServiceID item 9 | - | U32
41898 | 0xA3AA | 1 | Occurrence item 9: | - | U8
41899 | 0xA3AB | 2 | ServiceID item 10 | - | U32
41901 | 0xA3AD | 1 | Occurrence item 10: | - | U8
41902 | 0xA3AE | 2 | ServiceID item 11 | - | U32
41904 | 0xA3B0 | 1 | Occurrence item 11: | - | U8
41905 | 0xA3B1 | 2 | ServiceID item 12 | - | U32
41907 | 0xA3B3 | 1 | Occurrence item 12: | - | U8

## Trend log

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
41978 | 0xA3FA | Command | 2 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
41978 | 0xA3FA | 1 | Start record number (0 to 65534) or 65535 for last record | - | U16
41979 | 0xA3FB | 1 | Item number 0 : Item 1 1 : Item 2 2 : Item 3 3 : Item 4 4 : Item 5 5 : Item 6 6 : Item 7 7 : Item 8 8 : Item 9 9 : Item 10 10 : Item 11 11 : Item 12 12 : Item 13 13 : Item 14 14 : Item 15 15 : Item 16 16 : Item 17 17 : Item 18 18 : Item 19 19 : Item 20 | - | U8

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
41980 | 0xA3FC | Header | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
41980 | 0xA3FC | 1 | Next record number | - | U16
41981 | 0xA3FD | 1 | Items count (20 per record) | - | U16
41982 | 0xA3FE | 1 | Item size | - | U16
41983 | 0xA3FF | 1 | Integration period duration | min | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
41984 | 0xA400 | Data | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
41984 | 0xA400 | 2 | Date | s | DATETIME
41986 | 0xA402 | 2 | Point value | - | S32

## Trend log raw

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42064 | 0xA450 | Command | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42064 | 0xA450 | 1 | Start record number (0 to 65534) or 65535 for last record | - | U16

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42080 | 0xA460 | Header | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42080 | 0xA460 | 1 | Next record number | - | U16
42081 | 0xA461 | 1 | Items count (2 per record) | - | U16
42082 | 0xA462 | 1 | Item size | - | U16
42083 | 0xA463 | 1 | Integration period duration | min | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42084 | 0xA464 | Data | 58 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42084 | 0xA464 | 2 | Date | - | DATETIME
42086 | 0xA466 | 2 | Trend item 1 | - | S32
42088 | 0xA468 | 2 | Trend item 2 | - | S32
42090 | 0xA46A | 2 | Trend item 3 | - | S32
42092 | 0xA46C | 2 | Trend item 4 | - | S32
42094 | 0xA46E | 2 | Trend item 5 | - | S32
42096 | 0xA470 | 2 | Trend item 6 | - | S32
42098 | 0xA472 | 2 | Trend item 7 | - | S32
42100 | 0xA474 | 2 | Trend item 8 | - | S32
42102 | 0xA476 | 2 | Trend item 9 | - | S32
42104 | 0xA478 | 2 | Trend item 10 | - | S32
42106 | 0xA47A | 2 | Trend item 11 | - | S32
42108 | 0xA47C | 2 | Trend item 12 | - | S32
42110 | 0xA47E | 2 | Reserved | - | -
42112 | 0xA480 | 2 | Reserved | - | -
42114 | 0xA482 | 2 | Reserved | - | -
42116 | 0xA484 | 2 | Reserved | - | -
42118 | 0xA486 | 2 | Reserved | - | -
42120 | 0xA488 | 2 | Reserved | - | -
42122 | 0xA48A | 2 | Reserved | - | -
42124 | 0xA48C | 2 | Reserved | - | -
42126 | 0xA48E | 2 | Reserved | - | -
42128 | 0xA490 | 2 | Reserved | - | -
42130 | 0xA492 | 2 | Reserved | - | -
42132 | 0xA494 | 2 | Reserved | - | -
42134 | 0xA496 | 2 | Reserved | - | -
42136 | 0xA498 | 2 | Reserved | - | -
42138 | 0xA49A | 2 | Reserved | - | -
42140 | 0xA49C | 2 | Reserved | - | -

# Quality events

## EN50160 events in progress #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42240 | 0xA500 | Info | 46 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42240 | 0xA500 | 1 | Event state 0 : Unactive 1 : Active | - | U16
42241 | 0xA501 | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16
42242 | 0xA502 | 4 | Start date | - | DATETIME_MS
42246 | 0xA506 | 4 | End date | - | DATETIME_MS
42250 | 0xA50A | 1 | Net/Load 0 : Net 1 : Load1 2 : Load2 3 : Load3 4 : Load4 6 : Undefined | - | U8
42251 | 0xA50B | 1 | Line mask | - | U16_HEX
42252 | 0xA50C | 1 | Start mask | - | U16_HEX
42253 | 0xA50D | 1 | End mask | - | U16_HEX
42254 | 0xA50E | 1 | Trig ratio | % | U16
42255 | 0xA50F | 1 | Ret trig ratio | % | U16
42256 | 0xA510 | 2 | Bit weight VU | V / 1000 | U32
42258 | 0xA512 | 2 | Bit weight I1 | A / 100000 | U32
42260 | 0xA514 | 2 | Bit weight I2 | A / 100000 | U32
42262 | 0xA516 | 2 | Bit weight I3 | A / 100000 | U32
42264 | 0xA518 | 2 | Bit weight In | A / 100000 | U32
42266 | 0xA51A | 1 | V1ref | - | U16
42267 | 0xA51B | 1 | V2ref | - | U16
42268 | 0xA51C | 1 | V3ref | - | U16
42269 | 0xA51D | 1 | U12ref | - | U16
42270 | 0xA51E | 1 | U23ref | - | U16
42271 | 0xA51F | 1 | U31ref | - | U16
42272 | 0xA520 | 1 | I1ref | - | U16
42273 | 0xA521 | 1 | I2ref | - | U16
42274 | 0xA522 | 1 | I3ref | - | U16
42275 | 0xA523 | 1 | Inref | - | U16
42276 | 0xA524 | 1 | V1 min/max | - | U16
42277 | 0xA525 | 1 | V2 min/max | - | U16
42278 | 0xA526 | 1 | V3 min/max | - | U16
42279 | 0xA527 | 1 | U12 min/max | - | U16
42280 | 0xA528 | 1 | U23 min/max | - | U16
42281 | 0xA529 | 1 | U31 min/max | - | U16
42282 | 0xA52A | 1 | I1 min/max | - | U16
42283 | 0xA52B | 1 | I2 min/max | - | U16
42284 | 0xA52C | 1 | I3 min/max | - | U16
42285 | 0xA52D | 1 | In min/max | - | U16

## EN50160 events in progress #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42286 | 0xA52E | Info | 46 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42286 | 0xA52E | 1 | Event state 0 : Unactive 1 : Active | - | U16
42287 | 0xA52F | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16
42288 | 0xA530 | 4 | Start date | - | DATETIME_MS
42292 | 0xA534 | 4 | End date | - | DATETIME_MS
42296 | 0xA538 | 1 | Net/Load 0 : Net 1 : Load1 2 : Load2 3 : Load3 4 : Load4 6 : Undefined | - | U8
42297 | 0xA539 | 1 | Line mask | - | U16_HEX
42298 | 0xA53A | 1 | Start mask | - | U16_HEX
42299 | 0xA53B | 1 | End mask | - | U16_HEX
42300 | 0xA53C | 1 | Trig ratio | % | U16
42301 | 0xA53D | 1 | Ret trig ratio | % | U16
42302 | 0xA53E | 2 | Bit weight VU | V / 1000 | U32
42304 | 0xA540 | 2 | Bit weight I1 | A / 100000 | U32
42306 | 0xA542 | 2 | Bit weight I2 | A / 100000 | U32
42308 | 0xA544 | 2 | Bit weight I3 | A / 100000 | U32
42310 | 0xA546 | 2 | Bit weight In | A / 100000 | U32
42312 | 0xA548 | 1 | V1ref | - | U16
42313 | 0xA549 | 1 | V2ref | - | U16
42314 | 0xA54A | 1 | V3ref | - | U16
42315 | 0xA54B | 1 | U12ref | - | U16
42316 | 0xA54C | 1 | U23ref | - | U16
42317 | 0xA54D | 1 | U31ref | - | U16
42318 | 0xA54E | 1 | I1ref | - | U16
42319 | 0xA54F | 1 | I2ref | - | U16
42320 | 0xA550 | 1 | I3ref | - | U16
42321 | 0xA551 | 1 | Inref | - | U16
42322 | 0xA552 | 1 | V1 min/max | - | U16
42323 | 0xA553 | 1 | V2 min/max | - | U16
42324 | 0xA554 | 1 | V3 min/max | - | U16
42325 | 0xA555 | 1 | U12 min/max | - | U16
42326 | 0xA556 | 1 | U23 min/max | - | U16
42327 | 0xA557 | 1 | U31 min/max | - | U16
42328 | 0xA558 | 1 | I1 min/max | - | U16
42329 | 0xA559 | 1 | I2 min/max | - | U16
42330 | 0xA55A | 1 | I3 min/max | - | U16
42331 | 0xA55B | 1 | In min/max | - | U16

## EN50160 events in progress #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42332 | 0xA55C | Info | 46 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42332 | 0xA55C | 1 | Event state 0 : Unactive 1 : Active | - | U16
42333 | 0xA55D | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16
42334 | 0xA55E | 4 | Start date | - | DATETIME_MS
42338 | 0xA562 | 4 | End date | - | DATETIME_MS
42342 | 0xA566 | 1 | Net/Load 0 : Net 1 : Load1 2 : Load2 3 : Load3 4 : Load4 6 : Undefined | - | U8
42343 | 0xA567 | 1 | Line mask | - | U16_HEX
42344 | 0xA568 | 1 | Start mask | - | U16_HEX
42345 | 0xA569 | 1 | End mask | - | U16_HEX
42346 | 0xA56A | 1 | Trig ratio | % | U16
42347 | 0xA56B | 1 | Ret trig ratio | % | U16
42348 | 0xA56C | 2 | Bit weight VU | V / 1000 | U32
42350 | 0xA56E | 2 | Bit weight I1 | A / 100000 | U32
42352 | 0xA570 | 2 | Bit weight I2 | A / 100000 | U32
42354 | 0xA572 | 2 | Bit weight I3 | A / 100000 | U32
42356 | 0xA574 | 2 | Bit weight In | A / 100000 | U32
42358 | 0xA576 | 1 | V1ref | - | U16
42359 | 0xA577 | 1 | V2ref | - | U16
42360 | 0xA578 | 1 | V3ref | - | U16
42361 | 0xA579 | 1 | U12ref | - | U16
42362 | 0xA57A | 1 | U23ref | - | U16
42363 | 0xA57B | 1 | U31ref | - | U16
42364 | 0xA57C | 1 | I1ref | - | U16
42365 | 0xA57D | 1 | I2ref | - | U16
42366 | 0xA57E | 1 | I3ref | - | U16
42367 | 0xA57F | 1 | Inref | - | U16
42368 | 0xA580 | 1 | V1 min/max | - | U16
42369 | 0xA581 | 1 | V2 min/max | - | U16
42370 | 0xA582 | 1 | V3 min/max | - | U16
42371 | 0xA583 | 1 | U12 min/max | - | U16
42372 | 0xA584 | 1 | U23 min/max | - | U16
42373 | 0xA585 | 1 | U31 min/max | - | U16
42374 | 0xA586 | 1 | I1 min/max | - | U16
42375 | 0xA587 | 1 | I2 min/max | - | U16
42376 | 0xA588 | 1 | I3 min/max | - | U16
42377 | 0xA589 | 1 | In min/max | - | U16

## Inrush events in progress #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42384 | 0xA590 | Info | 46 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42384 | 0xA590 | 1 | Event state 0 : Unactive 1 : Active | - | U16
42385 | 0xA591 | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16
42386 | 0xA592 | 4 | Start date | - | DATETIME_MS
42390 | 0xA596 | 4 | End date | - | DATETIME_MS
42394 | 0xA59A | 1 | Net/Load 0 : Net 1 : Load1 2 : Load2 3 : Load3 4 : Load4 6 : Undefined | - | U8
42395 | 0xA59B | 1 | Line mask | - | U16_HEX
42396 | 0xA59C | 1 | Start mask | - | U16_HEX
42397 | 0xA59D | 1 | End mask | - | U16_HEX
42398 | 0xA59E | 1 | Trig ratio | % | U16
42399 | 0xA59F | 1 | Ret trig ratio | % | U16
42400 | 0xA5A0 | 2 | Bit weight VU | V / 1000 | U32
42402 | 0xA5A2 | 2 | Bit weight I1 | A / 100000 | U32
42404 | 0xA5A4 | 2 | Bit weight I2 | A / 100000 | U32
42406 | 0xA5A6 | 2 | Bit weight I3 | A / 100000 | U32
42408 | 0xA5A8 | 2 | Bit weight In | A / 100000 | U32
42410 | 0xA5AA | 1 | V1ref | - | U16
42411 | 0xA5AB | 1 | V2ref | - | U16
42412 | 0xA5AC | 1 | V3ref | - | U16
42413 | 0xA5AD | 1 | U12ref | - | U16
42414 | 0xA5AE | 1 | U23ref | - | U16
42415 | 0xA5AF | 1 | U31ref | - | U16
42416 | 0xA5B0 | 1 | I1ref | - | U16
42417 | 0xA5B1 | 1 | I2ref | - | U16
42418 | 0xA5B2 | 1 | I3ref | - | U16
42419 | 0xA5B3 | 1 | Inref | - | U16
42420 | 0xA5B4 | 1 | V1 min/max | - | U16
42421 | 0xA5B5 | 1 | V2 min/max | - | U16
42422 | 0xA5B6 | 1 | V3 min/max | - | U16
42423 | 0xA5B7 | 1 | U12 min/max | - | U16
42424 | 0xA5B8 | 1 | U23 min/max | - | U16
42425 | 0xA5B9 | 1 | U31 min/max | - | U16
42426 | 0xA5BA | 1 | I1 min/max | - | U16
42427 | 0xA5BB | 1 | I2 min/max | - | U16
42428 | 0xA5BC | 1 | I3 min/max | - | U16
42429 | 0xA5BD | 1 | In min/max | - | U16

## Inrush events in progress #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42430 | 0xA5BE | Info | 46 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42430 | 0xA5BE | 1 | Event state 0 : Unactive 1 : Active | - | U16
42431 | 0xA5BF | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16
42432 | 0xA5C0 | 4 | Start date | - | DATETIME_MS
42436 | 0xA5C4 | 4 | End date | - | DATETIME_MS
42440 | 0xA5C8 | 1 | Net/Load 0 : Net 1 : Load1 2 : Load2 3 : Load3 4 : Load4 6 : Undefined | - | U8
42441 | 0xA5C9 | 1 | Line mask | - | U16_HEX
42442 | 0xA5CA | 1 | Start mask | - | U16_HEX
42443 | 0xA5CB | 1 | End mask | - | U16_HEX
42444 | 0xA5CC | 1 | Trig ratio | % | U16
42445 | 0xA5CD | 1 | Ret trig ratio | % | U16
42446 | 0xA5CE | 2 | Bit weight VU | V / 1000 | U32
42448 | 0xA5D0 | 2 | Bit weight I1 | A / 100000 | U32
42450 | 0xA5D2 | 2 | Bit weight I2 | A / 100000 | U32
42452 | 0xA5D4 | 2 | Bit weight I3 | A / 100000 | U32
42454 | 0xA5D6 | 2 | Bit weight In | A / 100000 | U32
42456 | 0xA5D8 | 1 | V1ref | - | U16
42457 | 0xA5D9 | 1 | V2ref | - | U16
42458 | 0xA5DA | 1 | V3ref | - | U16
42459 | 0xA5DB | 1 | U12ref | - | U16
42460 | 0xA5DC | 1 | U23ref | - | U16
42461 | 0xA5DD | 1 | U31ref | - | U16
42462 | 0xA5DE | 1 | I1ref | - | U16
42463 | 0xA5DF | 1 | I2ref | - | U16
42464 | 0xA5E0 | 1 | I3ref | - | U16
42465 | 0xA5E1 | 1 | Inref | - | U16
42466 | 0xA5E2 | 1 | V1 min/max | - | U16
42467 | 0xA5E3 | 1 | V2 min/max | - | U16
42468 | 0xA5E4 | 1 | V3 min/max | - | U16
42469 | 0xA5E5 | 1 | U12 min/max | - | U16
42470 | 0xA5E6 | 1 | U23 min/max | - | U16
42471 | 0xA5E7 | 1 | U31 min/max | - | U16
42472 | 0xA5E8 | 1 | I1 min/max | - | U16
42473 | 0xA5E9 | 1 | I2 min/max | - | U16
42474 | 0xA5EA | 1 | I3 min/max | - | U16
42475 | 0xA5EB | 1 | In min/max | - | U16

## Inrush events in progress #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42476 | 0xA5EC | Info | 46 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42476 | 0xA5EC | 1 | Event state 0 : Unactive 1 : Active | - | U16
42477 | 0xA5ED | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16
42478 | 0xA5EE | 4 | Start date | - | DATETIME_MS
42482 | 0xA5F2 | 4 | End date | - | DATETIME_MS
42486 | 0xA5F6 | 1 | Net/Load 0 : Net 1 : Load1 2 : Load2 3 : Load3 4 : Load4 6 : Undefined | - | U8
42487 | 0xA5F7 | 1 | Line mask | - | U16_HEX
42488 | 0xA5F8 | 1 | Start mask | - | U16_HEX
42489 | 0xA5F9 | 1 | End mask | - | U16_HEX
42490 | 0xA5FA | 1 | Trig ratio | % | U16
42491 | 0xA5FB | 1 | Ret trig ratio | % | U16
42492 | 0xA5FC | 2 | Bit weight VU | V / 1000 | U32
42494 | 0xA5FE | 2 | Bit weight I1 | A / 100000 | U32
42496 | 0xA600 | 2 | Bit weight I2 | A / 100000 | U32
42498 | 0xA602 | 2 | Bit weight I3 | A / 100000 | U32
42500 | 0xA604 | 2 | Bit weight In | A / 100000 | U32
42502 | 0xA606 | 1 | V1ref | - | U16
42503 | 0xA607 | 1 | V2ref | - | U16
42504 | 0xA608 | 1 | V3ref | - | U16
42505 | 0xA609 | 1 | U12ref | - | U16
42506 | 0xA60A | 1 | U23ref | - | U16
42507 | 0xA60B | 1 | U31ref | - | U16
42508 | 0xA60C | 1 | I1ref | - | U16
42509 | 0xA60D | 1 | I2ref | - | U16
42510 | 0xA60E | 1 | I3ref | - | U16
42511 | 0xA60F | 1 | Inref | - | U16
42512 | 0xA610 | 1 | V1 min/max | - | U16
42513 | 0xA611 | 1 | V2 min/max | - | U16
42514 | 0xA612 | 1 | V3 min/max | - | U16
42515 | 0xA613 | 1 | U12 min/max | - | U16
42516 | 0xA614 | 1 | U23 min/max | - | U16
42517 | 0xA615 | 1 | U31 min/max | - | U16
42518 | 0xA616 | 1 | I1 min/max | - | U16
42519 | 0xA617 | 1 | I2 min/max | - | U16
42520 | 0xA618 | 1 | I3 min/max | - | U16
42521 | 0xA619 | 1 | In min/max | - | U16

## Inrush events in progress #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42522 | 0xA61A | Info | 46 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42522 | 0xA61A | 1 | Event state 0 : Unactive 1 : Active | - | U16
42523 | 0xA61B | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16
42524 | 0xA61C | 4 | Start date | - | DATETIME_MS
42528 | 0xA620 | 4 | End date | - | DATETIME_MS
42532 | 0xA624 | 1 | Net/Load 0 : Net 1 : Load1 2 : Load2 3 : Load3 4 : Load4 6 : Undefined | - | U8
42533 | 0xA625 | 1 | Line mask | - | U16_HEX
42534 | 0xA626 | 1 | Start mask | - | U16_HEX
42535 | 0xA627 | 1 | End mask | - | U16_HEX
42536 | 0xA628 | 1 | Trig ratio | % | U16
42537 | 0xA629 | 1 | Ret trig ratio | % | U16
42538 | 0xA62A | 2 | Bit weight VU | V / 1000 | U32
42540 | 0xA62C | 2 | Bit weight I1 | A / 100000 | U32
42542 | 0xA62E | 2 | Bit weight I2 | A / 100000 | U32
42544 | 0xA630 | 2 | Bit weight I3 | A / 100000 | U32
42546 | 0xA632 | 2 | Bit weight In | A / 100000 | U32
42548 | 0xA634 | 1 | V1ref | - | U16
42549 | 0xA635 | 1 | V2ref | - | U16
42550 | 0xA636 | 1 | V3ref | - | U16
42551 | 0xA637 | 1 | U12ref | - | U16
42552 | 0xA638 | 1 | U23ref | - | U16
42553 | 0xA639 | 1 | U31ref | - | U16
42554 | 0xA63A | 1 | I1ref | - | U16
42555 | 0xA63B | 1 | I2ref | - | U16
42556 | 0xA63C | 1 | I3ref | - | U16
42557 | 0xA63D | 1 | Inref | - | U16
42558 | 0xA63E | 1 | V1 min/max | - | U16
42559 | 0xA63F | 1 | V2 min/max | - | U16
42560 | 0xA640 | 1 | V3 min/max | - | U16
42561 | 0xA641 | 1 | U12 min/max | - | U16
42562 | 0xA642 | 1 | U23 min/max | - | U16
42563 | 0xA643 | 1 | U31 min/max | - | U16
42564 | 0xA644 | 1 | I1 min/max | - | U16
42565 | 0xA645 | 1 | I2 min/max | - | U16
42566 | 0xA646 | 1 | I3 min/max | - | U16
42567 | 0xA647 | 1 | In min/max | - | U16

## EN50160 events settings

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42628 | 0xA684 | Settings | 7 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42628 | 0xA684 | 1 | Reference voltage 0 : Fixed reference voltage 1 : Sliding reference voltage | - | U16
42629 | 0xA685 | 1 | Dip (Udip) threshold | % | U16
42630 | 0xA686 | 1 | Dip (Udip) hysteresis | % | U16
42631 | 0xA687 | 1 | Swell (Uswl) threshold | % | U16
42632 | 0xA688 | 1 | Swell (Uswl) hysteresis | % | U16
42633 | 0xA689 | 1 | Interruption (Uint) threshold | % | U16
42634 | 0xA68A | 1 | Interruption (Uint) hysteresis | % | U16

## Inrush events settings - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42640 | 0xA690 | Settings | 2 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42640 | 0xA690 | 1 | Inrush current threshold | % | U16
42641 | 0xA691 | 1 | Inrush current hysteresis | % | U16

## Inrush events settings - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42648 | 0xA698 | Settings | 2 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42648 | 0xA698 | 1 | Inrush current threshold | % | U16
42649 | 0xA699 | 1 | Inrush current hysteresis | % | U16

## Inrush events settings - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42656 | 0xA6A0 | Settings | 2 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42656 | 0xA6A0 | 1 | Inrush current threshold | % | U16
42657 | 0xA6A1 | 1 | Inrush current hysteresis | % | U16

## Inrush events settings - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42664 | 0xA6A8 | Settings | 2 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42664 | 0xA6A8 | 1 | Inrush current threshold | % | U16
42665 | 0xA6A9 | 1 | Inrush current hysteresis | % | U16

## Quality events log

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42752 | 0xA700 | Command | 2 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42752 | 0xA700 | 1 | Start record number (0 to 65534) or 65535 for last record | - | U16
42753 | 0xA701 | 1 | Event type 0 : All 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42768 | 0xA710 | Header | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42768 | 0xA710 | 1 | Next record number | - | U16
42769 | 0xA711 | 1 | Items count (max 3 per request) | - | U16
42770 | 0xA712 | 1 | Item size (words) | - | U16
42771 | 0xA713 | 1 | Event type 0 : All 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
42772 | 0xA714 | Data | 45 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
42772 | 0xA714 | 1 | Event type 0 : Unknown 1 : Swell 2 : Dip 3 : Interruption 4 : Inrush current 5 : Trip | - | U16
42773 | 0xA715 | 4 | Start date | - | DATETIME_MS
42777 | 0xA719 | 4 | End date | - | DATETIME_MS
42781 | 0xA71D | 1 | Net/Load 0 : Net 1 : Load 1 2 : Load 2 3 : Load 3 4 : Load 4 6 : Undefined | - | U8
42782 | 0xA71E | 1 | Line mask | - | U16_HEX
42783 | 0xA71F | 1 | Start mask | - | U16_HEX
42784 | 0xA720 | 1 | End mask | - | U16_HEX
42785 | 0xA721 | 1 | Trig ratio | % | U16
42786 | 0xA722 | 1 | Ret trig ratio | % | U16
42787 | 0xA723 | 2 | Bit weight VU | V / 1000 | U32
42789 | 0xA725 | 2 | Bit weight I1 | A / 100000 | U32
42791 | 0xA727 | 2 | Bit weight I2 | A / 100000 | U32
42793 | 0xA729 | 2 | Bit weight I3 | A / 100000 | U32
42795 | 0xA72B | 2 | Bit weight In | A / 100000 | U32
42797 | 0xA72D | 1 | V1ref | - | U16
42798 | 0xA72E | 1 | V2ref | - | U16
42799 | 0xA72F | 1 | V3ref | - | U16
42800 | 0xA730 | 1 | U12ref | - | U16
42801 | 0xA731 | 1 | U23ref | - | U16
42802 | 0xA732 | 1 | U31ref | - | U16
42803 | 0xA733 | 1 | I1ref | - | U16
42804 | 0xA734 | 1 | I2ref | - | U16
42805 | 0xA735 | 1 | I3ref | - | U16
42806 | 0xA736 | 1 | Inref | - | U16
42807 | 0xA737 | 1 | V1 min/max | - | U16
42808 | 0xA738 | 1 | V2 min/max | - | U16
42809 | 0xA739 | 1 | V3 min/max | - | U16
42810 | 0xA73A | 1 | U12 min/max | - | U16
42811 | 0xA73B | 1 | U23 min/max | - | U16
42812 | 0xA73C | 1 | U31 min/max | - | U16
42813 | 0xA73D | 1 | I1 min/max | - | U16
42814 | 0xA73E | 1 | I2 min/max | - | U16
42815 | 0xA73F | 1 | I3 min/max | - | U16
42816 | 0xA740 | 1 | In min/max | - | U16

# LoadShedding

## LoadShedding settings - Load #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
43024 | 0xA810 | Settings | 5 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
43024 | 0xA810 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
43025 | 0xA811 | 1 | Output : 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
43026 | 0xA812 | 1 | Predictive power type : 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S | - | U16
43027 | 0xA813 | 2 | Activation threshold (in W, var or VA) | - | U32

## LoadShedding settings - Load #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
43032 | 0xA818 | Settings | 5 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
43032 | 0xA818 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
43033 | 0xA819 | 1 | Output : 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
43034 | 0xA81A | 1 | Predictive power type : 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S | - | U16
43035 | 0xA81B | 2 | Activation threshold (in W, var or VA) | - | U32

## LoadShedding settings - Load #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
43040 | 0xA820 | Settings | 5 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
43040 | 0xA820 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
43041 | 0xA821 | 1 | Output : 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
43042 | 0xA822 | 1 | Predictive power type : 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S | - | U16
43043 | 0xA823 | 2 | Activation threshold (in W, var or VA) | - | U32

## LoadShedding settings - Load #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
43048 | 0xA828 | Settings | 5 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
43048 | 0xA828 | 1 | Status : 0 : Disabled 1 : Enabled | - | U16
43049 | 0xA829 | 1 | Output : 0 : Output 1 1 : Output 2 2 : Output 3 3 : Output 4 4 : Output 5 5 : Output 6 6 : Output 7 7 : Output 8 255 : Not used | - | U16
43050 | 0xA82A | 1 | Predictive power type : 0 : P+ 1 : P- 2 : Q+ 3 : Q- 4 : S | - | U16
43051 | 0xA82B | 2 | Activation threshold (in W, var or VA) | - | U32

## LoadShedding commands state

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
43008 | 0xA800 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
43008 | 0xA800 | 1 | LoadShedding command 1 0 : Inactive 1 : Active | - | U8
43009 | 0xA801 | 1 | LoadShedding command 2 0 : Inactive 1 : Active | - | U8
43010 | 0xA802 | 1 | LoadShedding command 3 0 : Inactive 1 : Active | - | U8
43011 | 0xA803 | 1 | LoadShedding command 4 0 : Inactive 1 : Active | - | U8

# Common

## Evt EN50160 in Progress

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51984 | 0xCB10 | Info | 106 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51984 | 0xCB10 | 1 | Evt in progress: up to 4 different types (dip, swell, interruption, overload) | - | U16
51985 | 0xCB11 | 1 | Data size : 26 | - | U16
51986 | 0xCB12 | 4 | Date | s / 1000 | DATETIME_MS
51990 | 0xCB16 | 2 | Duration | s / 1000 | U32
51992 | 0xCB18 | 0 | Nature & Network type: Nature 1 : Swell 2 : Dip 3 : Interruption 4 : Overload current | - | U8_H
51992 | 0xCB18 | 1 | Nature & Network type: Network type 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8_L
51993 | 0xCB19 | 0 | Thresholds and Hysteresis: Threshold | % | U8_H
51993 | 0xCB19 | 1 | Thresholds and Hysteresis: Hysteresis | % | U8_L
51994 | 0xCB1A | 1 | Classification (following EN50160 norm) | A | U16
51995 | 0xCB1B | 0 | Start parameter and end parameter: start parameter | - | U8_H
51995 | 0xCB1B | 1 | Start parameter and end parameter: end parameter | - | U8_L
51996 | 0xCB1C | 2 | Nominal voltage : Vnom | V / 100 | U32
51998 | 0xCB1E | 2 | Nominal voltage : Unom | V / 100 | U32
52000 | 0xCB20 | 2 | Nominal current : Inom | A / 1000 | U32
52002 | 0xCB22 | 0 | Ref voltage (V1 & V2): V1 | % / 5 | S8_H
52002 | 0xCB22 | 1 | Ref voltage (V1 & V2): V2 | % / 5 | S8_L
52003 | 0xCB23 | 0 | Ref voltage (V3 & U12): V3 | % / 5 | S8_H
52003 | 0xCB23 | 1 | Ref voltage (V3 & U12): U12 | % / 5 | S8_L
52004 | 0xCB24 | 0 | Ref voltage (U23 & U31): U23 | % / 5 | S8_H
52004 | 0xCB24 | 1 | Ref voltage (U23 & U31): U31 | % / 5 | S8_L
52005 | 0xCB25 | 0 | Voltage delta (V1 & V2): V1 | % / 2 | S8_H
52005 | 0xCB25 | 1 | Voltage delta (V1 & V2): V2 | % / 2 | S8_L
52006 | 0xCB26 | 0 | Voltage delta (V3 & U12): V3 | % / 2 | S8_H
52006 | 0xCB26 | 1 | Voltage delta (V3 & U12): U12 | % / 2 | S8_L
52007 | 0xCB27 | 0 | Voltage delta (U23 & U31): U23 | % / 2 | S8_H
52007 | 0xCB27 | 1 | Voltage delta (U23 & U31): U31 | % / 2 | S8_L
52008 | 0xCB28 | 1 | Current delta I1 | % | U16
52009 | 0xCB29 | 1 | Current delta I2 | % | U16
52010 | 0xCB2A | 1 | Current delta I3 | % | U16
52011 | 0xCB2B | 1 | Current delta In | % | U16
52012 | 0xCB2C | 4 | Date | s / 1000 | DATETIME_MS
52016 | 0xCB30 | 2 | Duration | s / 1000 | U32
52018 | 0xCB32 | 0 | Nature & Network type: Nature 1 : Swell 2 : Dip 3 : Interruption 4 : Overload current | - | U8_H
52018 | 0xCB32 | 1 | Nature & Network type: Network type 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8_L
52019 | 0xCB33 | 0 | Thresholds and Hysteresis: Threshold | % | U8_H
52019 | 0xCB33 | 1 | Thresholds and Hysteresis: Hysteresis | % | U8_L
52020 | 0xCB34 | 1 | Classification (following EN50160 norm) | A | U16
52021 | 0xCB35 | 0 | Start parameter and end parameter: start parameter | - | U8_H
52021 | 0xCB35 | 1 | Start parameter and end parameter: end parameter | - | U8_L
52022 | 0xCB36 | 2 | Ref V Nominal | V / 100 | U32
52024 | 0xCB38 | 2 | Ref U Nominal | V / 100 | U32
52026 | 0xCB3A | 2 | Ref I Nominal | A / 1000 | U32
52028 | 0xCB3C | 0 | Sliding Ref voltage (V1 & V2): V1 | % / 5 | S8_H
52028 | 0xCB3C | 1 | Sliding Ref voltage (V1 & V2): V2 | % / 5 | S8_L
52029 | 0xCB3D | 0 | Sliding Ref voltage (V3 & U12): V3 | % / 5 | S8_H
52029 | 0xCB3D | 1 | Sliding Ref voltage (V3 & U12): U12 | % / 5 | S8_L
52030 | 0xCB3E | 0 | Sliding Ref voltage (U23 & U31): U23 | % / 5 | S8_H
52030 | 0xCB3E | 1 | Sliding Ref voltage (U23 & U31): U31 | % / 5 | S8_L
52031 | 0xCB3F | 0 | Voltage delta (V1 & V2): V1 | % / 2 | S8_H
52031 | 0xCB3F | 1 | Voltage delta (V1 & V2): V2 | % / 2 | S8_L
52032 | 0xCB40 | 0 | Voltage delta (V3 & U12): V3 | % / 2 | S8_H
52032 | 0xCB40 | 1 | Voltage delta (V3 & U12): U12 | % / 2 | S8_L
52033 | 0xCB41 | 0 | Voltage delta (U23 & U31): U23 | % / 2 | S8_H
52033 | 0xCB41 | 1 | Voltage delta (U23 & U31): U31 | % / 2 | S8_L
52034 | 0xCB42 | 1 | Current delta I1 | % | U16
52035 | 0xCB43 | 1 | Current delta I2 | % | U16
52036 | 0xCB44 | 1 | Current delta I3 | % | U16
52037 | 0xCB45 | 1 | Current delta In | % | U16
52038 | 0xCB46 | 4 | Date | s / 1000 | DATETIME_MS
52042 | 0xCB4A | 2 | Duration | s / 1000 | U32
52044 | 0xCB4C | 0 | Nature & Network type: Nature 1 : Swell 2 : Dip 3 : Interruption 4 : Overload current | - | U8_H
52044 | 0xCB4C | 1 | Nature & Network type: Network type 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8_L
52045 | 0xCB4D | 0 | Thresholds and Hysteresis: Threshold | % | U8_H
52045 | 0xCB4D | 1 | Thresholds and Hysteresis: Hysteresis | % | U8_L
52046 | 0xCB4E | 1 | Classification (following EN50160 norm) | A | U16
52047 | 0xCB4F | 0 | Start parameter and end parameter: start parameter | - | U8_H
52047 | 0xCB4F | 1 | Start parameter and end parameter: end parameter | - | U8_L
52048 | 0xCB50 | 2 | Ref V Nominal | V / 100 | U32
52050 | 0xCB52 | 2 | Ref U Nominal | V / 100 | U32
52052 | 0xCB54 | 2 | Ref I Nominal | A / 1000 | U32
52054 | 0xCB56 | 0 | Sliding Ref voltage (V1 & V2): V1 | % / 5 | S8_H
52054 | 0xCB56 | 1 | Sliding Ref voltage (V1 & V2): V2 | % / 5 | S8_L
52055 | 0xCB57 | 0 | Sliding Ref voltage (V3 & U12): V3 | % / 5 | S8_H
52055 | 0xCB57 | 1 | Sliding Ref voltage (V3 & U12): U12 | % / 5 | S8_L
52056 | 0xCB58 | 0 | Sliding Ref voltage (U23 & U31): U23 | % / 5 | S8_H
52056 | 0xCB58 | 1 | Sliding Ref voltage (U23 & U31): U31 | % / 5 | S8_L
52057 | 0xCB59 | 0 | Voltage delta (V1 & V2): V1 | % / 2 | S8_H
52057 | 0xCB59 | 1 | Voltage delta (V1 & V2): V2 | % / 2 | S8_L
52058 | 0xCB5A | 0 | Voltage delta (V3 & U12): V3 | % / 2 | S8_H
52058 | 0xCB5A | 1 | Voltage delta (V3 & U12): U12 | % / 2 | S8_L
52059 | 0xCB5B | 0 | Voltage delta (U23 & U31): U23 | % / 2 | S8_H
52059 | 0xCB5B | 1 | Voltage delta (U23 & U31): U31 | % / 2 | S8_L
52060 | 0xCB5C | 1 | Current delta I1 | % | U16
52061 | 0xCB5D | 1 | Current delta I2 | % | U16
52062 | 0xCB5E | 1 | Current delta I3 | % | U16
52063 | 0xCB5F | 1 | Current delta In | % | U16
52064 | 0xCB60 | 4 | Date | s / 1000 | DATETIME_MS
52068 | 0xCB64 | 2 | Duration | s / 1000 | U32
52070 | 0xCB66 | 0 | Nature & Network type: Nature 1 : Swell 2 : Dip 3 : Interruption 4 : Overload current | - | U8_H
52070 | 0xCB66 | 1 | Nature & Network type: Network type 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8_L
52071 | 0xCB67 | 0 | Thresholds and Hysteresis: Threshold | % | U8_H
52071 | 0xCB67 | 1 | Thresholds and Hysteresis: Hysteresis | % | U8_L
52072 | 0xCB68 | 1 | Classification (following EN50160 norm) | A | U16
52073 | 0xCB69 | 0 | Start parameter and end parameter: start parameter | - | U8_H
52073 | 0xCB69 | 1 | Start parameter and end parameter: end parameter | - | U8_L
52074 | 0xCB6A | 2 | Ref V Nominal | V / 100 | U32
52076 | 0xCB6C | 2 | Ref U Nominal | V / 100 | U32
52078 | 0xCB6E | 2 | Ref I Nominal | A / 1000 | U32
52080 | 0xCB70 | 0 | Sliding Ref voltage (V1 & V2): V1 | % / 5 | S8_H
52080 | 0xCB70 | 1 | Sliding Ref voltage (V1 & V2): V2 | % / 5 | S8_L
52081 | 0xCB71 | 0 | Sliding Ref voltage (V3 & U12): V3 | % / 5 | S8_H
52081 | 0xCB71 | 1 | Sliding Ref voltage (V3 & U12): U12 | % / 5 | S8_L
52082 | 0xCB72 | 0 | Sliding Ref voltage (U23 & U31): U23 | % / 5 | S8_H
52082 | 0xCB72 | 1 | Sliding Ref voltage (U23 & U31): U31 | % / 5 | S8_L
52083 | 0xCB73 | 0 | Voltage delta (V1 & V2): V1 | % / 2 | S8_H
52083 | 0xCB73 | 1 | Voltage delta (V1 & V2): V2 | % / 2 | S8_L
52084 | 0xCB74 | 0 | Voltage delta (V3 & U12): V3 | % / 2 | S8_H
52084 | 0xCB74 | 1 | Voltage delta (V3 & U12): U12 | % / 2 | S8_L
52085 | 0xCB75 | 0 | Voltage delta (U23 & U31): U23 | % / 2 | S8_H
52085 | 0xCB75 | 1 | Voltage delta (U23 & U31): U31 | % / 2 | S8_L
52086 | 0xCB76 | 1 | Current delta I1 | % | U16
52087 | 0xCB77 | 1 | Current delta I2 | % | U16
52088 | 0xCB78 | 1 | Current delta I3 | % | U16
52089 | 0xCB79 | 1 | Current delta In | % | U16

## Evt EN50160 log

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
62976 | 0xF600 | Command | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
62976 | 0xF600 | 1 | Action 0x0001 : Reset read pointer 0xFFFE : Get next data | - | U16_HEX

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
62992 | 0xF610 | Header | 2 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
62992 | 0xF610 | 1 | Record count (max. 4) | - | U8
62993 | 0xF611 | 1 | Record size (words) | - | U8

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
62994 | 0xF612 | Data | 26 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
62994 | 0xF612 | 4 | Date | s / 1000 | DATETIME_MS
62998 | 0xF616 | 2 | Duration | s / 1000 | U32
63000 | 0xF618 | 0 | Nature & Network type: Nature 1 : Swell 2 : Dip 3 : Interruption 4 : Overload current | - | U8_H
63000 | 0xF618 | 1 | Nature & Network type: Network type 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8_L
63001 | 0xF619 | 0 | Thresholds and Hysteresis: Threshold | % | U8_H
63001 | 0xF619 | 1 | Thresholds and Hysteresis: Hysteresis | % | U8_L
63002 | 0xF61A | 1 | Classification (following EN50160 norm) | A | U16
63003 | 0xF61B | 0 | Start parameter and end parameter: start parameter | - | U8_H
63003 | 0xF61B | 1 | Start parameter and end parameter: end parameter | - | U8_L
63004 | 0xF61C | 2 | Nominal voltage : Vnom | V / 100 | U32
63006 | 0xF61E | 2 | Nominal voltage : Unom | V / 100 | U32
63008 | 0xF620 | 2 | Nominal current : Inom | A / 1000 | U32
63010 | 0xF622 | 0 | Ref voltage (V1 & V2): V1 | % / 5 | S8_H
63010 | 0xF622 | 1 | Ref voltage (V1 & V2): V2 | % / 5 | S8_L
63011 | 0xF623 | 0 | Ref voltage (V3 & U12): V3 | % / 5 | S8_H
63011 | 0xF623 | 1 | Ref voltage (V3 & U12): U12 | % / 5 | S8_L
63012 | 0xF624 | 0 | Ref voltage (U23 & U31): U23 | % / 5 | S8_H
63012 | 0xF624 | 1 | Ref voltage (U23 & U31): U31 | % / 5 | S8_L
63013 | 0xF625 | 0 | Voltage delta (V1 & V2): V1 | % / 2 | S8_H
63013 | 0xF625 | 1 | Voltage delta (V1 & V2): V2 | % / 2 | S8_L
63014 | 0xF626 | 0 | Voltage delta (V3 & U12): V3 | % / 2 | S8_H
63014 | 0xF626 | 1 | Voltage delta (V3 & U12): U12 | % / 2 | S8_L
63015 | 0xF627 | 0 | Voltage delta (U23 & U31): U23 | % / 2 | S8_H
63015 | 0xF627 | 1 | Voltage delta (U23 & U31): U31 | % / 2 | S8_L
63016 | 0xF628 | 1 | Current delta I1 | % | U16
63017 | 0xF629 | 1 | Current delta I2 | % | U16
63018 | 0xF62A | 1 | Current delta I3 | % | U16
63019 | 0xF62B | 1 | Current delta In | % | U16

# Names

## Load Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46592 | 0xB600 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46592 | 0xB600 | 16 | Name | - | STRING_NORM

## Load Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46608 | 0xB610 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46608 | 0xB610 | 16 | Name | - | STRING_NORM

## Load Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46624 | 0xB620 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46624 | 0xB620 | 16 | Name | - | STRING_NORM

## Load Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46640 | 0xB630 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46640 | 0xB630 | 16 | Name | - | STRING_NORM

## Logical Input Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46848 | 0xB700 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46848 | 0xB700 | 16 | Name | - | STRING_NORM

## Logical Input Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46864 | 0xB710 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46864 | 0xB710 | 16 | Name | - | STRING_NORM

## Logical Input Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46880 | 0xB720 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46880 | 0xB720 | 16 | Name | - | STRING_NORM

## Logical Input Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46896 | 0xB730 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46896 | 0xB730 | 16 | Name | - | STRING_NORM

## Logical Input Name #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46912 | 0xB740 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46912 | 0xB740 | 16 | Name | - | STRING_NORM

## Logical Input Name #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46928 | 0xB750 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46928 | 0xB750 | 16 | Name | - | STRING_NORM

## Logical Input Name #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46944 | 0xB760 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46944 | 0xB760 | 16 | Name | - | STRING_NORM

## Logical Input Name #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46960 | 0xB770 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46960 | 0xB770 | 16 | Name | - | STRING_NORM

## Logical Input Name #9

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46976 | 0xB780 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46976 | 0xB780 | 16 | Name | - | STRING_NORM

## Logical Input Name #10

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
46992 | 0xB790 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
46992 | 0xB790 | 16 | Name | - | STRING_NORM

## Logical Output Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47232 | 0xB880 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47232 | 0xB880 | 16 | Name | - | STRING_NORM

## Logical Output Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47248 | 0xB890 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47248 | 0xB890 | 16 | Name | - | STRING_NORM

## Logical Output Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47264 | 0xB8A0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47264 | 0xB8A0 | 16 | Name | - | STRING_NORM

## Logical Output Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47280 | 0xB8B0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47280 | 0xB8B0 | 16 | Name | - | STRING_NORM

## Logical Output Name #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47296 | 0xB8C0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47296 | 0xB8C0 | 16 | Name | - | STRING_NORM

## Logical Output Name #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47312 | 0xB8D0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47312 | 0xB8D0 | 16 | Name | - | STRING_NORM

## Logical Output Name #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47328 | 0xB8E0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47328 | 0xB8E0 | 16 | Name | - | STRING_NORM

## Logical Output Name #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47344 | 0xB8F0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47344 | 0xB8F0 | 16 | Name | - | STRING_NORM

## Analog Input Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47552 | 0xB9C0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47552 | 0xB9C0 | 16 | Name | - | STRING_NORM

## Analog Input Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47568 | 0xB9D0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47568 | 0xB9D0 | 16 | Name | - | STRING_NORM

## Analog Input Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47584 | 0xB9E0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47584 | 0xB9E0 | 16 | Name | - | STRING_NORM

## Analog Input Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47600 | 0xB9F0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47600 | 0xB9F0 | 16 | Name | - | STRING_NORM

## Analog Input Name #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47616 | 0xBA00 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47616 | 0xBA00 | 16 | Name | - | STRING_NORM

## Analog Input Name #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47632 | 0xBA10 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47632 | 0xBA10 | 16 | Name | - | STRING_NORM

## Analog Input Name #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47648 | 0xBA20 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47648 | 0xBA20 | 16 | Name | - | STRING_NORM

## Analog Input Name #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47664 | 0xBA30 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47664 | 0xBA30 | 16 | Name | - | STRING_NORM

## Analog Output Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47872 | 0xBB00 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47872 | 0xBB00 | 16 | Name | - | STRING_NORM

## Analog Output Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47888 | 0xBB10 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47888 | 0xBB10 | 16 | Name | - | STRING_NORM

## Analog Output Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47904 | 0xBB20 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47904 | 0xBB20 | 16 | Name | - | STRING_NORM

## Analog Output Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47920 | 0xBB30 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47920 | 0xBB30 | 16 | Name | - | STRING_NORM

## Analog Output Name #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47936 | 0xBB40 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47936 | 0xBB40 | 16 | Name | - | STRING_NORM

## Analog Output Name #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47952 | 0xBB50 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47952 | 0xBB50 | 16 | Name | - | STRING_NORM

## Analog Output Name #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47968 | 0xBB60 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47968 | 0xBB60 | 16 | Name | - | STRING_NORM

## Analog Output Name #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
47984 | 0xBB70 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
47984 | 0xBB70 | 16 | Name | - | STRING_NORM

## Temperature Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48192 | 0xBC40 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48192 | 0xBC40 | 16 | Name | - | STRING_NORM

## Temperature Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48208 | 0xBC50 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48208 | 0xBC50 | 16 | Name | - | STRING_NORM

## Temperature Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48224 | 0xBC60 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48224 | 0xBC60 | 16 | Name | - | STRING_NORM

## Temperature Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48240 | 0xBC70 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48240 | 0xBC70 | 16 | Name | - | STRING_NORM

## Analog Alarm Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48448 | 0xBD40 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48448 | 0xBD40 | 16 | Name | - | STRING_NORM

## Analog Alarm Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48464 | 0xBD50 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48464 | 0xBD50 | 16 | Name | - | STRING_NORM

## Analog Alarm Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48480 | 0xBD60 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48480 | 0xBD60 | 16 | Name | - | STRING_NORM

## Analog Alarm Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48496 | 0xBD70 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48496 | 0xBD70 | 16 | Name | - | STRING_NORM

## Analog Alarm Name #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48512 | 0xBD80 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48512 | 0xBD80 | 16 | Name | - | STRING_NORM

## Analog Alarm Name #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48528 | 0xBD90 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48528 | 0xBD90 | 16 | Name | - | STRING_NORM

## Analog Alarm Name #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48544 | 0xBDA0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48544 | 0xBDA0 | 16 | Name | - | STRING_NORM

## Analog Alarm Name #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48560 | 0xBDB0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48560 | 0xBDB0 | 16 | Name | - | STRING_NORM

## Logical Alarm Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48768 | 0xBE80 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48768 | 0xBE80 | 16 | Name | - | STRING_NORM

## Logical Alarm Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48784 | 0xBE90 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48784 | 0xBE90 | 16 | Name | - | STRING_NORM

## Logical Alarm Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48800 | 0xBEA0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48800 | 0xBEA0 | 16 | Name | - | STRING_NORM

## Logical Alarm Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48816 | 0xBEB0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48816 | 0xBEB0 | 16 | Name | - | STRING_NORM

## Combination Alarm Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48960 | 0xBF40 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48960 | 0xBF40 | 16 | Name | - | STRING_NORM

## Combination Alarm Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48976 | 0xBF50 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48976 | 0xBF50 | 16 | Name | - | STRING_NORM

## Combination Alarm Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
48992 | 0xBF60 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
48992 | 0xBF60 | 16 | Name | - | STRING_NORM

## Combination Alarm Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49008 | 0xBF70 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49008 | 0xBF70 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49152 | 0xC000 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49152 | 0xC000 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49168 | 0xC010 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49168 | 0xC010 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49184 | 0xC020 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49184 | 0xC020 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49200 | 0xC030 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49200 | 0xC030 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49216 | 0xC040 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49216 | 0xC040 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49232 | 0xC050 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49232 | 0xC050 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49248 | 0xC060 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49248 | 0xC060 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49264 | 0xC070 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49264 | 0xC070 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #9

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49280 | 0xC080 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49280 | 0xC080 | 16 | Name | - | STRING_NORM

## Multi-fluid Feeder Name #10

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49296 | 0xC090 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49296 | 0xC090 | 16 | Name | - | STRING_NORM

## Tariff Name #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49536 | 0xC180 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49536 | 0xC180 | 16 | Name | - | STRING_NORM

## Tariff Name #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49552 | 0xC190 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49552 | 0xC190 | 16 | Name | - | STRING_NORM

## Tariff Name #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49568 | 0xC1A0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49568 | 0xC1A0 | 16 | Name | - | STRING_NORM

## Tariff Name #4

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49584 | 0xC1B0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49584 | 0xC1B0 | 16 | Name | - | STRING_NORM

## Tariff Name #5

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49600 | 0xC1C0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49600 | 0xC1C0 | 16 | Name | - | STRING_NORM

## Tariff Name #6

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49616 | 0xC1D0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49616 | 0xC1D0 | 16 | Name | - | STRING_NORM

## Tariff Name #7

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49632 | 0xC1E0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49632 | 0xC1E0 | 16 | Name | - | STRING_NORM

## Tariff Name #8

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
49648 | 0xC1F0 | Settings | 16 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
49648 | 0xC1F0 | 16 | Name | - | STRING_NORM