= Schneider Acti9 Smartlink Meter

Three-phase electricity meter for energy measurement via Modbus protocol.

== Overview

This bundle provides integration with Schneider Acti9 Smartlink meters, three-phase electricity meters designed for energy management in commercial and industrial installations. The component communicates with the meter through the Modbus TCP protocol, enabling real-time energy monitoring, power measurement, and comprehensive data collection in OpenEMS.

Schneider Acti9 Smartlink meters are part of Schneider Electric's distribution management system for reliable energy measurement and monitoring.

== Supported Devices

* https://www.schneider-electric.com/[Schneider Acti9 Smartlink Meter icon:external-link[]]

== Components

This bundle implements the following OpenEMS Component:

=== Schneider Acti9 Smartlink Meter

*Name*: Meter Schneider Acti9 Smartlink

*Factory-PID*: `Meter.Schneider.Acti9.Smartlink`

.Implemented Natures/Interfaces
* MeterSchneiderActi9Smartlink
* ElectricityMeter
* ModbusComponent
* OpenemsComponent

*Description*: Three-phase electricity meter for energy measurement via Modbus protocol.

.*Configuration*:

* `id` (String): Component ID for unique identification (default: "meter0")
* `alias` (String): Human-readable alias for the component
* `enabled` (Boolean): Enable/disable this component (default: true)
* `modbus_id` (String): ID of Modbus bridge for communication (default: "modbus0")
* `modbusUnitId` (Integer): Modbus Unit ID of the meter device (default: 1)
* `type` (Enum): Meter type - GRID, PRODUCTION, or CONSUMPTION (default: PRODUCTION)
* `invert` (Boolean): Invert all power and current values (default: false)

https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.meter.schneider.acti9.smartlink[Source Code icon:github[]]
