= Phoenix Contact EEM-MB370-24DC Meter

Three-phase electricity meter for energy measurement via Modbus protocol.

== Overview

This bundle provides integration with Phoenix Contact energy meters, specifically the EEM-MB370-24DC model. The component communicates with the meter through the Modbus TCP protocol, enabling real-time energy monitoring and comprehensive data collection in OpenEMS.

Phoenix Contact meters are designed for reliable energy measurement in commercial and industrial applications with robust industrial design and proven reliability.

== Supported Devices

* https://www.phoenixcontact.com/de-de/produkte/energiemessgeraet-eem-mb370-24dc-1127061[Phoenix Contact EEM-MB370-24DC icon:external-link[]]

== Components

This bundle implements the following OpenEMS Component:

=== Phoenix Contact Meter

*Name*: Meter Phoenix Contact

*Factory-PID*: `Meter.PhoenixContact`

.Implemented Natures/Interfaces
* PhoenixContactMeter
* ElectricityMeter
* ModbusComponent
* OpenemsComponent
* ModbusSlave

*Description*: Three-phase electricity meter for energy measurement via Modbus protocol.

.*Configuration*:

* `id` (String): Component ID for unique identification (default: "meter0")
* `alias` (String): Human-readable alias for the component
* `enabled` (Boolean): Enable/disable this component (default: true)
* `modbus_id` (String): ID of Modbus bridge for communication (default: "modbus0")
* `modbusUnitId` (Integer): Modbus Unit ID of the meter device (default: 1)
* `type` (Enum): Meter type - GRID, PRODUCTION, or CONSUMPTION (default: PRODUCTION)
* `invert` (Boolean): Invert power and current, swap production/consumption energy (default: false)

https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.meter.phoenixcontact[Source Code icon:github[]]