= FENECON Commercial Battery

High-performance lithium battery system for commercial and industrial energy storage (of year 2024).

== Overview

This bundle provides integration with the FENECON Commercial Battery (of year 2024), a modular lithium-based energy storage system designed for commercial and industrial applications. The system communicates via Modbus for precise charge/discharge control, thermal management, and state monitoring.

== Components

This bundle implements the following OpenEMS Components:

=== FENECON Commercial Battery

*Name*: Battery FENECON Commercial

*Factory-PID*: `Battery.Fenecon.Commercial`

.Implemented Natures/Interfaces
* BatteryFeneconCommercial
* Battery
* ModbusComponent
* OpenemsComponent
* EventHandler
* ModbusSlave
* StartStoppable

*Description*: Modbus interface for the FENECON Commercial Battery system. Manages charging and discharging of the battery pack, monitors state of charge, temperature, cell voltages, and health status. Supports relay-based automatic start/stop control for safety and operational optimization.

.*Configuration*:

* `id` (String): Component ID for unique identification (default: "battery0")
* `alias` (String): Human-readable alias for the component
* `enabled` (Boolean): Enable/disable this component (default: true)
* `startStop` (StartStopConfig): Start/stop behavior - AUTO, ALWAYS_ON, or ALWAYS_OFF (default: AUTO)
* `modbus_id` (String): ID of the Modbus bridge to use (default: "modbus0")
* `modbusUnitId` (Integer): Modbus Unit-ID of the battery device (default: 1)
* `batteryStartStopRelay` (String): IO channel for automatic start/stop relay control (default: "io0/Relay7")

https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.battery.fenecon.commercial[Source Code icon:github[]]