# General

# Identification

## Product identification

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50000 | 0xC350 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50000 | 0xC350 | 4 | "SOCO" | - | STRING_16
50004 | 0xC354 | 1 | Product order ID (Countis:100, Protection:200, Atys:300, Diris:400) | - | U16
50005 | 0xC355 | 1 | Product ID (EX: 1000 ATS3) | - | U16
50006 | 0xC356 | 1 | JBUS Table Version (EX: 101 Version 1.01) | - | U16
50007 | 0xC357 | 1 | Product software version (EX: 100 Version 1.00) | - | U16
50008 | 0xC358 | 1 | Serial_AA_SS | - | U16_HEX
50009 | 0xC359 | 1 | Serial_SST_L | - | U16_HEX
50010 | 0xC35A | 1 | Serial_order | - | U16
50011 | 0xC35B | 2 | Serial_Reserve | - | U32
50013 | 0xC35D | 4 | See "Code table" tab for more details | - | U64_HEX
50017 | 0xC361 | 1 | Customization data loaded (True/False) | - | U8
50018 | 0xC362 | 1 | Product version (Major) | - | U16
50019 | 0xC363 | 1 | Product version (Minor) | - | U16
50020 | 0xC364 | 1 | Product version (Revision) | - | U16
50021 | 0xC365 | 1 | Product version (Build) | - | U16
50022 | 0xC366 | 3 | Product build date | - | DATETIME_3
50025 | 0xC369 | 1 | Software technical base version (Major) | - | U16
50026 | 0xC36A | 1 | Software technical base version (Minor) | - | U16
50027 | 0xC36B | 1 | Software technical base version (Revision) | - | U16
50028 | 0xC36C | 1 | Customization version (Major) | - | U16
50029 | 0xC36D | 1 | Customization version (Minor) | - | U16
50030 | 0xC36E | 4 | Product VLO (EX : "880100") | - | STRING_NORM
50034 | 0xC372 | 4 | Customization VLO (EX : "880700") | - | STRING_NORM
50038 | 0xC376 | 4 | Software technical base VLO (EX : "880600") | - | STRING_NORM
50042 | 0xC37A | 8 | Vendor name (EX : "SOCOMEC") | - | STRING_NORM
50050 | 0xC382 | 8 | Product name (EX : "DIRIS A40R") | - | STRING_NORM
50058 | 0xC38A | 8 | Extended name | - | STRING_NORM

## Communication board information

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38912 | 0x9800 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38912 | 0x9800 | 1 | Communication Board version (Major) | - | U16
38913 | 0x9801 | 1 | Communication Board version (Minor) | - | U16
38914 | 0x9802 | 1 | Communication Board version (Revision) | - | U16
38915 | 0x9803 | 1 | Communication Board version (Build) | - | U16
38916 | 0x9804 | 3 | Communication Board build date | - | DATETIME_3
38919 | 0x9807 | 4 | Communication Board VLO (EX : "880100") | - | STRING_NORM

# Common settings

## Network Setting

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57344 | 0xE000 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57344 | 0xE000 | 1 | Network Type : 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8
57345 | 0xE001 | 1 | Current Transformer secondary : 1 : 1 A 5 : 5 A | A | U8
57346 | 0xE002 | 1 | Current Transformer primary | A | U16
57347 | 0xE003 | 1 | Reserved | - | -
57348 | 0xE004 | 1 | Reserved | - | -
57349 | 0xE005 | 1 | Reserved | - | -
57350 | 0xE006 | 1 | Reserved | - | -
57351 | 0xE007 | 1 | Reserved | - | -
57352 | 0xE008 | 2 | Reserved | - | -
57354 | 0xE00A | 1 | Reserved | - | -
57355 | 0xE00B | 1 | Synchronisation Top for P+ : time in seconds (60s, 300s, 480s, 600s, 900s, 1200s, 1800s, 3600s) | s | U16

## Hour/Date setting ( Write 6 words in one time Function 16)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57600 | 0xE100 | Settings | 6 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57600 | 0xE100 | 1 | Day | - | U8
57601 | 0xE101 | 1 | Month | - | U8
57602 | 0xE102 | 1 | Year | - | U16
57603 | 0xE103 | 1 | Hour | - | U8
57604 | 0xE104 | 1 | Minute | - | U8
57605 | 0xE105 | 1 | Second | - | U8

# Actions

## Action system

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57856 | 0xE200 | Commands | 1 | NONE | READ | WRITE | READ | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57856 | 0xE200 | 1 | Action : 0xA1 : Product Configuration storage 0xB2 : Produit reset | - | U8_HEX

# Application

# Measurement

# Common

## Metrology Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50512 | 0xC550 | Info | 62 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50512 | 0xC550 | 2 | Reserved | - | -
50514 | 0xC552 | 2 | Phase to Phase Voltage: U12 | V / 100 | U32
50516 | 0xC554 | 2 | Phase to Phase Voltage: U23 | V / 100 | U32
50518 | 0xC556 | 2 | Phase to Phase Voltage: U31 | V / 100 | U32
50520 | 0xC558 | 2 | Simple voltage : V1 | V / 100 | U32
50522 | 0xC55A | 2 | Simple voltage : V2 | V / 100 | U32
50524 | 0xC55C | 2 | Simple voltage : V3 | V / 100 | U32
50526 | 0xC55E | 2 | Frequency : F | Hz / 100 | U32
50528 | 0xC560 | 2 | Current : I1 | A / 1000 | U32
50530 | 0xC562 | 2 | Current : I2 | A / 1000 | U32
50532 | 0xC564 | 2 | Current : I3 | A / 1000 | U32
50534 | 0xC566 | 2 | Neutral Current : In | A / 1000 | U32
50536 | 0xC568 | 2 | ? Active Power +/- : P | W / 0.1 | S32
50538 | 0xC56A | 2 | ? Reactive Power +/- : Q | var / 0.1 | S32
50540 | 0xC56C | 2 | ? Apparent Power : S | VA / 0.1 | U32
50542 | 0xC56E | 2 | ? Power Factor : -: leading et + : lagging : PF | - / 1000 | S32
50544 | 0xC570 | 2 | Active Power phase 1 +/- : P1 | W / 0.1 | S32
50546 | 0xC572 | 2 | Active Power phase 2 +/- : P2 | W / 0.1 | S32
50548 | 0xC574 | 2 | Active Power phase 3 +/- : P3 | W / 0.1 | S32
50550 | 0xC576 | 2 | Reactive Power phase 1 +/- : Q1 | var / 0.1 | S32
50552 | 0xC578 | 2 | Reactive Power phase 2 +/- : Q2 | var / 0.1 | S32
50554 | 0xC57A | 2 | Reactive Power phase 3 +/- : Q3 | var / 0.1 | S32
50556 | 0xC57C | 2 | Apparent Power phase 1 : S1 | VA / 0.1 | U32
50558 | 0xC57E | 2 | Apparent Power phase 2 : S2 | VA / 0.1 | U32
50560 | 0xC580 | 2 | Apparent Power phase 3 : S3 | VA / 0.1 | U32
50562 | 0xC582 | 2 | Power Factor phase 1 -: leading and + : lagging : PF1 | - / 1000 | S32
50564 | 0xC584 | 2 | Power Factor phase 2 -: leading and + : lagging : PF2 | - / 1000 | S32
50566 | 0xC586 | 2 | Power Factor phase 3 -: leading and + : lagging : PF3 | - / 1000 | S32
50568 | 0xC588 | 2 | Reserved | - | -
50570 | 0xC58A | 2 | Reserved | - | -
50572 | 0xC58C | 2 | Reserved | - | -

## Energies

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50768 | 0xC650 | Info | 65 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50768 | 0xC650 | 2 | Reserved | - | -
50770 | 0xC652 | 2 | Total Positive Active Energy (not resettable) : Ea+ | Wh / 0.001 | U32
50772 | 0xC654 | 2 | Total Positive Reactive Energy (not resettable) : Er + | varh / 0.001 | U32
50774 | 0xC656 | 2 | Reserved | - | -
50776 | 0xC658 | 2 | Total Negative Active Energy (not resettable) : Ea- | Wh / 0.001 | U32
50778 | 0xC65A | 2 | Total Negative Reactive Energy (not resettable) : Er - | varh / 0.001 | U32
50780 | 0xC65C | 2 | Partial Positive Active Energy: Ea+ | Wh / 0.001 | U32
50782 | 0xC65E | 2 | Partial Positive Reactive Energy: Er + | varh / 0.001 | U32
50784 | 0xC660 | 2 | Reserved | - | -
50786 | 0xC662 | 2 | Partial Negative Active Energy : Ea- | Wh / 0.001 | U32
50788 | 0xC664 | 2 | Partial Negative Reactive Energy : Er - | varh / 0.001 | U32
50790 | 0xC666 | 2 | Reserved | - | -
50792 | 0xC668 | 2 | Reserved | - | -
50794 | 0xC66A | 2 | Reserved | - | -
50796 | 0xC66C | 2 | Reserved | - | -
50798 | 0xC66E | 2 | Reserved | - | -
50800 | 0xC670 | 2 | Reserved | - | -
50802 | 0xC672 | 2 | Reserved | - | -
50804 | 0xC674 | 2 | Reserved | - | -
50806 | 0xC676 | 2 | Reserved | - | -
50808 | 0xC678 | 2 | Reserved | - | -
50810 | 0xC67A | 2 | Reserved | - | -
50812 | 0xC67C | 2 | Reserved | - | -
50814 | 0xC67E | 2 | Reserved | - | -
50816 | 0xC680 | 2 | Reserved | - | -
50818 | 0xC682 | 2 | Reserved | - | -
50820 | 0xC684 | 2 | Reserved | - | -
50822 | 0xC686 | 2 | Reserved | - | -
50824 | 0xC688 | 2 | Reserved | - | -
50826 | 0xC68A | 2 | Last date for Record average P/Q/S in second since 01/01/2000 | s | U32
50828 | 0xC68C | 1 | Last average (P+) | W | U16
50829 | 0xC68D | 1 | Reserved | - | -
50830 | 0xC68E | 1 | Reserved | - | -
50831 | 0xC68F | 1 | Reserved | - | -
50832 | 0xC690 | 1 | Reserved | - | -

## Energies in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50944 | 0xC700 | Info | 65 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50944 | 0xC700 | 2 | Reserved | - | -
50946 | 0xC702 | 2 | Total Positive Active Energy (not resettable) : Ea+ | Wh / 0.1 | U32
50948 | 0xC704 | 2 | Total Positive Reactive Energy (not resettable) : Er + | varh / 0.1 | U32
50950 | 0xC706 | 2 | Reserved | - | -
50952 | 0xC708 | 2 | Total Negative Active Energy (not resettable) : Ea- | Wh / 0.1 | U32
50954 | 0xC70A | 2 | Total Negative Reactive Energy (not resettable) : Er - | varh / 0.1 | U32
50956 | 0xC70C | 2 | Partial Positive Active Energy: Ea+ | Wh / 0.1 | U32
50958 | 0xC70E | 2 | Partial Positive Reactive Energy: Er + | varh / 0.1 | U32
50960 | 0xC710 | 2 | Reserved | - | -
50962 | 0xC712 | 2 | Partial Negative Active Energy : Ea- | Wh / 0.1 | U32
50964 | 0xC714 | 2 | Partial Negative Reactive Energy : Er - | varh / 0.1 | U32
50966 | 0xC716 | 2 | Reserved | - | -
50968 | 0xC718 | 2 | Reserved | - | -
50970 | 0xC71A | 2 | Reserved | - | -
50972 | 0xC71C | 2 | Reserved | - | -
50974 | 0xC71E | 2 | Reserved | - | -
50976 | 0xC720 | 2 | Reserved | - | -
50978 | 0xC722 | 2 | Reserved | - | -
50980 | 0xC724 | 2 | Reserved | - | -
50982 | 0xC726 | 2 | Reserved | - | -
50984 | 0xC728 | 2 | Reserved | - | -
50986 | 0xC72A | 2 | Reserved | - | -
50988 | 0xC72C | 2 | Reserved | - | -
50990 | 0xC72E | 2 | Reserved | - | -
50992 | 0xC730 | 2 | Reserved | - | -
50994 | 0xC732 | 2 | Reserved | - | -
50996 | 0xC734 | 2 | Reserved | - | -
50998 | 0xC736 | 2 | Reserved | - | -
51000 | 0xC738 | 2 | Reserved | - | -
51002 | 0xC73A | 2 | Last date for Record average P/Q/S in second since 01/01/2000 | s | U32
51004 | 0xC73C | 1 | Last average (P+) | W | U16
51005 | 0xC73D | 1 | Reserved | - | -
51006 | 0xC73E | 1 | Reserved | - | -
51007 | 0xC73F | 1 | Reserved | - | -
51008 | 0xC740 | 1 | Reserved | - | -

## Energies per tariff

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50848 | 0xC6A0 | Info | 50 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50848 | 0xC6A0 | 1 | 0 >: Tariff number <: 8 | - | U8
50849 | 0xC6A1 | 1 | Tariff number in progress ( 1 to 8 ) | - | U8
50850 | 0xC6A2 | 2 | Positive Active Energies 1 | Wh / 100 | U32
50852 | 0xC6A4 | 2 | Positive Active Energies 2 | h / 100 | U32
50854 | 0xC6A6 | 2 | Positive Active Energies 3 | h / 100 | U32
50856 | 0xC6A8 | 2 | Positive Active Energies 4 | h / 100 | U32
50858 | 0xC6AA | 2 | Reserved | - | -
50860 | 0xC6AC | 2 | Reserved | - | -
50862 | 0xC6AE | 2 | Reserved | - | -
50864 | 0xC6B0 | 2 | Reserved | - | -
50866 | 0xC6B2 | 2 | Positive Reactive Enegies 1 | varh / 100 | U32
50868 | 0xC6B4 | 2 | Positive Reactive Enegies 2 | h / 100 | U32
50870 | 0xC6B6 | 2 | Positive Reactive Enegies 3 | h / 100 | U32
50872 | 0xC6B8 | 2 | Positive Reactive Enegies 4 | h / 100 | U32
50874 | 0xC6BA | 2 | Reserved | - | -
50876 | 0xC6BC | 2 | Reserved | - | -
50878 | 0xC6BE | 2 | Reserved | - | -
50880 | 0xC6C0 | 2 | Reserved | - | -
50882 | 0xC6C2 | 2 | Reserved | - | -
50884 | 0xC6C4 | 2 | Reserved | - | -
50886 | 0xC6C6 | 2 | Reserved | - | -
50888 | 0xC6C8 | 2 | Reserved | - | -
50890 | 0xC6CA | 2 | Reserved | - | -
50892 | 0xC6CC | 2 | Reserved | - | -
50894 | 0xC6CE | 2 | Reserved | - | -
50896 | 0xC6D0 | 2 | Reserved | - | -

## Energies per tariff in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51200 | 0xC800 | Info | 50 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51200 | 0xC800 | 1 | 0 >: Tariff number <: 8 | - | U8
51201 | 0xC801 | 1 | Tariff number in progress ( 1 to 8 ) | - | U8
51202 | 0xC802 | 2 | Positive Active Energies 1 | Wh / 0.1 | U32
51204 | 0xC804 | 2 | Positive Active Energies 2 | Wh / 0.1 | U32
51206 | 0xC806 | 2 | Positive Active Energies 3 | Wh / 0.1 | U32
51208 | 0xC808 | 2 | Positive Active Energies 4 | Wh / 0.1 | U32
51210 | 0xC80A | 2 | Positive Active Energies 5 | h / 100 | U32
51212 | 0xC80C | 2 | Positive Active Energies 6 | h / 100 | U32
51214 | 0xC80E | 2 | Positive Active Energies 7 | h / 100 | U32
51216 | 0xC810 | 2 | Positive Active Energies 8 | h / 100 | U32
51218 | 0xC812 | 2 | Positive Reactive Enegies 1 | varh / 0.1 | U32
51220 | 0xC814 | 2 | Positive Reactive Enegies 2 | varh / 0.1 | U32
51222 | 0xC816 | 2 | Positive Reactive Enegies 3 | varh / 0.1 | U32
51224 | 0xC818 | 2 | Positive Reactive Enegies 4 | varh / 0.1 | U32
51226 | 0xC81A | 2 | Positive Reactive Enegies 5 | h / 100 | U32
51228 | 0xC81C | 2 | Positive Reactive Enegies 6 | h / 100 | U32
51230 | 0xC81E | 2 | Positive Reactive Enegies 7 | h / 100 | U32
51232 | 0xC820 | 2 | Positive Reactive Enegies 8 | h / 100 | U32
51234 | 0xC822 | 2 | Reserved | - | -
51236 | 0xC824 | 2 | Reserved | - | -
51238 | 0xC826 | 2 | Reserved | - | -
51240 | 0xC828 | 2 | Reserved | - | -
51242 | 0xC82A | 2 | Reserved | - | -
51244 | 0xC82C | 2 | Reserved | - | -
51246 | 0xC82E | 2 | Reserved | - | -
51248 | 0xC830 | 2 | Reserved | - | -

## Metrology No Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51280 | 0xC850 | Info | 35 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51280 | 0xC850 | 1 | Reserved | - | -
51281 | 0xC851 | 1 | Phase to Phase Voltage: U12 | V / 100 | U16
51282 | 0xC852 | 1 | Phase to Phase Voltage: U23 | V / 100 | U16
51283 | 0xC853 | 1 | Phase to Phase Voltage: U31 | V / 100 | U16
51284 | 0xC854 | 1 | Simple voltage : V1 | V / 100 | U16
51285 | 0xC855 | 1 | Simple voltage : V2 | V / 100 | U16
51286 | 0xC856 | 1 | Simple voltage : V3 | V / 100 | U16
51287 | 0xC857 | 1 | Frequency : F | Hz / 100 | U16
51288 | 0xC858 | 1 | Current : I1 | A / 1000 | U16
51289 | 0xC859 | 1 | Current : I2 | A / 1000 | U16
51290 | 0xC85A | 1 | Current : I3 | A / 1000 | U16
51291 | 0xC85B | 1 | Neutral Current : In | A / 1000 | U16
51292 | 0xC85C | 1 | ? active Power +/- : P | W / 0.1 | S16
51293 | 0xC85D | 1 | ? reactive Power +/- : Q | var / 0.1 | S16
51294 | 0xC85E | 1 | ? apparent power : S | VA / 0.1 | U16
51295 | 0xC85F | 1 | ? power factor : -: leading and + : lagging : PF | - / 1000 | S16
51296 | 0xC860 | 1 | Active Power phase 1 +/- : P1 | W / 0.1 | S16
51297 | 0xC861 | 1 | Active Power phase 2 +/- : P2 | W / 0.1 | S16
51298 | 0xC862 | 1 | Active Power phase 3 +/- : P3 | W / 0.1 | S16
51299 | 0xC863 | 1 | Reactive Power phase 1 +/- : Q1 | var / 0.1 | S16
51300 | 0xC864 | 1 | Reactive Power phase 2 +/- : Q2 | var / 0.1 | S16
51301 | 0xC865 | 1 | Reactive Power phase 3 +/- : Q3 | var / 0.1 | S16
51302 | 0xC866 | 1 | Apparent power phase 1 : S1 | VA / 0.1 | U16
51303 | 0xC867 | 1 | Apparent power phase 2 : S2 | VA / 0.1 | U16
51304 | 0xC868 | 1 | Apparent power phase 3 : S3 | VA / 0.1 | U16
51305 | 0xC869 | 1 | Power Factor phase 1 -: leading and + : lagging : PF1 | - / 1000 | S16
51306 | 0xC86A | 1 | Power Factor phase 2 -: leading and + : lagging : PF2 | - / 1000 | S16
51307 | 0xC86B | 1 | Power Factor phase 3 -: leading and + : lagging : PF3 | - / 1000 | S16
51308 | 0xC86C | 1 | Reserved | - | -
51309 | 0xC86D | 1 | Reserved | - | -
51310 | 0xC86E | 1 | Reserved | - | -
51311 | 0xC86F | 1 | Total Positive Active Energy (not resettable) : Ea+ | Wh / 1E-06 | U16
51312 | 0xC870 | 1 | Total Positive Reactive Energy (not resettable) : Er + | varh / 1E-06 | U16
51313 | 0xC871 | 1 | Total Negative Active Energy (not resettable) : Ea- | Wh / 1E-06 | U16
51314 | 0xC872 | 1 | Total Negative Reactive Energy (not resettable) : Er - | varh / 1E-06 | U16

# Specific

## Table Overflow

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36864 | 0x9000 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36864 | 0x9000 | 2 | Value of the meter overflow (10Wh) : 999 999 999 | Wh / 0.1 | U32
36866 | 0x9002 | 1 | Nb Overflow Total Ea + | - | U16
36867 | 0x9003 | 1 | Nb Overflow Total Er + | - | U16
36868 | 0x9004 | 1 | Nb Overflow Total Ea - | - | U16
36869 | 0x9005 | 1 | Nb Overflow Total Er - | - | U16
36870 | 0x9006 | 1 | Reserved | - | -
36871 | 0x9007 | 1 | Nb Overflow Total Ea T1 | - | U16
36872 | 0x9008 | 1 | Nb Overflow Total Ea T2 | - | U16
36873 | 0x9009 | 1 | Nb Overflow Total Ea T3 | - | U16
36874 | 0x900A | 1 | Nb Overflow Total Ea T4 | - | U8

## Temporal Active Index

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36896 | 0x9020 | Info | 24 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36896 | 0x9020 | 2 | Ea + for day n-1 | Wh / 0.001 | U32
36898 | 0x9022 | 2 | Reserved | - | -
36900 | 0x9024 | 2 | Ea + for day n | Wh / 0.001 | U32
36902 | 0x9026 | 2 | Reserved | - | -
36904 | 0x9028 | 2 | Ea + for Week n-1 | Wh / 0.001 | U32
36906 | 0x902A | 2 | Reserved | - | -
36908 | 0x902C | 2 | Ea + for Week n | Wh / 0.001 | U32
36910 | 0x902E | 2 | Reserved | - | -
36912 | 0x9030 | 2 | Ea + for Month n-1 | Wh / 0.001 | U32
36914 | 0x9032 | 2 | Reserved | - | -
36916 | 0x9034 | 2 | Ea + for Month n | Wh / 0.001 | U32
36918 | 0x9036 | 2 | Reserved | - | -

## Temporal Active Index in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36928 | 0x9040 | Info | 24 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36928 | 0x9040 | 2 | Ea + for day n-1 | Wh / 0.1 | U32
36930 | 0x9042 | 2 | Reserved | - | -
36932 | 0x9044 | 2 | Ea + for day n | Wh / 0.1 | U32
36934 | 0x9046 | 2 | Reserved | - | -
36936 | 0x9048 | 2 | Ea + for Week n-1 | Wh / 0.1 | U32
36938 | 0x904A | 2 | Reserved | - | -
36940 | 0x904C | 2 | Ea + for Week n | Wh / 0.1 | U32
36942 | 0x904E | 2 | Reserved | - | -
36944 | 0x9050 | 2 | Ea + for Month n-1 | Wh / 0.1 | U32
36946 | 0x9052 | 2 | Reserved | - | -
36948 | 0x9054 | 2 | Ea + for Month n | Wh / 0.1 | U32
36950 | 0x9056 | 2 | Reserved | - | -

## Energies (Full scale)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37376 | 0x9200 | Info | 43 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37376 | 0x9200 | 4 | Total Positive Active Energy (not resettable) : Ea+ | Wh / 0.001 | U64
37380 | 0x9204 | 4 | Total Positive Reactive Energy (not resettable) : Er + | varh / 0.001 | U64
37384 | 0x9208 | 4 | Reserved | - | -
37388 | 0x920C | 4 | Total Negative Active Energy (not resettable) : Ea- | Wh / 0.001 | U64
37392 | 0x9210 | 4 | Total Negative Reactive Energy (not resettable) : Er - | varh / 0.001 | U64
37396 | 0x9214 | 4 | Partial Positive Active Energy: Ea+ | Wh / 0.001 | U64
37400 | 0x9218 | 4 | Partial Positive Reactive Energy: Er + | varh / 0.001 | U64
37404 | 0x921C | 4 | Reserved | - | -
37408 | 0x9220 | 4 | Partial Negative Active Energy : Ea- | Wh / 0.001 | U64
37412 | 0x9224 | 4 | Partial Negative Reactive Energy : Er - | varh / 0.001 | U64
37416 | 0x9228 | 2 | Last date for Record average P in second since 01/01/2000 | s | U32
37418 | 0x922A | 1 | Last average P+ | W | U16

## Energies per tariff (Full scale)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37632 | 0x9300 | Info | 34 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37632 | 0x9300 | 1 | 0 > Tariff number <= 4 | - | U8
37633 | 0x9301 | 1 | Tariff number in progress (1 to 4) | - | U8
37634 | 0x9302 | 4 | Total Positive Active Energie Tariff 1 | Wh / 0.001 | U64
37638 | 0x9306 | 4 | Total Positive Active Energie Tariff 2 | Wh / 0.001 | U64
37642 | 0x930A | 4 | Total Positive Active Energie Tariff 3 | Wh / 0.001 | U64
37646 | 0x930E | 4 | Total Positive Active Energie Tariff 4 | Wh / 0.001 | U64
37650 | 0x9312 | 4 | Partial Positive Active Energie Tariff 1 | Wh / 0.001 | U64
37654 | 0x9316 | 4 | Partial Positive Active Energie Tariff 2 | Wh / 0.001 | U64
37658 | 0x931A | 4 | Partial Positive Active Energie Tariff 3 | Wh / 0.001 | U64
37662 | 0x931E | 4 | Partial Positive Active Energie Tariff 4 | Wh / 0.001 | U64

## Energies in Unit/100 (Full scale)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37888 | 0x9400 | Info | 43 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37888 | 0x9400 | 4 | Total Positive Active Energy (not resettable) : Ea+ | Wh / 0.1 | U64
37892 | 0x9404 | 4 | Total Positive Reactive Energy (not resettable) : Er + | varh / 0.1 | U64
37896 | 0x9408 | 4 | Reserved | - | -
37900 | 0x940C | 4 | Total Negative Active Energy (not resettable) : Ea- | Wh / 0.1 | U64
37904 | 0x9410 | 4 | Total Negative Reactive Energy (not resettable) : Er - | varh / 0.1 | U64
37908 | 0x9414 | 4 | Partial Positive Active Energy: Ea+ | Wh / 0.1 | U64
37912 | 0x9418 | 4 | Partial Positive Reactive Energy: Er + | varh / 0.1 | U64
37916 | 0x941C | 4 | Reserved | - | -
37920 | 0x9420 | 4 | Partial Negative Active Energy : Ea- | Wh / 0.1 | U64
37924 | 0x9424 | 4 | Partial Negative Reactive Energy : Er - | varh / 0.1 | U64
37928 | 0x9428 | 2 | Last date for Record average P in second since 01/01/2000 | s | U32
37930 | 0x942A | 1 | Last average P+ | W | U16

## Energies per tariff in Unit/100 (Full scale)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38144 | 0x9500 | Info | 34 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38144 | 0x9500 | 1 | 0 > Tariff number <= 4 | - | U8
38145 | 0x9501 | 1 | Tariff number in progress (1 to 4) | - | U8
38146 | 0x9502 | 4 | Total Positive Active Energie Tariff 1 | Wh / 0.1 | U64
38150 | 0x9506 | 4 | Total Positive Active Energie Tariff 2 | Wh / 0.1 | U64
38154 | 0x950A | 4 | Total Positive Active Energie Tariff 3 | Wh / 0.1 | U64
38158 | 0x950E | 4 | Total Positive Active Energie Tariff 4 | Wh / 0.1 | U64
38162 | 0x9512 | 4 | Partial Positive Active Energie Tariff 1 | Wh / 0.1 | U64
38166 | 0x9516 | 4 | Partial Positive Active Energie Tariff 2 | Wh / 0.1 | U64
38170 | 0x951A | 4 | Partial Positive Active Energie Tariff 3 | Wh / 0.1 | U64
38174 | 0x951E | 4 | Partial Positive Active Energie Tariff 4 | Wh / 0.1 | U64

## Maximum Values

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
37120 | 0x9100 | Info | 20 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
37120 | 0x9100 | 2 | Maximum I1 | A / 1000 | U32
37122 | 0x9102 | 2 | Maximum I2 | A / 1000 | U32
37124 | 0x9104 | 2 | Maximum I3 | A / 1000 | U32
37126 | 0x9106 | 2 | Maximum In | A / 1000 | U32
37128 | 0x9108 | 2 | Maximum P+ | W / 1000 | U32
37130 | 0x910A | 2 | Maximum P- | W / 1000 | U32
37132 | 0x910C | 2 | Maximum Q+ | var / 1000 | U32
37134 | 0x910E | 2 | Maximum Q- | var / 1000 | U32
37136 | 0x9110 | 2 | Maximum S | VA / 1000 | U32
37138 | 0x9112 | 1 | Maximum cos(phi)+ | - / 1000 | U16
37139 | 0x9113 | 1 | Maximum cos(phi)- | - / 1000 | U16

# Settings

## Set Tariff

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38656 | 0x9700 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38656 | 0x9700 | 1 | Set Tariff (1 to 4) | - | U8

# Actions

## Partial reset

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40512 | 0x9E40 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40512 | 0x9E40 | 1 | Reset Partial (mix values is possible): 0x0001 : Tariff 1 positive active energy (Ea+) 0x0002 : Tariff 2 positive active energy (Ea+) 0x0004 : Tariff 3 positive active energy (Ea+) 0x0008 : Tariff 4 positive active energy (Ea+) 0x0010 : Negative active energy (Ea-) 0x0020 : Positive reactive energy (Er+) 0x0040 : Negative reactive energy (Er-) 0x000F : All partial energies per tariff 0xFFFF : All partial energies | - | U16_HEX

## Maximum reset

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40513 | 0x9E41 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40513 | 0x9E41 | 1 | Reset Max (mix values is possible): 0x0001 : Max of phase 1 current (I1) 0x0002 : Max of phase 2 current (I2) 0x0004 : Max of phase 3 current (I3) 0x0008 : Max of phase N current (IN) 0x0010 : Max of positive active power (P+) 0x0020 : Max of negative active power (P-) 0x0040 : Max of positive reactive power (Q+) 0x0080 : Max of positive reactive power (Q-) 0x0100 : Max of apparent power (S) 0x0200 : Max of positive cos(phi) 0x0400 : Max of negative cos(phi) 0xFFFF : All max | - | U16_HEX

# Monitoring

# Quality

## Quality Values

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
38400 | 0x9600 | Info | 22 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
38400 | 0x9600 | 2 | THD Value for I1 | % / 100 | U32
38402 | 0x9602 | 2 | THD Value for I2 | % / 100 | U32
38404 | 0x9604 | 2 | THD Value for I3 | % / 100 | U32
38406 | 0x9606 | 2 | THD Value for V1 | % / 100 | U32
38408 | 0x9608 | 2 | THD Value for V2 | % / 100 | U32
38410 | 0x960A | 2 | THD Value for V3 | % / 100 | U32
38412 | 0x960C | 2 | THD Value for U12 | % / 100 | U32
38414 | 0x960E | 2 | THD Value for U23 | % / 100 | U32
38416 | 0x9610 | 2 | THD Value for U31 | % / 100 | U32
38418 | 0x9612 | 1 | cos(phi) L1 | - / 1000 | S16
38419 | 0x9613 | 1 | cos(phi) L2 | - / 1000 | S16
38420 | 0x9614 | 1 | cos(phi) L3 | - / 1000 | S16
38421 | 0x9615 | 1 | cos(phi) Total | - / 1000 | S16

# Load Curve

## Load curve P+

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61440 | 0xF000 | Command | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61440 | 0xF000 | 1 | Action 0x0001 : Reset read pointer 0xFFFE : Get next data | - | U16_HEX

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61456 | 0xF010 | Header | 6 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61456 | 0xF010 | 1 | Record count ( Maximum 29 ) | - | U8
61457 | 0xF011 | 1 | Record size : 4 see below the data record description | W | U8
61458 | 0xF012 | 1 | Integration period | min | U16
61459 | 0xF013 | 1 | Physical Unit : 0 0 : W 1 : W 2 : var 3 : var 4 : VA 5 : None 6 : J 7 : Pulse 8 : m3 9 : Nm3 20 : kW 22 : kVAr 24 : kVA 26 : kJ 27 : kilo-Pulse | - | U8
61460 | 0xF014 | 1 | Numerator Rate | - | U16
61461 | 0xF015 | 1 | Denominator Rate | - | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61462 | 0xF016 | Data | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61462 | 0xF016 | 2 | Date | s | DATETIME
61464 | 0xF018 | 1 | Full/incomplete period 0 : full integration period 1 : incomplete integration period | - | U8
61465 | 0xF019 | 1 | Value without CT*VT rate | - | U16

# Industrialization

## Indus Mode and MID status

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40544 | 0x9E60 | Info | 2 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40544 | 0x9E60 | 1 | Indus Mode (0: indus mode disabled, 1: indus mode enabled) | - | U8
40545 | 0x9E61 | 1 | MID status (0: non-MID product, 1: MID product | - | U8