--X33F-LB08-0PZ4-609140a6 Content-Disposition: form-data; name=""; filename="COUNTIS-E48-ETHERNET_COMMUNICATION-TABLE_2019-07_CMT_201-146_EN.html" Content-Type: application/octet-stream ﻿

# Identification

## Product

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50000 | 0xC350 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50000 | 0xC350 | 4 | "SOCO" | - | STRING_16
50004 | 0xC354 | 1 | Product order ID (Countis:100, Protection:200, Atys:300, Diris:400) | - | U16
50005 | 0xC355 | 1 | Product ID (EX: 1000 ATS3) | - | U16
50006 | 0xC356 | 1 | JBUS Table Version (EX: 101 Version 1.01) | - | U16
50007 | 0xC357 | 1 | Product software version (EX: 100 Version 1.00) | - | U16
50008 | 0xC358 | 1 | Serial_AA_SS | - | U16_HEX
50009 | 0xC359 | 1 | Serial_SST_L | - | U16_HEX
50010 | 0xC35A | 1 | Serial_order | - | U16
50011 | 0xC35B | 2 | Serial_Reserve | - | U32
50013 | 0xC35D | 4 | See "Code table" tab for more details | - | U64_HEX
50017 | 0xC361 | 1 | Customization data loaded (True/False) | - | U8
50018 | 0xC362 | 1 | Product version (Major) | - | U16
50019 | 0xC363 | 1 | Product version (Minor) | - | U16
50020 | 0xC364 | 1 | Product version (Revision) | - | U16
50021 | 0xC365 | 1 | Product version (Build) | - | U16
50022 | 0xC366 | 3 | Product build date | - | DATETIME_3
50025 | 0xC369 | 1 | Software technical base version (Major) | - | U16
50026 | 0xC36A | 1 | Software technical base version (Minor) | - | U16
50027 | 0xC36B | 1 | Software technical base version (Revision) | - | U16
50028 | 0xC36C | 1 | COM board software major verion | - | U16
50029 | 0xC36D | 1 | Customization version (Minor) | - | U16
50030 | 0xC36E | 4 | Product VLO (EX : "880100") | - | STRING_NORM
50034 | 0xC372 | 4 | Customization VLO (EX : "880700") | - | STRING_NORM
50038 | 0xC376 | 4 | Software technical base VLO (EX : "880600") | - | STRING_NORM
50042 | 0xC37A | 8 | Vendor name (EX : "SOCOMEC") | - | STRING_NORM
50050 | 0xC382 | 8 | Product name (EX : "DIRIS A40R") | - | STRING_NORM
50058 | 0xC38A | 8 | Extended name | - | STRING_NORM

# Visualization

# Measurement

## Metrology Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50512 | 0xC550 | Info | 62 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50512 | 0xC550 | 2 | Reserved | - | -
50514 | 0xC552 | 2 | Phase to Phase Voltage: U12 | V 10⁻² | U32
50516 | 0xC554 | 2 | Phase to Phase Voltage: U23 | V 10⁻² | U32
50518 | 0xC556 | 2 | Phase to Phase Voltage: U31 | V 10⁻² | U32
50520 | 0xC558 | 2 | Simple voltage : V1 | V 10⁻² | U32
50522 | 0xC55A | 2 | Simple voltage : V2 | V 10⁻² | U32
50524 | 0xC55C | 2 | Simple voltage : V3 | V 10⁻² | U32
50526 | 0xC55E | 2 | Frequency : F | Hz 10⁻² | U32
50528 | 0xC560 | 2 | Current : I1 | mA | U32
50530 | 0xC562 | 2 | Current : I2 | mA | U32
50532 | 0xC564 | 2 | Current : I3 | mA | U32
50534 | 0xC566 | 2 | Neutral Current : In | mA | U32
50536 | 0xC568 | 2 | ? Active Power +/- : P | W 10 | S32
50538 | 0xC56A | 2 | ? Reactive Power +/- : Q | var 10 | S32
50540 | 0xC56C | 2 | ? Apparent Power : S | VA 10 | U32
50542 | 0xC56E | 2 | ? Power Factor : -: leading et + : lagging : PF | - / 1000 | S32
50544 | 0xC570 | 2 | Active Power phase 1 +/- : P1 | W 10 | S32
50546 | 0xC572 | 2 | Active Power phase 2 +/- : P2 | W 10 | S32
50548 | 0xC574 | 2 | Active Power phase 3 +/- : P3 | W 10 | S32
50550 | 0xC576 | 2 | Reactive Power phase 1 +/- : Q1 | var 10 | S32
50552 | 0xC578 | 2 | Reactive Power phase 2 +/- : Q2 | var 10 | S32
50554 | 0xC57A | 2 | Reactive Power phase 3 +/- : Q3 | var 10 | S32
50556 | 0xC57C | 2 | Apparent Power phase 1 : S1 | VA 10 | U32
50558 | 0xC57E | 2 | Apparent Power phase 2 : S2 | VA 10 | U32
50560 | 0xC580 | 2 | Apparent Power phase 3 : S3 | VA 10 | U32
50562 | 0xC582 | 2 | Power Factor phase 1 -: leading and + : lagging : PF1 | - / 1000 | S32
50564 | 0xC584 | 2 | Power Factor phase 2 -: leading and + : lagging : PF2 | - / 1000 | S32
50566 | 0xC586 | 2 | Power Factor phase 3 -: leading and + : lagging : PF3 | - / 1000 | S32
50568 | 0xC588 | 2 | System value I Sys : ( I1+I2+I3) / 3 | mA | U32
50570 | 0xC58A | 2 | System value U Sys : (U12 + U23 + U31 ) / 3 | V 10⁻² | U32
50572 | 0xC58C | 2 | System value V Sys : (V1 + V2 + V3 ) / 3 | V 10⁻² | U32

## Metrology No Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51280 | 0xC850 | Info | 36 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51280 | 0xC850 | 1 | Reserved | - | -
51281 | 0xC851 | 1 | Phase to Phase Voltage: U12 | V 10⁻² | U16
51282 | 0xC852 | 1 | Phase to Phase Voltage: U23 | V 10⁻² | U16
51283 | 0xC853 | 1 | Phase to Phase Voltage: U31 | V 10⁻² | U16
51284 | 0xC854 | 1 | Simple voltage : V1 | V 10⁻² | U16
51285 | 0xC855 | 1 | Simple voltage : V2 | V 10⁻² | U16
51286 | 0xC856 | 1 | Simple voltage : V3 | V 10⁻² | U16
51287 | 0xC857 | 1 | Frequency : F | Hz 10⁻² | U16
51288 | 0xC858 | 1 | Reserved | - | -
51289 | 0xC859 | 1 | Reserved | - | -
51290 | 0xC85A | 1 | Reserved | - | -
51291 | 0xC85B | 1 | Reserved | - | -
51292 | 0xC85C | 1 | ? active Power +/- : P | W 10 | S16
51293 | 0xC85D | 1 | ? reactive Power +/- : Q | var 10 | S16
51294 | 0xC85E | 1 | ? apparent power : S | VA 10 | U16
51295 | 0xC85F | 1 | ? power factor : -: leading and + : lagging : PF | - / 1000 | S16
51296 | 0xC860 | 1 | Active Power phase 1 +/- : P1 | W 10 | S16
51297 | 0xC861 | 1 | Active Power phase 2 +/- : P2 | W 10 | S16
51298 | 0xC862 | 1 | Active Power phase 3 +/- : P3 | W 10 | S16
51299 | 0xC863 | 1 | Reactive Power phase 1 +/- : Q1 | var 10 | S16
51300 | 0xC864 | 1 | Reactive Power phase 2 +/- : Q2 | var 10 | S16
51301 | 0xC865 | 1 | Reactive Power phase 3 +/- : Q3 | var 10 | S16
51302 | 0xC866 | 1 | Apparent power phase 1 : S1 | VA 10 | U16
51303 | 0xC867 | 1 | Apparent power phase 2 : S2 | VA 10 | U16
51304 | 0xC868 | 1 | Apparent power phase 3 : S3 | VA 10 | U16
51305 | 0xC869 | 1 | Power Factor phase 1 -: leading and + : lagging : PF1 | - / 1000 | S16
51306 | 0xC86A | 1 | Power Factor phase 2 -: leading and + : lagging : PF2 | - / 1000 | S16
51307 | 0xC86B | 1 | Power Factor phase 3 -: leading and + : lagging : PF3 | - / 1000 | S16
51308 | 0xC86C | 1 | System value I Sys : ( I1+I2+I3) / 3 | mA | U16
51309 | 0xC86D | 1 | System value U Sys : (U12 + U23 + U31 ) / 3 | V 10⁻² | U16
51310 | 0xC86E | 1 | System value V Sys : (V1 + V2 + V3 ) / 3 | V 10⁻² | U16
51311 | 0xC86F | 1 | Total Positive Active Energy (no resetable) : Ea+ | Wh / 1E-06 | U16
51312 | 0xC870 | 1 | Total Positive Reactive Energy (no resetable) : Er + | varh / 1E-06 | U16
51313 | 0xC871 | 1 | Total Negative Active Energy (no resetable) : Ea- | Wh / 1E-06 | U16
51314 | 0xC872 | 1 | Total Negative Reactive Energy (no resetable) : Er - | varh / 1E-06 | U16
51315 | 0xC873 | 1 | Reserved | - | -

## Energies

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50768 | 0xC650 | Info | 65 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50768 | 0xC650 | 2 | Reserved | - | -
50770 | 0xC652 | 2 | Total Positive Active Energy (no resetable) : Ea+ | kWh | U32
50772 | 0xC654 | 2 | Total Positive Reactive Energy (no resetable) : Er + | varh 10³ | U32
50774 | 0xC656 | 2 | Total Apparent Energy (no resetable) : Eap | kVAh | U32
50776 | 0xC658 | 2 | Total Negative Active Energy (no resetable) : Ea- | kWh | U32
50778 | 0xC65A | 2 | Total Negative Reactive Energy (no resetable) : Er - | varh 10³ | U32
50780 | 0xC65C | 2 | Partial Positive Active Energy: Ea+ | kWh | U32
50782 | 0xC65E | 2 | Partial Positive Reactive Energy: Er + | varh 10³ | U32
50784 | 0xC660 | 2 | Partial Apparent Energy : Eap | kVAh | U32
50786 | 0xC662 | 2 | Partial Negative Active Energy : Ea- | kWh | U32
50788 | 0xC664 | 2 | Partial Negative Reactive Energy : Er - | varh 10³ | U32
50790 | 0xC666 | 2 | Reserved | - | -
50792 | 0xC668 | 2 | Reserved | - | -
50794 | 0xC66A | 2 | Reserved | - | -
50796 | 0xC66C | 2 | Reserved | - | -
50798 | 0xC66E | 2 | Reserved | - | -
50800 | 0xC670 | 2 | Reserved | - | -
50802 | 0xC672 | 2 | Reserved | - | -
50804 | 0xC674 | 2 | Reserved | - | -
50806 | 0xC676 | 2 | Reserved | - | -
50808 | 0xC678 | 2 | Reserved | - | -
50810 | 0xC67A | 2 | Reserved | - | -
50812 | 0xC67C | 2 | Reserved | - | -
50814 | 0xC67E | 2 | Reserved | - | -
50816 | 0xC680 | 2 | Reserved | - | -
50818 | 0xC682 | 2 | Reserved | - | -
50820 | 0xC684 | 2 | Reserved | - | -
50822 | 0xC686 | 2 | Reserved | - | -
50824 | 0xC688 | 2 | Reserved | - | -
50826 | 0xC68A | 2 | Last date for Record average P/Q/S in second since 01/01/2000 | - | DATETIME
50828 | 0xC68C | 1 | Last average (P+) | W | U16
50829 | 0xC68D | 1 | Reserved | - | -
50830 | 0xC68E | 1 | Reserved | - | -
50831 | 0xC68F | 1 | Reserved | - | -
50832 | 0xC690 | 1 | Reserved | - | -

## Energies in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50944 | 0xC700 | Info | 65 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50944 | 0xC700 | 2 | Reserved | - | -
50946 | 0xC702 | 2 | Total Positive Active Energy (no resetable) : Ea+ | Wh 10 | U32
50948 | 0xC704 | 2 | Total Positive Reactive Energy (no resetable) : Er + | varh 10 | U32
50950 | 0xC706 | 2 | Total Apparent Energy (no resetable) : Eap | VAh 10 | U32
50952 | 0xC708 | 2 | Total Negative Active Energy (no resetable) : Ea- | Wh 10 | U32
50954 | 0xC70A | 2 | Total Negative Reactive Energy (no resetable) : Er - | varh 10 | U32
50956 | 0xC70C | 2 | Partial Positive Active Energy: Ea+ | Wh 10 | U32
50958 | 0xC70E | 2 | Partial Positive Reactive Energy: Er + | varh 10 | U32
50960 | 0xC710 | 2 | Partial Apparent Energy : Eap | VAh 10 | U32
50962 | 0xC712 | 2 | Partial Negative Active Energy : Ea- | Wh 10 | U32
50964 | 0xC714 | 2 | Partial Negative Reactive Energy : Er - | varh 10 | U32
50966 | 0xC716 | 2 | Reserved | - | -
50968 | 0xC718 | 2 | Reserved | - | -
50970 | 0xC71A | 2 | Reserved | - | -
50972 | 0xC71C | 2 | Reserved | - | -
50974 | 0xC71E | 2 | Reserved | - | -
50976 | 0xC720 | 2 | Reserved | - | -
50978 | 0xC722 | 2 | Reserved | - | -
50980 | 0xC724 | 2 | Reserved | - | -
50982 | 0xC726 | 2 | Reserved | - | -
50984 | 0xC728 | 2 | Reserved | - | -
50986 | 0xC72A | 2 | Reserved | - | -
50988 | 0xC72C | 2 | Reserved | - | -
50990 | 0xC72E | 2 | Reserved | - | -
50992 | 0xC730 | 2 | Reserved | - | -
50994 | 0xC732 | 2 | Reserved | - | -
50996 | 0xC734 | 2 | Reserved | - | -
50998 | 0xC736 | 2 | Reserved | - | -
51000 | 0xC738 | 2 | Reserved | - | -
51002 | 0xC73A | 2 | Last date for Record average P/Q/S in second since 01/01/2000 | - | U32
51004 | 0xC73C | 1 | Last average (P+) | W | U16
51005 | 0xC73D | 1 | Reserved | - | -
51006 | 0xC73E | 1 | Reserved | - | -
51007 | 0xC73F | 1 | Reserved | - | -
51008 | 0xC740 | 1 | Reserved | - | -

## Energies per tariff

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50848 | 0xC6A0 | Info | 50 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50848 | 0xC6A0 | 1 | 1 >= Tariff number <= 4 | - | U8
50849 | 0xC6A1 | 1 | Tariff number in progress ( 1 to 4 ) 1 : Tariff 1 2 : Tariff 2 3 : Tariff 3 4 : Tariff 4 | - | U8
50850 | 0xC6A2 | 2 | Positive Active Energies 1 | kWh | U32
50852 | 0xC6A4 | 2 | Positive Active Energies 2 | kWh | U32
50854 | 0xC6A6 | 2 | Positive Active Energies 3 | kWh | U32
50856 | 0xC6A8 | 2 | Positive Active Energies 4 | kWh | U32
50858 | 0xC6AA | 2 | Reserved | - | -
50860 | 0xC6AC | 2 | Reserved | - | -
50862 | 0xC6AE | 2 | Reserved | - | -
50864 | 0xC6B0 | 2 | Reserved | - | -
50866 | 0xC6B2 | 2 | Positive Reactive Enegies 1 | varh 10³ | U32
50868 | 0xC6B4 | 2 | Positive Reactive Enegies 2 | varh 10³ | U32
50870 | 0xC6B6 | 2 | Positive Reactive Enegies 3 | varh 10³ | U32
50872 | 0xC6B8 | 2 | Positive Reactive Enegies 4 | varh 10³ | U32
50874 | 0xC6BA | 2 | Reserved | - | -
50876 | 0xC6BC | 2 | Reserved | - | -
50878 | 0xC6BE | 2 | Reserved | - | -
50880 | 0xC6C0 | 2 | Reserved | - | -
50882 | 0xC6C2 | 2 | Time Counter 1 | h 10⁻² | U32
50884 | 0xC6C4 | 2 | Time Counter 2 | h 10⁻² | U32
50886 | 0xC6C6 | 2 | Time Counter 3 | h 10⁻² | U32
50888 | 0xC6C8 | 2 | Time Counter 4 | h 10⁻² | U32
50890 | 0xC6CA | 2 | Reserved | - | -
50892 | 0xC6CC | 2 | Reserved | - | -
50894 | 0xC6CE | 2 | Reserved | - | -
50896 | 0xC6D0 | 2 | Reserved | - | -

## Energies per tariff in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51200 | 0xC800 | Info | 50 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51200 | 0xC800 | 1 | 1 >= Tariff number <= 4 | - | U8
51201 | 0xC801 | 1 | Tariff number in progress ( 1 to 4 ) 1 : Tariff 1 2 : Tariff 2 3 : Tariff 3 4 : Tariff 4 | - | U8
51202 | 0xC802 | 2 | Positive Active Energies 1 | Wh 10 | U32
51204 | 0xC804 | 2 | Positive Active Energies 2 | Wh 10 | U32
51206 | 0xC806 | 2 | Positive Active Energies 3 | Wh 10 | U32
51208 | 0xC808 | 2 | Positive Active Energies 4 | Wh 10 | U32
51210 | 0xC80A | 2 | Reserved | - | -
51212 | 0xC80C | 2 | Reserved | - | -
51214 | 0xC80E | 2 | Reserved | - | -
51216 | 0xC810 | 2 | Reserved | - | -
51218 | 0xC812 | 2 | Positive Reactive Enegies 1 | varh 10 | U32
51220 | 0xC814 | 2 | Positive Reactive Enegies 2 | varh 10 | U32
51222 | 0xC816 | 2 | Positive Reactive Enegies 3 | varh 10 | U32
51224 | 0xC818 | 2 | Positive Reactive Enegies 4 | varh 10 | U32
51226 | 0xC81A | 2 | Reserved | - | -
51228 | 0xC81C | 2 | Reserved | - | -
51230 | 0xC81E | 2 | Reserved | - | -
51232 | 0xC820 | 2 | Reserved | - | -
51234 | 0xC822 | 2 | Time Counter 1 | h 10⁻² | U32
51236 | 0xC824 | 2 | Time Counter 2 | h 10⁻² | U32
51238 | 0xC826 | 2 | Time Counter 3 | h 10⁻² | U32
51240 | 0xC828 | 2 | Time Counter 4 | h 10⁻² | U32
51242 | 0xC82A | 2 | Reserved | - | -
51244 | 0xC82C | 2 | Reserved | - | -
51246 | 0xC82E | 2 | Reserved | - | -
51248 | 0xC830 | 2 | Reserved | - | -

## Energy measurement - Line #1

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
19840 | 0x4D80 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
19840 | 0x4D80 | 1 | Reserved | - | -
19841 | 0x4D81 | 2 | Reserved | - | -
19843 | 0x4D83 | 2 | Total Positive active Energy : Ea+ | kWh | U32
19845 | 0x4D85 | 1 | Total Residual positive active Energy : rEa+ | Wh 10⁻¹ | U16
19846 | 0x4D86 | 2 | Total Negative active Energy : Ea- | kWh | U32
19848 | 0x4D88 | 1 | Total Residual negative active Energy : rEa- | Wh 10⁻¹ | U16
19849 | 0x4D89 | 2 | Total Positive reactive Energy : Er+ | varh 10³ | U32
19851 | 0x4D8B | 1 | Total Residual positive reactive Energy : rEr+ | varh 10⁻¹ | U16
19852 | 0x4D8C | 2 | Total Negative reactive Energy : Er- | varh 10³ | U32
19854 | 0x4D8E | 1 | Total Residual negative reactive Energy : rEr- | varh 10⁻¹ | U16
19855 | 0x4D8F | 2 | Total Apparent Energy : Eap | kVAh | U32
19857 | 0x4D91 | 1 | Total Residual apparent Energy : rEap | VAh 10⁻¹ | U16
19858 | 0x4D92 | 2 | Total positive lagging reactive Energy : Er+ (lagging) | varh 10³ | U32
19860 | 0x4D94 | 1 | Total Residual positive lagging reactive Energy : rEr+ (lagging) | varh 10⁻¹ | U16
19861 | 0x4D95 | 2 | Total negative lagging reactive Energy : Er- (lagging) | varh 10³ | U32
19863 | 0x4D97 | 1 | Total Residual negative lagging reactive Energy : rEr- (lagging) | varh 10⁻¹ | U16
19864 | 0x4D98 | 2 | Total positive leading reactive Energy : Er+ (leading) | varh 10³ | U32
19866 | 0x4D9A | 1 | Total Residual positive leading reactive Energy : rEr+ (leading) | varh 10⁻¹ | U16
19867 | 0x4D9B | 2 | Total negative leading reactive Energy : Er- (leading) | varh 10³ | U32
19869 | 0x4D9D | 1 | Total Residual negative leading reactive Energy : rEr- (leading) | varh 10⁻¹ | U16
19870 | 0x4D9E | 2 | Reserved | - | -
19872 | 0x4DA0 | 2 | Reserved | - | -
19874 | 0x4DA2 | 1 | Reserved | - | -
19875 | 0x4DA3 | 2 | Reserved | - | -
19877 | 0x4DA5 | 1 | Reserved | - | -
19878 | 0x4DA6 | 2 | Reserved | - | -
19880 | 0x4DA8 | 1 | Reserved | - | -
19881 | 0x4DA9 | 2 | Reserved | - | -
19883 | 0x4DAB | 1 | Reserved | - | -
19884 | 0x4DAC | 2 | Reserved | - | -
19886 | 0x4DAE | 1 | Reserved | - | -
19887 | 0x4DAF | 2 | Reserved | - | -
19889 | 0x4DB1 | 2 | Reserved | - | -
19891 | 0x4DB3 | 2 | Reserved | - | -
19893 | 0x4DB5 | 1 | Reserved | - | -
19894 | 0x4DB6 | 2 | Reserved | - | -
19896 | 0x4DB8 | 1 | Reserved | - | -
19897 | 0x4DB9 | 2 | Reserved | - | -
19899 | 0x4DBB | 1 | Reserved | - | -
19900 | 0x4DBC | 2 | Reserved | - | -
19902 | 0x4DBE | 1 | Reserved | - | -
19903 | 0x4DBF | 2 | Reserved | - | -
19905 | 0x4DC1 | 1 | Reserved | - | -

## Energy measurement - Line #2

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
21888 | 0x5580 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
21888 | 0x5580 | 1 | Reserved | - | -
21889 | 0x5581 | 2 | Reserved | - | -
21891 | 0x5583 | 2 | Total Positive active Energy : Ea+ | kWh | U32
21893 | 0x5585 | 1 | Total Residual positive active Energy : rEa+ | Wh 10⁻¹ | U16
21894 | 0x5586 | 2 | Total Negative active Energy : Ea- | kWh | U32
21896 | 0x5588 | 1 | Total Residual negative active Energy : rEa- | Wh 10⁻¹ | U16
21897 | 0x5589 | 2 | Total Positive reactive Energy : Er+ | varh 10³ | U32
21899 | 0x558B | 1 | Total Residual positive reactive Energy : rEr+ | varh 10⁻¹ | U16
21900 | 0x558C | 2 | Total Negative reactive Energy : Er- | varh 10³ | U32
21902 | 0x558E | 1 | Total Residual negative reactive Energy : rEr- | varh 10⁻¹ | U16
21903 | 0x558F | 2 | Total Apparent Energy : Eap | kVAh | U32
21905 | 0x5591 | 1 | Total Residual apparent Energy : rEap | VAh 10⁻¹ | U16
21906 | 0x5592 | 2 | Total positive lagging reactive Energy : Er+ (lagging) | varh 10³ | U32
21908 | 0x5594 | 1 | Total Residual positive lagging reactive Energy : rEr+ (lagging) | varh 10⁻¹ | U16
21909 | 0x5595 | 2 | Total negative lagging reactive Energy : Er- (lagging) | varh 10³ | U32
21911 | 0x5597 | 1 | Total Residual negative lagging reactive Energy : rEr- (lagging) | varh 10⁻¹ | U16
21912 | 0x5598 | 2 | Total positive leading reactive Energy : Er+ (leading) | varh 10³ | U32
21914 | 0x559A | 1 | Total Residual positive leading reactive Energy : rEr+ (leading) | varh 10⁻¹ | U16
21915 | 0x559B | 2 | Total negative leading reactive Energy : Er- (leading) | varh 10³ | U32
21917 | 0x559D | 1 | Total Residual negative leading reactive Energy : rEr- (leading) | varh 10⁻¹ | U16
21918 | 0x559E | 2 | Reserved | - | -
21920 | 0x55A0 | 2 | Reserved | - | -
21922 | 0x55A2 | 1 | Reserved | - | -
21923 | 0x55A3 | 2 | Reserved | - | -
21925 | 0x55A5 | 1 | Reserved | - | -
21926 | 0x55A6 | 2 | Reserved | - | -
21928 | 0x55A8 | 1 | Reserved | - | -
21929 | 0x55A9 | 2 | Reserved | - | -
21931 | 0x55AB | 1 | Reserved | - | -
21932 | 0x55AC | 2 | Reserved | - | -
21934 | 0x55AE | 1 | Reserved | - | -
21935 | 0x55AF | 2 | Reserved | - | -
21937 | 0x55B1 | 2 | Reserved | - | -
21939 | 0x55B3 | 2 | Reserved | - | -
21941 | 0x55B5 | 1 | Reserved | - | -
21942 | 0x55B6 | 2 | Reserved | - | -
21944 | 0x55B8 | 1 | Reserved | - | -
21945 | 0x55B9 | 2 | Reserved | - | -
21947 | 0x55BB | 1 | Reserved | - | -
21948 | 0x55BC | 2 | Reserved | - | -
21950 | 0x55BE | 1 | Reserved | - | -
21951 | 0x55BF | 2 | Reserved | - | -
21953 | 0x55C1 | 1 | Reserved | - | -

## Energy measurement - Line #3

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
23936 | 0x5D80 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
23936 | 0x5D80 | 1 | Reserved | - | -
23937 | 0x5D81 | 2 | Reserved | - | -
23939 | 0x5D83 | 2 | Total Positive active Energy : Ea+ | kWh | U32
23941 | 0x5D85 | 1 | Total Residual positive active Energy : rEa+ | Wh 10⁻¹ | U16
23942 | 0x5D86 | 2 | Total Negative active Energy : Ea- | kWh | U32
23944 | 0x5D88 | 1 | Total Residual negative active Energy : rEa- | Wh 10⁻¹ | U16
23945 | 0x5D89 | 2 | Total Positive reactive Energy : Er+ | varh 10³ | U32
23947 | 0x5D8B | 1 | Total Residual positive reactive Energy : rEr+ | varh 10⁻¹ | U16
23948 | 0x5D8C | 2 | Total Negative reactive Energy : Er- | varh 10³ | U32
23950 | 0x5D8E | 1 | Total Residual negative reactive Energy : rEr- | varh 10⁻¹ | U16
23951 | 0x5D8F | 2 | Total Apparent Energy : Eap | kVAh | U32
23953 | 0x5D91 | 1 | Total Residual apparent Energy : rEap | VAh 10⁻¹ | U16
23954 | 0x5D92 | 2 | Total positive lagging reactive Energy : Er+ (lagging) | varh 10³ | U32
23956 | 0x5D94 | 1 | Total Residual positive lagging reactive Energy : rEr+ (lagging) | varh 10⁻¹ | U16
23957 | 0x5D95 | 2 | Total negative lagging reactive Energy : Er- (lagging) | varh 10³ | U32
23959 | 0x5D97 | 1 | Total Residual negative lagging reactive Energy : rEr- (lagging) | varh 10⁻¹ | U16
23960 | 0x5D98 | 2 | Total positive leading reactive Energy : Er+ (leading) | varh 10³ | U32
23962 | 0x5D9A | 1 | Total Residual positive leading reactive Energy : rEr+ (leading) | varh 10⁻¹ | U16
23963 | 0x5D9B | 2 | Total negative leading reactive Energy : Er- (leading) | varh 10³ | U32
23965 | 0x5D9D | 1 | Total Residual negative leading reactive Energy : rEr- (leading) | varh 10⁻¹ | U16
23966 | 0x5D9E | 2 | Reserved | - | -
23968 | 0x5DA0 | 2 | Reserved | - | -
23970 | 0x5DA2 | 1 | Reserved | - | -
23971 | 0x5DA3 | 2 | Reserved | - | -
23973 | 0x5DA5 | 1 | Reserved | - | -
23974 | 0x5DA6 | 2 | Reserved | - | -
23976 | 0x5DA8 | 1 | Reserved | - | -
23977 | 0x5DA9 | 2 | Reserved | - | -
23979 | 0x5DAB | 1 | Reserved | - | -
23980 | 0x5DAC | 2 | Reserved | - | -
23982 | 0x5DAE | 1 | Reserved | - | -
23983 | 0x5DAF | 2 | Reserved | - | -
23985 | 0x5DB1 | 2 | Reserved | - | -
23987 | 0x5DB3 | 2 | Reserved | - | -
23989 | 0x5DB5 | 1 | Reserved | - | -
23990 | 0x5DB6 | 2 | Reserved | - | -
23992 | 0x5DB8 | 1 | Reserved | - | -
23993 | 0x5DB9 | 2 | Reserved | - | -
23995 | 0x5DBB | 1 | Reserved | - | -
23996 | 0x5DBC | 2 | Reserved | - | -
23998 | 0x5DBE | 1 | Reserved | - | -
23999 | 0x5DBF | 2 | Reserved | - | -
24001 | 0x5DC1 | 1 | Reserved | - | -

## Energy measurement - Total

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
25984 | 0x6580 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
25984 | 0x6580 | 1 | Reserved | - | -
25985 | 0x6581 | 2 | Reserved | - | -
25987 | 0x6583 | 2 | Total Positive active Energy : Ea+ | kWh | U32
25989 | 0x6585 | 1 | Total Residual positive active Energy : rEa+ | Wh 10⁻¹ | U16
25990 | 0x6586 | 2 | Total Negative active Energy : Ea- | kWh | U32
25992 | 0x6588 | 1 | Total Residual negative active Energy : rEa- | Wh 10⁻¹ | U16
25993 | 0x6589 | 2 | Total Positive reactive Energy : Er+ | varh 10³ | U32
25995 | 0x658B | 1 | Total Residual positive reactive Energy : rEr+ | varh 10⁻¹ | U16
25996 | 0x658C | 2 | Total Negative reactive Energy : Er- | varh 10³ | U32
25998 | 0x658E | 1 | Total Residual negative reactive Energy : rEr- | varh 10⁻¹ | U16
25999 | 0x658F | 2 | Total Apparent Energy : Eap | kVAh | U32
26001 | 0x6591 | 1 | Total Residual apparent Energy : rEap | VAh 10⁻¹ | U16
26002 | 0x6592 | 2 | Total positive lagging reactive Energy : Er+ (lagging) | varh 10³ | U32
26004 | 0x6594 | 1 | Total Residual positive lagging reactive Energy : rEr+ (lagging) | varh 10⁻¹ | U16
26005 | 0x6595 | 2 | Total negative lagging reactive Energy : Er- (lagging) | varh 10³ | U32
26007 | 0x6597 | 1 | Total Residual negative lagging reactive Energy : rEr- (lagging) | varh 10⁻¹ | U16
26008 | 0x6598 | 2 | Total positive leading reactive Energy : Er+ (leading) | varh 10³ | U32
26010 | 0x659A | 1 | Total Residual positive leading reactive Energy : rEr+ (leading) | varh 10⁻¹ | U16
26011 | 0x659B | 2 | Total negative leading reactive Energy : Er- (leading) | varh 10³ | U32
26013 | 0x659D | 1 | Total Residual negative leading reactive Energy : rEr- (leading) | varh 10⁻¹ | U16
26014 | 0x659E | 2 | Reserved | - | -
26016 | 0x65A0 | 2 | Reserved | - | -
26018 | 0x65A2 | 1 | Reserved | - | -
26019 | 0x65A3 | 2 | Reserved | - | -
26021 | 0x65A5 | 1 | Reserved | - | -
26022 | 0x65A6 | 2 | Reserved | - | -
26024 | 0x65A8 | 1 | Reserved | - | -
26025 | 0x65A9 | 2 | Reserved | - | -
26027 | 0x65AB | 1 | Reserved | - | -
26028 | 0x65AC | 2 | Reserved | - | -
26030 | 0x65AE | 1 | Reserved | - | -
26031 | 0x65AF | 2 | Reserved | - | -
26033 | 0x65B1 | 2 | Reserved | - | -
26035 | 0x65B3 | 2 | Reserved | - | -
26037 | 0x65B5 | 1 | Reserved | - | -
26038 | 0x65B6 | 2 | Reserved | - | -
26040 | 0x65B8 | 1 | Reserved | - | -
26041 | 0x65B9 | 2 | Reserved | - | -
26043 | 0x65BB | 1 | Reserved | - | -
26044 | 0x65BC | 2 | Reserved | - | -
26046 | 0x65BE | 1 | Reserved | - | -
26047 | 0x65BF | 2 | Reserved | - | -
26049 | 0x65C1 | 1 | Reserved | - | -

## Tariff meter (total) - Line #1 (EA)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20224 | 0x4F00 | Info | 33 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20224 | 0x4F00 | 1 | Tariff number in progress ( 1 to 4 ) 1 : Tariff 1 2 : Tariff 2 3 : Tariff 3 4 : Tariff 4 | - | U16
20225 | 0x4F01 | 2 | T1 - Ea+ | kWh | U32
20227 | 0x4F03 | 2 | T2 - Ea+ | kWh | U32
20229 | 0x4F05 | 2 | T3 - Ea+ | kWh | U32
20231 | 0x4F07 | 2 | T4 - Ea+ | kWh | U32
20233 | 0x4F09 | 2 | Reserved | - | -
20235 | 0x4F0B | 2 | Reserved | - | -
20237 | 0x4F0D | 2 | Reserved | - | -
20239 | 0x4F0F | 2 | Reserved | - | -
20241 | 0x4F11 | 2 | T1 - Ea- | kWh | U32
20243 | 0x4F13 | 2 | T2 - Ea- | kWh | U32
20245 | 0x4F15 | 2 | T3 - Ea- | kWh | U32
20247 | 0x4F17 | 2 | T4 - Ea- | kWh | U32
20249 | 0x4F19 | 2 | Reserved | - | -
20251 | 0x4F1B | 2 | Reserved | - | -
20253 | 0x4F1D | 2 | Reserved | - | -
20255 | 0x4F1F | 2 | Reserved | - | -

## Tariff meter (total) - Line #1 (ER)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20257 | 0x4F21 | Info | 96 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20257 | 0x4F21 | 2 | T1 - Er+ | varh 10³ | U32
20259 | 0x4F23 | 2 | T2 - Er+ | varh 10³ | U32
20261 | 0x4F25 | 2 | T3 - Er+ | varh 10³ | U32
20263 | 0x4F27 | 2 | T4 - Er+ | varh 10³ | U32
20265 | 0x4F29 | 2 | Reserved | - | -
20267 | 0x4F2B | 2 | Reserved | - | -
20269 | 0x4F2D | 2 | Reserved | - | -
20271 | 0x4F2F | 2 | Reserved | - | -
20273 | 0x4F31 | 2 | T1 - Er+ (lagging) | varh 10³ | U32
20275 | 0x4F33 | 2 | T2 - Er+ (lagging) | varh 10³ | U32
20277 | 0x4F35 | 2 | T3 - Er+ (lagging) | varh 10³ | U32
20279 | 0x4F37 | 2 | T4 - Er+ (lagging) | varh 10³ | U32
20281 | 0x4F39 | 2 | Reserved | - | -
20283 | 0x4F3B | 2 | Reserved | - | -
20285 | 0x4F3D | 2 | Reserved | - | -
20287 | 0x4F3F | 2 | Reserved | - | -
20289 | 0x4F41 | 2 | T1 - Er+ (leading) | varh 10³ | U32
20291 | 0x4F43 | 2 | T2 - Er+ (leading) | varh 10³ | U32
20293 | 0x4F45 | 2 | T3 - Er+ (leading) | varh 10³ | U32
20295 | 0x4F47 | 2 | T4 - Er+ (leading) | varh 10³ | U32
20297 | 0x4F49 | 2 | Reserved | - | -
20299 | 0x4F4B | 2 | Reserved | - | -
20301 | 0x4F4D | 2 | Reserved | - | -
20303 | 0x4F4F | 2 | Reserved | - | -
20305 | 0x4F51 | 2 | T1 - Er- | varh 10³ | U32
20307 | 0x4F53 | 2 | T2 - Er- | varh 10³ | U32
20309 | 0x4F55 | 2 | T3 - Er- | varh 10³ | U32
20311 | 0x4F57 | 2 | T4 - Er- | varh 10³ | U32
20313 | 0x4F59 | 2 | Reserved | - | -
20315 | 0x4F5B | 2 | Reserved | - | -
20317 | 0x4F5D | 2 | Reserved | - | -
20319 | 0x4F5F | 2 | Reserved | - | -
20321 | 0x4F61 | 2 | T1 - Er- (lagging) | varh 10³ | U32
20323 | 0x4F63 | 2 | T2 - Er- (lagging) | varh 10³ | U32
20325 | 0x4F65 | 2 | T3 - Er- (lagging) | varh 10³ | U32
20327 | 0x4F67 | 2 | T4 - Er- (lagging) | varh 10³ | U32
20329 | 0x4F69 | 2 | Reserved | - | -
20331 | 0x4F6B | 2 | Reserved | - | -
20333 | 0x4F6D | 2 | Reserved | - | -
20335 | 0x4F6F | 2 | Reserved | - | -
20337 | 0x4F71 | 2 | T1 - Er- (leading) | varh 10³ | U32
20339 | 0x4F73 | 2 | T2 - Er- (leading) | varh 10³ | U32
20341 | 0x4F75 | 2 | T3 - Er- (leading) | varh 10³ | U32
20343 | 0x4F77 | 2 | T4 - Er- (leading) | varh 10³ | U32
20345 | 0x4F79 | 2 | Reserved | - | -
20347 | 0x4F7B | 2 | Reserved | - | -
20349 | 0x4F7D | 2 | Reserved | - | -
20351 | 0x4F7F | 2 | Reserved | - | -

## Tariff meter (total) - Line #1 (ES)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
20353 | 0x4F81 | Info | 16 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
20353 | 0x4F81 | 2 | T1 - Eap | kVAh | U32
20355 | 0x4F83 | 2 | T2 - Eap | kVAh | U32
20357 | 0x4F85 | 2 | T3 - Eap | kVAh | U32
20359 | 0x4F87 | 2 | T4 - Eap | kVAh | U32
20361 | 0x4F89 | 2 | Reserved | - | -
20363 | 0x4F8B | 2 | Reserved | - | -
20365 | 0x4F8D | 2 | Reserved | - | -
20367 | 0x4F8F | 2 | Reserved | - | -

## Tariff meter (total) - Line #2 (EA)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22272 | 0x5700 | Info | 33 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22272 | 0x5700 | 1 | Tariff number in progress ( 1 to 4 ) 1 : Tariff 1 2 : Tariff 2 3 : Tariff 3 4 : Tariff 4 | - | U16
22273 | 0x5701 | 2 | T1 - Ea+ | kWh | U32
22275 | 0x5703 | 2 | T2 - Ea+ | kWh | U32
22277 | 0x5705 | 2 | T3 - Ea+ | kWh | U32
22279 | 0x5707 | 2 | T4 - Ea+ | kWh | U32
22281 | 0x5709 | 2 | Reserved | - | -
22283 | 0x570B | 2 | Reserved | - | -
22285 | 0x570D | 2 | Reserved | - | -
22287 | 0x570F | 2 | Reserved | - | -
22289 | 0x5711 | 2 | T1 - Ea- | kWh | U32
22291 | 0x5713 | 2 | T2 - Ea- | kWh | U32
22293 | 0x5715 | 2 | T3 - Ea- | kWh | U32
22295 | 0x5717 | 2 | T4 - Ea- | kWh | U32
22297 | 0x5719 | 2 | Reserved | - | -
22299 | 0x571B | 2 | Reserved | - | -
22301 | 0x571D | 2 | Reserved | - | -
22303 | 0x571F | 2 | Reserved | - | -

## Tariff meter (total) - Line #2 (ER)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22305 | 0x5721 | Info | 96 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22305 | 0x5721 | 2 | T1 - Er+ | varh 10³ | U32
22307 | 0x5723 | 2 | T2 - Er+ | varh 10³ | U32
22309 | 0x5725 | 2 | T3 - Er+ | varh 10³ | U32
22311 | 0x5727 | 2 | T4 - Er+ | varh 10³ | U32
22313 | 0x5729 | 2 | Reserved | - | -
22315 | 0x572B | 2 | Reserved | - | -
22317 | 0x572D | 2 | Reserved | - | -
22319 | 0x572F | 2 | Reserved | - | -
22321 | 0x5731 | 2 | T1 - Er+ (lagging) | varh 10³ | U32
22323 | 0x5733 | 2 | T2 - Er+ (lagging) | varh 10³ | U32
22325 | 0x5735 | 2 | T3 - Er+ (lagging) | varh 10³ | U32
22327 | 0x5737 | 2 | T4 - Er+ (lagging) | varh 10³ | U32
22329 | 0x5739 | 2 | Reserved | - | -
22331 | 0x573B | 2 | Reserved | - | -
22333 | 0x573D | 2 | Reserved | - | -
22335 | 0x573F | 2 | Reserved | - | -
22337 | 0x5741 | 2 | T1 - Er+ (leading) | varh 10³ | U32
22339 | 0x5743 | 2 | T2 - Er+ (leading) | varh 10³ | U32
22341 | 0x5745 | 2 | T3 - Er+ (leading) | varh 10³ | U32
22343 | 0x5747 | 2 | T4 - Er+ (leading) | varh 10³ | U32
22345 | 0x5749 | 2 | Reserved | - | -
22347 | 0x574B | 2 | Reserved | - | -
22349 | 0x574D | 2 | Reserved | - | -
22351 | 0x574F | 2 | Reserved | - | -
22353 | 0x5751 | 2 | T1 - Er- | varh 10³ | U32
22355 | 0x5753 | 2 | T2 - Er- | varh 10³ | U32
22357 | 0x5755 | 2 | T3 - Er- | varh 10³ | U32
22359 | 0x5757 | 2 | T4 - Er- | varh 10³ | U32
22361 | 0x5759 | 2 | Reserved | - | -
22363 | 0x575B | 2 | Reserved | - | -
22365 | 0x575D | 2 | Reserved | - | -
22367 | 0x575F | 2 | Reserved | - | -
22369 | 0x5761 | 2 | T1 - Er- (lagging) | varh 10³ | U32
22371 | 0x5763 | 2 | T2 - Er- (lagging) | varh 10³ | U32
22373 | 0x5765 | 2 | T3 - Er- (lagging) | varh 10³ | U32
22375 | 0x5767 | 2 | T4 - Er- (lagging) | varh 10³ | U32
22377 | 0x5769 | 2 | Reserved | - | -
22379 | 0x576B | 2 | Reserved | - | -
22381 | 0x576D | 2 | Reserved | - | -
22383 | 0x576F | 2 | Reserved | - | -
22385 | 0x5771 | 2 | T1 - Er- (leading) | varh 10³ | U32
22387 | 0x5773 | 2 | T2 - Er- (leading) | varh 10³ | U32
22389 | 0x5775 | 2 | T3 - Er- (leading) | varh 10³ | U32
22391 | 0x5777 | 2 | T4 - Er- (leading) | varh 10³ | U32
22393 | 0x5779 | 2 | Reserved | - | -
22395 | 0x577B | 2 | Reserved | - | -
22397 | 0x577D | 2 | Reserved | - | -
22399 | 0x577F | 2 | Reserved | - | -

## Tariff meter (total) - Line #2_(ES)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
22401 | 0x5781 | Info | 16 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
22401 | 0x5781 | 2 | T1 - Eap | kVAh | U32
22403 | 0x5783 | 2 | T2 - Eap | kVAh | U32
22405 | 0x5785 | 2 | T3 - Eap | kVAh | U32
22407 | 0x5787 | 2 | T4 - Eap | kVAh | U32
22409 | 0x5789 | 2 | Reserved | - | -
22411 | 0x578B | 2 | Reserved | - | -
22413 | 0x578D | 2 | Reserved | - | -
22415 | 0x578F | 2 | Reserved | - | -

## Tariff meter (total) - Line #3 (EA)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24320 | 0x5F00 | Info | 33 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24320 | 0x5F00 | 1 | Tariff number in progress ( 1 to 4 ) 1 : Tariff 1 2 : Tariff 2 3 : Tariff 3 4 : Tariff 4 | - | U16
24321 | 0x5F01 | 2 | T1 - Ea+ | kWh | U32
24323 | 0x5F03 | 2 | T2 - Ea+ | kWh | U32
24325 | 0x5F05 | 2 | T3 - Ea+ | kWh | U32
24327 | 0x5F07 | 2 | T4 - Ea+ | kWh | U32
24329 | 0x5F09 | 2 | Reserved | - | -
24331 | 0x5F0B | 2 | Reserved | - | -
24333 | 0x5F0D | 2 | Reserved | - | -
24335 | 0x5F0F | 2 | Reserved | - | -
24337 | 0x5F11 | 2 | T1 - Ea- | kWh | U32
24339 | 0x5F13 | 2 | T2 - Ea- | kWh | U32
24341 | 0x5F15 | 2 | T3 - Ea- | kWh | U32
24343 | 0x5F17 | 2 | T4 - Ea- | kWh | U32
24345 | 0x5F19 | 2 | Reserved | - | -
24347 | 0x5F1B | 2 | Reserved | - | -
24349 | 0x5F1D | 2 | Reserved | - | -
24351 | 0x5F1F | 2 | Reserved | - | -

## Tariff meter (total) - Line #3 (ER)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24353 | 0x5F21 | Info | 96 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24353 | 0x5F21 | 2 | T1 - Er+ | varh 10³ | U32
24355 | 0x5F23 | 2 | T2 - Er+ | varh 10³ | U32
24357 | 0x5F25 | 2 | T3 - Er+ | varh 10³ | U32
24359 | 0x5F27 | 2 | T4 - Er+ | varh 10³ | U32
24361 | 0x5F29 | 2 | Reserved | - | -
24363 | 0x5F2B | 2 | Reserved | - | -
24365 | 0x5F2D | 2 | Reserved | - | -
24367 | 0x5F2F | 2 | Reserved | - | -
24369 | 0x5F31 | 2 | T1 - Er+ (lagging) | varh 10³ | U32
24371 | 0x5F33 | 2 | T2 - Er+ (lagging) | varh 10³ | U32
24373 | 0x5F35 | 2 | T3 - Er+ (lagging) | varh 10³ | U32
24375 | 0x5F37 | 2 | T4 - Er+ (lagging) | varh 10³ | U32
24377 | 0x5F39 | 2 | Reserved | - | -
24379 | 0x5F3B | 2 | Reserved | - | -
24381 | 0x5F3D | 2 | Reserved | - | -
24383 | 0x5F3F | 2 | Reserved | - | -
24385 | 0x5F41 | 2 | T1 - Er+ (leading) | varh 10³ | U32
24387 | 0x5F43 | 2 | T2 - Er+ (leading) | varh 10³ | U32
24389 | 0x5F45 | 2 | T3 - Er+ (leading) | varh 10³ | U32
24391 | 0x5F47 | 2 | T4 - Er+ (leading) | varh 10³ | U32
24393 | 0x5F49 | 2 | Reserved | - | -
24395 | 0x5F4B | 2 | Reserved | - | -
24397 | 0x5F4D | 2 | Reserved | - | -
24399 | 0x5F4F | 2 | Reserved | - | -
24401 | 0x5F51 | 2 | T1 - Er- | varh 10³ | U32
24403 | 0x5F53 | 2 | T2 - Er- | varh 10³ | U32
24405 | 0x5F55 | 2 | T3 - Er- | varh 10³ | U32
24407 | 0x5F57 | 2 | T4 - Er- | varh 10³ | U32
24409 | 0x5F59 | 2 | Reserved | - | -
24411 | 0x5F5B | 2 | Reserved | - | -
24413 | 0x5F5D | 2 | Reserved | - | -
24415 | 0x5F5F | 2 | Reserved | - | -
24417 | 0x5F61 | 2 | T1 - Er- (lagging) | varh 10³ | U32
24419 | 0x5F63 | 2 | T2 - Er- (lagging) | varh 10³ | U32
24421 | 0x5F65 | 2 | T3 - Er- (lagging) | varh 10³ | U32
24423 | 0x5F67 | 2 | T4 - Er- (lagging) | varh 10³ | U32
24425 | 0x5F69 | 2 | Reserved | - | -
24427 | 0x5F6B | 2 | Reserved | - | -
24429 | 0x5F6D | 2 | Reserved | - | -
24431 | 0x5F6F | 2 | Reserved | - | -
24433 | 0x5F71 | 2 | T1 - Er- (leading) | varh 10³ | U32
24435 | 0x5F73 | 2 | T2 - Er- (leading) | varh 10³ | U32
24437 | 0x5F75 | 2 | T3 - Er- (leading) | varh 10³ | U32
24439 | 0x5F77 | 2 | T4 - Er- (leading) | varh 10³ | U32
24441 | 0x5F79 | 2 | Reserved | - | -
24443 | 0x5F7B | 2 | Reserved | - | -
24445 | 0x5F7D | 2 | Reserved | - | -
24447 | 0x5F7F | 2 | Reserved | - | -

## Tariff meter (total) - Line #3 (ES)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
24449 | 0x5F81 | Info | 16 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
24449 | 0x5F81 | 2 | T1 - Eap | kVAh | U32
24451 | 0x5F83 | 2 | T2 - Eap | kVAh | U32
24453 | 0x5F85 | 2 | T3 - Eap | kVAh | U32
24455 | 0x5F87 | 2 | T4 - Eap | kVAh | U32
24457 | 0x5F89 | 2 | Reserved | - | -
24459 | 0x5F8B | 2 | Reserved | - | -
24461 | 0x5F8D | 2 | Reserved | - | -
24463 | 0x5F8F | 2 | Reserved | - | -

## Tariff meter (total) - Total (EA)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26368 | 0x6700 | Info | 33 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26368 | 0x6700 | 1 | Tariff number in progress 1 : Tariff 1 2 : Tariff 2 3 : Tariff 3 4 : Tariff 4 | - | U16
26369 | 0x6701 | 2 | T1 - Ea+ | kWh | U32
26371 | 0x6703 | 2 | T2 - Ea+ | kWh | U32
26373 | 0x6705 | 2 | T3 - Ea+ | kWh | U32
26375 | 0x6707 | 2 | T4 - Ea+ | kWh | U32
26377 | 0x6709 | 2 | Reserved | - | -
26379 | 0x670B | 2 | Reserved | - | -
26381 | 0x670D | 2 | Reserved | - | -
26383 | 0x670F | 2 | Reserved | - | -
26385 | 0x6711 | 2 | T1 - Ea- | kWh | U32
26387 | 0x6713 | 2 | T2 - Ea- | kWh | U32
26389 | 0x6715 | 2 | T3 - Ea- | kWh | U32
26391 | 0x6717 | 2 | T4 - Ea- | kWh | U32
26393 | 0x6719 | 2 | Reserved | - | -
26395 | 0x671B | 2 | Reserved | - | -
26397 | 0x671D | 2 | Reserved | - | -
26399 | 0x671F | 2 | Reserved | - | -

## Tariff meter (total) - Total (ER)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26401 | 0x6721 | Info | 96 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26401 | 0x6721 | 2 | T1 - Er+ | varh 10³ | U32
26403 | 0x6723 | 2 | T2 - Er+ | varh 10³ | U32
26405 | 0x6725 | 2 | T3 - Er+ | varh 10³ | U32
26407 | 0x6727 | 2 | T4 - Er+ | varh 10³ | U32
26409 | 0x6729 | 2 | Reserved | - | -
26411 | 0x672B | 2 | Reserved | - | -
26413 | 0x672D | 2 | Reserved | - | -
26415 | 0x672F | 2 | Reserved | - | -
26417 | 0x6731 | 2 | T1 - Er+ (lagging) | varh 10³ | U32
26419 | 0x6733 | 2 | T2 - Er+ (lagging) | varh 10³ | U32
26421 | 0x6735 | 2 | T3 - Er+ (lagging) | varh 10³ | U32
26423 | 0x6737 | 2 | T4 - Er+ (lagging) | varh 10³ | U32
26425 | 0x6739 | 2 | Reserved | - | -
26427 | 0x673B | 2 | Reserved | - | -
26429 | 0x673D | 2 | Reserved | - | -
26431 | 0x673F | 2 | Reserved | - | -
26433 | 0x6741 | 2 | T1 - Er+ (leading) | varh 10³ | U32
26435 | 0x6743 | 2 | T2 - Er+ (leading) | varh 10³ | U32
26437 | 0x6745 | 2 | T3 - Er+ (leading) | varh 10³ | U32
26439 | 0x6747 | 2 | T4 - Er+ (leading) | varh 10³ | U32
26441 | 0x6749 | 2 | Reserved | - | -
26443 | 0x674B | 2 | Reserved | - | -
26445 | 0x674D | 2 | Reserved | - | -
26447 | 0x674F | 2 | Reserved | - | -
26449 | 0x6751 | 2 | T1 - Er- | varh 10³ | U32
26451 | 0x6753 | 2 | T2 - Er- | varh 10³ | U32
26453 | 0x6755 | 2 | T3 - Er- | varh 10³ | U32
26455 | 0x6757 | 2 | T4 - Er- | varh 10³ | U32
26457 | 0x6759 | 2 | Reserved | - | -
26459 | 0x675B | 2 | Reserved | - | -
26461 | 0x675D | 2 | Reserved | - | -
26463 | 0x675F | 2 | Reserved | - | -
26465 | 0x6761 | 2 | T1 - Er- (lagging) | varh 10³ | U32
26467 | 0x6763 | 2 | T2 - Er- (lagging) | varh 10³ | U32
26469 | 0x6765 | 2 | T3 - Er- (lagging) | varh 10³ | U32
26471 | 0x6767 | 2 | T4 - Er- (lagging) | varh 10³ | U32
26473 | 0x6769 | 2 | Reserved | - | -
26475 | 0x676B | 2 | Reserved | - | -
26477 | 0x676D | 2 | Reserved | - | -
26479 | 0x676F | 2 | Reserved | - | -
26481 | 0x6771 | 2 | T1 - Er- (leading) | varh 10³ | U32
26483 | 0x6773 | 2 | T2 - Er- (leading) | varh 10³ | U32
26485 | 0x6775 | 2 | T3 - Er- (leading) | varh 10³ | U32
26487 | 0x6777 | 2 | T4 - Er- (leading) | varh 10³ | U32
26489 | 0x6779 | 2 | Reserved | - | -
26491 | 0x677B | 2 | Reserved | - | -
26493 | 0x677D | 2 | Reserved | - | -
26495 | 0x677F | 2 | Reserved | - | -

## Tariff meter (total) - Total (ES)

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
26497 | 0x6781 | Info | 16 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
26497 | 0x6781 | 2 | T1 - Eap | kVAh | U32
26499 | 0x6783 | 2 | T2 - Eap | kVAh | U32
26501 | 0x6785 | 2 | T3 - Eap | kVAh | U32
26503 | 0x6787 | 2 | T4 - Eap | kVAh | U32
26505 | 0x6789 | 2 | Reserved | - | -
26507 | 0x678B | 2 | Reserved | - | -
26509 | 0x678D | 2 | Reserved | - | -
26511 | 0x678F | 2 | Reserved | - | -

## Partial active energy by tariff

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
32768 | 0x8000 | Info | 48 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
32768 | 0x8000 | 2 | Partial positive active Energy : Ea+ Tariff 1 | kWh | U32
32770 | 0x8002 | 1 | Partial Residual positive active Energy : rEa+ Tariff 1 | Wh 10⁻¹ | U16
32771 | 0x8003 | 2 | Partial positive active Energy : Ea+ Tariff 2 | kWh | U32
32773 | 0x8005 | 1 | Partial Residual positive active Energy : rEa+ Tariff 2 | Wh 10⁻¹ | U16
32774 | 0x8006 | 2 | Partial positive active Energy : Ea+ Tariff 3 | kWh | U32
32776 | 0x8008 | 1 | Partial Residual positive active Energy : rEa+ Tariff 3 | Wh 10⁻¹ | U16
32777 | 0x8009 | 2 | Partial positive active Energy : Ea+ Tariff 4 | kWh | U32
32779 | 0x800B | 1 | Partial Residual positive active Energy : rEa+ Tariff 4 | Wh 10⁻¹ | U16
32780 | 0x800C | 2 | Reserved | - | -
32782 | 0x800E | 1 | Reserved | - | -
32783 | 0x800F | 2 | Reserved | - | -
32785 | 0x8011 | 1 | Reserved | - | -
32786 | 0x8012 | 2 | Reserved | - | -
32788 | 0x8014 | 1 | Reserved | - | -
32789 | 0x8015 | 2 | Reserved | - | -
32791 | 0x8017 | 1 | Reserved | - | -
32792 | 0x8018 | 2 | Partial negative active Energy : Ea- Tariff 1 | kWh | U32
32794 | 0x801A | 1 | Partial Residual negative active Energy : rEa- Tariff 1 | Wh 10⁻¹ | U16
32795 | 0x801B | 2 | Partial negative active Energy : Ea- Tariff 2 | kWh | U32
32797 | 0x801D | 1 | Partial Residual negative active Energy : rEa- Tariff 2 | Wh 10⁻¹ | U16
32798 | 0x801E | 2 | Partial negative active Energy : Ea- Tariff 3 | kWh | U32
32800 | 0x8020 | 1 | Partial Residual negative active Energy : rEa- Tariff 3 | Wh 10⁻¹ | U16
32801 | 0x8021 | 2 | Partial negative active Energy : Ea- Tariff 4 | kWh | U32
32803 | 0x8023 | 1 | Partial Residual negative active Energy : rEa- Tariff 4 | Wh 10⁻¹ | U16
32804 | 0x8024 | 2 | Reserved | - | -
32806 | 0x8026 | 1 | Reserved | - | -
32807 | 0x8027 | 2 | Reserved | - | -
32809 | 0x8029 | 1 | Reserved | - | -
32810 | 0x802A | 2 | Reserved | - | -
32812 | 0x802C | 1 | Reserved | - | -
32813 | 0x802D | 2 | Reserved | - | -
32815 | 0x802F | 1 | Reserved | - | -

## Net energy consumption

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
33024 | 0x8100 | Info | 6 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
33024 | 0x8100 | 2 | Net active energy consumption (?(Ea+-Ea-) by tariff) | kWh | S32
33026 | 0x8102 | 1 | Net Residual active energy consumption (?(Ea+-Ea-) by tariff) | Wh 10⁻¹ | S16
33027 | 0x8103 | 2 | Net reactive energy consumption (?(Er+-Er-) by tariff) | varh 10³ | S32
33029 | 0x8105 | 1 | Net Residual reactive energy consumption (?(Er+-Er-) by tariff) | varh 10⁻¹ | S16

## Load curve P+

### Command

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61440 | 0xF000 | Command | 1 | NONE | WRITE_MANY | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61440 | 0xF000 | 1 | Action 0x0001 : Reset read pointer 0xFFFE : Get next data | - | U16_HEX

### Header

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61456 | 0xF010 | Header | 6 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61456 | 0xF010 | 1 | Record count ( Maximum 29 ) | - | U8
61457 | 0xF011 | 1 | Record size : 4 see below the data record description | W | U8
61458 | 0xF012 | 1 | Integration period | s | U16
61459 | 0xF013 | 1 | Physical Unit : 0 0 : W 1 : W 2 : var 3 : var 4 : VA 5 : None 6 : J 7 : Pulse 8 : m3 9 : Nm3 20 : kW 22 : kVAr 24 : kVA 26 : kJ 27 : kilo-Pulse | - | U8
61460 | 0xF014 | 1 | Numerator Rate | - | U16
61461 | 0xF015 | 1 | Denominator Rate | - | U16

### Data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
61462 | 0xF016 | Data | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
61462 | 0xF016 | 2 | Date | - | DATETIME
61464 | 0xF018 | 1 | Full/incomplete period 0 : full integration period 1 : incomplete integration period | - | U8
61465 | 0xF019 | 1 | Value without CT*VT rate | W | U16

# Specific

## Table Overflow

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36864 | 0x9000 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36864 | 0x9000 | 2 | Value of the meter overflow (10Wh) : 999 999 999 | Wh 10 | U32
36866 | 0x9002 | 1 | Nb Overflow Total Ea + | - | U8
36867 | 0x9003 | 1 | Nb Overflow Total Er + | - | U8
36868 | 0x9004 | 1 | Nb Overflow Total Ea - | - | U8
36869 | 0x9005 | 1 | Nb Overflow Total Er - | - | U8
36870 | 0x9006 | 1 | Nb Overflow Total Eap | - | U8
36871 | 0x9007 | 1 | Nb Overflow Total Ea T1 | - | U8
36872 | 0x9008 | 1 | Nb Overflow Total Ea T2 | - | U8
36873 | 0x9009 | 1 | Nb Overflow Total Ea T3 | - | U8
36874 | 0x900A | 1 | Nb Overflow Total Ea T4 | - | U8

## Temporal Active Index

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36896 | 0x9020 | Info | 24 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36896 | 0x9020 | 2 | Ea + for day n-1 | kWh | U32
36898 | 0x9022 | 2 | Ea - for day n-1 | kWh | U32
36900 | 0x9024 | 2 | Ea + for day n | kWh | U32
36902 | 0x9026 | 2 | Ea - for day n | kWh | U32
36904 | 0x9028 | 2 | Ea + for Week n-1 | kWh | U32
36906 | 0x902A | 2 | Ea - for Week n-1 | kWh | U32
36908 | 0x902C | 2 | Ea + for Week n | kWh | U32
36910 | 0x902E | 2 | Ea - for Week n | kWh | U32
36912 | 0x9030 | 2 | Ea + for Month n-1 | kWh | U32
36914 | 0x9032 | 2 | Ea - for Month n-1 | kWh | U32
36916 | 0x9034 | 2 | Ea + for Month n | kWh | U32
36918 | 0x9036 | 2 | Ea - for Month n | kWh | U32

## Temporal Active Index in Unit/100

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36928 | 0x9040 | Info | 24 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36928 | 0x9040 | 2 | Ea + for day n-1 | Wh 10 | U32
36930 | 0x9042 | 2 | Ea - for day n-1 | Wh 10 | U32
36932 | 0x9044 | 2 | Ea + for day n | Wh 10 | U32
36934 | 0x9046 | 2 | Ea - for day n | Wh 10 | U32
36936 | 0x9048 | 2 | Ea + for Week n-1 | Wh 10 | U32
36938 | 0x904A | 2 | Ea - for Week n-1 | Wh 10 | U32
36940 | 0x904C | 2 | Ea + for Week n | Wh 10 | U32
36942 | 0x904E | 2 | Ea - for Week n | Wh 10 | U32
36944 | 0x9050 | 2 | Ea + for Month n-1 | Wh 10 | U32
36946 | 0x9052 | 2 | Ea - for Month n-1 | Wh 10 | U32
36948 | 0x9054 | 2 | Ea + for Month n | Wh 10 | U32
36950 | 0x9056 | 2 | Ea - for Month n | Wh 10 | U32

## Current without CT

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40576 | 0x9E80 | Info | 6 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40576 | 0x9E80 | 2 | Current: I1 | mA | U32
40578 | 0x9E82 | 2 | Current: I2 | mA | U32
40580 | 0x9E84 | 2 | Current: I3 | mA | U32

# Settings

# Gateway

## Network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
29184 | 0x7200 | Settings | 7 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
29184 | 0x7200 | 2 | IP address | - | U32_IP
29186 | 0x7202 | 2 | Subnet mask | - | U32_IP
29188 | 0x7204 | 2 | Gateway | - | U32_IP
29190 | 0x7206 | 1 | DHCP Enable | - | U8

# Modbus slave

## General slave connection

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
29440 | 0x7300 | Settings | 1 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
29440 | 0x7300 | 1 | Slave Address | - | U8

# Measurement

## Electrical network

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57344 | 0xE000 | Settings | 10 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57344 | 0xE000 | 1 | Network Type : 0 : 1P+N (1BL) 1 : 2P (2BL) 2 : 3P (3BL) 3 : 3P (3NBL) 4 : 3P+N (4BL) 5 : 3P+N (4NBL) | - | U8
57345 | 0xE001 | 1 | Current Transformer secondary : 1 : 1 A 5 : 5 A | - | U8
57346 | 0xE002 | 1 | Current Transformer primary | A | U16
57347 | 0xE003 | 1 | Reserved | - | -
57348 | 0xE004 | 1 | Reserved | - | -
57349 | 0xE005 | 1 | Reserved | - | -
57350 | 0xE006 | 1 | Reserved | - | -
57351 | 0xE007 | 1 | Reserved | - | -
57352 | 0xE008 | 2 | Reserved | - | -

## Energy measurement

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57354 | 0xE00A | Settings | 2 | NONE | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57354 | 0xE00A | 1 | Internal/External Top 0 : internal 1 : external | - | U8
57355 | 0xE00B | 1 | Synchronisation Top for P+/- Q+/- : time in seconds ( 1mn, 5mn, 8mn, 10mn, 15mn, 20mn, 30mn, 60mn) 60 : 1 min 120 : 2 min 180 : 3 min 240 : 4 min 300 : 5 min 360 : 6 min 480 : 8 min 600 : 10 min 720 : 12 min 900 : 15 min 1200 : 20 min 1800 : 30 min 3600 : 60 min | s | U16

# Time management

## Date and time

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57600 | 0xE100 | Settings | 6 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57600 | 0xE100 | 1 | Day | - | U8
57601 | 0xE101 | 1 | Month | - | U8
57602 | 0xE102 | 1 | Year | - | U16
57603 | 0xE103 | 1 | Hour | - | U8
57604 | 0xE104 | 1 | Minute | - | U8
57605 | 0xE105 | 1 | Second | - | U8

## Date and time extended

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
29952 | 0x7500 | Settings | 7 | NONE | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
29952 | 0x7500 | 1 | Day | - | U16
29953 | 0x7501 | 1 | Month | - | U16
29954 | 0x7502 | 1 | Year | - | U16
29955 | 0x7503 | 1 | Hour | h | U16
29956 | 0x7504 | 1 | Minute | min | U16
29957 | 0x7505 | 1 | Second | s | U16
29958 | 0x7506 | 1 | Millisecond | s 10⁻³ | U16

## Time synchro and SNTP server

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
30208 | 0x7600 | Settings | 27 | USER | READ | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
30208 | 0x7600 | 1 | Activation 0 : Disabled 1 : Enabled | - | U16
30209 | 0x7601 | 25 | SNTP server IP address | - | STRING_NORM

# Commands

## Set Tariff

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40480 | 0x9E20 | Commands | 2 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40480 | 0x9E20 | 1 | Reserved | - | -
40481 | 0x9E21 | 1 | Tariff Number to set 1 : Tariff 1 2 : Tariff 2 3 : Tariff 3 4 : Tariff 4 | - | U8

# System

## Action system

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57856 | 0xE200 | Commands | 1 | USER | NONE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57856 | 0xE200 | 1 | Reserved | - | -

# Reset

## Value reset

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57888 | 0xE220 | Commands | 5 | NONE | NONE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57888 | 0xE220 | 1 | Reserved | - | -
57889 | 0xE221 | 1 | Reserved | - | -
57890 | 0xE222 | 1 | Reset Partial Energies 0x0000 : None 0x0001 : Partial Ea+ 0x0002 : Partial Er+ 0x0004 : Partial Eap 0x0008 : Partial Ea- 0x0010 : Partial Er- 0x001F : Reset ALL TOT Partial | - | U16_HEX
57891 | 0xE223 | 1 | Reserved | - | -
57892 | 0xE224 | 1 | Reset Tarif Partial Energies 0x0000 : None 0x0001 : Tariff counter 1 0x0002 : Tariff counter 2 0x0004 : Tariff counter 3 0x0008 : Tariff counter 4 0xFFFF : Reset All Partial | - | U16_HEX

## Partial Energies Reset

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40512 | 0x9E40 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40512 | 0x9E40 | 1 | Reset 0x00 : None 0x01 : Max P 0x20 : Partial Energies | - | U8_HEX

# Industrialization

## Indus Mode and MID status

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40544 | 0x9E60 | Info | 2 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40544 | 0x9E60 | 1 | Indus Mode (0: indus mode disabled, 1: indus mode enabled) | - | U8
40545 | 0x9E61 | 1 | MID status (0: non-MID product, 1: MID product | - | U8

## COM Board Product ID

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
40608 | 0x9EA0 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
40608 | 0x9EA0 | 1 | Product ID :0x01: E3x/E4x COM Board0x02: E63 COM Board | - | U8

--X33F-LB08-0PZ4-609140a6--