= ESS §14a EnWG Controller

Established by law (for Germany), this controller lowers active power to `-4200 W` in response to grid operator limitations, aiming to alleviate load on transformers.

Link to legislative text:
https://www.gesetze-im-internet.de/enwg_2005/__14a.html

https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.controller.ess.limiter14a[Source Code icon:github[]]