= Symmetric Timeslot Peak-Shaving

Applies peak-shaving within a configured timeslot at the grid using a symmetric energy storage system. Outside of the timeslot the battery recharges. 

This Controller can be used for "Atypische Netznutzung" applications in Germany, e.g. "Hochlastzeitfenster".

https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.controller.symmetric.timeslotpeakshaving[Source Code icon:github[]]