# General

# Identification

## Product identification

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50000 | 0xC350 | Info | 66 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50000 | 0xC350 | 4 | "SOCO" | - | STRING_16
50004 | 0xC354 | 1 | Product order ID (Countis:100, Protection:200, Atys:300, Diris:400) | - | U16
50005 | 0xC355 | 1 | Product ID (EX: 1000 ATS3) | - | U16
50006 | 0xC356 | 1 | JBUS Table Version (EX: 101 Version 1.01) | - | U16
50007 | 0xC357 | 1 | Product software version (EX: 100 Version 1.00) | - | U16
50008 | 0xC358 | 1 | Serial_AA_SS | - | U16_HEX
50009 | 0xC359 | 1 | Serial_SST_L | - | U16_HEX
50010 | 0xC35A | 1 | Serial_order | - | U16
50011 | 0xC35B | 2 | Serial_Reserve | - | U32
50013 | 0xC35D | 4 | See "Code table" tab for more details | - | U64_HEX
50017 | 0xC361 | 1 | Customization data loaded (True/False) | - | U8
50018 | 0xC362 | 1 | Product version (Major) | - | U16
50019 | 0xC363 | 1 | Product version (Minor) | - | U16
50020 | 0xC364 | 1 | Product version (Revision) | - | U16
50021 | 0xC365 | 1 | Product version (Build) | - | U16
50022 | 0xC366 | 3 | Product build date | - | DATETIME_3
50025 | 0xC369 | 1 | Software technical base version (Major) | - | U16
50026 | 0xC36A | 1 | Software technical base version (Minor) | - | U16
50027 | 0xC36B | 1 | Software technical base version (Revision) | - | U16
50028 | 0xC36C | 1 | Customization version (Major) | - | U16
50029 | 0xC36D | 1 | Customization version (Minor) | - | U16
50030 | 0xC36E | 4 | Product VLO (EX : "880100") | - | STRING_NORM
50034 | 0xC372 | 4 | Customization VLO (EX : "880700") | - | STRING_NORM
50038 | 0xC376 | 4 | Software technical base VLO (EX : "880600") | - | STRING_NORM
50042 | 0xC37A | 8 | Vendor name (EX : "SOCOMEC") | - | STRING_NORM
50050 | 0xC382 | 8 | Product name (EX : "DIRIS A40R") | - | STRING_NORM
50058 | 0xC38A | 8 | Extended name | - | STRING_NORM

## Table Option

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36096 | 0x8D00 | Info | 1 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36096 | 0x8D00 | 1 | Product option code (bit field) :bit 1: Metering Optionbit 2: Communication optionbit 3: 3 inputs / 1 output option | - | U8

## Customization specific data

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
4096 | 0x1000 | Info | 138 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
4096 | 0x1000 | 1 | Customisation specific data loaded0x0000 : FALSE0x0001 : TRUE | - | U8
4097 | 0x1001 | 1 | Retrofit activated0x0000 : FALSE0x0001 : TRUE | - | U8
4098 | 0x1002 | 8 | TC list :TC 1 / TC2 / TC3 / TC4 / TC5 / TC6 / TC7 / TC8 | A | U32[]
4106 | 0x100A | 16 | TC gain correction X1 2 words : 1 TC correction | - | U32[]
4122 | 0x101A | 16 | TC gain correction X2 2 words : 1 TC correction | - | U32[]
4138 | 0x102A | 16 | TC gain correction Y1 2 words : 1 TC correction | - | U32[]
4154 | 0x103A | 16 | TC gain correction Y2 2 words : 1 TC correction | - | U32[]
4170 | 0x104A | 16 | TC phasys correction X1 2 words : 1 TC correction | - | U32[]
4186 | 0x105A | 16 | TC phasys correction X2 2 words : 1 TC correction | - | U32[]
4202 | 0x106A | 16 | TC phasys correction Y1 2 words : 1 TC correction | - | U32[]
4218 | 0x107A | 16 | TC phasys correction Y2 2 words : 1 TC correction | - | U32[]

# Common settings

## Network Setting

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57344 | 0xE000 | Settings | 12 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57344 | 0xE000 | 1 | Network Type : 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8
57345 | 0xE001 | 1 | Current Transformer secondary : 1 : 1 A 5 : 5 A | - | U8
57346 | 0xE002 | 1 | Current Transformer primary | A | U16
57347 | 0xE003 | 1 | Reserved | - | -
57348 | 0xE004 | 1 | Reserved | - | -
57349 | 0xE005 | 1 | Reserved | - | -
57350 | 0xE006 | 1 | Reserved | - | -
57351 | 0xE007 | 1 | Reserved | - | -
57352 | 0xE008 | 2 | Reserved | - | -
57354 | 0xE00A | 1 | Reserved | - | -
57355 | 0xE00B | 1 | Reserved | - | -

# Actions

## Action system

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
57856 | 0xE200 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
57856 | 0xE200 | 1 | Action : 0xA1 : Product Configuration storage 0xB2 : Produit reset 0xC3 : Load Factory Config | - | U8_HEX

# Application

## Table Setup

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36352 | 0x8E00 | Settings | 18 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36352 | 0x8E00 | 1 | Network Type 0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8
36353 | 0x8E01 | 1 | Current Transformer secondary: 0 : 1A 5 : 5A | A | U8
36354 | 0x8E02 | 1 | Current Transformer primary | A | U8
36355 | 0x8E03 | 1 | Reserved | - | U8
36356 | 0x8E04 | 1 | Synchronisation of I AVG/MAX: 2 : 2 seconds 5 : 5 minutes 8 : 8 minutes 10 : 10 minutes 15 : 15 minutes 30 : 30 minutes 60 : 60 minutes | - | U8
36357 | 0x8E05 | 1 | Synchronisation of P/Q/S AVG/MAX: 2 : 2 secondes 5 : 5 minutes 8 : 8 minutes 10 : 10 minutes 15 : 15 minutes 30 : 30 minutes 60 : 60 minutes | - | U8
36358 | 0x8E06 | 1 | OUT : pulse output allocation: 0 : kWh+ 1 : kVar+ 2 : kWh- 3 : kVarh- 4 : kVAh 5 : Alarm 6 : Command | - | U8
36359 | 0x8E07 | 1 | OUT : pulse output value : 0 : 0,1 kWh/kvarh 1 : 1 kWh/kvarh 2 : 10 kWh/kvarh 3 : 100 kWh/kvarh 4 : 1000 kWh/kvarh 5 : 10000 kWh/kvarh | - | U8
36360 | 0x8E08 | 1 | OUT : pulse output duration: 1 : 100ms 2 : 200ms 3 : 300ms 4 : 400ms 5 : 500ms 6 : 600ms 7 : 700ms 8 : 800ms 9 : 900ms | - | U8
36361 | 0x8E09 | 1 | Hour meter allocation: 1 : Auxiliary power supply 2 : Currents 3 : phase to phase voltage 4 : Input 1 5 : Input2 6 : Input3 | - | U8
36362 | 0x8E0A | 1 | Hour meter trigger threshold | - | U16
36363 | 0x8E0B | 1 | Alarm Type: 1 : I 2 : In 3 : U 4 : V 5 : ?P+ 6 : ?Q+ 7 : ?S+ 8 : ?PFC 9 : ?PFL 10 : THDU 11 : THDV 12 : THDI 13 : HOUR 14 : F 15 : Temperature | - | U8
36364 | 0x8E0C | 1 | Alarm Specified time (1-999) | s | U8
36365 | 0x8E0D | 1 | Alarm upper Threshold | - | U16
36366 | 0x8E0E | 1 | Alarm Lower Threshold | - | U16
36367 | 0x8E0F | 1 | Alarm Hysteresis(0-99) | - | U8
36368 | 0x8E10 | 1 | Relay State: 0 : Normally Open 1 : Normally Closed | - | U8
36369 | 0x8E11 | 1 | Reactive Power Calculation: 0 : With Harmonic (IEC61557-12) 1 : Without Harmonic | - | U8

# Measurement

# Common

## Metrology Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50512 | 0xC550 | Info | 74 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50512 | 0xC550 | 2 | Hour Meter | h 10⁻² | U32
50514 | 0xC552 | 2 | Phase to Phase Voltage: U12 | V 10⁻² | U32
50516 | 0xC554 | 2 | Phase to Phase Voltage: U23 | V 10⁻² | U32
50518 | 0xC556 | 2 | Phase to Phase Voltage: U31 | V 10⁻² | U32
50520 | 0xC558 | 2 | Simple voltage : V1 | V 10⁻² | U32
50522 | 0xC55A | 2 | Simple voltage : V2 | V 10⁻² | U32
50524 | 0xC55C | 2 | Simple voltage : V3 | V 10⁻² | U32
50526 | 0xC55E | 2 | Frequency : F | Hz 10⁻² | U32
50528 | 0xC560 | 2 | Current : I1 | mA | U32
50530 | 0xC562 | 2 | Current : I2 | mA | U32
50532 | 0xC564 | 2 | Current : I3 | mA | U32
50534 | 0xC566 | 2 | Neutral Current : In | mA | U32
50536 | 0xC568 | 2 | ? Active Power +/- : P | W 10 | S32
50538 | 0xC56A | 2 | ? Reactive Power +/- : Q | var 10 | S32
50540 | 0xC56C | 2 | ? Apparent Power : S | VA 10 | U32
50542 | 0xC56E | 2 | ? Power Factor : -: leading et + : lagging : PF | - / 1000 | S32
50544 | 0xC570 | 2 | Active Power phase 1 +/- : P1 | W 10 | S32
50546 | 0xC572 | 2 | Active Power phase 2 +/- : P2 | W 10 | S32
50548 | 0xC574 | 2 | Active Power phase 3 +/- : P3 | W 10 | S32
50550 | 0xC576 | 2 | Reactive Power phase 1 +/- : Q1 | var 10 | S32
50552 | 0xC578 | 2 | Reactive Power phase 2 +/- : Q2 | var 10 | S32
50554 | 0xC57A | 2 | Reactive Power phase 3 +/- : Q3 | var 10 | S32
50556 | 0xC57C | 2 | Apparent Power phase 1 : S1 | VA 10 | U32
50558 | 0xC57E | 2 | Apparent Power phase 2 : S2 | VA 10 | U32
50560 | 0xC580 | 2 | Apparent Power phase 3 : S3 | VA 10 | U32
50562 | 0xC582 | 2 | Power Factor phase 1 -: leading and + : lagging : PF1 | - / 1000 | S32
50564 | 0xC584 | 2 | Power Factor phase 2 -: leading and + : lagging : PF2 | - / 1000 | S32
50566 | 0xC586 | 2 | Power Factor phase 3 -: leading and + : lagging : PF3 | - / 1000 | S32
50568 | 0xC588 | 2 | Reserved | - | -
50570 | 0xC58A | 2 | Reserved | - | -
50572 | 0xC58C | 2 | Reserved | - | -
50574 | 0xC58E | 2 | Total power factor | - / 1000 | S32
50576 | 0xC590 | 2 | Power factor : PF1 | - / 1000 | S32
50578 | 0xC592 | 2 | Power factor : PF2 | - / 1000 | S32
50580 | 0xC594 | 2 | Power factor : PF3 | - / 1000 | S32
50582 | 0xC596 | 1 | Total Power Factor Type 0 : undefined 1 : leading 2 : lagging | - | U8
50583 | 0xC597 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U8
50584 | 0xC598 | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U8
50585 | 0xC599 | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U8

## Energies

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50768 | 0xC650 | Info | 65 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50768 | 0xC650 | 2 | Hour meter | h 10⁻² | U32
50770 | 0xC652 | 2 | Reserved | - | -
50772 | 0xC654 | 2 | Reserved | - | -
50774 | 0xC656 | 2 | Reserved | - | -
50776 | 0xC658 | 2 | Reserved | - | -
50778 | 0xC65A | 2 | Reserved | - | -
50780 | 0xC65C | 2 | Partial Positive Active Energy: Ea+ | kWh | U32
50782 | 0xC65E | 2 | Partial Positive Reactive Energy: Er + | varh 10³ | U32
50784 | 0xC660 | 2 | Partial Apparent Energy : Es | kVAh | U32
50786 | 0xC662 | 2 | Partial Negative Active Energy : Ea- | kWh | U32
50788 | 0xC664 | 2 | Partial Negative Reactive Energy : Er - | varh 10³ | U32
50790 | 0xC666 | 2 | Reserved | - | -
50792 | 0xC668 | 2 | Reserved | - | -
50794 | 0xC66A | 2 | Reserved | - | -
50796 | 0xC66C | 2 | Reserved | - | -
50798 | 0xC66E | 2 | Reserved | - | -
50800 | 0xC670 | 2 | Reserved | - | -
50802 | 0xC672 | 2 | Reserved | - | -
50804 | 0xC674 | 2 | Reserved | - | -
50806 | 0xC676 | 2 | Reserved | - | -
50808 | 0xC678 | 2 | Reserved | - | -
50810 | 0xC67A | 2 | Reserved | - | -
50812 | 0xC67C | 2 | Reserved | - | -
50814 | 0xC67E | 2 | Reserved | - | -
50816 | 0xC680 | 2 | Reserved | - | -
50818 | 0xC682 | 2 | Reserved | - | -
50820 | 0xC684 | 2 | Reserved | - | -
50822 | 0xC686 | 2 | Reserved | - | -
50824 | 0xC688 | 2 | Reserved | - | -
50826 | 0xC68A | 2 | Reserved | - | -
50828 | 0xC68C | 1 | Reserved | - | -
50829 | 0xC68D | 1 | Reserved | - | -
50830 | 0xC68E | 1 | Reserved | - | -
50831 | 0xC68F | 1 | Reserved | - | -
50832 | 0xC690 | 1 | Reserved | - | -

## Statistique Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51024 | 0xC750 | Info | 70 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51024 | 0xC750 | 2 | Reserved | - | -
51026 | 0xC752 | 2 | Reserved | - | -
51028 | 0xC754 | 2 | Reserved | - | -
51030 | 0xC756 | 2 | Reserved | - | -
51032 | 0xC758 | 2 | Reserved | - | -
51034 | 0xC75A | 2 | Reserved | - | -
51036 | 0xC75C | 2 | Reserved | - | -
51038 | 0xC75E | 2 | Reserved | - | -
51040 | 0xC760 | 2 | Reserved | - | -
51042 | 0xC762 | 2 | Reserved | - | -
51044 | 0xC764 | 2 | Reserved | - | -
51046 | 0xC766 | 2 | Reserved | - | -
51048 | 0xC768 | 2 | Reserved | - | -
51050 | 0xC76A | 2 | Reserved | - | -
51052 | 0xC76C | 2 | Reserved | - | -
51054 | 0xC76E | 2 | Reserved | - | -
51056 | 0xC770 | 2 | Reserved | - | -
51058 | 0xC772 | 2 | Reserved | - | -
51060 | 0xC774 | 2 | Reserved | - | -
51062 | 0xC776 | 2 | Reserved | - | -
51064 | 0xC778 | 2 | Reserved | - | -
51066 | 0xC77A | 2 | Reserved | - | -
51068 | 0xC77C | 2 | Reserved | - | -
51070 | 0xC77E | 2 | Max/avg I1 | mA | U32
51072 | 0xC780 | 2 | Max/avg I2 | mA | U32
51074 | 0xC782 | 2 | Max/avg I3 | mA | U32
51076 | 0xC784 | 2 | Max/avg In | mA | U32
51078 | 0xC786 | 2 | Max/avg P+ | W 10 | U32
51080 | 0xC788 | 2 | Reserved | - | -
51082 | 0xC78A | 2 | Max/avg Q+ | var 10 | U32
51084 | 0xC78C | 2 | Reserved | - | -
51086 | 0xC78E | 2 | Max/avg S | VA 10 | U32
51088 | 0xC790 | 1 | Reserved | - | -
51089 | 0xC791 | 1 | Reserved | - | -
51090 | 0xC792 | 1 | Reserved | - | -
51091 | 0xC793 | 1 | Reserved | - | -
51092 | 0xC794 | 1 | Reserved | - | -
51093 | 0xC795 | 1 | Reserved | - | -

## Metrology No Affected by current and voltage transformers

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51280 | 0xC850 | Info | 43 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51280 | 0xC850 | 1 | Hour Meter | h | U16
51281 | 0xC851 | 1 | Phase to Phase Voltage: U12 | V 10⁻² | U16
51282 | 0xC852 | 1 | Phase to Phase Voltage: U23 | V 10⁻² | U16
51283 | 0xC853 | 1 | Phase to Phase Voltage: U31 | V 10⁻² | U16
51284 | 0xC854 | 1 | Simple voltage : V1 | V 10⁻² | U16
51285 | 0xC855 | 1 | Simple voltage : V2 | V 10⁻² | U16
51286 | 0xC856 | 1 | Simple voltage : V3 | V 10⁻² | U16
51287 | 0xC857 | 1 | Frequency : F | Hz 10⁻² | U16
51288 | 0xC858 | 1 | Current : I1 | mA | U16
51289 | 0xC859 | 1 | Current : I2 | mA | U16
51290 | 0xC85A | 1 | Current : I3 | mA | U16
51291 | 0xC85B | 1 | Neutral Current : In | mA | U16
51292 | 0xC85C | 1 | ? active Power +/- : P | W 10 | S16
51293 | 0xC85D | 1 | ? reactive Power +/- : Q | var 10 | S16
51294 | 0xC85E | 1 | ? apparent power : S | VA 10 | U16
51295 | 0xC85F | 1 | ? power factor : -: leading and + : lagging : PF | - / 1000 | S16
51296 | 0xC860 | 1 | Active Power phase 1 +/- : P1 | W 10 | S16
51297 | 0xC861 | 1 | Active Power phase 2 +/- : P2 | W 10 | S16
51298 | 0xC862 | 1 | Active Power phase 3 +/- : P3 | W 10 | S16
51299 | 0xC863 | 1 | Reactive Power phase 1 +/- : Q1 | var 10 | S16
51300 | 0xC864 | 1 | Reactive Power phase 2 +/- : Q2 | var 10 | S16
51301 | 0xC865 | 1 | Reactive Power phase 3 +/- : Q3 | var 10 | S16
51302 | 0xC866 | 1 | Apparent power phase 1 : S1 | VA 10 | U16
51303 | 0xC867 | 1 | Apparent power phase 2 : S2 | VA 10 | U16
51304 | 0xC868 | 1 | Apparent power phase 3 : S3 | VA 10 | U16
51305 | 0xC869 | 1 | Power Factor phase 1 -: leading and + : lagging : PF1 | - / 1000 | S16
51306 | 0xC86A | 1 | Power Factor phase 2 -: leading and + : lagging : PF2 | - / 1000 | S16
51307 | 0xC86B | 1 | Power Factor phase 3 -: leading and + : lagging : PF3 | - / 1000 | S16
51308 | 0xC86C | 1 | Reserved | - | -
51309 | 0xC86D | 1 | Reserved | - | -
51310 | 0xC86E | 1 | Reserved | - | -
51311 | 0xC86F | 1 | Total Positive Active Energy (not resettable) : Ea+ | Wh / 1E-06 | U16
51312 | 0xC870 | 1 | Total Negative Active Energy (not resettable) : Ea - | Wh / 1E-06 | U16
51313 | 0xC871 | 1 | Total Positive Reactive Energy (not resettable) : Er + | varh / 1E-06 | U16
51314 | 0xC872 | 1 | Total Negative Reactive Energy (not resettable) : Er - | varh / 1E-06 | U16
51315 | 0xC873 | 1 | Total power factor | - / 1000 | S16
51316 | 0xC874 | 1 | Power factor : PF1 | - / 1000 | S16
51317 | 0xC875 | 1 | Power factor : PF2 | - / 1000 | S16
51318 | 0xC876 | 1 | Power factor : PF3 | - / 1000 | S16
51319 | 0xC877 | 1 | Total Power Factor Type 0 : undefined 1 : leading 2 : lagging | - | U16
51320 | 0xC878 | 1 | Power factor type : sPF1 0 : undefined 1 : leading 2 : lagging | - | U16
51321 | 0xC879 | 1 | Power factor type : sPF2 0 : undefined 1 : leading 2 : lagging | - | U16
51322 | 0xC87A | 1 | Power factor type : sPF3 0 : undefined 1 : leading 2 : lagging | - | U16

## THD

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51536 | 0xC950 | Info | 10 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51536 | 0xC950 | 1 | thd U12 | % / 10 | U16
51537 | 0xC951 | 1 | thd U23 | % / 10 | U16
51538 | 0xC952 | 1 | thd U31 | % / 10 | U16
51539 | 0xC953 | 1 | thd V1 | % / 10 | U16
51540 | 0xC954 | 1 | thd V2 | % / 10 | U16
51541 | 0xC955 | 1 | thd V3 | % / 10 | U16
51542 | 0xC956 | 1 | thd I1 | % / 10 | U16
51543 | 0xC957 | 1 | thd I2 | % / 10 | U16
51544 | 0xC958 | 1 | thd I3 | % / 10 | U16
51545 | 0xC959 | 1 | Reserved | - | -

# Specific

## Measurement CT/VT affected

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
768 | 0x0300 | Info | 150 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
768 | 0x0300 | 2 | Phase 1 Current | mA | U32
770 | 0x0302 | 2 | Phase 2 Current | mA | U32
772 | 0x0304 | 2 | Phase 3 Current | mA | U32
774 | 0x0306 | 2 | Neutral Current | mA | U32
776 | 0x0308 | 2 | Phase to Phase Voltage: U12 | V 10⁻² | U32
778 | 0x030A | 2 | Phase to Phase Voltage: U23 | V 10⁻² | U32
780 | 0x030C | 2 | Phase to Phase Voltage: U31 | V 10⁻² | U32
782 | 0x030E | 2 | Phase to Neutral voltage phase 1 | V 10⁻² | U32
784 | 0x0310 | 2 | Phase to Neutral voltage phase 2 | V 10⁻² | U32
786 | 0x0312 | 2 | Phase to Neutral voltage phase 3 | V 10⁻² | U32
788 | 0x0314 | 2 | Frequency | Hz 10⁻² | U32
790 | 0x0316 | 2 | ? active power +/- : P | W 10 | S32
792 | 0x0318 | 2 | ? reactive power +/- : Q | var 10 | S32
794 | 0x031A | 2 | ? apparent power : S | VA 10 | U32
796 | 0x031C | 2 | ? power factor : -: leadiing et + : lagging : PF | - / 1000 | S32
798 | 0x031E | 2 | Active Power phase1 +/- | W 10 | S32
800 | 0x0320 | 2 | Active Power phase2 +/- | W 10 | S32
802 | 0x0322 | 2 | Active Power phase3 +/- | W 10 | S32
804 | 0x0324 | 2 | Reactive Power phase1 +/- | var 10 | S32
806 | 0x0326 | 2 | Reactive Power phase2 +/- | var 10 | S32
808 | 0x0328 | 2 | Reactive Power phase3 +/- | var 10 | S32
810 | 0x032A | 2 | Apparent Power phase1 | VA 10 | U32
812 | 0x032C | 2 | Apparent Power phase2 | VA 10 | U32
814 | 0x032E | 2 | Apparent Power phase3 | VA 10 | U32
816 | 0x0330 | 2 | Power factor phase 1 -:leading and +: lagging | - / 1000 | S32
818 | 0x0332 | 2 | Power factor phase 2 -:leading and +: lagging | - / 1000 | S32
820 | 0x0334 | 2 | Power factor phase 3 -:leading and +: lagging | - / 1000 | S32
822 | 0x0336 | 16 | R?serv? constructeur | - | U32[]
838 | 0x0346 | 2 | max/avg I1 | mA | U32
840 | 0x0348 | 2 | max/avg I2 | mA | U32
842 | 0x034A | 2 | max/avg I3 | mA | U32
844 | 0x034C | 2 | max/avg ?active power + | W 10 | U32
846 | 0x034E | 2 | reserved | - | U32
848 | 0x0350 | 2 | max/avg ?reactive power + | var 10 | U32
850 | 0x0352 | 2 | Reserved | - | U32
852 | 0x0354 | 2 | max/avg ? apparent power | VA 10 | U32
854 | 0x0356 | 2 | Hour Meter | h 10⁻² | U32
856 | 0x0358 | 2 | Active Energy + | kWh | U32
858 | 0x035A | 2 | Reactive Energy + | varh 10³ | U32
860 | 0x035C | 56 | Reserved | - | U32[]
916 | 0x0394 | 2 | max/avg In | mA | U32

## Measurement NO CT/VT affected

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
1792 | 0x0700 | Info | 100 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
1792 | 0x0700 | 1 | Phase 1 Current | mA | U16
1793 | 0x0701 | 1 | Phase 2 Current | mA | U16
1794 | 0x0702 | 1 | Phase 3 Current | mA | U16
1795 | 0x0703 | 1 | Neutral Current | mA | U16
1796 | 0x0704 | 1 | Phase to Phase Voltage: U12 | V 10⁻² | U16
1797 | 0x0705 | 1 | Phase to Phase Voltage: U23 | V 10⁻² | U16
1798 | 0x0706 | 1 | Phase to Phase Voltage: U31 | V 10⁻² | U16
1799 | 0x0707 | 1 | Phase to Neutral voltage phase 1 | V 10⁻² | U16
1800 | 0x0708 | 1 | Phase to Neutral voltage phase 2 | V 10⁻² | U16
1801 | 0x0709 | 1 | Phase to Neutral voltage phase 3 | V 10⁻² | U16
1802 | 0x070A | 1 | Frequency | Hz 10⁻² | U16
1803 | 0x070B | 1 | ? active power +/- : P | W 10 | S16
1804 | 0x070C | 1 | ? reactive power +/- : Q | var 10 | S16
1805 | 0x070D | 1 | ? apparent power : S | VA 10 | U16
1806 | 0x070E | 1 | ? power factor : -: leadiing et + : lagging : PF | - / 1000 | S16
1807 | 0x070F | 1 | Active Power phase1 +/- | W 10 | S16
1808 | 0x0710 | 1 | Active Power phase2 +/- | W 10 | S16
1809 | 0x0711 | 1 | Active Power phase3 +/- | W 10 | S16
1810 | 0x0712 | 1 | Reactive Power phase1 +/- | var 10 | S16
1811 | 0x0713 | 1 | Reactive Power phase2 +/- | var 10 | S16
1812 | 0x0714 | 1 | Reactive Power phase3 +/- | var 10 | S16
1813 | 0x0715 | 1 | Apparent Power phase1 | VA 10 | U16
1814 | 0x0716 | 1 | Apparent Power phase2 | VA 10 | U16
1815 | 0x0717 | 1 | Apparent Power phase3 | VA 10 | U16
1816 | 0x0718 | 1 | Power factor phase 1 -:leading and +: lagging | - / 1000 | S16
1817 | 0x0719 | 1 | Power factor phase 2 -:leading and +: lagging | - / 1000 | S16
1818 | 0x071A | 1 | Power factor phase 3 -:leading and +: lagging | - / 1000 | S16
1819 | 0x071B | 8 | R?serv? constructeur | - | U16[]
1827 | 0x0723 | 1 | max/avg I1 | mA | U16
1828 | 0x0724 | 1 | max/avg I2 | mA | U16
1829 | 0x0725 | 1 | max/avg I3 | mA | U16
1830 | 0x0726 | 1 | max/avg ?active power + | W 10 | U16
1831 | 0x0727 | 1 | reserved | - | U16
1832 | 0x0728 | 1 | max/avg ?reactive power + | var 10 | U16
1833 | 0x0729 | 1 | Reserved | - | U16
1834 | 0x072A | 1 | max/avg ? apparent power | VA 10 | U16
1835 | 0x072B | 1 | Active Energy +<10 000 | kWh | U16
1836 | 0x072C | 1 | Active Energy +>10 000 | kWh | U16
1837 | 0x072D | 1 | Reactive Energy+< 10 000 | varh 10³ | U16
1838 | 0x072E | 1 | Reactive Energy +>10 000 | varh 10³ | U16
1839 | 0x072F | 52 | R?serv? constructeur | - | U16[]
1891 | 0x0763 | 1 | Max / AVG In | mA | U16

## Tariff Energy

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
50848 | 0xC6A0 | Info | 50 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
50848 | 0xC6A0 | 1 | Total Tariff Count | - | U8
50849 | 0xC6A1 | 1 | Current Tariff No | - | U8
50850 | 0xC6A2 | 2 | Active Energy Tariff 1 | kWh | U32
50852 | 0xC6A4 | 2 | Active Energy Tariff 2 | kWh | U32
50854 | 0xC6A6 | 12 | Reserved | - | -
50866 | 0xC6B2 | 2 | Reactive Energy Tariff 1 | varh 10³ | U32
50868 | 0xC6B4 | 2 | Reactive Energy Tariff 2 | varh 10³ | U32
50870 | 0xC6B6 | 12 | Reserved | - | -
50882 | 0xC6C2 | 16 | Reserved | - | -

## THD

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
2304 | 0x0900 | Info | 11 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
2304 | 0x0900 | 1 | I1 | % / 10 | U16
2305 | 0x0901 | 1 | I2 | % / 10 | U16
2306 | 0x0902 | 1 | I3 | % / 10 | U16
2307 | 0x0903 | 1 | Reserved | - | -
2308 | 0x0904 | 1 | U12 | % / 10 | U16
2309 | 0x0905 | 1 | U23 | % / 10 | U16
2310 | 0x0906 | 1 | U31 | % / 10 | U16
2311 | 0x0907 | 1 | V1 | % / 10 | U16
2312 | 0x0908 | 1 | V2 | % / 10 | U16
2313 | 0x0909 | 1 | V3 | % / 10 | U16
2314 | 0x090A | 1 | Reserved | - | -

# Actions

## Reset ( These values could be combine all )

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
1024 | 0x0400 | Commands | 1 | NONE | WRITE | WRITE

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
1024 | 0x0400 | 1 | Reset 0x0001 : Max3I 0x0002 : Max P+,Q+,S 0x0040 : Hour meter 0x0080 : kWh+ 0x0100 : kvarh+ 0x0200 : kVAh 0x0400 : kWh- 0x0800 : kvarh- 0x1000 : All energies | - | U16_HEX

# Monitoring

# Alarms

## Alarme

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36176 | 0x8D50 | Info | 7 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36176 | 0x8D50 | 1 | Current alarm on lower threshold cause:0 : No Alarm / 1 : I1 / 2 : I2 / 3 : I3 / 4 : IN / 5 : U12 / 6 : U23 / 7 : U31 / 8 : ?P+ / 9 : ?Q+ / 10 : ?S / 11 : F / 12 : ?PFL / 15: thdI1 / 16: thdI2 / 17 : thdI3 / 18 : thdU12 / 19 : thdU23 / 20 : thdU31 / 21 : Hour / 22: V1 / 23 : V2 / 24 : V3 / 26: thdV1 / 27 : thdV2 / 28 : thd V3 / 31 : ?PFC / 32 : ?Temperature | - / 1000 | U8
36177 | 0x8D51 | 2 | Current alarm on lower threshold : min value | - | U32
36179 | 0x8D53 | 1 | Current alarm on upper threshold cause:0 : No Alarm / 1 : I1 / 2 : I2 / 3 : I3 / 4 : IN / 5 : U12 / 6 : U23 / 7 : U31 / 8 : ?P+ / 9 : ?Q+ / 10 : ?S / 11 : F / 12 : ?PFL / 15: thdI1 / 16: thdI2 / 17 : thdI3 / 18 : thdU12 / 19 : thdU23 / 20 : thdU31 / 21 : Hour / 22: V1 / 23 : V2 / 24 : V3 / 26: thdV1 / 27 : thdV2 / 28 : thd V3 / 31 : ?PFC/ 32 : ?Temperature | - / 1000 | U8
36180 | 0x8D54 | 2 | Current alarm on upper threshold : max value | - | U32
36182 | 0x8D56 | 1 | Current alarm duration | s | U8

# Extensions

## Temperatures

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51456 | 0xC900 | Info | 8 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51456 | 0xC900 | 1 | Internal module Temperature present | - | U8
51457 | 0xC901 | 1 | Module Temperature | - | S16
51458 | 0xC902 | 1 | Number of external Temperature sensors | - | U8
51459 | 0xC903 | 1 | Reserved | - | -
51460 | 0xC904 | 1 | Reserved | - | -
51461 | 0xC905 | 1 | Reserved | - | -
51462 | 0xC906 | 1 | Reserved | - | -
51463 | 0xC907 | 1 | Reserved | - | -

## Input/Output state

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
51968 | 0xCB00 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
51968 | 0xCB00 | 1 | Input count | - | U8
51969 | 0xCB01 | 1 | Input State: Bit 0 : Input 1 Open or ClosedBit x : Input x Open or Closed | - | U8
51970 | 0xCB02 | 1 | Output count | - | U8
51971 | 0xCB03 | 1 | Output State: Bit 0 : Output 1 Open or ClosedBit x : Output x Open or Closed | - | U8

# Industrialization

## Table Indus

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36816 | 0x8FD0 | Settings | 45 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36816 | 0x8FD0 | 2 | Courant Inject? en Calib | - | U32
36818 | 0x8FD2 | 2 | Tension simple Inject? en Calib | - | U32
36820 | 0x8FD4 | 1 | Action Calib | A | U8
36821 | 0x8FD5 | 1 | Set Relais Impul | A | U8
36822 | 0x8FD6 | 1 | Clr Relais Impulsion | A | U8
36823 | 0x8FD7 | 2 | Code Constructeur | - | S32
36825 | 0x8FD9 | 4 | Coef G?n?rale Courant | A | U16[]
36829 | 0x8FDD | 4 | Coef G?n?rale Tension | A | U16[]
36833 | 0x8FE1 | 4 | D?phasage Phase 1 | A | U16[]
36837 | 0x8FE5 | 4 | D?phasage Phase 2 | A | U16[]
36841 | 0x8FE9 | 4 | D?phasage Phase 3 | A | U16[]
36845 | 0x8FED | 1 | Offset IN | - | U8
36846 | 0x8FEE | 1 | Gain IN | - | U8
36847 | 0x8FEF | 1 | Offset I1 | - | U8
36848 | 0x8FF0 | 1 | Gain I1 | - | U8
36849 | 0x8FF1 | 1 | Offset I2 | - | U8
36850 | 0x8FF2 | 1 | Gain I2 | - | U8
36851 | 0x8FF3 | 1 | Offset I3 | - | U8
36852 | 0x8FF4 | 1 | Gain I3 | - | U8
36853 | 0x8FF5 | 1 | Offset VN | - | U8
36854 | 0x8FF6 | 1 | Gain VN | - | U8
36855 | 0x8FF7 | 1 | Offset V1 | - | U8
36856 | 0x8FF8 | 1 | Gain V1 | - | U8
36857 | 0x8FF9 | 1 | Offset V2 | - | U8
36858 | 0x8FFA | 1 | Gain V2 | - | U8
36859 | 0x8FFB | 1 | Offset V3 | - | U8
36860 | 0x8FFC | 1 | Gain V3 | - | U8

## Table Indus Temperature ( only available for the Diris A10 )

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
36384 | 0x8E20 | Info | 3 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
36384 | 0x8E20 | 1 | Offset calibration ( 0 - 1024 ) | - | U8
36385 | 0x8E21 | 1 | Offset Int/Ext ( default : 0 ) | ? / 10 | U8
36386 | 0x8E22 | 1 | Valeur Convert ( N : 0-1024) | - | U8

# Legacy

## Measurement

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
2816 | 0x0B00 | Info | 40 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
2816 | 0x0B00 | 1 | Current : I1 | mA | U16
2817 | 0x0B01 | 1 | Current : I2 | mA | U16
2818 | 0x0B02 | 1 | Current : I3 | mA | U16
2819 | 0x0B03 | 1 | Neutral Current : In | mA | U16
2820 | 0x0B04 | 1 | Phase to Phase Voltage: U12 | V 10⁻² | U16
2821 | 0x0B05 | 1 | Phase to Phase Voltage: U23 | V 10⁻² | U16
2822 | 0x0B06 | 1 | Phase to Phase Voltage: U31 | V 10⁻² | U16
2823 | 0x0B07 | 1 | Simple voltage : V1 | V 10⁻² | U16
2824 | 0x0B08 | 1 | Simple voltage : V2 | V 10⁻² | U16
2825 | 0x0B09 | 1 | Simple voltage : V3 | V 10⁻² | U16
2826 | 0x0B0A | 1 | Frequency : Fr | Hz 10⁻² | U16
2827 | 0x0B0B | 1 | Total Active Power +/- : P | W 10 | S16
2828 | 0x0B0C | 1 | Total Reactive Power +/- : Q | var 10 | S16
2829 | 0x0B0D | 1 | Total apparent power : S | VA 10 | U16
2830 | 0x0B0E | 1 | ? Power factor : -: capacitif et + : inductif : PF | - / 1000 | S16
2831 | 0x0B0F | 1 | I 1 AVG MAX | mA | U16
2832 | 0x0B10 | 1 | I 2 AVG MAX | mA | U16
2833 | 0x0B11 | 1 | I 3 AVG MAX | mA | U16
2834 | 0x0B12 | 1 | In AVG MAX | mA | U16
2835 | 0x0B13 | 1 | P+ AVG MAX | W 10 | U16
2836 | 0x0B14 | 1 | Active Energy +<10 000 | kWh | U16
2837 | 0x0B15 | 1 | Active Energy +>10 000 | kWh | U16
2838 | 0x0B16 | 1 | Reactive Energy+< 10 000 | varh 10³ | U16
2839 | 0x0B17 | 1 | Reactive Energy +>10 000 | varh 10³ | U16
2840 | 0x0B18 | 1 | Hour Meter +<10000 | h 10⁻² | U16
2841 | 0x0B19 | 1 | Hour Meter +>10000 | h 10⁻² | U16
2842 | 0x0B1A | 1 | Active Power phase1 +/- | W 10 | S16
2843 | 0x0B1B | 1 | Active Power phase2 +/- | W 10 | S16
2844 | 0x0B1C | 1 | Active Power phase3 +/- | W 10 | S16
2845 | 0x0B1D | 1 | Reactive Power phase1 +/- | var 10 | S16
2846 | 0x0B1E | 1 | Reactive Power phase2 +/- | var 10 | S16
2847 | 0x0B1F | 1 | Reactive Power phase3 +/- | var 10 | S16
2848 | 0x0B20 | 1 | Apparent Power phase1 | VA 10 | U16
2849 | 0x0B21 | 1 | Apparent Power phase2 | VA 10 | U16
2850 | 0x0B22 | 1 | Apparent Power phase3 | VA 10 | U16
2851 | 0x0B23 | 1 | Power factor phase 1-: leading and +: lagging | - / 1000 | S16
2852 | 0x0B24 | 1 | Power factor phase 2-: leading and +: lagging | - / 1000 | S16
2853 | 0x0B25 | 1 | Power factor phase 3-: leading and +: lagging | - / 1000 | S16
2854 | 0x0B26 | 1 | Q+ AVG MAX | var 10 | U16
2855 | 0x0B27 | 1 | S AVG MAX | VA 10 | U16

## Alarme

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
1280 | 0x0500 | Info | 7 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
1280 | 0x0500 | 1 | Current alarm on lower threshold cause:0 : No Alarm / 1 : I1 / 2 : I2 / 3 : I3 / 4 : IN / 5 : U12 / 6 : U23 / 7 : U31 / 8 : ?P+ / 9 : ?Q+ / 10 : ?S / 11 : F / 12 : ?PFL / 15: thdI1 / 16: thdI2 / 17 : thdI3 / 18 : thdU12 / 19 : thdU23 / 20 : thdU31 / 21 : Hour / 22: V1 / 23 : V2 / 24 : V3 / 26: thdV1 / 27 : thdV2 / 28 : thd V3 / 31 : ?PFC/ 32 : ?Temperature | - / 1000 | U8
1281 | 0x0501 | 2 | Current alarm on lower threshold : min value | - | S32
1283 | 0x0503 | 1 | Current alarm on upper threshold cause:0 : No Alarm / 1 : I1 / 2 : I2 / 3 : I3 / 4 : IN / 5 : U12 / 6 : U23 / 7 : U31 / 8 : ?P+ / 9 : ?Q+ / 10 : ?S / 11 : F / 12 : ?PFL / 15: thdI1 / 16: thdI2 / 17 : thdI3 / 18 : thdU12 / 19 : thdU23 / 20 : thdU31 / 21 : Hour / 22: V1 / 23 : V2 / 24 : V3 / 26: thdV1 / 27 : thdV2 / 28 : thd V3 / 31 : ?PFC/ 32 : ?Temperature | - / 1000 | U8
1284 | 0x0504 | 2 | Current alarm on upper threshold : max value | - | S32
1286 | 0x0506 | 1 | Current alarm duration | s | U8

## Option

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
256 | 0x0100 | Info | 4 | NONE | READ | READ

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
256 | 0x0100 | 1 | Reserved | - | -
257 | 0x0101 | 1 | Reserved | - | -
258 | 0x0102 | 1 | Reserved | - | -
259 | 0x0103 | 1 | Reserved | - | -

## Setup

Dec start address | Hex start address | Type | Size | Lock level | Locked fcts | Unlocked fcts
--- | --- | --- | --- | --- | --- | ---
512 | 0x0200 | Settings | 108 | NONE | READ | WRITE | WRITE_MANY | READ | WRITE | WRITE_MANY

Dec address | Hex address | Words count | Description | Unit | Data type
--- | --- | --- | --- | --- | ---
512 | 0x0200 | 1 | Network Type :0 : 1BL 1 : 2BL 2 : 3BL 3 : 3NBL 4 : 4BL 5 : 4NBL | - | U8
513 | 0x0201 | 1 | Current Transformer secondary : 1: 1 A 5: 5 A | A | U8
514 | 0x0202 | 1 | Current Transformer primary | A | U8
515 | 0x0203 | 4 | Reserved | - | U16[]
519 | 0x0207 | 1 | Synchronisation of I AVG/MAX: Synchronisation of I AVG/MAX:2 : 2 seconds 5 : 5 minutes 8 : 8 minutes 10 : 10 Minutes 15 : 15 minutes 20 : 20 minutes 30 : 30 minutes 60 : 60 minutes | - | U8
520 | 0x0208 | 1 | Synchronisation of P/Q/S AVG/MAXSynchronisation of I AVG/MAX:2 : 2 seconds 5 : 5 minutes 8 : 8 minutes 10 : 10 Minutes 15 : 15 minutes 20 : 20 minutes 30 : 30 minutes 60 : 60 minutes | - | U8
521 | 0x0209 | 1 | OUT : pulse output allocation :0 : kWh+1 : kvarh +2 :Alarm3 : Command | - | U8
522 | 0x020A | 1 | OUT : pulse output value :0 : 0,1 kWh/kvarh1 : 1 kWh/kvarh2 : 10 kWh/kvarh3 : 100 kWh/kvarh4 : 1000 kWh/kvarh5 : 10000 kWh/kvarh | - | U8
523 | 0x020B | 1 | OUT : pulse output duration :1 : 100ms2 : 200ms3 : 300ms4 : 400ms5 : 500ms6 : 600ms7 : 700ms8 : 800ms9 : 900ms | - | U8
524 | 0x020C | 27 | R?serve Constructeur | - | U16[]
551 | 0x0227 | 1 | Alarm Type :1 : I2 : In3 : U4 : V5 : ?P+6 : ?Q+7 : ?S+8 : ?PFC9 : ?PFL10 : THDU11 : THDV12 : THDI13 : HOUR14 : F 15 : Temperature | - | U8
552 | 0x0228 | 1 | Alarm upper Threshold | - | U16
553 | 0x0229 | 1 | Reserved | - | U8
554 | 0x022A | 1 | Alarm Lower Threshold | - | U16
555 | 0x022B | 1 | Reserved | - | U8
556 | 0x022C | 1 | Alarm Hysteresis(0-99) | - | U8
557 | 0x022D | 1 | Alarm Specified time (1-999) | - | U16
558 | 0x022E | 1 | Relay State :0 : Normally Open1 : Normally Closed | - | U8
559 | 0x022F | 58 | Reserved | - | U16[]
617 | 0x0269 | 1 | Hour meter allocation1 : Auxiliary power supply2 : Currents3 : phase to phase voltage4 : Input 1 | - | U8
618 | 0x026A | 1 | Hour meter trigger threshold | - | U16
619 | 0x026B | 1 | Reserved | - | U8