= IO Analog Controller

Controller that sets a analog output according to the configured inputs to OFF|AUTOMATIC|ON.

In AUTOMATIC mode the output is set dynamically depending on the current surplus power.
 
https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.controller.io.analog[Source Code icon:github[]]