= Hybrid-Ess Surplus-Feed-To-Grid Controller

Controls a Hybrid Battery Inverter (i.e. integrated Energy Storage System) so, that the surplus DC production of its chargers gets fed to grid.

https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.controller.ess.hybrid.surplusfeedtogrid[Source Code icon:github[]]