= ESS Fix State Of Charge

Sets active power constraints for charging/discharging of a symmetric energy storage system, to reach a final SoC under the constraints below.

- State of Charge should be reached at a certain time or as fast as possible
- State of Charge is held for a configured time or optionally until a specific end condition is fulfilled


https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.controller.ess.fixstateofcharge[Source Code icon:github[]]