= IO Channel-Single-Threshold

Generic Controller that sets a digital output according to the value of given Channel -- e.g., turn a relay on or off, when configured input channel/SoC is above or below a given threshold respectively.

Documentation: https://docs.fenecon.de/en/fems/fems-app/App_Schwellwertsteuerung.html

https://github.com/OpenEMS/openems/tree/develop/io.openems.edge.controller.io.channelsinglethreshold[Source Code icon:github[]]
