# USB Echo
Read from USB input and write to output

## Resources
- https://github.com/esp-rs/esp-idf-hal/issues/200#issuecomment-1483922405

## TODO
- Once a safe Rust API is available, replace the unsafe C calls with safe Rust calls