# ISC License
#
# Copyright (C) 2024 Microchip Technology Inc. and its subsidiaries
#
# Permission to use, copy, modify, and/or distribute this software for any
# purpose with or without fee is hereby granted, provided that the above
# copyright notice and this permission notice appear in all copies.
#
# THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
# WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
# MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
# ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
# WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
# ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
# OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.

# asynchronous read
ram block $__uSRAM_AR_ {

	#(LSRAM cost)/3
	cost 43;

	# INIT supported
	init any;

	abits 6;
	widths 12 per_port;

	# single write enable wire
	port sw "W" {
		clock posedge;

		# collision not supported, but write takes precedence and read data is invalid while writing to
		# the same address
		wrtrans all new;

		optional;
	}
	port ar "R" {
		optional;
	}
}

# synchronous read
# NOTE: synchronous read can be realized by the address pipeline register or data pipeline register.
#		This assumes address is synchronized
ram block $__uSRAM_SR_ {

	cost 42;

	init any;
	abits 6;
widths 12 per_port;

	port sw "W" {
		clock posedge;

		# collision not supported
		wrtrans all new;

		optional;
	}
	port sr "R" {
		clock posedge;
		rden;
		rdinit none;
		optional;
	}
}
