A simple example design, based on the Numato Labs Mimas V2 board
================================================================

This example uses Yosys for synthesis and Xilinx ISE
for place&route and bit-stream creation.

To synthesize:
  bash run.sh
