Internal formats
================

Yosys uses two different internal formats. The first is used to store an
abstract syntax tree (AST) of a Verilog input file. This format is simply called
AST and is generated by the Verilog Frontend. This data structure is consumed by
a subsystem called AST Frontend [1]_. This AST Frontend then generates a design
in Yosys' main internal format, the
Register-Transfer-Level-Intermediate-Language (RTLIL) representation. It does
that by first performing a number of simplifications within the AST
representation and then generating RTLIL from the simplified AST data structure.

The RTLIL representation is used by all passes as input and outputs. This has
the following advantages over using different representational formats between
different passes:

-  The passes can be rearranged in a different order and passes can be removed
   or inserted.

-  Passes can simply pass-thru the parts of the design they don't change without
   the need to convert between formats. In fact Yosys passes output the same
   data structure they received as input and performs all changes in place.

-  All passes use the same interface, thus reducing the effort required to
   understand a pass when reading the Yosys source code, e.g. when adding
   additional features.

The RTLIL representation is basically a netlist representation with the
following additional features:

-  An internal cell library with fixed-function cells to represent RTL datapath
   and register cells as well as logical gate-level cells (single-bit gates and
   registers).

-  Support for multi-bit values that can use individual bits from wires as well
   as constant bits to represent coarse-grain netlists.

-  Support for basic behavioural constructs (if-then-else structures and
   multi-case switches with a sensitivity list for updating the outputs).

-  Support for multi-port memories.

The use of RTLIL also has the disadvantage of having a very powerful format
between all passes, even when doing gate-level synthesis where the more advanced
features are not needed. In order to reduce complexity for passes that operate
on a low-level representation, these passes check the features used in the input
RTLIL and fail to run when unsupported high-level constructs are used. In such
cases a pass that transforms the higher-level constructs to lower-level
constructs must be called from the synthesis script first.

.. toctree::
   :maxdepth: 3

   rtlil_rep

.. [1]
   In Yosys the term pass is only used to refer to commands that operate on the
   RTLIL data structure.
