ADDRESS   :0x4de3c
LEN_BYTES :25
ORIGINAL  :#3df3ff # Kanal Status[END]
TRANSLATED:#3df3ff # CH Status[END]

ADDRESS   :0x4ef90
LEN_BYTES :10
ORIGINAL  :Hauptmenü[END]
TRANSLATED:Allgemein[END]

ADDRESS   :0x4f564
LEN_BYTES :10
ORIGINAL  :Hauptmenü[END]
TRANSLATED:Allgemein[END]

ADDRESS   :0x4ef9c
LEN_BYTES :20
ORIGINAL  :Modell Einstellungen[END]
TRANSLATED:Modell[END]

ADDRESS   :0x4f5c4
LEN_BYTES :20
ORIGINAL  :Modell Einstellungen[END]
TRANSLATED:Modell[END]

ADDRESS   :0x81cc
LEN_BYTES :20
ORIGINAL  :Modell Einstellungen[END]
TRANSLATED:Modell[END]

ADDRESS   :0x4efb4
LEN_BYTES :28
ORIGINAL  :Fernsteuerungs Einstellungen[END]
TRANSLATED:Fernbedienung[END]

ADDRESS   :0x4fa40
LEN_BYTES :28
ORIGINAL  :Fernsteuerungs Einstellungen[END]
TRANSLATED:Fernbedienung[END]

ADDRESS   :0x4efd4
LEN_BYTES :21
ORIGINAL  :Receiver installiert.[END]
TRANSLATED:Empfänger[END]

ADDRESS   :0x4fadc
LEN_BYTES :21
ORIGINAL  :Receiver installiert.[END]
TRANSLATED:Empfänger[END]

ADDRESS   :0x7cb8
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:CH [END]

ADDRESS   :0xa228
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:CH [END]

ADDRESS   :0x1373c
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:CH [END]

ADDRESS   :0x150e8
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:CH [END]

ADDRESS   :0x1a290
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:CH [END]

ADDRESS   :0xd774
LEN_BYTES :7
ORIGINAL  :Zurück[END]
TRANSLATED:Rück[END]

ADDRESS   :0xd7a4
LEN_BYTES :9
ORIGINAL  :Vorwärts[END]
TRANSLATED:Vorw[END]

ADDRESS   :0x18a9c
LEN_BYTES :14
ORIGINAL  :Schlüssel Typ[END]
TRANSLATED:Schaltertyp[END]

ADDRESS   :0x18b24
LEN_BYTES :52
ORIGINAL  :Selbstverriegelnd
Momenttaster
Dreistufen
Vierstufen[END]
TRANSLATED:Schalter
Druck
Drei-Zustand
Vier-Zustand[END]

ADDRESS   :0x1a234
LEN_BYTES :14
ORIGINAL  :Überschreiben[END]
TRANSLATED:Zuordnung[END]

ADDRESS   :0x8d98
LEN_BYTES :4
COMMENT   :Should be fine, there are nulls past this string
ORIGINAL  :Sart[END]
TRANSLATED:Starten[END]

ADDRESS   :0x8d20
LEN_BYTES :12
ORIGINAL  :Speed Regler[END]
TRANSLATED:Tempomat[END]

ADDRESS   :0x19510
LEN_BYTES :7
ORIGINAL  :Kanal 1[END]
TRANSLATED:CH 1[END]

ADDRESS   :0x96bc
LEN_BYTES :7
ORIGINAL  :Kanal 2[END]
TRANSLATED:CH 2[END]

ADDRESS   :0x177a0
LEN_BYTES :7
ORIGINAL  :Kanal 3[END]
TRANSLATED:CH 3[END]

ADDRESS   :0x19534
LEN_BYTES :7
ORIGINAL  :Kanal 4[END]
TRANSLATED:CH 4[END]

ADDRESS   :0x122cc
LEN_BYTES :7
ORIGINAL  :Kanal 8[END]
TRANSLATED:CH 8[END]

ADDRESS   :0x24170
LEN_BYTES :8
ORIGINAL  :Kanal 10[END]
TRANSLATED:CH 10[END]

ADDRESS   :0xbc58
LEN_BYTES :9
ORIGINAL  :Standard-[END]
TRANSLATED:Vorwahl [END]

ADDRESS   :0xf920
LEN_BYTES :9
ORIGINAL  :Standard-[END]
TRANSLATED:Vorwahl [END]

ADDRESS   :0xf48c
LEN_BYTES :15
ORIGINAL  :Gas/Brems Kurve[END]
TRANSLATED:Gas Kurve[END]

ADDRESS   :0x11cf0
LEN_BYTES :9
ORIGINAL  :Gyromodus[END]
TRANSLATED:Gyroskop[END]

ADDRESS   :0x11d54
LEN_BYTES :11
ORIGINAL  :Einschalten[END]
TRANSLATED:Starten[END]

ADDRESS   :0x121e4
LEN_BYTES :13
ORIGINAL  :Einstellknopf[END]
TRANSLATED:Setting[END]

ADDRESS   :0x12264
LEN_BYTES :14
ORIGINAL  :Aktueller Wert[END]
TRANSLATED:Wert[END]

ADDRESS   :0x14e10
LEN_BYTES :12
COMMENT   :Should be fine, there are nulls past this string
ORIGINAL  :Antriebsrate[END]
TRANSLATED:Vorwärtsrate[END]

ADDRESS   :0x14e60
LEN_BYTES :9
COMMENT   :Should be fine, there are nulls past this string
ORIGINAL  :Bremsrate[END]
TRANSLATED:Rücksrate[END]

ADDRESS   :0x14eac
LEN_BYTES :12
ORIGINAL  :Linke Stufe [END]
TRANSLATED:Linke
Rate[END]

ADDRESS   :0x14efc
LEN_BYTES :12
ORIGINAL  :Rechte Stufe[END]
TRANSLATED:Rechte
Rate[END]

ADDRESS   :0x177cc
LEN_BYTES :15
ORIGINAL  :Steigerungsrate[END]
TRANSLATED:Aufwärts[END]

ADDRESS   :0x8238
LEN_BYTES :14
ORIGINAL  :Modell Auswahl[END]
TRANSLATED:Modell Wahl[END]

ADDRESS   :0x88a0
LEN_BYTES :21
ORIGINAL  :Modell zurücksetzten[END]
TRANSLATED:Modell zurückset.[END]

ADDRESS   :0xa7dc
LEN_BYTES :16
ORIGINAL  :Trainings Modell[END]
TRANSLATED:Trainings Modus[END]

ADDRESS   :0xad18
LEN_BYTES :20
ORIGINAL  :Gashebel Einstellung[END]
TRANSLATED:Gas Einstellung[END]

ADDRESS   :0xb244
ORIGINAL  :Stop/Zurücksetzen Knopf[END]
TRANSLATED:Stop/Zzr. Knopf[END]

ADDRESS   :0xb348
LEN_BYTES :29
ORIGINAL  :Schließen
Helligkeit
Dynamik[END]
TRANSLATED:Aus
Statik
Dynamik[END]

ADDRESS   :0xe774
LEN_BYTES :15
ORIGINAL  :Startton An/Aus[END]
TRANSLATED:Startton[END]

ADDRESS   :0xe7e0
LEN_BYTES :9
ORIGINAL  :Singalton[END]
TRANSLATED:Signalton[END]

ADDRESS   :0xec14
LEN_BYTES :20
ORIGINAL  :Stumm
Nur Alarm
Alle[END]
TRANSLATED:Aus
Nur Alarm
Alle[END]

ADDRESS   :0xefbc
LEN_BYTES :40
ORIGINAL  :Schließen
1 min 
3 min 
10 min 
30 min [END]
TRANSLATED:Aus
1 min
3 min
10 min
30 min[END]

ADDRESS   :0x1d714
LEN_BYTES :14
ORIGINAL  :Leerlauf Alarm[END]
TRANSLATED:Leerlauf Alm[END]

ADDRESS   :0x1d780
LEN_BYTES :34
ORIGINAL  :Schließen 
15 min 
30 min 
60 min[END]
TRANSLATED:Aus
15 min
30 min
60 min[END]

ADDRESS   :0x1dc68
LEN_BYTES :54
ORIGINAL  :Schließen 
Leerlauf 5 m 
Leerlauf 10 m 
Leerlauf 20 m[END]
TRANSLATED:Aus
Leerlauf 5 m
Leerlauf 10 m
Leerlauf 20 m[END]

ADDRESS   :0x1ddc0
LEN_BYTES :14
ORIGINAL  :Spannung Alarm[END]
TRANSLATED:Spannung Alm[END]

ADDRESS   :0x130b0
LEN_BYTES :17
ORIGINAL  :Aktuelle Spannung[END]
TRANSLATED:Spannung Akt.[END]

ADDRESS   :0x1e2d4
LEN_BYTES :20
ORIGINAL  :Spannung Kalibrieren[END]
TRANSLATED:Spannung Kalib[END]

ADDRESS   :0x144cc
LEN_BYTES :36
ORIGINAL  :Zurücksetzen auf Werkseinstellungen[END]
TRANSLATED:Werkreset[END]

ADDRESS   :0x1fe70
LEN_BYTES :11
ORIGINAL  :RF abkommen[END]
TRANSLATED:RF Stand.[END]

ADDRESS   :0x3bb8
LEN_BYTES :9
ORIGINAL  :Gyromodus[END]
TRANSLATED:Gyroskop[END]

ADDRESS   :0x19984
LEN_BYTES :12
ORIGINAL  :Linke Stufe [END]
TRANSLATED:Links[END]

ADDRESS   :0x19a40
LEN_BYTES :12
ORIGINAL  :Rechte Stufe[END]
TRANSLATED:Rechts[END]

ADDRESS   :0x23738
LEN_BYTES :24
ORIGINAL  :Servoarm-Schwenkregelung[END]
TRANSLATED:Servoschwenk[END]

ADDRESS   :0x23c50
LEN_BYTES :13
ORIGINAL  :Umschalttaste[END]
TRANSLATED:Starten[END]

ADDRESS   :0x23cd4
LEN_BYTES :15
ORIGINAL  :Geschwindigkeit[END]
TRANSLATED:Tempo[END]
