ADDRESS   :0x143e0
LEN_BYTES :54
ORIGINAL  :官网: www.dumborc.com

硬件: V1.0.0
软件: V1.1.9[END]
TRANSLATED:官网:
www.dumborc.com
软件: V1.1.9
ELynx V0.8.3a[END]

ADDRESS   :0x1441c
LEN_BYTES :60
ORIGINAL  :Über uns:
www.dumborc.com
Hardware: V1.0.0
Software: V1.1.9[END]
TRANSLATED:Über uns:
www.dumborc.com
Software: V1.1.9
ELynx V0.8.3a[END]

ADDRESS   :0x14464
LEN_BYTES :59
ORIGINAL  :About Us:
www.dumborc.com
Hardware: V1.0.0
Software: V1.1.9[END]
TRANSLATED:About Us:
www.dumborc.com
Software: V1.1.9
ELynx V0.8.3a[END]

ADDRESS   :0x6f0c8
LEN_BYTES :70
ORIGINAL  :À propos de nous:
www.dumborc.com
Matériel: V1.0.0
Logiciels: V1.1.9[END]
TRANSLATED:À propos de nous:
www.dumborc.com
Logiciels: V1.1.9
ELynx V0.8.3a[END]

ADDRESS   :0x6f110
LEN_BYTES :83
ORIGINAL  :サポート:
www.dumborc.com
ハードウェア: V1.0.0
ソフトウェア: V1.1.9[END]
TRANSLATED:サポート:
www.dumborc.com
ソフトウェア: V1.1.9
ELynx V0.8.3a[END]

ADDRESS   :0x4fcfc
LEN_BYTES :44
ORIGINAL  :English
简体中文
Germany
French
Japanese[END]
TRANSLATED:English
简体中文
Deutsch
French
Japanese[END]

ADDRESS   :0x1f2a8
LEN_BYTES :4
ORIGINAL  :%s ![END]
TRANSLATED:%s[END]

ADDRESS   :0x1f2b0
LEN_BYTES :46
ORIGINAL  :Only P series receivers support this interface[END]
TRANSLATED:Only for P series receivers![END]

ADDRESS   :0x20138
LEN_BYTES :4
ORIGINAL  :%s ![END]
TRANSLATED:%s[END]

ADDRESS   :0x20140
LEN_BYTES :46
ORIGINAL  :Only P series receivers support this interface[END]
TRANSLATED:Only for P series receivers![END]

ADDRESS   :0x21e54
LEN_BYTES :12
ORIGINAL  :Rudder Speed[END]
TRANSLATED:Servo Freq.[END]

ADDRESS   :0x1abf0
LEN_BYTES :1
ORIGINAL  :M[END]
TRANSLATED:L[END]

ADDRESS   :0x1b058
LEN_BYTES :1
ORIGINAL  :S[END]
TRANSLATED:F[END]

ADDRESS   :0x1c388
LEN_BYTES :1
ORIGINAL  :M[END]
TRANSLATED:L[END]

ADDRESS   :0x1c7f0
LEN_BYTES :1
ORIGINAL  :S[END]
TRANSLATED:F[END]
