ADDRESS   :0x698
LEN_BYTES :6
ORIGINAL  :xTFI[END]
TRANSLATED:xTFI[END]

ADDRESS   :0x6dc
LEN_BYTES :4
ORIGINAL  :zD2[END]
TRANSLATED:zD2[END]

ADDRESS   :0x868
LEN_BYTES :4
ORIGINAL  :!0K[END]
TRANSLATED:!0K[END]

ADDRESS   :0xee8
LEN_BYTES :6
ORIGINAL  :𵅰F[END]
TRANSLATED:𵅰F[END]

ADDRESS   :0xfd8
LEN_BYTES :6
ORIGINAL  :%d.%dV[END]
TRANSLATED:%d.%dV[END]

ADDRESS   :0x1014
LEN_BYTES :6
ORIGINAL  ::Ip:H[END]
TRANSLATED::Ip:H[END]

ADDRESS   :0x1464
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x153c
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x16b4
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x178c
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x1c8c
LEN_BYTES :4
ORIGINAL  :cтH[END]
TRANSLATED:cтH[END]

ADDRESS   :0x1f8c
LEN_BYTES :12
ORIGINAL  :#24d8a8 #[END]
TRANSLATED:#24d8a8 #[END]

ADDRESS   :0x20c8
LEN_BYTES :6
ORIGINAL  :!IpH[END]
TRANSLATED:!IpH[END]

ADDRESS   :0x248c
LEN_BYTES :10
ORIGINAL  :2:ID1 %X

[END]
TRANSLATED:2:ID1 %X

[END]

ADDRESS   :0x2498
LEN_BYTES :10
ORIGINAL  :2:ID2 %X

[END]
TRANSLATED:2:ID2 %X

[END]

ADDRESS   :0x24a4
LEN_BYTES :10
ORIGINAL  :2:ID3 %X

[END]
TRANSLATED:2:ID3 %X

[END]

ADDRESS   :0x24b0
LEN_BYTES :13
ORIGINAL  :2:Secret %X

[END]
TRANSLATED:2:Secret %X

[END]

ADDRESS   :0x24c0
LEN_BYTES :20
ORIGINAL  :2:Rolling_code:%X 

[END]
TRANSLATED:2:Rolling_code:%X 

[END]

ADDRESS   :0x24d8
LEN_BYTES :34
ORIGINAL  :2:Hardware_version_code ADDR: %s

[END]
TRANSLATED:2:Hardware_version_code ADDR: %s

[END]

ADDRESS   :0x24fc
LEN_BYTES :15
ORIGINAL  :Check Error !

[END]
TRANSLATED:Check Error !

[END]

ADDRESS   :0x250c
LEN_BYTES :12
ORIGINAL  :Check OK .

[END]
TRANSLATED:Check OK .

[END]

ADDRESS   :0x2698
LEN_BYTES :4
ORIGINAL  :EѐH[END]
TRANSLATED:EѐH[END]

ADDRESS   :0x2790
LEN_BYTES :4
ORIGINAL  :ĲVH[END]
TRANSLATED:ĲVH[END]

ADDRESS   :0x2850
LEN_BYTES :6
ORIGINAL  :0Hx1H[END]
TRANSLATED:0Hx1H[END]

ADDRESS   :0x2bf4
LEN_BYTES :12
ORIGINAL  :HdHHdpG#gE[END]
TRANSLATED:HdHHdpG#gE[END]

ADDRESS   :0x2cd0
LEN_BYTES :4
ORIGINAL  : pjH[END]
TRANSLATED: pjH[END]

ADDRESS   :0x2d28
LEN_BYTES :4
ORIGINAL  : pXH[END]
TRANSLATED: pXH[END]

ADDRESS   :0x2eb0
LEN_BYTES :4
ORIGINAL  : p2H[END]
TRANSLATED: p2H[END]

ADDRESS   :0x3b74
LEN_BYTES :4
ORIGINAL  :5I4H[END]
TRANSLATED:5I4H[END]

ADDRESS   :0x3b80
LEN_BYTES :4
ORIGINAL  :L!1H[END]
TRANSLATED:L!1H[END]

ADDRESS   :0x3bac
LEN_BYTES :9
ORIGINAL  :陀螺仪[END]
TRANSLATED:陀螺仪[END]

ADDRESS   :0x3bb8
LEN_BYTES :9
ORIGINAL  :Gyromodus[END]
TRANSLATED:Gyromodus[END]

ADDRESS   :0x3bc4
LEN_BYTES :10
ORIGINAL  :gyromètre[END]
TRANSLATED:gyromètre[END]

ADDRESS   :0x3bd0
LEN_BYTES :12
ORIGINAL  :ジャイロ[END]
TRANSLATED:ジャイロ[END]

ADDRESS   :0x3be0
LEN_BYTES :4
ORIGINAL  :Gyro[END]
TRANSLATED:Gyro[END]

ADDRESS   :0x3bf4
LEN_BYTES :6
ORIGINAL  :相位[END]
TRANSLATED:相位[END]

ADDRESS   :0x3bfc
LEN_BYTES :5
ORIGINAL  :Phase[END]
TRANSLATED:Phase[END]

ADDRESS   :0x3c04
LEN_BYTES :12
ORIGINAL  :フェーズ[END]
TRANSLATED:フェーズ[END]

ADDRESS   :0x3c18
LEN_BYTES :12
ORIGINAL  :感度通道[END]
TRANSLATED:感度通道[END]

ADDRESS   :0x3c28
LEN_BYTES :6
ORIGINAL  :Sen CH[END]
TRANSLATED:Sen CH[END]

ADDRESS   :0x3c30
LEN_BYTES :21
ORIGINAL  :感度チャンネル[END]
TRANSLATED:感度チャンネル[END]

ADDRESS   :0x3f54
LEN_BYTES :4
ORIGINAL  :MIaH[END]
TRANSLATED:MIaH[END]

ADDRESS   :0x4048
LEN_BYTES :41
ORIGINAL  :NULL
CH2
CH3
CH4
CH5
CH6
CH7
CH8
CH9
CH10[END]
TRANSLATED:NULL
CH2
CH3
CH4
CH5
CH6
CH7
CH8
CH9
CH10[END]

ADDRESS   :0x4094
LEN_BYTES :9
ORIGINAL  :灵敏度[END]
TRANSLATED:灵敏度[END]

ADDRESS   :0x40a4
LEN_BYTES :6
ORIGINAL  :感度[END]
TRANSLATED:感度[END]

ADDRESS   :0x40b8
LEN_BYTES :7
ORIGINAL  :%d.%d%s[END]
TRANSLATED:%d.%d%s[END]

ADDRESS   :0x40c8
LEN_BYTES :15
ORIGINAL  :手轮介入比[END]
TRANSLATED:手轮介入比[END]

ADDRESS   :0x42fc
LEN_BYTES :9
ORIGINAL  :缓回中[END]
TRANSLATED:缓回中[END]

ADDRESS   :0x44c8
LEN_BYTES :4
ORIGINAL  :V1.1[END]
TRANSLATED:V1.1[END]

ADDRESS   :0x44d8
LEN_BYTES :10
ORIGINAL  :ID1:%04X

[END]
TRANSLATED:ID1:%04X

[END]

ADDRESS   :0x44e4
LEN_BYTES :10
ORIGINAL  :ID2:%04X

[END]
TRANSLATED:ID2:%04X

[END]

ADDRESS   :0x44f0
LEN_BYTES :10
ORIGINAL  :ID3:%04X

[END]
TRANSLATED:ID3:%04X

[END]

ADDRESS   :0x44fc
LEN_BYTES :11
ORIGINAL  :CODE:%04X

[END]
TRANSLATED:CODE:%04X

[END]

ADDRESS   :0x4508
LEN_BYTES :18
ORIGINAL  :u32RollCode:%04X

[END]
TRANSLATED:u32RollCode:%04X

[END]

ADDRESS   :0x4d90
LEN_BYTES :4
ORIGINAL  :転H[END]
TRANSLATED:転H[END]

ADDRESS   :0x4e50
LEN_BYTES :6
ORIGINAL  :uIpuH[END]
TRANSLATED:uIpuH[END]

ADDRESS   :0x4f18
LEN_BYTES :4
ORIGINAL  :CIp[END]
TRANSLATED:CIp[END]

ADDRESS   :0x4f6c
LEN_BYTES :6
ORIGINAL  :.Ip.H[END]
TRANSLATED:.Ip.H[END]

ADDRESS   :0x540c
LEN_BYTES :6
ORIGINAL  :ќ[END]
TRANSLATED:ќ[END]

ADDRESS   :0x544c
LEN_BYTES :6
ORIGINAL  :ј=[END]
TRANSLATED:ј=[END]

ADDRESS   :0x5cc0
LEN_BYTES :6
ORIGINAL  :xIpvH[END]
TRANSLATED:xIpvH[END]

ADDRESS   :0x5ce4
LEN_BYTES :6
ORIGINAL  :oIpmH[END]
TRANSLATED:oIpmH[END]

ADDRESS   :0x5d08
LEN_BYTES :6
ORIGINAL  :fIpfH[END]
TRANSLATED:fIpfH[END]

ADDRESS   :0x5d14
LEN_BYTES :4
ORIGINAL  :deH[END]
TRANSLATED:deH[END]

ADDRESS   :0x6c00
LEN_BYTES :7
ORIGINAL  :提示:[END]
TRANSLATED:提示:[END]

ADDRESS   :0x6c10
LEN_BYTES :10
ORIGINAL  :Hinweis...[END]
TRANSLATED:Hinweis...[END]

ADDRESS   :0x6c1c
LEN_BYTES :11
ORIGINAL  :Remarque...[END]
TRANSLATED:Remarque...[END]

ADDRESS   :0x6c28
LEN_BYTES :9
ORIGINAL  :通知...[END]
TRANSLATED:通知...[END]

ADDRESS   :0x6c34
LEN_BYTES :7
ORIGINAL  :Hint...[END]
TRANSLATED:Hint...[END]

ADDRESS   :0x6c3c
LEN_BYTES :7
ORIGINAL  :警告![END]
TRANSLATED:警告![END]

ADDRESS   :0x6c44
LEN_BYTES :8
ORIGINAL  :Warnung![END]
TRANSLATED:Warnung![END]

ADDRESS   :0x6c50
LEN_BYTES :7
ORIGINAL  :Alarme![END]
TRANSLATED:Alarme![END]

ADDRESS   :0x6c58
LEN_BYTES :8
ORIGINAL  :Warning![END]
TRANSLATED:Warning![END]

ADDRESS   :0x6c68
LEN_BYTES :14
ORIGINAL  :复制成功.
[END]
TRANSLATED:复制成功.
[END]

ADDRESS   :0x6c7c
LEN_BYTES :11
ORIGINAL  :Model %d
%s[END]
TRANSLATED:Model %d
%s[END]

ADDRESS   :0x6c88
LEN_BYTES :15
ORIGINAL  :Kopie erfolgr. [END]
TRANSLATED:Kopie erfolgr. [END]

ADDRESS   :0x6c98
LEN_BYTES :12
ORIGINAL  :Modell %d
%s[END]
TRANSLATED:Modell %d
%s[END]

ADDRESS   :0x6ca8
LEN_BYTES :16
ORIGINAL  :Copie réussie. [END]
TRANSLATED:Copie réussie. [END]

ADDRESS   :0x6cbc
LEN_BYTES :13
ORIGINAL  :Modèle %d
%s[END]
TRANSLATED:Modèle %d
%s[END]

ADDRESS   :0x6ccc
LEN_BYTES :15
ORIGINAL  :コピー完了[END]
TRANSLATED:コピー完了[END]

ADDRESS   :0x6cdc
LEN_BYTES :15
ORIGINAL  :モデル %d
%s[END]
TRANSLATED:モデル %d
%s[END]

ADDRESS   :0x6cec
LEN_BYTES :14
ORIGINAL  :Copy success. [END]
TRANSLATED:Copy success. [END]

ADDRESS   :0x6cfc
LEN_BYTES :14
ORIGINAL  :粘贴成功.
[END]
TRANSLATED:粘贴成功.
[END]

ADDRESS   :0x6d1c
LEN_BYTES :13
ORIGINAL  :Model %d 
 %s[END]
TRANSLATED:Model %d 
 %s[END]

ADDRESS   :0x6d2c
LEN_BYTES :14
ORIGINAL  :Einf. Erfolgr.[END]
TRANSLATED:Einf. Erfolgr.[END]

ADDRESS   :0x6d48
LEN_BYTES :15
ORIGINAL  : Modell %d 
 %s[END]
TRANSLATED: Modell %d 
 %s[END]

ADDRESS   :0x6d58
LEN_BYTES :18
ORIGINAL  :Insérer. se fait.[END]
TRANSLATED:Insérer. se fait.[END]

ADDRESS   :0x6d7c
LEN_BYTES :13
ORIGINAL  :dèle %d 
 %s[END]
TRANSLATED:dèle %d 
 %s[END]

ADDRESS   :0x6d8c
LEN_BYTES :18
ORIGINAL  :ペースト完了[END]
TRANSLATED:ペースト完了[END]

ADDRESS   :0x6db0
LEN_BYTES :17
ORIGINAL  :モデル %d 
 %s[END]
TRANSLATED:モデル %d 
 %s[END]

ADDRESS   :0x6dc4
LEN_BYTES :19
ORIGINAL  :Paste successfully.[END]
TRANSLATED:Paste successfully.[END]

ADDRESS   :0x6dd8
LEN_BYTES :15
ORIGINAL  :粘贴失败!

[END]
TRANSLATED:粘贴失败!

[END]

ADDRESS   :0x6de8
LEN_BYTES :14
ORIGINAL  :Einf. Fehler ![END]
TRANSLATED:Einf. Fehler ![END]

ADDRESS   :0x6df8
LEN_BYTES :20
ORIGINAL  :Défaut de collage ![END]
TRANSLATED:Défaut de collage ![END]

ADDRESS   :0x6e10
LEN_BYTES :16
ORIGINAL  :コピー失敗![END]
TRANSLATED:コピー失敗![END]

ADDRESS   :0x6e24
LEN_BYTES :15
ORIGINAL  :Paste failure ![END]
TRANSLATED:Paste failure ![END]

ADDRESS   :0x6e80
LEN_BYTES :4
ORIGINAL  :IIHH[END]
TRANSLATED:IIHH[END]

ADDRESS   :0x6efc
LEN_BYTES :4
ORIGINAL  :Z!+H[END]
TRANSLATED:Z!+H[END]

ADDRESS   :0x70f8
LEN_BYTES :29
ORIGINAL  :%s
%s
%s
%s
%s
%s
%s
%s
%s
%s[END]
TRANSLATED:%s
%s
%s
%s
%s
%s
%s
%s
%s
%s[END]

ADDRESS   :0x711c
LEN_BYTES :5
ORIGINAL  :Exit
[END]
TRANSLATED:Exit
[END]

ADDRESS   :0x7304
LEN_BYTES :13
ORIGINAL  :PPM IN MODE

[END]
TRANSLATED:PPM IN MODE

[END]

ADDRESS   :0x7414
LEN_BYTES :14
ORIGINAL  :PPM OUT MODE

[END]
TRANSLATED:PPM OUT MODE

[END]

ADDRESS   :0x7430
LEN_BYTES :4
ORIGINAL  :pG%H[END]
TRANSLATED:pG%H[END]

ADDRESS   :0x7620
LEN_BYTES :6
ORIGINAL  : 0 p.H[END]
TRANSLATED: 0 p.H[END]

ADDRESS   :0x779c
LEN_BYTES :4
ORIGINAL  : pH[END]
TRANSLATED: pH[END]

ADDRESS   :0x7c20
LEN_BYTES :12
ORIGINAL  :舵量浏览[END]
TRANSLATED:舵量浏览[END]

ADDRESS   :0x7c30
LEN_BYTES :13
ORIGINAL  :Kanal Anzeige[END]
TRANSLATED:Kanal Anzeige[END]

ADDRESS   :0x7c40
LEN_BYTES :19
ORIGINAL  :Indicateur de canal[END]
TRANSLATED:Indicateur de canal[END]

ADDRESS   :0x7c54
LEN_BYTES :21
ORIGINAL  :チャンネル表示[END]
TRANSLATED:チャンネル表示[END]

ADDRESS   :0x7c6c
LEN_BYTES :14
ORIGINAL  :Rudder reading[END]
TRANSLATED:Rudder reading[END]

ADDRESS   :0x7ca8
LEN_BYTES :6
ORIGINAL  :通道[END]
TRANSLATED:通道[END]

ADDRESS   :0x7cb0
LEN_BYTES :4
ORIGINAL  :%s%d[END]
TRANSLATED:%s%d[END]

ADDRESS   :0x7cb8
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:Kanal [END]

ADDRESS   :0x7d88
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x80fc
LEN_BYTES :4
ORIGINAL  :pIbH[END]
TRANSLATED:pIbH[END]

ADDRESS   :0x81bc
LEN_BYTES :12
ORIGINAL  :模型设置[END]
TRANSLATED:模型设置[END]

ADDRESS   :0x81cc
LEN_BYTES :20
ORIGINAL  :Modell Einstellungen[END]
TRANSLATED:Modell Einstellungen[END]

ADDRESS   :0x81e4
LEN_BYTES :19
ORIGINAL  :Réglage du modèle[END]
TRANSLATED:Réglage du modèle[END]

ADDRESS   :0x81f8
LEN_BYTES :27
ORIGINAL  :モデルセッティング[END]
TRANSLATED:モデルセッティング[END]

ADDRESS   :0x8214
LEN_BYTES :14
ORIGINAL  :Model Settings[END]
TRANSLATED:Model Settings[END]

ADDRESS   :0x8228
LEN_BYTES :12
ORIGINAL  :模型选择[END]
TRANSLATED:模型选择[END]

ADDRESS   :0x8238
LEN_BYTES :14
ORIGINAL  :Modell Auswahl[END]
TRANSLATED:Modell Auswahl[END]

ADDRESS   :0x8248
LEN_BYTES :21
ORIGINAL  :Sélection du modèle[END]
TRANSLATED:Sélection du modèle[END]

ADDRESS   :0x8260
LEN_BYTES :21
ORIGINAL  :モデルセレクト[END]
TRANSLATED:モデルセレクト[END]

ADDRESS   :0x8278
LEN_BYTES :12
ORIGINAL  :Model Select[END]
TRANSLATED:Model Select[END]

ADDRESS   :0x8294
LEN_BYTES :29
ORIGINAL  :%s
%s
%s
%s
%s
%s
%s
%s
%s
%s[END]
TRANSLATED:%s
%s
%s
%s
%s
%s
%s
%s
%s
%s[END]

ADDRESS   :0x86d4
LEN_BYTES :15
ORIGINAL  :模型重命名[END]
TRANSLATED:模型重命名[END]

ADDRESS   :0x86e4
LEN_BYTES :15
ORIGINAL  :Modell umbennen[END]
TRANSLATED:Modell umbennen[END]

ADDRESS   :0x86f4
LEN_BYTES :19
ORIGINAL  :Renommer le modèle[END]
TRANSLATED:Renommer le modèle[END]

ADDRESS   :0x8708
LEN_BYTES :18
ORIGINAL  :モデルネーム[END]
TRANSLATED:モデルネーム[END]

ADDRESS   :0x871c
LEN_BYTES :14
ORIGINAL  :Model renaming[END]
TRANSLATED:Model renaming[END]

ADDRESS   :0x8738
LEN_BYTES :12
ORIGINAL  :模型复制[END]
TRANSLATED:模型复制[END]

ADDRESS   :0x8748
LEN_BYTES :15
ORIGINAL  :Modell kopieren[END]
TRANSLATED:Modell kopieren[END]

ADDRESS   :0x8758
LEN_BYTES :13
ORIGINAL  :Modèle Copie[END]
TRANSLATED:Modèle Copie[END]

ADDRESS   :0x8768
LEN_BYTES :18
ORIGINAL  :モデルコピー[END]
TRANSLATED:モデルコピー[END]

ADDRESS   :0x877c
LEN_BYTES :10
ORIGINAL  :Model Copy[END]
TRANSLATED:Model Copy[END]

ADDRESS   :0x8790
LEN_BYTES :12
ORIGINAL  :模型粘贴[END]
TRANSLATED:模型粘贴[END]

ADDRESS   :0x87a0
LEN_BYTES :16
ORIGINAL  :Modell einfügen[END]
TRANSLATED:Modell einfügen[END]

ADDRESS   :0x87b4
LEN_BYTES :19
ORIGINAL  :Insérer un modèle[END]
TRANSLATED:Insérer un modèle[END]

ADDRESS   :0x87c8
LEN_BYTES :21
ORIGINAL  :モデルペースト[END]
TRANSLATED:モデルペースト[END]

ADDRESS   :0x87e0
LEN_BYTES :11
ORIGINAL  :Model Paste[END]
TRANSLATED:Model Paste[END]

ADDRESS   :0x8890
LEN_BYTES :12
ORIGINAL  :模型重置[END]
TRANSLATED:模型重置[END]

ADDRESS   :0x88a0
LEN_BYTES :21
ORIGINAL  :Modell zurücksetzten[END]
TRANSLATED:Modell zurücksetzten[END]

ADDRESS   :0x88b8
LEN_BYTES :25
ORIGINAL  :Réinitialiser le modèle[END]
TRANSLATED:Réinitialiser le modèle[END]

ADDRESS   :0x88d4
LEN_BYTES :21
ORIGINAL  :モデルリセット[END]
TRANSLATED:モデルリセット[END]

ADDRESS   :0x88ec
LEN_BYTES :11
ORIGINAL  :Model Reset[END]
TRANSLATED:Model Reset[END]

ADDRESS   :0x8bf0
LEN_BYTES :4
ORIGINAL  :dIqH[END]
TRANSLATED:dIqH[END]

ADDRESS   :0x8bfc
LEN_BYTES :4
ORIGINAL  :P!nH[END]
TRANSLATED:P!nH[END]

ADDRESS   :0x8d10
LEN_BYTES :12
ORIGINAL  :定速巡航[END]
TRANSLATED:定速巡航[END]

ADDRESS   :0x8d20
LEN_BYTES :12
ORIGINAL  :Speed Regler[END]
TRANSLATED:Speed Regler[END]

ADDRESS   :0x8d30
LEN_BYTES :17
ORIGINAL  :Contr. De vitesse[END]
TRANSLATED:Contr. De vitesse[END]

ADDRESS   :0x8d44
LEN_BYTES :30
ORIGINAL  :クルーズコントロール[END]
TRANSLATED:クルーズコントロール[END]

ADDRESS   :0x8d64
LEN_BYTES :14
ORIGINAL  :Cruise control[END]
TRANSLATED:Cruise control[END]

ADDRESS   :0x8d88
LEN_BYTES :12
ORIGINAL  :巡航按键[END]
TRANSLATED:巡航按键[END]

ADDRESS   :0x8d98
LEN_BYTES :4
ORIGINAL  :Sart[END]
TRANSLATED:Sart[END]

ADDRESS   :0x8da0
LEN_BYTES :5
ORIGINAL  :Start[END]
TRANSLATED:Start[END]

ADDRESS   :0x8da8
LEN_BYTES :12
ORIGINAL  :スタート[END]
TRANSLATED:スタート[END]

ADDRESS   :0x8dbc
LEN_BYTES :24
ORIGINAL  :NULL
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:NULL
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0x91e4
LEN_BYTES :12
ORIGINAL  :巡航旋钮[END]
TRANSLATED:巡航旋钮[END]

ADDRESS   :0x91f4
LEN_BYTES :7
ORIGINAL  :Setting[END]
TRANSLATED:Setting[END]

ADDRESS   :0x91fc
LEN_BYTES :18
ORIGINAL  :セッティング[END]
TRANSLATED:セッティング[END]

ADDRESS   :0x9218
LEN_BYTES :14
ORIGINAL  :NULL
VR-5
VR-6[END]
TRANSLATED:NULL
VR-5
VR-6[END]

ADDRESS   :0x923c
LEN_BYTES :12
ORIGINAL  :巡航模式[END]
TRANSLATED:巡航模式[END]

ADDRESS   :0x924c
LEN_BYTES :4
ORIGINAL  :Mode[END]
TRANSLATED:Mode[END]

ADDRESS   :0x9254
LEN_BYTES :9
ORIGINAL  :モード[END]
TRANSLATED:モード[END]

ADDRESS   :0x9264
LEN_BYTES :17
ORIGINAL  :模式 1
模式 2[END]
TRANSLATED:模式 1
模式 2[END]

ADDRESS   :0x9278
LEN_BYTES :13
ORIGINAL  :mode 1
mode 2[END]
TRANSLATED:mode 1
mode 2[END]

ADDRESS   :0x9288
LEN_BYTES :21
ORIGINAL  :モード1
モード2[END]
TRANSLATED:モード1
モード2[END]

ADDRESS   :0x92a4
LEN_BYTES :20
ORIGINAL  :模式2
巡航速度[END]
TRANSLATED:模式2
巡航速度[END]

ADDRESS   :0x92bc
LEN_BYTES :6
ORIGINAL  :Mode 2[END]
TRANSLATED:Mode 2[END]

ADDRESS   :0x92c4
LEN_BYTES :24
ORIGINAL  :モード２スピード[END]
TRANSLATED:モード２スピード[END]

ADDRESS   :0x92e0
LEN_BYTES :13
ORIGINAL  :Mode 2 
speed[END]
TRANSLATED:Mode 2 
speed[END]

ADDRESS   :0x96b4
LEN_BYTES :7
ORIGINAL  :通道2[END]
TRANSLATED:通道2[END]

ADDRESS   :0x96bc
LEN_BYTES :7
ORIGINAL  :Kanal 2[END]
TRANSLATED:Kanal 2[END]

ADDRESS   :0x96d4
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x96e0
LEN_BYTES :7
ORIGINAL  :状态:[END]
TRANSLATED:状态:[END]

ADDRESS   :0x96e8
LEN_BYTES :7
ORIGINAL  :Status:[END]
TRANSLATED:Status:[END]

ADDRESS   :0x96f0
LEN_BYTES :15
ORIGINAL  :ステータス[END]
TRANSLATED:ステータス[END]

ADDRESS   :0x9780
LEN_BYTES :4
ORIGINAL  :QIp[END]
TRANSLATED:QIp[END]

ADDRESS   :0x979c
LEN_BYTES :6
ORIGINAL  :MHxMH[END]
TRANSLATED:MHxMH[END]

ADDRESS   :0x97d0
LEN_BYTES :4
ORIGINAL  :=Ip[END]
TRANSLATED:=Ip[END]

ADDRESS   :0x98e0
LEN_BYTES :15
ORIGINAL  :paste error !

[END]
TRANSLATED:paste error !

[END]

ADDRESS   :0x9974
LEN_BYTES :6
ORIGINAL  :7IpF[END]
TRANSLATED:7IpF[END]

ADDRESS   :0x99ac
LEN_BYTES :6
ORIGINAL  :,IpF[END]
TRANSLATED:,IpF[END]

ADDRESS   :0x9a90
LEN_BYTES :6
ORIGINAL  :AKU_NH[END]
TRANSLATED:AKU_NH[END]

ADDRESS   :0x9c08
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x9cf4
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0xa1b0
LEN_BYTES :12
ORIGINAL  :通道相位[END]
TRANSLATED:通道相位[END]

ADDRESS   :0xa1c0
LEN_BYTES :12
ORIGINAL  :Kanal Status[END]
TRANSLATED:Kanal Status[END]

ADDRESS   :0xa1d0
LEN_BYTES :19
ORIGINAL  :Phase de la chaîne[END]
TRANSLATED:Phase de la chaîne[END]

ADDRESS   :0xa1e4
LEN_BYTES :30
ORIGINAL  :チャンネルステータス[END]
TRANSLATED:チャンネルステータス[END]

ADDRESS   :0xa204
LEN_BYTES :13
ORIGINAL  :Channel Phase[END]
TRANSLATED:Channel Phase[END]

ADDRESS   :0xa218
LEN_BYTES :6
ORIGINAL  :通道[END]
TRANSLATED:通道[END]

ADDRESS   :0xa220
LEN_BYTES :4
ORIGINAL  :%s%d[END]
TRANSLATED:%s%d[END]

ADDRESS   :0xa228
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:Kanal [END]

ADDRESS   :0xa234
LEN_BYTES :6
ORIGINAL  :正相[END]
TRANSLATED:正相[END]

ADDRESS   :0xa240
LEN_BYTES :12
ORIGINAL  :ノーマル[END]
TRANSLATED:ノーマル[END]

ADDRESS   :0xa390
LEN_BYTES :6
ORIGINAL  :反相[END]
TRANSLATED:反相[END]

ADDRESS   :0xa39c
LEN_BYTES :12
ORIGINAL  :リバース[END]
TRANSLATED:リバース[END]

ADDRESS   :0xa6a8
LEN_BYTES :4
ORIGINAL  :fIuH[END]
TRANSLATED:fIuH[END]

ADDRESS   :0xa6c8
LEN_BYTES :4
ORIGINAL  :n!mH[END]
TRANSLATED:n!mH[END]

ADDRESS   :0xa7cc
LEN_BYTES :12
ORIGINAL  :教练模式[END]
TRANSLATED:教练模式[END]

ADDRESS   :0xa7dc
LEN_BYTES :16
ORIGINAL  :Trainings Modell[END]
TRANSLATED:Trainings Modell[END]

ADDRESS   :0xa7fc
LEN_BYTES :11
ORIGINAL  :traînement[END]
TRANSLATED:traînement[END]

ADDRESS   :0xa808
LEN_BYTES :27
ORIGINAL  :トレーニングモード[END]
TRANSLATED:トレーニングモード[END]

ADDRESS   :0xa824
LEN_BYTES :14
ORIGINAL  :Coaching model[END]
TRANSLATED:Coaching model[END]

ADDRESS   :0xa848
LEN_BYTES :12
ORIGINAL  :输入模式[END]
TRANSLATED:输入模式[END]

ADDRESS   :0xa858
LEN_BYTES :7
ORIGINAL  :Eingabe[END]
TRANSLATED:Eingabe[END]

ADDRESS   :0xa860
LEN_BYTES :7
ORIGINAL  :Entrée[END]
TRANSLATED:Entrée[END]

ADDRESS   :0xa868
LEN_BYTES :15
ORIGINAL  :インプット[END]
TRANSLATED:インプット[END]

ADDRESS   :0xa878
LEN_BYTES :5
ORIGINAL  :Input[END]
TRANSLATED:Input[END]

ADDRESS   :0xa884
LEN_BYTES :13
ORIGINAL  :输出模式 [END]
TRANSLATED:输出模式 [END]

ADDRESS   :0xa894
LEN_BYTES :7
ORIGINAL  :Ausgabe[END]
TRANSLATED:Ausgabe[END]

ADDRESS   :0xa89c
LEN_BYTES :6
ORIGINAL  :Sortie[END]
TRANSLATED:Sortie[END]

ADDRESS   :0xa8a4
LEN_BYTES :18
ORIGINAL  :アウトプット[END]
TRANSLATED:アウトプット[END]

ADDRESS   :0xa8b8
LEN_BYTES :6
ORIGINAL  :Output[END]
TRANSLATED:Output[END]

ADDRESS   :0xacd4
LEN_BYTES :10
ORIGINAL  :计时器 [END]
TRANSLATED:计时器 [END]

ADDRESS   :0xace0
LEN_BYTES :5
ORIGINAL  :Timer[END]
TRANSLATED:Timer[END]

ADDRESS   :0xace8
LEN_BYTES :9
ORIGINAL  :Minuterie[END]
TRANSLATED:Minuterie[END]

ADDRESS   :0xacf4
LEN_BYTES :12
ORIGINAL  :タイマー[END]
TRANSLATED:タイマー[END]

ADDRESS   :0xad08
LEN_BYTES :12
ORIGINAL  :扳机启动[END]
TRANSLATED:扳机启动[END]

ADDRESS   :0xad18
LEN_BYTES :20
ORIGINAL  :Gashebel Einstellung[END]
TRANSLATED:Gashebel Einstellung[END]

ADDRESS   :0xad30
LEN_BYTES :26
ORIGINAL  :Réglage du levier des gaz[END]
TRANSLATED:Réglage du levier des gaz[END]

ADDRESS   :0xad4c
LEN_BYTES :36
ORIGINAL  :スロットルトリガーの調整[END]
TRANSLATED:スロットルトリガーの調整[END]

ADDRESS   :0xad74
LEN_BYTES :15
ORIGINAL  :Trigger priming[END]
TRANSLATED:Trigger priming[END]

ADDRESS   :0xad94
LEN_BYTES :13
ORIGINAL  :启动 按键[END]
TRANSLATED:启动 按键[END]

ADDRESS   :0xada4
LEN_BYTES :10
ORIGINAL  :Startknopf[END]
TRANSLATED:Startknopf[END]

ADDRESS   :0xadb0
LEN_BYTES :20
ORIGINAL  :Bouton de démarrage[END]
TRANSLATED:Bouton de démarrage[END]

ADDRESS   :0xadc8
LEN_BYTES :21
ORIGINAL  :スタートボダン[END]
TRANSLATED:スタートボダン[END]

ADDRESS   :0xade0
LEN_BYTES :12
ORIGINAL  :Start button[END]
TRANSLATED:Start button[END]

ADDRESS   :0xadf8
LEN_BYTES :23
ORIGINAL  :无
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:无
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0xae10
LEN_BYTES :23
ORIGINAL  :無
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:無
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0xae28
LEN_BYTES :24
ORIGINAL  :NULL
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:NULL
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0xb138
LEN_BYTES :6
ORIGINAL  :fHhxH[END]
TRANSLATED:fHhxH[END]

ADDRESS   :0xb22c
LEN_BYTES :20
ORIGINAL  :停止/复位 按键[END]
TRANSLATED:停止/复位 按键[END]

ADDRESS   :0xb244
LEN_BYTES :24
ORIGINAL  :Stop/Zurücksetzen Knopf[END]
TRANSLATED:Stop/Zurücksetzen Knopf[END]

ADDRESS   :0xb260
LEN_BYTES :17
ORIGINAL  :Bouton Stop/Reset[END]
TRANSLATED:Bouton Stop/Reset[END]

ADDRESS   :0xb274
LEN_BYTES :34
ORIGINAL  :ストップ/リセットボタン[END]
TRANSLATED:ストップ/リセットボタン[END]

ADDRESS   :0xb298
LEN_BYTES :17
ORIGINAL  :Stop/Reset button[END]
TRANSLATED:Stop/Reset button[END]

ADDRESS   :0xb2dc
LEN_BYTES :10
ORIGINAL  :LED 模式[END]
TRANSLATED:LED 模式[END]

ADDRESS   :0xb2e8
LEN_BYTES :9
ORIGINAL  :LED Modus[END]
TRANSLATED:LED Modus[END]

ADDRESS   :0xb2f4
LEN_BYTES :15
ORIGINAL  :Modèle de Lamp[END]
TRANSLATED:Modèle de Lamp[END]

ADDRESS   :0xb304
LEN_BYTES :12
ORIGINAL  :LEDモード[END]
TRANSLATED:LEDモード[END]

ADDRESS   :0xb314
LEN_BYTES :8
ORIGINAL  :LED Mode[END]
TRANSLATED:LED Mode[END]

ADDRESS   :0xb324
LEN_BYTES :32
ORIGINAL  :   关闭 
   常亮 
   动态 [END]
TRANSLATED:   关闭 
   常亮 
   动态 [END]

ADDRESS   :0xb348
LEN_BYTES :29
ORIGINAL  :Schließen
Helligkeit
Dynamik[END]
TRANSLATED:Schließen
Helligkeit
Dynamik[END]

ADDRESS   :0xb368
LEN_BYTES :25
ORIGINAL  :Fermer
Lumineux
Dynamique[END]
TRANSLATED:Fermer
Lumineux
Dynamique[END]

ADDRESS   :0xb384
LEN_BYTES :32
ORIGINAL  :オフ
点灯
ダイナミック[END]
TRANSLATED:オフ
点灯
ダイナミック[END]

ADDRESS   :0xb3a8
LEN_BYTES :20
ORIGINAL  :Close
Bright
Dynamic[END]
TRANSLATED:Close
Bright
Dynamic[END]

ADDRESS   :0xb7d4
LEN_BYTES :12
ORIGINAL  :转向曲线[END]
TRANSLATED:转向曲线[END]

ADDRESS   :0xb7e4
LEN_BYTES :9
ORIGINAL  :Lenkkurve[END]
TRANSLATED:Lenkkurve[END]

ADDRESS   :0xb7f0
LEN_BYTES :19
ORIGINAL  :Courbe de direction[END]
TRANSLATED:Courbe de direction[END]

ADDRESS   :0xb804
LEN_BYTES :27
ORIGINAL  :ステアリングカーブ[END]
TRANSLATED:ステアリングカーブ[END]

ADDRESS   :0xb820
LEN_BYTES :14
ORIGINAL  :Steering Curve[END]
TRANSLATED:Steering Curve[END]

ADDRESS   :0xba78
LEN_BYTES :4
ORIGINAL  :5!HC[END]
TRANSLATED:5!HC[END]

ADDRESS   :0xbc48
LEN_BYTES :6
ORIGINAL  :预设[END]
TRANSLATED:预设[END]

ADDRESS   :0xbc50
LEN_BYTES :4
ORIGINAL  :%s%d[END]
TRANSLATED:%s%d[END]

ADDRESS   :0xbc58
LEN_BYTES :9
ORIGINAL  :Standard-[END]
TRANSLATED:Standard-[END]

ADDRESS   :0xbc64
LEN_BYTES :6
ORIGINAL  :conçu[END]
TRANSLATED:conçu[END]

ADDRESS   :0xbc6c
LEN_BYTES :15
ORIGINAL  :初期設定値[END]
TRANSLATED:初期設定値[END]

ADDRESS   :0xbc7c
LEN_BYTES :7
ORIGINAL  :Presets[END]
TRANSLATED:Presets[END]

ADDRESS   :0xbca0
LEN_BYTES :5
ORIGINAL  :Punkt[END]
TRANSLATED:Punkt[END]

ADDRESS   :0xbca8
LEN_BYTES :5
ORIGINAL  :Point[END]
TRANSLATED:Point[END]

ADDRESS   :0xbcb0
LEN_BYTES :12
ORIGINAL  :ポイント[END]
TRANSLATED:ポイント[END]

ADDRESS   :0xbec0
LEN_BYTES :6
ORIGINAL  := [END]
TRANSLATED:= [END]

ADDRESS   :0xc708
LEN_BYTES :8
ORIGINAL  :C bS Hb[END]
TRANSLATED:C bS Hb[END]

ADDRESS   :0xcd4c
LEN_BYTES :4
ORIGINAL  :RIQH[END]
TRANSLATED:RIQH[END]

ADDRESS   :0xcde8
LEN_BYTES :12
ORIGINAL  :通道行程[END]
TRANSLATED:通道行程[END]

ADDRESS   :0xcdf8
LEN_BYTES :9
ORIGINAL  :Endpunkte[END]
TRANSLATED:Endpunkte[END]

ADDRESS   :0xce04
LEN_BYTES :9
ORIGINAL  :Point FIN[END]
TRANSLATED:Point FIN[END]

ADDRESS   :0xce10
LEN_BYTES :21
ORIGINAL  :エンドポイント[END]
TRANSLATED:エンドポイント[END]

ADDRESS   :0xce28
LEN_BYTES :9
ORIGINAL  :END Point[END]
TRANSLATED:END Point[END]

ADDRESS   :0xce44
LEN_BYTES :9
ORIGINAL  :转向舵[END]
TRANSLATED:转向舵[END]

ADDRESS   :0xce50
LEN_BYTES :7
ORIGINAL  :Lenkung[END]
TRANSLATED:Lenkung[END]

ADDRESS   :0xce58
LEN_BYTES :9
ORIGINAL  :Direction[END]
TRANSLATED:Direction[END]

ADDRESS   :0xce64
LEN_BYTES :18
ORIGINAL  :ステアリング[END]
TRANSLATED:ステアリング[END]

ADDRESS   :0xce78
LEN_BYTES :8
ORIGINAL  :Steering[END]
TRANSLATED:Steering[END]

ADDRESS   :0xce8c
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0xd2b8
LEN_BYTES :5
ORIGINAL  :Links[END]
TRANSLATED:Links[END]

ADDRESS   :0xd2c0
LEN_BYTES :7
ORIGINAL  :Gauche [END]
TRANSLATED:Gauche [END]

ADDRESS   :0xd2c8
LEN_BYTES :4
ORIGINAL  :Left[END]
TRANSLATED:Left[END]

ADDRESS   :0xd2ec
LEN_BYTES :6
ORIGINAL  :Rechts[END]
TRANSLATED:Rechts[END]

ADDRESS   :0xd2f4
LEN_BYTES :6
ORIGINAL  :Droite[END]
TRANSLATED:Droite[END]

ADDRESS   :0xd2fc
LEN_BYTES :5
ORIGINAL  :Right[END]
TRANSLATED:Right[END]

ADDRESS   :0xd30c
LEN_BYTES :6
ORIGINAL  :油门[END]
TRANSLATED:油门[END]

ADDRESS   :0xd318
LEN_BYTES :14
ORIGINAL  :Accélérateur[END]
TRANSLATED:Accélérateur[END]

ADDRESS   :0xd328
LEN_BYTES :15
ORIGINAL  :スロットル[END]
TRANSLATED:スロットル[END]

ADDRESS   :0xd5dc
LEN_BYTES :6
ORIGINAL  :nHxnH[END]
TRANSLATED:nHxnH[END]

ADDRESS   :0xd630
LEN_BYTES :6
ORIGINAL  :XHhYH[END]
TRANSLATED:XHhYH[END]

ADDRESS   :0xd640
LEN_BYTES :4
ORIGINAL  :IIVH[END]
TRANSLATED:IIVH[END]

ADDRESS   :0xd734
LEN_BYTES :8
ORIGINAL  :Throttle[END]
TRANSLATED:Throttle[END]

ADDRESS   :0xd774
LEN_BYTES :7
ORIGINAL  :Zurück[END]
TRANSLATED:Zurück[END]

ADDRESS   :0xd77c
LEN_BYTES :5
ORIGINAL  :Avant[END]
TRANSLATED:Avant[END]

ADDRESS   :0xd784
LEN_BYTES :6
ORIGINAL  :後進[END]
TRANSLATED:後進[END]

ADDRESS   :0xd78c
LEN_BYTES :4
ORIGINAL  :Back[END]
TRANSLATED:Back[END]

ADDRESS   :0xd7a4
LEN_BYTES :9
ORIGINAL  :Vorwärts[END]
TRANSLATED:Vorwärts[END]

ADDRESS   :0xd7b0
LEN_BYTES :8
ORIGINAL  :Arrière[END]
TRANSLATED:Arrière[END]

ADDRESS   :0xd7bc
LEN_BYTES :6
ORIGINAL  :前進[END]
TRANSLATED:前進[END]

ADDRESS   :0xd7c4
LEN_BYTES :5
ORIGINAL  :Front[END]
TRANSLATED:Front[END]

ADDRESS   :0xdb64
LEN_BYTES :6
ORIGINAL  :BHxBH[END]
TRANSLATED:BHxBH[END]

ADDRESS   :0xdbb8
LEN_BYTES :6
ORIGINAL  :,Hh-H[END]
TRANSLATED:,Hh-H[END]

ADDRESS   :0xdbf0
LEN_BYTES :7
ORIGINAL  :旋钮5[END]
TRANSLATED:旋钮5[END]

ADDRESS   :0xdbfc
LEN_BYTES :11
ORIGINAL  :Drehknopf 5[END]
TRANSLATED:Drehknopf 5[END]

ADDRESS   :0xdc08
LEN_BYTES :16
ORIGINAL  :Bouton rotatif 5[END]
TRANSLATED:Bouton rotatif 5[END]

ADDRESS   :0xdc1c
LEN_BYTES :22
ORIGINAL  :ロータリーノブ5[END]
TRANSLATED:ロータリーノブ5[END]

ADDRESS   :0xdc34
LEN_BYTES :13
ORIGINAL  :Rotary Knob 5[END]
TRANSLATED:Rotary Knob 5[END]

ADDRESS   :0xdc60
LEN_BYTES :6
ORIGINAL  :最小[END]
TRANSLATED:最小[END]

ADDRESS   :0xdf5c
LEN_BYTES :6
ORIGINAL  :gHxhH[END]
TRANSLATED:gHxhH[END]

ADDRESS   :0xdfb0
LEN_BYTES :6
ORIGINAL  :PHhSH[END]
TRANSLATED:PHhSH[END]

ADDRESS   :0xdfc0
LEN_BYTES :4
ORIGINAL  :RIPH[END]
TRANSLATED:RIPH[END]

ADDRESS   :0xe088
LEN_BYTES :6
ORIGINAL  :最大[END]
TRANSLATED:最大[END]

ADDRESS   :0xe09c
LEN_BYTES :7
ORIGINAL  :旋钮6[END]
TRANSLATED:旋钮6[END]

ADDRESS   :0xe0a4
LEN_BYTES :11
ORIGINAL  :Drehknopf 6[END]
TRANSLATED:Drehknopf 6[END]

ADDRESS   :0xe0b0
LEN_BYTES :16
ORIGINAL  :Bouton rotatif 6[END]
TRANSLATED:Bouton rotatif 6[END]

ADDRESS   :0xe0c4
LEN_BYTES :22
ORIGINAL  :ロータリーノブ6[END]
TRANSLATED:ロータリーノブ6[END]

ADDRESS   :0xe0dc
LEN_BYTES :13
ORIGINAL  :Rotary Knob 6[END]
TRANSLATED:Rotary Knob 6[END]

ADDRESS   :0xe194
LEN_BYTES :6
ORIGINAL  :GHxIH[END]
TRANSLATED:GHxIH[END]

ADDRESS   :0xe1e8
LEN_BYTES :6
ORIGINAL  :1Hh4H[END]
TRANSLATED:1Hh4H[END]

ADDRESS   :0xe1f8
LEN_BYTES :4
ORIGINAL  :3I1H[END]
TRANSLATED:3I1H[END]

ADDRESS   :0xe5f4
LEN_BYTES :4
ORIGINAL  :d!uH[END]
TRANSLATED:d!uH[END]

ADDRESS   :0xe6b4
LEN_BYTES :6
ORIGINAL  :EHhZH[END]
TRANSLATED:EHhZH[END]

ADDRESS   :0xe6f8
LEN_BYTES :12
ORIGINAL  :声音设置[END]
TRANSLATED:声音设置[END]

ADDRESS   :0xe708
LEN_BYTES :16
ORIGINAL  :Toneinstellungen[END]
TRANSLATED:Toneinstellungen[END]

ADDRESS   :0xe71c
LEN_BYTES :17
ORIGINAL  :Réglages sonores[END]
TRANSLATED:Réglages sonores[END]

ADDRESS   :0xe730
LEN_BYTES :30
ORIGINAL  :サウンドセッティング[END]
TRANSLATED:サウンドセッティング[END]

ADDRESS   :0xe750
LEN_BYTES :14
ORIGINAL  :Sound Settings[END]
TRANSLATED:Sound Settings[END]

ADDRESS   :0xe764
LEN_BYTES :15
ORIGINAL  :开关机声音[END]
TRANSLATED:开关机声音[END]

ADDRESS   :0xe774
LEN_BYTES :15
ORIGINAL  :Startton An/Aus[END]
TRANSLATED:Startton An/Aus[END]

ADDRESS   :0xe784
LEN_BYTES :24
ORIGINAL  :Son de démarrage On/Off[END]
TRANSLATED:Son de démarrage On/Off[END]

ADDRESS   :0xe7a0
LEN_BYTES :9
ORIGINAL  :始動音[END]
TRANSLATED:始動音[END]

ADDRESS   :0xe7ac
LEN_BYTES :18
ORIGINAL  :Power_on/off sound[END]
TRANSLATED:Power_on/off sound[END]

ADDRESS   :0xe7d0
LEN_BYTES :13
ORIGINAL  :声音类型 [END]
TRANSLATED:声音类型 [END]

ADDRESS   :0xe7e0
LEN_BYTES :9
ORIGINAL  :Singalton[END]
TRANSLATED:Singalton[END]

ADDRESS   :0xe7ec
LEN_BYTES :17
ORIGINAL  :Type de tonalité[END]
TRANSLATED:Type de tonalité[END]

ADDRESS   :0xe800
LEN_BYTES :21
ORIGINAL  :サウンドタイプ[END]
TRANSLATED:サウンドタイプ[END]

ADDRESS   :0xe818
LEN_BYTES :9
ORIGINAL  :Tone Type[END]
TRANSLATED:Tone Type[END]

ADDRESS   :0xebf0
LEN_BYTES :28
ORIGINAL  :  静音 
仅报警 
全部 [END]
TRANSLATED:  静音 
仅报警 
全部 [END]

ADDRESS   :0xec14
LEN_BYTES :20
ORIGINAL  :Stumm
Nur Alarm
Alle[END]
TRANSLATED:Stumm
Nur Alarm
Alle[END]

ADDRESS   :0xec2c
LEN_BYTES :17
ORIGINAL  :Muet 
Alarme
Tous[END]
TRANSLATED:Muet 
Alarme
Tous[END]

ADDRESS   :0xec40
LEN_BYTES :35
ORIGINAL  :消音
アラームのみ
すべて[END]
TRANSLATED:消音
アラームのみ
すべて[END]

ADDRESS   :0xec64
LEN_BYTES :18
ORIGINAL  :Mute 
ALM Only
All[END]
TRANSLATED:Mute 
ALM Only
All[END]

ADDRESS   :0xeca4
LEN_BYTES :10
ORIGINAL  :背光灯 [END]
TRANSLATED:背光灯 [END]

ADDRESS   :0xecb0
LEN_BYTES :22
ORIGINAL  :Hintergrundbeleuchtung[END]
TRANSLATED:Hintergrundbeleuchtung[END]

ADDRESS   :0xecc8
LEN_BYTES :17
ORIGINAL  :Rétro-éclairage[END]
TRANSLATED:Rétro-éclairage[END]

ADDRESS   :0xecdc
LEN_BYTES :24
ORIGINAL  :バックライト設定[END]
TRANSLATED:バックライト設定[END]

ADDRESS   :0xecf8
LEN_BYTES :9
ORIGINAL  :Backlight[END]
TRANSLATED:Backlight[END]

ADDRESS   :0xed08
LEN_BYTES :13
ORIGINAL  :背光亮度 [END]
TRANSLATED:背光亮度 [END]

ADDRESS   :0xed18
LEN_BYTES :10
ORIGINAL  :Helligkeit[END]
TRANSLATED:Helligkeit[END]

ADDRESS   :0xed24
LEN_BYTES :14
ORIGINAL  :La luminosité[END]
TRANSLATED:La luminosité[END]

ADDRESS   :0xed34
LEN_BYTES :27
ORIGINAL  :バックライト明るさ[END]
TRANSLATED:バックライト明るさ[END]

ADDRESS   :0xed50
LEN_BYTES :10
ORIGINAL  :Brightness[END]
TRANSLATED:Brightness[END]

ADDRESS   :0xed7c
LEN_BYTES :6
ORIGINAL  :pHhnH[END]
TRANSLATED:pHhnH[END]

ADDRESS   :0xed88
LEN_BYTES :4
ORIGINAL  :d!lH[END]
TRANSLATED:d!lH[END]

ADDRESS   :0xef48
LEN_BYTES :13
ORIGINAL  :自动熄灭 [END]
TRANSLATED:自动熄灭 [END]

ADDRESS   :0xef58
LEN_BYTES :8
ORIGINAL  :Auto Off[END]
TRANSLATED:Auto Off[END]

ADDRESS   :0xef64
LEN_BYTES :11
ORIGINAL  :Arrêt auto[END]
TRANSLATED:Arrêt auto[END]

ADDRESS   :0xef70
LEN_BYTES :15
ORIGINAL  :オートオフ[END]
TRANSLATED:オートオフ[END]

ADDRESS   :0xef8c
LEN_BYTES :47
ORIGINAL  :  关闭 
1分钟 
3分钟 
10分钟 
30分钟 [END]
TRANSLATED:  关闭 
1分钟 
3分钟 
10分钟 
30分钟 [END]

ADDRESS   :0xefbc
LEN_BYTES :40
ORIGINAL  :Schließen
1 min 
3 min 
10 min 
30 min [END]
TRANSLATED:Schließen
1 min 
3 min 
10 min 
30 min [END]

ADDRESS   :0xefe8
LEN_BYTES :37
ORIGINAL  :Fermer 
1 min 
3 min 
10 min 
30 min [END]
TRANSLATED:Fermer 
1 min 
3 min 
10 min 
30 min [END]

ADDRESS   :0xf010
LEN_BYTES :32
ORIGINAL  :オフ
1 分
3 分
10 分
30 分[END]
TRANSLATED:オフ
1 分
3 分
10 分
30 分[END]

ADDRESS   :0xf034
LEN_BYTES :36
ORIGINAL  :Close 
1 min 
3 min 
10 min 
30 min [END]
TRANSLATED:Close 
1 min 
3 min 
10 min 
30 min [END]

ADDRESS   :0xf478
LEN_BYTES :19
ORIGINAL  :油门/刹车曲线[END]
TRANSLATED:油门/刹车曲线[END]

ADDRESS   :0xf48c
LEN_BYTES :15
ORIGINAL  :Gas/Brems Kurve[END]
TRANSLATED:Gas/Brems Kurve[END]

ADDRESS   :0xf4a8
LEN_BYTES :12
ORIGINAL  :élér/frein[END]
TRANSLATED:élér/frein[END]

ADDRESS   :0xf4b8
LEN_BYTES :37
ORIGINAL  :スロットル/ブレーキカーブ[END]
TRANSLATED:スロットル/ブレーキカーブ[END]

ADDRESS   :0xf4e0
LEN_BYTES :20
ORIGINAL  :Throttle/Brake Curve[END]
TRANSLATED:Throttle/Brake Curve[END]

ADDRESS   :0xf76c
LEN_BYTES :4
ORIGINAL  :5!HC[END]
TRANSLATED:5!HC[END]

ADDRESS   :0xf910
LEN_BYTES :6
ORIGINAL  :预设[END]
TRANSLATED:预设[END]

ADDRESS   :0xf918
LEN_BYTES :4
ORIGINAL  :%s%d[END]
TRANSLATED:%s%d[END]

ADDRESS   :0xf920
LEN_BYTES :9
ORIGINAL  :Standard-[END]
TRANSLATED:Standard-[END]

ADDRESS   :0xf92c
LEN_BYTES :6
ORIGINAL  :conçu[END]
TRANSLATED:conçu[END]

ADDRESS   :0xf934
LEN_BYTES :15
ORIGINAL  :初期設定値[END]
TRANSLATED:初期設定値[END]

ADDRESS   :0xf944
LEN_BYTES :7
ORIGINAL  :Presets[END]
TRANSLATED:Presets[END]

ADDRESS   :0xf968
LEN_BYTES :5
ORIGINAL  :Punkt[END]
TRANSLATED:Punkt[END]

ADDRESS   :0xf970
LEN_BYTES :5
ORIGINAL  :Point[END]
TRANSLATED:Point[END]

ADDRESS   :0xf978
LEN_BYTES :12
ORIGINAL  :ポイント[END]
TRANSLATED:ポイント[END]

ADDRESS   :0xfb88
LEN_BYTES :6
ORIGINAL  :iPL[END]
TRANSLATED:iPL[END]

ADDRESS   :0xff4c
LEN_BYTES :6
ORIGINAL  :?Hx;H[END]
TRANSLATED:?Hx;H[END]

ADDRESS   :0x10368
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x10614
LEN_BYTES :8
ORIGINAL  :C bS Hb[END]
TRANSLATED:C bS Hb[END]

ADDRESS   :0x10bf8
LEN_BYTES :6
ORIGINAL  :YHhhH[END]
TRANSLATED:YHhhH[END]

ADDRESS   :0x10cd8
LEN_BYTES :12
ORIGINAL  :Double ratio[END]
TRANSLATED:Double ratio[END]

ADDRESS   :0x10ce8
LEN_BYTES :9
ORIGINAL  :双比率[END]
TRANSLATED:双比率[END]

ADDRESS   :0x10cf4
LEN_BYTES :44
ORIGINAL  :D/R  ステアリングデュアルレート[END]
TRANSLATED:D/R  ステアリングデュアルレート[END]

ADDRESS   :0x10d2c
LEN_BYTES :18
ORIGINAL  :转向比率切换[END]
TRANSLATED:转向比率切换[END]

ADDRESS   :0x10d40
LEN_BYTES :22
ORIGINAL  :ステアリング D/R[END]
TRANSLATED:ステアリング D/R[END]

ADDRESS   :0x10d58
LEN_BYTES :6
ORIGINAL  :ST D/R[END]
TRANSLATED:ST D/R[END]

ADDRESS   :0x10d64
LEN_BYTES :40
ORIGINAL  :NULL
K-3
K-4
K-8
K-9
K-10
SW-7
VR-5
VR-6[END]
TRANSLATED:NULL
K-3
K-4
K-8
K-9
K-10
SW-7
VR-5
VR-6[END]

ADDRESS   :0x10db8
LEN_BYTES :18
ORIGINAL  :油门比率切换[END]
TRANSLATED:油门比率切换[END]

ADDRESS   :0x111bc
LEN_BYTES :19
ORIGINAL  :スロットル D/R[END]
TRANSLATED:スロットル D/R[END]

ADDRESS   :0x111d0
LEN_BYTES :6
ORIGINAL  :TH D/R[END]
TRANSLATED:TH D/R[END]

ADDRESS   :0x11214
LEN_BYTES :7
ORIGINAL  :通道1[END]
TRANSLATED:通道1[END]

ADDRESS   :0x11228
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x11680
LEN_BYTES :7
ORIGINAL  :通道2[END]
TRANSLATED:通道2[END]

ADDRESS   :0x11c28
LEN_BYTES :6
ORIGINAL  :cHxZH[END]
TRANSLATED:cHxZH[END]

ADDRESS   :0x11c34
LEN_BYTES :4
ORIGINAL  :aIXH[END]
TRANSLATED:aIXH[END]

ADDRESS   :0x11c8c
LEN_BYTES :4
ORIGINAL  :+IBH[END]
TRANSLATED:+IBH[END]

ADDRESS   :0x11ce0
LEN_BYTES :15
ORIGINAL  :陀螺仪混控[END]
TRANSLATED:陀螺仪混控[END]

ADDRESS   :0x11cf0
LEN_BYTES :9
ORIGINAL  :Gyromodus[END]
TRANSLATED:Gyromodus[END]

ADDRESS   :0x11cfc
LEN_BYTES :15
ORIGINAL  :Mode gyromètre[END]
TRANSLATED:Mode gyromètre[END]

ADDRESS   :0x11d0c
LEN_BYTES :24
ORIGINAL  :ジャイロミックス[END]
TRANSLATED:ジャイロミックス[END]

ADDRESS   :0x11d28
LEN_BYTES :8
ORIGINAL  :Gyro MIX[END]
TRANSLATED:Gyro MIX[END]

ADDRESS   :0x11d44
LEN_BYTES :12
ORIGINAL  :使能开关[END]
TRANSLATED:使能开关[END]

ADDRESS   :0x11d54
LEN_BYTES :11
ORIGINAL  :Einschalten[END]
TRANSLATED:Einschalten[END]

ADDRESS   :0x11d60
LEN_BYTES :14
ORIGINAL  :Mise en marche[END]
TRANSLATED:Mise en marche[END]

ADDRESS   :0x11d70
LEN_BYTES :27
ORIGINAL  :キーを有効にする。[END]
TRANSLATED:キーを有効にする。[END]

ADDRESS   :0x11d8c
LEN_BYTES :10
ORIGINAL  :Enable Key[END]
TRANSLATED:Enable Key[END]

ADDRESS   :0x11d9c
LEN_BYTES :24
ORIGINAL  :NULL
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:NULL
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0x121d4
LEN_BYTES :12
ORIGINAL  :调整旋钮[END]
TRANSLATED:调整旋钮[END]

ADDRESS   :0x121e4
LEN_BYTES :13
ORIGINAL  :Einstellknopf[END]
TRANSLATED:Einstellknopf[END]

ADDRESS   :0x121f4
LEN_BYTES :19
ORIGINAL  :Bouton de calibrage[END]
TRANSLATED:Bouton de calibrage[END]

ADDRESS   :0x12208
LEN_BYTES :12
ORIGINAL  :ノブ調整[END]
TRANSLATED:ノブ調整[END]

ADDRESS   :0x12218
LEN_BYTES :14
ORIGINAL  :Adjusting Knob[END]
TRANSLATED:Adjusting Knob[END]

ADDRESS   :0x12234
LEN_BYTES :14
ORIGINAL  :NULL
VR-5
VR-6[END]
TRANSLATED:NULL
VR-5
VR-6[END]

ADDRESS   :0x12258
LEN_BYTES :9
ORIGINAL  :当前值[END]
TRANSLATED:当前值[END]

ADDRESS   :0x12264
LEN_BYTES :14
ORIGINAL  :Aktueller Wert[END]
TRANSLATED:Aktueller Wert[END]

ADDRESS   :0x12274
LEN_BYTES :15
ORIGINAL  :Valeur actuelle[END]
TRANSLATED:Valeur actuelle[END]

ADDRESS   :0x12284
LEN_BYTES :12
ORIGINAL  :カレント[END]
TRANSLATED:カレント[END]

ADDRESS   :0x12294
LEN_BYTES :13
ORIGINAL  :Current Value[END]
TRANSLATED:Current Value[END]

ADDRESS   :0x122b0
LEN_BYTES :5
ORIGINAL  :%d.%d[END]
TRANSLATED:%d.%d[END]

ADDRESS   :0x122c4
LEN_BYTES :7
ORIGINAL  :通道8[END]
TRANSLATED:通道8[END]

ADDRESS   :0x122cc
LEN_BYTES :7
ORIGINAL  :Kanal 8[END]
TRANSLATED:Kanal 8[END]

ADDRESS   :0x12384
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x12558
LEN_BYTES :4
ORIGINAL  :OєH[END]
TRANSLATED:OєH[END]

ADDRESS   :0x127c0
LEN_BYTES :4
ORIGINAL  :%d%s[END]
TRANSLATED:%d%s[END]

ADDRESS   :0x129a8
LEN_BYTES :6
ORIGINAL  :5IpF[END]
TRANSLATED:5IpF[END]

ADDRESS   :0x12a84
LEN_BYTES :6
ORIGINAL  :%d.%dV[END]
TRANSLATED:%d.%dV[END]

ADDRESS   :0x12b28
LEN_BYTES :6
ORIGINAL  :,IpF[END]
TRANSLATED:,IpF[END]

ADDRESS   :0x12be8
LEN_BYTES :5
ORIGINAL  :%d.%d[END]
TRANSLATED:%d.%d[END]

ADDRESS   :0x12f0c
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x13080
LEN_BYTES :20
ORIGINAL  :当前电压        [END]
TRANSLATED:当前电压        [END]

ADDRESS   :0x13098
LEN_BYTES :17
ORIGINAL  :%s      %d.%02d V[END]
TRANSLATED:%s      %d.%02d V[END]

ADDRESS   :0x130b0
LEN_BYTES :17
ORIGINAL  :Aktuelle Spannung[END]
TRANSLATED:Aktuelle Spannung[END]

ADDRESS   :0x130c4
LEN_BYTES :12
ORIGINAL  :%s %d.%02d V[END]
TRANSLATED:%s %d.%02d V[END]

ADDRESS   :0x130d4
LEN_BYTES :16
ORIGINAL  :Tension actuelle[END]
TRANSLATED:Tension actuelle[END]

ADDRESS   :0x130e8
LEN_BYTES :13
ORIGINAL  :%s  %d.%02d V[END]
TRANSLATED:%s  %d.%02d V[END]

ADDRESS   :0x130f8
LEN_BYTES :12
ORIGINAL  :電圧表示[END]
TRANSLATED:電圧表示[END]

ADDRESS   :0x13108
LEN_BYTES :15
ORIGINAL  :Current Voltage[END]
TRANSLATED:Current Voltage[END]

ADDRESS   :0x13158
LEN_BYTES :6
ORIGINAL  :#Ip#H[END]
TRANSLATED:#Ip#H[END]

ADDRESS   :0x13200
LEN_BYTES :5
ORIGINAL  :%d.%d[END]
TRANSLATED:%d.%d[END]

ADDRESS   :0x13218
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x136b0
LEN_BYTES :12
ORIGINAL  :辅助微调[END]
TRANSLATED:辅助微调[END]

ADDRESS   :0x136c0
LEN_BYTES :17
ORIGINAL  :Feineinstellungen[END]
TRANSLATED:Feineinstellungen[END]

ADDRESS   :0x136d4
LEN_BYTES :12
ORIGINAL  :Trim neutre [END]
TRANSLATED:Trim neutre [END]

ADDRESS   :0x136e4
LEN_BYTES :15
ORIGINAL  :サブトリム[END]
TRANSLATED:サブトリム[END]

ADDRESS   :0x136f4
LEN_BYTES :8
ORIGINAL  :SUB Trim[END]
TRANSLATED:SUB Trim[END]

ADDRESS   :0x1372c
LEN_BYTES :6
ORIGINAL  :通道[END]
TRANSLATED:通道[END]

ADDRESS   :0x13734
LEN_BYTES :4
ORIGINAL  :%s%d[END]
TRANSLATED:%s%d[END]

ADDRESS   :0x1373c
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:Kanal [END]

ADDRESS   :0x13930
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x13c04
LEN_BYTES :6
ORIGINAL  :eHhuH[END]
TRANSLATED:eHhuH[END]

ADDRESS   :0x13c14
LEN_BYTES :4
ORIGINAL  :sIrH[END]
TRANSLATED:sIrH[END]

ADDRESS   :0x13c2c
LEN_BYTES :4
ORIGINAL  :FInH[END]
TRANSLATED:FInH[END]

ADDRESS   :0x13c54
LEN_BYTES :6
ORIGINAL  :bHhcH[END]
TRANSLATED:bHhcH[END]

ADDRESS   :0x13c60
LEN_BYTES :4
ORIGINAL  :_!aH[END]
TRANSLATED:_!aH[END]

ADDRESS   :0x13d50
LEN_BYTES :7
ORIGINAL  :校准 [END]
TRANSLATED:校准 [END]

ADDRESS   :0x13d58
LEN_BYTES :12
ORIGINAL  :Kalibrierung[END]
TRANSLATED:Kalibrierung[END]

ADDRESS   :0x13d68
LEN_BYTES :9
ORIGINAL  :Calibrage[END]
TRANSLATED:Calibrage[END]

ADDRESS   :0x13d74
LEN_BYTES :27
ORIGINAL  :キャリブレーション[END]
TRANSLATED:キャリブレーション[END]

ADDRESS   :0x13d90
LEN_BYTES :11
ORIGINAL  :Calibration[END]
TRANSLATED:Calibration[END]

ADDRESS   :0x13da0
LEN_BYTES :10
ORIGINAL  :转向轮 [END]
TRANSLATED:转向轮 [END]

ADDRESS   :0x13dac
LEN_BYTES :7
ORIGINAL  :Lenkung[END]
TRANSLATED:Lenkung[END]

ADDRESS   :0x13db4
LEN_BYTES :9
ORIGINAL  :Direction[END]
TRANSLATED:Direction[END]

ADDRESS   :0x13dc0
LEN_BYTES :18
ORIGINAL  :ステアリング[END]
TRANSLATED:ステアリング[END]

ADDRESS   :0x13dd4
LEN_BYTES :8
ORIGINAL  :Steering[END]
TRANSLATED:Steering[END]

ADDRESS   :0x13dec
LEN_BYTES :7
ORIGINAL  :开始 [END]
TRANSLATED:开始 [END]

ADDRESS   :0x13df4
LEN_BYTES :5
ORIGINAL  :Start[END]
TRANSLATED:Start[END]

ADDRESS   :0x13dfc
LEN_BYTES :10
ORIGINAL  :Démarrage[END]
TRANSLATED:Démarrage[END]

ADDRESS   :0x13e08
LEN_BYTES :12
ORIGINAL  :スタート[END]
TRANSLATED:スタート[END]

ADDRESS   :0x140c8
LEN_BYTES :4
ORIGINAL  :_!lH[END]
TRANSLATED:_!lH[END]

ADDRESS   :0x141fc
LEN_BYTES :7
ORIGINAL  :扳机 [END]
TRANSLATED:扳机 [END]

ADDRESS   :0x1420c
LEN_BYTES :14
ORIGINAL  :Accélération[END]
TRANSLATED:Accélération[END]

ADDRESS   :0x1421c
LEN_BYTES :15
ORIGINAL  :スロットル[END]
TRANSLATED:スロットル[END]

ADDRESS   :0x1422c
LEN_BYTES :7
ORIGINAL  :Trottle[END]
TRANSLATED:Trottle[END]

ADDRESS   :0x14250
LEN_BYTES :7
ORIGINAL  :按键 [END]
TRANSLATED:按键 [END]

ADDRESS   :0x14258
LEN_BYTES :6
ORIGINAL  :Tasten[END]
TRANSLATED:Tasten[END]

ADDRESS   :0x14260
LEN_BYTES :7
ORIGINAL  :Boutons[END]
TRANSLATED:Boutons[END]

ADDRESS   :0x14268
LEN_BYTES :9
ORIGINAL  :ボタン[END]
TRANSLATED:ボタン[END]

ADDRESS   :0x14274
LEN_BYTES :7
ORIGINAL  :Buttons[END]
TRANSLATED:Buttons[END]

ADDRESS   :0x142a4
LEN_BYTES :4
ORIGINAL  :mI\H[END]
TRANSLATED:mI\H[END]

ADDRESS   :0x142b0
LEN_BYTES :4
ORIGINAL  :kIYH[END]
TRANSLATED:kIYH[END]

ADDRESS   :0x142f8
LEN_BYTES :4
ORIGINAL  :lIkH[END]
TRANSLATED:lIkH[END]

ADDRESS   :0x14304
LEN_BYTES :4
ORIGINAL  :jIhH[END]
TRANSLATED:jIhH[END]

ADDRESS   :0x143cc
LEN_BYTES :4
ORIGINAL  :WI6H[END]
TRANSLATED:WI6H[END]

ADDRESS   :0x143e0
LEN_BYTES :54
ORIGINAL  :官网: www.dumborc.com

硬件: V1.0.0
软件: V1.1.9[END]
TRANSLATED:官网: www.dumborc.com

硬件: V1.0.0
软件: V1.1.9[END]

ADDRESS   :0x1441c
LEN_BYTES :60
ORIGINAL  :Über uns:
www.dumborc.com
Hardware: V1.0.0
Software: V1.1.9[END]
TRANSLATED:Über uns:
www.dumborc.com
Hardware: V1.0.0
Software: V1.1.9[END]

ADDRESS   :0x14464
LEN_BYTES :59
ORIGINAL  :About Us:
www.dumborc.com
Hardware: V1.0.0
Software: V1.1.9[END]
TRANSLATED:About Us:
www.dumborc.com
Hardware: V1.0.0
Software: V1.1.9[END]

ADDRESS   :0x144b8
LEN_BYTES :19
ORIGINAL  :恢复出厂设置 [END]
TRANSLATED:恢复出厂设置 [END]

ADDRESS   :0x144cc
LEN_BYTES :36
ORIGINAL  :Zurücksetzen auf Werkseinstellungen[END]
TRANSLATED:Zurücksetzen auf Werkseinstellungen[END]

ADDRESS   :0x14508
LEN_BYTES :5
ORIGINAL  :usine[END]
TRANSLATED:usine[END]

ADDRESS   :0x14510
LEN_BYTES :9
ORIGINAL  :初期化[END]
TRANSLATED:初期化[END]

ADDRESS   :0x1451c
LEN_BYTES :13
ORIGINAL  :Factory Reset[END]
TRANSLATED:Factory Reset[END]

ADDRESS   :0x14938
LEN_BYTES :12
ORIGINAL  :坦克混控[END]
TRANSLATED:坦克混控[END]

ADDRESS   :0x14948
LEN_BYTES :11
ORIGINAL  :Panzermodus[END]
TRANSLATED:Panzermodus[END]

ADDRESS   :0x14954
LEN_BYTES :23
ORIGINAL  :Mélange de réservoirs[END]
TRANSLATED:Mélange de réservoirs[END]

ADDRESS   :0x1496c
LEN_BYTES :21
ORIGINAL  :タンクミックス[END]
TRANSLATED:タンクミックス[END]

ADDRESS   :0x14984
LEN_BYTES :8
ORIGINAL  :Tank MIX[END]
TRANSLATED:Tank MIX[END]

ADDRESS   :0x14e00
LEN_BYTES :12
ORIGINAL  :前进比率[END]
TRANSLATED:前进比率[END]

ADDRESS   :0x14e10
LEN_BYTES :12
ORIGINAL  :Antriebsrate[END]
TRANSLATED:Antriebsrate[END]

ADDRESS   :0x14e20
LEN_BYTES :13
ORIGINAL  :Taux de front[END]
TRANSLATED:Taux de front[END]

ADDRESS   :0x14e30
LEN_BYTES :18
ORIGINAL  :前進スピード[END]
TRANSLATED:前進スピード[END]

ADDRESS   :0x14e44
LEN_BYTES :11
ORIGINAL  :Front Ratio[END]
TRANSLATED:Front Ratio[END]

ADDRESS   :0x14e50
LEN_BYTES :12
ORIGINAL  :后退比率[END]
TRANSLATED:后退比率[END]

ADDRESS   :0x14e60
LEN_BYTES :9
ORIGINAL  :Bremsrate[END]
TRANSLATED:Bremsrate[END]

ADDRESS   :0x14e6c
LEN_BYTES :15
ORIGINAL  :Taux de rupture[END]
TRANSLATED:Taux de rupture[END]

ADDRESS   :0x14e7c
LEN_BYTES :18
ORIGINAL  :後進スピード[END]
TRANSLATED:後進スピード[END]

ADDRESS   :0x14e90
LEN_BYTES :11
ORIGINAL  :Break Ratio[END]
TRANSLATED:Break Ratio[END]

ADDRESS   :0x14e9c
LEN_BYTES :12
ORIGINAL  :左转比率[END]
TRANSLATED:左转比率[END]

ADDRESS   :0x14eac
LEN_BYTES :12
ORIGINAL  :Linke Stufe [END]
TRANSLATED:Linke Stufe [END]

ADDRESS   :0x14ebc
LEN_BYTES :14
ORIGINAL  :Taux de gauche[END]
TRANSLATED:Taux de gauche[END]

ADDRESS   :0x14ecc
LEN_BYTES :19
ORIGINAL  :左折ス
ピード[END]
TRANSLATED:左折ス
ピード[END]

ADDRESS   :0x14ee0
LEN_BYTES :10
ORIGINAL  :Left Ratio[END]
TRANSLATED:Left Ratio[END]

ADDRESS   :0x14eec
LEN_BYTES :12
ORIGINAL  :右转比率[END]
TRANSLATED:右转比率[END]

ADDRESS   :0x14efc
LEN_BYTES :12
ORIGINAL  :Rechte Stufe[END]
TRANSLATED:Rechte Stufe[END]

ADDRESS   :0x14f0c
LEN_BYTES :13
ORIGINAL  :Taux de droit[END]
TRANSLATED:Taux de droit[END]

ADDRESS   :0x14f1c
LEN_BYTES :19
ORIGINAL  :右折ス
ピード[END]
TRANSLATED:右折ス
ピード[END]

ADDRESS   :0x14f30
LEN_BYTES :11
ORIGINAL  :Right Ratio[END]
TRANSLATED:Right Ratio[END]

ADDRESS   :0x150d8
LEN_BYTES :6
ORIGINAL  :通道[END]
TRANSLATED:通道[END]

ADDRESS   :0x150e0
LEN_BYTES :4
ORIGINAL  :%s%d[END]
TRANSLATED:%s%d[END]

ADDRESS   :0x150e8
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:Kanal [END]

ADDRESS   :0x150fc
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x15280
LEN_BYTES :4
ORIGINAL  :1Ip[END]
TRANSLATED:1Ip[END]

ADDRESS   :0x156c4
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x15758
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x15ce0
LEN_BYTES :12
ORIGINAL  :辅助通道[END]
TRANSLATED:辅助通道[END]

ADDRESS   :0x15cf0
LEN_BYTES :9
ORIGINAL  :AUX Kanal[END]
TRANSLATED:AUX Kanal[END]

ADDRESS   :0x15cfc
LEN_BYTES :18
ORIGINAL  :Canal auxiliaires [END]
TRANSLATED:Canal auxiliaires [END]

ADDRESS   :0x15d10
LEN_BYTES :18
ORIGINAL  :AUXチャンネル[END]
TRANSLATED:AUXチャンネル[END]

ADDRESS   :0x15d24
LEN_BYTES :11
ORIGINAL  :AUX Channel[END]
TRANSLATED:AUX Channel[END]

ADDRESS   :0x15d50
LEN_BYTES :4
ORIGINAL  :K-10[END]
TRANSLATED:K-10[END]

ADDRESS   :0x16030
LEN_BYTES :4
ORIGINAL  :XnZH[END]
TRANSLATED:XnZH[END]

ADDRESS   :0x161a0
LEN_BYTES :4
ORIGINAL  :%c%d[END]
TRANSLATED:%c%d[END]

ADDRESS   :0x1680c
LEN_BYTES :4
ORIGINAL  :+0I[END]
TRANSLATED:+0I[END]

ADDRESS   :0x17130
LEN_BYTES :4
ORIGINAL  :oInH[END]
TRANSLATED:oInH[END]

ADDRESS   :0x1713c
LEN_BYTES :4
ORIGINAL  :P!kH[END]
TRANSLATED:P!kH[END]

ADDRESS   :0x17248
LEN_BYTES :12
ORIGINAL  :绞盘混控[END]
TRANSLATED:绞盘混控[END]

ADDRESS   :0x17258
LEN_BYTES :11
ORIGINAL  :Windenmodus[END]
TRANSLATED:Windenmodus[END]

ADDRESS   :0x17264
LEN_BYTES :10
ORIGINAL  :Treuil MIX[END]
TRANSLATED:Treuil MIX[END]

ADDRESS   :0x17270
LEN_BYTES :24
ORIGINAL  :ウインチミックス[END]
TRANSLATED:ウインチミックス[END]

ADDRESS   :0x1728c
LEN_BYTES :9
ORIGINAL  :Winch MIX[END]
TRANSLATED:Winch MIX[END]

ADDRESS   :0x172a4
LEN_BYTES :12
ORIGINAL  :上升按键[END]
TRANSLATED:上升按键[END]

ADDRESS   :0x172b4
LEN_BYTES :9
ORIGINAL  :Aufwärts[END]
TRANSLATED:Aufwärts[END]

ADDRESS   :0x172c0
LEN_BYTES :12
ORIGINAL  :Vers le haut[END]
TRANSLATED:Vers le haut[END]

ADDRESS   :0x172d0
LEN_BYTES :15
ORIGINAL  :出しボタン[END]
TRANSLATED:出しボタン[END]

ADDRESS   :0x172e0
LEN_BYTES :8
ORIGINAL  :Rise key[END]
TRANSLATED:Rise key[END]

ADDRESS   :0x172f4
LEN_BYTES :19
ORIGINAL  :K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0x1771c
LEN_BYTES :12
ORIGINAL  :下降按键[END]
TRANSLATED:下降按键[END]

ADDRESS   :0x1772c
LEN_BYTES :8
ORIGINAL  :Abwärts[END]
TRANSLATED:Abwärts[END]

ADDRESS   :0x17738
LEN_BYTES :11
ORIGINAL  :Vers le bas[END]
TRANSLATED:Vers le bas[END]

ADDRESS   :0x17744
LEN_BYTES :15
ORIGINAL  :巻きボタン[END]
TRANSLATED:巻きボタン[END]

ADDRESS   :0x17754
LEN_BYTES :8
ORIGINAL  :Drop key[END]
TRANSLATED:Drop key[END]

ADDRESS   :0x17794
LEN_BYTES :8
ORIGINAL  :通道 3[END]
TRANSLATED:通道 3[END]

ADDRESS   :0x177a0
LEN_BYTES :7
ORIGINAL  :Kanal 3[END]
TRANSLATED:Kanal 3[END]

ADDRESS   :0x177b4
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x177bc
LEN_BYTES :12
ORIGINAL  :上升比率[END]
TRANSLATED:上升比率[END]

ADDRESS   :0x177cc
LEN_BYTES :15
ORIGINAL  :Steigerungsrate[END]
TRANSLATED:Steigerungsrate[END]

ADDRESS   :0x177e4
LEN_BYTES :11
ORIGINAL  :ugmentation[END]
TRANSLATED:ugmentation[END]

ADDRESS   :0x177f0
LEN_BYTES :18
ORIGINAL  :出しスピード[END]
TRANSLATED:出しスピード[END]

ADDRESS   :0x17804
LEN_BYTES :12
ORIGINAL  :Rising ratio[END]
TRANSLATED:Rising ratio[END]

ADDRESS   :0x17b14
LEN_BYTES :6
ORIGINAL  :停止[END]
TRANSLATED:停止[END]

ADDRESS   :0x17b1c
LEN_BYTES :4
ORIGINAL  :Stop[END]
TRANSLATED:Stop[END]

ADDRESS   :0x17b24
LEN_BYTES :12
ORIGINAL  :ストップ[END]
TRANSLATED:ストップ[END]

ADDRESS   :0x17b3c
LEN_BYTES :12
ORIGINAL  :下降比率[END]
TRANSLATED:下降比率[END]

ADDRESS   :0x17b4c
LEN_BYTES :18
ORIGINAL  :巻きスピード[END]
TRANSLATED:巻きスピード[END]

ADDRESS   :0x17b60
LEN_BYTES :13
ORIGINAL  :Decline ratio[END]
TRANSLATED:Decline ratio[END]

ADDRESS   :0x18578
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x18a8c
LEN_BYTES :12
ORIGINAL  :按键类型[END]
TRANSLATED:按键类型[END]

ADDRESS   :0x18a9c
LEN_BYTES :14
ORIGINAL  :Schlüssel Typ[END]
TRANSLATED:Schlüssel Typ[END]

ADDRESS   :0x18aac
LEN_BYTES :12
ORIGINAL  :Type de clé[END]
TRANSLATED:Type de clé[END]

ADDRESS   :0x18abc
LEN_BYTES :18
ORIGINAL  :ボタンタイプ[END]
TRANSLATED:ボタンタイプ[END]

ADDRESS   :0x18ad0
LEN_BYTES :8
ORIGINAL  :Key Type[END]
TRANSLATED:Key Type[END]

ADDRESS   :0x18af8
LEN_BYTES :4
ORIGINAL  :K-10[END]
TRANSLATED:K-10[END]

ADDRESS   :0x18b08
LEN_BYTES :27
ORIGINAL  :自锁
点动
三段
四段[END]
TRANSLATED:自锁
点动
三段
四段[END]

ADDRESS   :0x18b24
LEN_BYTES :52
ORIGINAL  :Selbstverriegelnd
Momenttaster
Dreistufen
Vierstufen[END]
TRANSLATED:Selbstverriegelnd
Momenttaster
Dreistufen
Vierstufen[END]

ADDRESS   :0x18b5c
LEN_BYTES :60
ORIGINAL  :Auto-verrouillage
Instantané
Trois vitesses
Quatre vitesses[END]
TRANSLATED:Auto-verrouillage
Instantané
Trois vitesses
Quatre vitesses[END]

ADDRESS   :0x18b9c
LEN_BYTES :63
ORIGINAL  :じこほじ
しゅんかんどうさ
さんだん
よんだん[END]
TRANSLATED:じこほじ
しゅんかんどうさ
さんだん
よんだん[END]

ADDRESS   :0x18bdc
LEN_BYTES :45
ORIGINAL  :Self-locking
Momentary
Three-speed
Four-speed[END]
TRANSLATED:Self-locking
Momentary
Three-speed
Four-speed[END]

ADDRESS   :0x19050
LEN_BYTES :12
ORIGINAL  :转向混控[END]
TRANSLATED:转向混控[END]

ADDRESS   :0x19070
LEN_BYTES :12
ORIGINAL  :正相使能[END]
TRANSLATED:正相使能[END]

ADDRESS   :0x19080
LEN_BYTES :9
ORIGINAL  :同位相[END]
TRANSLATED:同位相[END]

ADDRESS   :0x1908c
LEN_BYTES :7
ORIGINAL  :NOR KEY[END]
TRANSLATED:NOR KEY[END]

ADDRESS   :0x1909c
LEN_BYTES :24
ORIGINAL  :NULL
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:NULL
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0x190c4
LEN_BYTES :12
ORIGINAL  :反相使能[END]
TRANSLATED:反相使能[END]

ADDRESS   :0x194cc
LEN_BYTES :9
ORIGINAL  :逆位相[END]
TRANSLATED:逆位相[END]

ADDRESS   :0x194d8
LEN_BYTES :7
ORIGINAL  :REV KEY[END]
TRANSLATED:REV KEY[END]

ADDRESS   :0x19508
LEN_BYTES :7
ORIGINAL  :通道1[END]
TRANSLATED:通道1[END]

ADDRESS   :0x19510
LEN_BYTES :7
ORIGINAL  :Kanal 1[END]
TRANSLATED:Kanal 1[END]

ADDRESS   :0x1952c
LEN_BYTES :7
ORIGINAL  :通道4[END]
TRANSLATED:通道4[END]

ADDRESS   :0x19534
LEN_BYTES :7
ORIGINAL  :Kanal 4[END]
TRANSLATED:Kanal 4[END]

ADDRESS   :0x19974
LEN_BYTES :12
ORIGINAL  :左转比率[END]
TRANSLATED:左转比率[END]

ADDRESS   :0x19984
LEN_BYTES :12
ORIGINAL  :Linke Stufe [END]
TRANSLATED:Linke Stufe [END]

ADDRESS   :0x19994
LEN_BYTES :14
ORIGINAL  :Taux de gauche[END]
TRANSLATED:Taux de gauche[END]

ADDRESS   :0x199a4
LEN_BYTES :19
ORIGINAL  :左折ス
ピード[END]
TRANSLATED:左折ス
ピード[END]

ADDRESS   :0x199b8
LEN_BYTES :10
ORIGINAL  :Left Ratio[END]
TRANSLATED:Left Ratio[END]

ADDRESS   :0x19a30
LEN_BYTES :12
ORIGINAL  :右转比率[END]
TRANSLATED:右转比率[END]

ADDRESS   :0x19a40
LEN_BYTES :12
ORIGINAL  :Rechte Stufe[END]
TRANSLATED:Rechte Stufe[END]

ADDRESS   :0x19a50
LEN_BYTES :13
ORIGINAL  :Taux de droit[END]
TRANSLATED:Taux de droit[END]

ADDRESS   :0x19a60
LEN_BYTES :19
ORIGINAL  :右折ス
ピード[END]
TRANSLATED:右折ス
ピード[END]

ADDRESS   :0x19a74
LEN_BYTES :11
ORIGINAL  :Right Ratio[END]
TRANSLATED:Right Ratio[END]

ADDRESS   :0x19e84
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x1a228
LEN_BYTES :9
ORIGINAL  :重映射[END]
TRANSLATED:重映射[END]

ADDRESS   :0x1a234
LEN_BYTES :14
ORIGINAL  :Überschreiben[END]
TRANSLATED:Überschreiben[END]

ADDRESS   :0x1a244
LEN_BYTES :9
ORIGINAL  :Remappage[END]
TRANSLATED:Remappage[END]

ADDRESS   :0x1a250
LEN_BYTES :27
ORIGINAL  :チャンネル配置設定[END]
TRANSLATED:チャンネル配置設定[END]

ADDRESS   :0x1a26c
LEN_BYTES :9
ORIGINAL  :Remapping[END]
TRANSLATED:Remapping[END]

ADDRESS   :0x1a280
LEN_BYTES :6
ORIGINAL  :通道[END]
TRANSLATED:通道[END]

ADDRESS   :0x1a288
LEN_BYTES :4
ORIGINAL  :%s%d[END]
TRANSLATED:%s%d[END]

ADDRESS   :0x1a290
LEN_BYTES :6
ORIGINAL  :Kanal [END]
TRANSLATED:Kanal [END]

ADDRESS   :0x1a2a4
LEN_BYTES :40
ORIGINAL  :NULL
K-3
K-4
VR-5
VR-6
SW-7
K-8
K-9
K-10[END]
TRANSLATED:NULL
K-3
K-4
VR-5
VR-6
SW-7
K-8
K-9
K-10[END]

ADDRESS   :0x1a2dc
LEN_BYTES :4
ORIGINAL  :1[END]
TRANSLATED:1[END]

ADDRESS   :0x1a6fc
LEN_BYTES :12
ORIGINAL  :程序混控[END]
TRANSLATED:程序混控[END]

ADDRESS   :0x1a710
LEN_BYTES :12
ORIGINAL  :Programm MIX[END]
TRANSLATED:Programm MIX[END]

ADDRESS   :0x1a720
LEN_BYTES :13
ORIGINAL  :Programme MIX[END]
TRANSLATED:Programme MIX[END]

ADDRESS   :0x1a730
LEN_BYTES :27
ORIGINAL  :プログラムミックス[END]
TRANSLATED:プログラムミックス[END]

ADDRESS   :0x1a74c
LEN_BYTES :11
ORIGINAL  :Program MIX[END]
TRANSLATED:Program MIX[END]

ADDRESS   :0x1a764
LEN_BYTES :12
ORIGINAL  :使能开关[END]
TRANSLATED:使能开关[END]

ADDRESS   :0x1a774
LEN_BYTES :6
ORIGINAL  :EN KEY[END]
TRANSLATED:EN KEY[END]

ADDRESS   :0x1a77c
LEN_BYTES :18
ORIGINAL  :有効化ボタン[END]
TRANSLATED:有効化ボタン[END]

ADDRESS   :0x1a798
LEN_BYTES :24
ORIGINAL  :NULL
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:NULL
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0x1ac00
LEN_BYTES :44
ORIGINAL  :8FCH1
CH2
CH3
CH4
CH5
CH6
CH7
CH8
CH9
CH10[END]
TRANSLATED:8FCH1
CH2
CH3
CH4
CH5
CH6
CH7
CH8
CH9
CH10[END]

ADDRESS   :0x1b040
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x1b068
LEN_BYTES :6
ORIGINAL  :8F[END]
TRANSLATED:8F[END]

ADDRESS   :0x1b080
LEN_BYTES :6
ORIGINAL  :反相[END]
TRANSLATED:反相[END]

ADDRESS   :0x1b3c4
LEN_BYTES :12
ORIGINAL  :リバース[END]
TRANSLATED:リバース[END]

ADDRESS   :0x1b400
LEN_BYTES :6
ORIGINAL  :正相[END]
TRANSLATED:正相[END]

ADDRESS   :0x1b40c
LEN_BYTES :12
ORIGINAL  :ノーマル[END]
TRANSLATED:ノーマル[END]

ADDRESS   :0x1b858
LEN_BYTES :6
ORIGINAL  :AKU_DH[END]
TRANSLATED:AKU_DH[END]

ADDRESS   :0x1b9a4
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x1be94
LEN_BYTES :12
ORIGINAL  :程序混控[END]
TRANSLATED:程序混控[END]

ADDRESS   :0x1bea8
LEN_BYTES :12
ORIGINAL  :Programm MIX[END]
TRANSLATED:Programm MIX[END]

ADDRESS   :0x1beb8
LEN_BYTES :13
ORIGINAL  :Programme MIX[END]
TRANSLATED:Programme MIX[END]

ADDRESS   :0x1bec8
LEN_BYTES :27
ORIGINAL  :プログラムミックス[END]
TRANSLATED:プログラムミックス[END]

ADDRESS   :0x1bee4
LEN_BYTES :11
ORIGINAL  :Program MIX[END]
TRANSLATED:Program MIX[END]

ADDRESS   :0x1befc
LEN_BYTES :12
ORIGINAL  :使能开关[END]
TRANSLATED:使能开关[END]

ADDRESS   :0x1bf0c
LEN_BYTES :6
ORIGINAL  :EN KEY[END]
TRANSLATED:EN KEY[END]

ADDRESS   :0x1bf14
LEN_BYTES :18
ORIGINAL  :有効化ボタン[END]
TRANSLATED:有効化ボタン[END]

ADDRESS   :0x1bf30
LEN_BYTES :24
ORIGINAL  :NULL
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:NULL
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0x1c398
LEN_BYTES :44
ORIGINAL  :8FCH1
CH2
CH3
CH4
CH5
CH6
CH7
CH8
CH9
CH10[END]
TRANSLATED:8FCH1
CH2
CH3
CH4
CH5
CH6
CH7
CH8
CH9
CH10[END]

ADDRESS   :0x1c7d8
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x1c800
LEN_BYTES :6
ORIGINAL  :8F[END]
TRANSLATED:8F[END]

ADDRESS   :0x1c818
LEN_BYTES :6
ORIGINAL  :反相[END]
TRANSLATED:反相[END]

ADDRESS   :0x1cb5c
LEN_BYTES :12
ORIGINAL  :リバース[END]
TRANSLATED:リバース[END]

ADDRESS   :0x1cb98
LEN_BYTES :6
ORIGINAL  :正相[END]
TRANSLATED:正相[END]

ADDRESS   :0x1cba4
LEN_BYTES :12
ORIGINAL  :ノーマル[END]
TRANSLATED:ノーマル[END]

ADDRESS   :0x1cea0
LEN_BYTES :6
ORIGINAL  :AKU_DH[END]
TRANSLATED:AKU_DH[END]

ADDRESS   :0x1cfec
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x1d100
LEN_BYTES :4
ORIGINAL  :ֲ[END]
TRANSLATED:ֲ[END]

ADDRESS   :0x1d54c
LEN_BYTES :6
ORIGINAL  :lHhH[END]
TRANSLATED:lHhH[END]

ADDRESS   :0x1d6cc
LEN_BYTES :7
ORIGINAL  :电源 [END]
TRANSLATED:电源 [END]

ADDRESS   :0x1d6d4
LEN_BYTES :5
ORIGINAL  :Strom[END]
TRANSLATED:Strom[END]

ADDRESS   :0x1d6dc
LEN_BYTES :9
ORIGINAL  :Puissance[END]
TRANSLATED:Puissance[END]

ADDRESS   :0x1d6e8
LEN_BYTES :12
ORIGINAL  :電源設定[END]
TRANSLATED:電源設定[END]

ADDRESS   :0x1d6f8
LEN_BYTES :5
ORIGINAL  :Power[END]
TRANSLATED:Power[END]

ADDRESS   :0x1d704
LEN_BYTES :13
ORIGINAL  :闲置报警 [END]
TRANSLATED:闲置报警 [END]

ADDRESS   :0x1d714
LEN_BYTES :14
ORIGINAL  :Leerlauf Alarm[END]
TRANSLATED:Leerlauf Alarm[END]

ADDRESS   :0x1d724
LEN_BYTES :17
ORIGINAL  :Alarme au ralenti[END]
TRANSLATED:Alarme au ralenti[END]

ADDRESS   :0x1d738
LEN_BYTES :9
ORIGINAL  :警告音[END]
TRANSLATED:警告音[END]

ADDRESS   :0x1d744
LEN_BYTES :10
ORIGINAL  :Idle Alarm[END]
TRANSLATED:Idle Alarm[END]

ADDRESS   :0x1d758
LEN_BYTES :39
ORIGINAL  :  关闭 
15分钟 
30分钟 
60分钟 [END]
TRANSLATED:  关闭 
15分钟 
30分钟 
60分钟 [END]

ADDRESS   :0x1d780
LEN_BYTES :34
ORIGINAL  :Schließen 
15 min 
30 min 
60 min[END]
TRANSLATED:Schließen 
15 min 
30 min 
60 min[END]

ADDRESS   :0x1d7a4
LEN_BYTES :30
ORIGINAL  :Fermer 
15 min 
30 min 
60 min[END]
TRANSLATED:Fermer 
15 min 
30 min 
60 min[END]

ADDRESS   :0x1d7c4
LEN_BYTES :27
ORIGINAL  :オフ
15 分
30 分
60 分[END]
TRANSLATED:オフ
15 分
30 分
60 分[END]

ADDRESS   :0x1d7e0
LEN_BYTES :29
ORIGINAL  :Close 
15 min 
30 min 
60 min[END]
TRANSLATED:Close 
15 min 
30 min 
60 min[END]

ADDRESS   :0x1d92c
LEN_BYTES :4
ORIGINAL  :H[END]
TRANSLATED:H[END]

ADDRESS   :0x1dbd4
LEN_BYTES :13
ORIGINAL  :自动关机 [END]
TRANSLATED:自动关机 [END]

ADDRESS   :0x1dbe4
LEN_BYTES :8
ORIGINAL  :Auto Off[END]
TRANSLATED:Auto Off[END]

ADDRESS   :0x1dbf8
LEN_BYTES :11
ORIGINAL  :Arrêt auto[END]
TRANSLATED:Arrêt auto[END]

ADDRESS   :0x1dc04
LEN_BYTES :24
ORIGINAL  :オートパワーオフ[END]
TRANSLATED:オートパワーオフ[END]

ADDRESS   :0x1dc2c
LEN_BYTES :56
ORIGINAL  :  关闭 
闲置5分钟 
闲置10分钟 
闲置20分钟 [END]
TRANSLATED:  关闭 
闲置5分钟 
闲置10分钟 
闲置20分钟 [END]

ADDRESS   :0x1dc68
LEN_BYTES :54
ORIGINAL  :Schließen 
Leerlauf 5 m 
Leerlauf 10 m 
Leerlauf 20 m[END]
TRANSLATED:Schließen 
Leerlauf 5 m 
Leerlauf 10 m 
Leerlauf 20 m[END]

ADDRESS   :0x1dca0
LEN_BYTES :44
ORIGINAL  :Fermer 
Idle 5 min 
Idle 10 min 
Idle 20 min[END]
TRANSLATED:Fermer 
Idle 5 min 
Idle 10 min 
Idle 20 min[END]

ADDRESS   :0x1dcd0
LEN_BYTES :26
ORIGINAL  :オフ
5 分
10 分
20 分[END]
TRANSLATED:オフ
5 分
10 分
20 分[END]

ADDRESS   :0x1dcec
LEN_BYTES :43
ORIGINAL  :Close 
Idle 5 min 
Idle 10 min 
Idle 20 min[END]
TRANSLATED:Close 
Idle 5 min 
Idle 10 min 
Idle 20 min[END]

ADDRESS   :0x1dd30
LEN_BYTES :13
ORIGINAL  :电池类型 [END]
TRANSLATED:电池类型 [END]

ADDRESS   :0x1dd40
LEN_BYTES :12
ORIGINAL  :Batterie Typ[END]
TRANSLATED:Batterie Typ[END]

ADDRESS   :0x1dd50
LEN_BYTES :16
ORIGINAL  :Type de batterie[END]
TRANSLATED:Type de batterie[END]

ADDRESS   :0x1dd64
LEN_BYTES :24
ORIGINAL  :バッテリータイプ[END]
TRANSLATED:バッテリータイプ[END]

ADDRESS   :0x1dd80
LEN_BYTES :12
ORIGINAL  :Battery Type[END]
TRANSLATED:Battery Type[END]

ADDRESS   :0x1dd94
LEN_BYTES :18
ORIGINAL  :   4AA
2S
3S
4NiMh[END]
TRANSLATED:   4AA
2S
3S
4NiMh[END]

ADDRESS   :0x1ddb0
LEN_BYTES :13
ORIGINAL  :电压报警 [END]
TRANSLATED:电压报警 [END]

ADDRESS   :0x1ddc0
LEN_BYTES :14
ORIGINAL  :Spannung Alarm[END]
TRANSLATED:Spannung Alarm[END]

ADDRESS   :0x1e1b0
LEN_BYTES :17
ORIGINAL  :Alarme de tension[END]
TRANSLATED:Alarme de tension[END]

ADDRESS   :0x1e1c8
LEN_BYTES :21
ORIGINAL  :低電圧アラーム[END]
TRANSLATED:低電圧アラーム[END]

ADDRESS   :0x1e1e0
LEN_BYTES :13
ORIGINAL  :Voltage alarm[END]
TRANSLATED:Voltage alarm[END]

ADDRESS   :0x1e204
LEN_BYTES :6
ORIGINAL  :%d.%dV[END]
TRANSLATED:%d.%dV[END]

ADDRESS   :0x1e22c
LEN_BYTES :20
ORIGINAL  :当前电压        [END]
TRANSLATED:当前电压        [END]

ADDRESS   :0x1e244
LEN_BYTES :17
ORIGINAL  :%s      %d.%02d V[END]
TRANSLATED:%s      %d.%02d V[END]

ADDRESS   :0x1e258
LEN_BYTES :17
ORIGINAL  :Aktuelle Spannung[END]
TRANSLATED:Aktuelle Spannung[END]

ADDRESS   :0x1e26c
LEN_BYTES :12
ORIGINAL  :%s %d.%02d V[END]
TRANSLATED:%s %d.%02d V[END]

ADDRESS   :0x1e27c
LEN_BYTES :16
ORIGINAL  :Tension actuelle[END]
TRANSLATED:Tension actuelle[END]

ADDRESS   :0x1e290
LEN_BYTES :13
ORIGINAL  :%s  %d.%02d V[END]
TRANSLATED:%s  %d.%02d V[END]

ADDRESS   :0x1e2a0
LEN_BYTES :12
ORIGINAL  :電圧表示[END]
TRANSLATED:電圧表示[END]

ADDRESS   :0x1e2b0
LEN_BYTES :15
ORIGINAL  :Current Voltage[END]
TRANSLATED:Current Voltage[END]

ADDRESS   :0x1e2c4
LEN_BYTES :13
ORIGINAL  :电压校准 [END]
TRANSLATED:电压校准 [END]

ADDRESS   :0x1e2d4
LEN_BYTES :20
ORIGINAL  :Spannung Kalibrieren[END]
TRANSLATED:Spannung Kalibrieren[END]

ADDRESS   :0x1e2ec
LEN_BYTES :25
ORIGINAL  :Étalonnage de la tension[END]
TRANSLATED:Étalonnage de la tension[END]

ADDRESS   :0x1e308
LEN_BYTES :12
ORIGINAL  :電圧校正[END]
TRANSLATED:電圧校正[END]

ADDRESS   :0x1e318
LEN_BYTES :18
ORIGINAL  :Voltage Calibrator[END]
TRANSLATED:Voltage Calibrator[END]

ADDRESS   :0x1e440
LEN_BYTES :6
ORIGINAL  :Yh[END]
TRANSLATED:Yh[END]

ADDRESS   :0x1e5c0
LEN_BYTES :6
ORIGINAL  :DIpDH[END]
TRANSLATED:DIpDH[END]

ADDRESS   :0x1e814
LEN_BYTES :6
ORIGINAL  :IIpIH[END]
TRANSLATED:IIpIH[END]

ADDRESS   :0x1e834
LEN_BYTES :6
ORIGINAL  :CIpAH[END]
TRANSLATED:CIpAH[END]

ADDRESS   :0x1f208
LEN_BYTES :18
ORIGINAL  :设置陀螺舵量[END]
TRANSLATED:设置陀螺舵量[END]

ADDRESS   :0x1f21c
LEN_BYTES :10
ORIGINAL  :Set GY EPA[END]
TRANSLATED:Set GY EPA[END]

ADDRESS   :0x1f228
LEN_BYTES :18
ORIGINAL  :ジャイロ設定[END]
TRANSLATED:ジャイロ設定[END]

ADDRESS   :0x1f244
LEN_BYTES :18
ORIGINAL  :设置失控保护[END]
TRANSLATED:设置失控保护[END]

ADDRESS   :0x1f258
LEN_BYTES :6
ORIGINAL  :Set FS[END]
TRANSLATED:Set FS[END]

ADDRESS   :0x1f260
LEN_BYTES :27
ORIGINAL  :フェイルセーフ設定[END]
TRANSLATED:フェイルセーフ設定[END]

ADDRESS   :0x1f27c
LEN_BYTES :40
ORIGINAL  :仅P系列接收机支持本界面调参[END]
TRANSLATED:仅P系列接收机支持本界面调参[END]

ADDRESS   :0x1f2a8
LEN_BYTES :4
ORIGINAL  :%s ![END]
TRANSLATED:%s ![END]

ADDRESS   :0x1f2b0
LEN_BYTES :46
ORIGINAL  :Only P series receivers support this interface[END]
TRANSLATED:Only P series receivers support this interface[END]

ADDRESS   :0x1f2e4
LEN_BYTES :6
ORIGINAL  :=Hx
[END]
TRANSLATED:=Hx
[END]

ADDRESS   :0x1f820
LEN_BYTES :7
ORIGINAL  :%d.%d%s[END]
TRANSLATED:%d.%d%s[END]

ADDRESS   :0x1f9f4
LEN_BYTES :7
ORIGINAL  :%d.%d%s[END]
TRANSLATED:%d.%d%s[END]

ADDRESS   :0x1fd54
LEN_BYTES :4
ORIGINAL  :tIYH[END]
TRANSLATED:tIYH[END]

ADDRESS   :0x1fdec
LEN_BYTES :4
ORIGINAL  :_!OH[END]
TRANSLATED:_!OH[END]

ADDRESS   :0x1fe30
LEN_BYTES :9
ORIGINAL  :接收机[END]
TRANSLATED:接收机[END]

ADDRESS   :0x1fe3c
LEN_BYTES :8
ORIGINAL  :Receiver[END]
TRANSLATED:Receiver[END]

ADDRESS   :0x1fe48
LEN_BYTES :9
ORIGINAL  :Réglages[END]
TRANSLATED:Réglages[END]

ADDRESS   :0x1fe54
LEN_BYTES :9
ORIGINAL  :受信機[END]
TRANSLATED:受信機[END]

ADDRESS   :0x1fe60
LEN_BYTES :12
ORIGINAL  :通讯协议[END]
TRANSLATED:通讯协议[END]

ADDRESS   :0x1fe70
LEN_BYTES :11
ORIGINAL  :RF abkommen[END]
TRANSLATED:RF abkommen[END]

ADDRESS   :0x1fe7c
LEN_BYTES :16
ORIGINAL  :Protocoles de RF[END]
TRANSLATED:Protocoles de RF[END]

ADDRESS   :0x1fe90
LEN_BYTES :30
ORIGINAL  :無線周波数プロトコル[END]
TRANSLATED:無線周波数プロトコル[END]

ADDRESS   :0x1feb0
LEN_BYTES :11
ORIGINAL  :RF protocol[END]
TRANSLATED:RF protocol[END]

ADDRESS   :0x1fec4
LEN_BYTES :13
ORIGINAL  :标准
快速[END]
TRANSLATED:标准
快速[END]

ADDRESS   :0x1fed4
LEN_BYTES :14
ORIGINAL  :Normal
Schnell[END]
TRANSLATED:Normal
Schnell[END]

ADDRESS   :0x1fee4
LEN_BYTES :13
ORIGINAL  :Norme
Rapides[END]
TRANSLATED:Norme
Rapides[END]

ADDRESS   :0x1fef4
LEN_BYTES :26
ORIGINAL  :ノーマル
ファ-スト[END]
TRANSLATED:ノーマル
ファ-スト[END]

ADDRESS   :0x1ff10
LEN_BYTES :11
ORIGINAL  :Normal
Fast[END]
TRANSLATED:Normal
Fast[END]

ADDRESS   :0x1ff70
LEN_BYTES :6
ORIGINAL  :THhTH[END]
TRANSLATED:THhTH[END]

ADDRESS   :0x1ff7c
LEN_BYTES :4
ORIGINAL  :_!RH[END]
TRANSLATED:_!RH[END]

ADDRESS   :0x200d4
LEN_BYTES :6
ORIGINAL  :对码[END]
TRANSLATED:对码[END]

ADDRESS   :0x200dc
LEN_BYTES :6
ORIGINAL  :Binde![END]
TRANSLATED:Binde![END]

ADDRESS   :0x200e4
LEN_BYTES :7
ORIGINAL  :Reliure[END]
TRANSLATED:Reliure[END]

ADDRESS   :0x200ec
LEN_BYTES :12
ORIGINAL  :バインド[END]
TRANSLATED:バインド[END]

ADDRESS   :0x200fc
LEN_BYTES :7
ORIGINAL  :Binding[END]
TRANSLATED:Binding[END]

ADDRESS   :0x2010c
LEN_BYTES :40
ORIGINAL  :仅P系列接收机支持本界面调参[END]
TRANSLATED:仅P系列接收机支持本界面调参[END]

ADDRESS   :0x20138
LEN_BYTES :4
ORIGINAL  :%s ![END]
TRANSLATED:%s ![END]

ADDRESS   :0x20140
LEN_BYTES :46
ORIGINAL  :Only P series receivers support this interface[END]
TRANSLATED:Only P series receivers support this interface[END]

ADDRESS   :0x202f0
LEN_BYTES :4
ORIGINAL  :jIh[END]
TRANSLATED:jIh[END]

ADDRESS   :0x202fc
LEN_BYTES :6
ORIGINAL  :AB
F-[END]
TRANSLATED:AB
F-[END]

ADDRESS   :0x204b4
LEN_BYTES :36
ORIGINAL  :%s 信号强度 
      #000000 %d%s#[END]
TRANSLATED:%s 信号强度 
      #000000 %d%s#[END]

ADDRESS   :0x204dc
LEN_BYTES :36
ORIGINAL  :%s 受信感度 
      #000000 %d%s#[END]
TRANSLATED:%s 受信感度 
      #000000 %d%s#[END]

ADDRESS   :0x20504
LEN_BYTES :28
ORIGINAL  :%s RSSI 
      #000000 %d%s#[END]
TRANSLATED:%s RSSI 
      #000000 %d%s#[END]

ADDRESS   :0x20524
LEN_BYTES :34
ORIGINAL  :%s 信号强度 
      #000000 无[END]
TRANSLATED:%s 信号强度 
      #000000 无[END]

ADDRESS   :0x20548
LEN_BYTES :34
ORIGINAL  :%s 受信感度 
      #000000 無[END]
TRANSLATED:%s 受信感度 
      #000000 無[END]

ADDRESS   :0x2056c
LEN_BYTES :28
ORIGINAL  :%s RSSI 
      #000000 NULL#[END]
TRANSLATED:%s RSSI 
      #000000 NULL#[END]

ADDRESS   :0x21304
LEN_BYTES :8
ORIGINAL  : x%IpH[END]
TRANSLATED: x%IpH[END]

ADDRESS   :0x21524
LEN_BYTES :37
ORIGINAL  :%s 回传电压
      #000000 %d.%dV#[END]
TRANSLATED:%s 回传电压
      #000000 %d.%dV#[END]

ADDRESS   :0x2154c
LEN_BYTES :32
ORIGINAL  :%s EXT Vol 
      #000000 %d.%dV[END]
TRANSLATED:%s EXT Vol 
      #000000 %d.%dV[END]

ADDRESS   :0x21570
LEN_BYTES :32
ORIGINAL  :%s EXT Ten 
      #000000 %d.%dV[END]
TRANSLATED:%s EXT Ten 
      #000000 %d.%dV[END]

ADDRESS   :0x21594
LEN_BYTES :35
ORIGINAL  :%s EXT 電圧 
      #000000 %d.%dV[END]
TRANSLATED:%s EXT 電圧 
      #000000 %d.%dV[END]

ADDRESS   :0x215bc
LEN_BYTES :35
ORIGINAL  :%s 回传电压
       #000000 无#[END]
TRANSLATED:%s 回传电压
       #000000 无#[END]

ADDRESS   :0x215e0
LEN_BYTES :31
ORIGINAL  :%s EXT Vol 
      #000000 NULL#[END]
TRANSLATED:%s EXT Vol 
      #000000 NULL#[END]

ADDRESS   :0x21600
LEN_BYTES :31
ORIGINAL  :%s EXT Ten 
      #000000 NULL#[END]
TRANSLATED:%s EXT Ten 
      #000000 NULL#[END]

ADDRESS   :0x21620
LEN_BYTES :33
ORIGINAL  :%s EXT 電圧 
      #000000 無#[END]
TRANSLATED:%s EXT 電圧 
      #000000 無#[END]

ADDRESS   :0x218b0
LEN_BYTES :22
ORIGINAL  :~Ip~Ip~Ipd ~Ip~Ip[END]
TRANSLATED:~Ip~Ip~Ipd ~Ip~Ip[END]

ADDRESS   :0x21924
LEN_BYTES :16
ORIGINAL  :tIp tIp sIp[END]
TRANSLATED:tIp tIp sIp[END]

ADDRESS   :0x21b8c
LEN_BYTES :6
ORIGINAL  :Z Ip[END]
TRANSLATED:Z Ip[END]

ADDRESS   :0x21c54
LEN_BYTES :6
ORIGINAL  :xHhuH[END]
TRANSLATED:xHhuH[END]

ADDRESS   :0x21e44
LEN_BYTES :12
ORIGINAL  :舵机速度[END]
TRANSLATED:舵机速度[END]

ADDRESS   :0x21e54
LEN_BYTES :12
ORIGINAL  :Rudder Speed[END]
TRANSLATED:Rudder Speed[END]

ADDRESS   :0x21e64
LEN_BYTES :15
ORIGINAL  :サーボ速度[END]
TRANSLATED:サーボ速度[END]

ADDRESS   :0x21e7c
LEN_BYTES :21
ORIGINAL  :67HZ
250HZ
50HZ
300HZ[END]
TRANSLATED:67HZ
250HZ
50HZ
300HZ[END]

ADDRESS   :0x21f78
LEN_BYTES :4
ORIGINAL  :A5H[END]
TRANSLATED:A5H[END]

ADDRESS   :0x22614
LEN_BYTES :4
ORIGINAL  :pGF[END]
TRANSLATED:pGF[END]

ADDRESS   :0x23210
LEN_BYTES :6
ORIGINAL  :6Ip6H[END]
TRANSLATED:6Ip6H[END]

ADDRESS   :0x23238
LEN_BYTES :4
ORIGINAL  :.I/H[END]
TRANSLATED:.I/H[END]

ADDRESS   :0x23724
LEN_BYTES :18
ORIGINAL  :舵机摆动控制[END]
TRANSLATED:舵机摆动控制[END]

ADDRESS   :0x23738
LEN_BYTES :24
ORIGINAL  :Servoarm-Schwenkregelung[END]
TRANSLATED:Servoarm-Schwenkregelung[END]

ADDRESS   :0x23754
LEN_BYTES :33
ORIGINAL  :Contrôle de balancement du servo[END]
TRANSLATED:Contrôle de balancement du servo[END]

ADDRESS   :0x23778
LEN_BYTES :27
ORIGINAL  :サーボスイング制御[END]
TRANSLATED:サーボスイング制御[END]

ADDRESS   :0x23794
LEN_BYTES :19
ORIGINAL  :Servo Swing Control[END]
TRANSLATED:Servo Swing Control[END]

ADDRESS   :0x237b8
LEN_BYTES :6
ORIGINAL  :模式[END]
TRANSLATED:模式[END]

ADDRESS   :0x237c0
LEN_BYTES :5
ORIGINAL  :Modus[END]
TRANSLATED:Modus[END]

ADDRESS   :0x237c8
LEN_BYTES :4
ORIGINAL  :Mode[END]
TRANSLATED:Mode[END]

ADDRESS   :0x237d0
LEN_BYTES :12
ORIGINAL  :モード‌[END]
TRANSLATED:モード‌[END]

ADDRESS   :0x237e4
LEN_BYTES :15
ORIGINAL  :模式1
模式2[END]
TRANSLATED:模式1
模式2[END]

ADDRESS   :0x237f4
LEN_BYTES :21
ORIGINAL  :Modus‌ 1
Modus‌ 2[END]
TRANSLATED:Modus‌ 1
Modus‌ 2[END]

ADDRESS   :0x2380c
LEN_BYTES :19
ORIGINAL  :Mode‌ 1
Mode‌ 2[END]
TRANSLATED:Mode‌ 1
Mode‌ 2[END]

ADDRESS   :0x23820
LEN_BYTES :21
ORIGINAL  :モード1
モード2[END]
TRANSLATED:モード1
モード2[END]

ADDRESS   :0x23a14
LEN_BYTES :6
ORIGINAL  :x 
#F[END]
TRANSLATED:x 
#F[END]

ADDRESS   :0x23b10
LEN_BYTES :4
ORIGINAL  :jIzH[END]
TRANSLATED:jIzH[END]

ADDRESS   :0x23b68
LEN_BYTES :4
ORIGINAL  :/IdH[END]
TRANSLATED:/IdH[END]

ADDRESS   :0x23c40
LEN_BYTES :12
ORIGINAL  :速度切换[END]
TRANSLATED:速度切换[END]

ADDRESS   :0x23c50
LEN_BYTES :13
ORIGINAL  :Umschalttaste[END]
TRANSLATED:Umschalttaste[END]

ADDRESS   :0x23c60
LEN_BYTES :21
ORIGINAL  :Bouton de commutation[END]
TRANSLATED:Bouton de commutation[END]

ADDRESS   :0x23c78
LEN_BYTES :21
ORIGINAL  :切り替えボタン[END]
TRANSLATED:切り替えボタン[END]

ADDRESS   :0x23c90
LEN_BYTES :6
ORIGINAL  :Switch[END]
TRANSLATED:Switch[END]

ADDRESS   :0x23c9c
LEN_BYTES :24
ORIGINAL  :NULL
K-3
K-4
K-8
K-9
K10[END]
TRANSLATED:NULL
K-3
K-4
K-8
K-9
K10[END]

ADDRESS   :0x23cc4
LEN_BYTES :12
ORIGINAL  :速度设置[END]
TRANSLATED:速度设置[END]

ADDRESS   :0x23cd4
LEN_BYTES :15
ORIGINAL  :Geschwindigkeit[END]
TRANSLATED:Geschwindigkeit[END]

ADDRESS   :0x23ce4
LEN_BYTES :7
ORIGINAL  :Vitesse[END]
TRANSLATED:Vitesse[END]

ADDRESS   :0x23cec
LEN_BYTES :6
ORIGINAL  :速度[END]
TRANSLATED:速度[END]

ADDRESS   :0x23cf4
LEN_BYTES :5
ORIGINAL  :Speed[END]
TRANSLATED:Speed[END]

ADDRESS   :0x23d00
LEN_BYTES :14
ORIGINAL  :NULL
VR-5
VR-6[END]
TRANSLATED:NULL
VR-5
VR-6[END]

ADDRESS   :0x24140
LEN_BYTES :6
ORIGINAL  :%d.%dS[END]
TRANSLATED:%d.%dS[END]

ADDRESS   :0x24154
LEN_BYTES :6
ORIGINAL  :͔h[END]
TRANSLATED:͔h[END]

ADDRESS   :0x24164
LEN_BYTES :8
ORIGINAL  :通道10[END]
TRANSLATED:通道10[END]

ADDRESS   :0x24170
LEN_BYTES :8
ORIGINAL  :Kanal 10[END]
TRANSLATED:Kanal 10[END]

ADDRESS   :0x2417c
LEN_BYTES :4
ORIGINAL  :CH10[END]
TRANSLATED:CH10[END]

ADDRESS   :0x24190
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x2419c
LEN_BYTES :7
ORIGINAL  :状态:[END]
TRANSLATED:状态:[END]

ADDRESS   :0x241a4
LEN_BYTES :7
ORIGINAL  :Status:[END]
TRANSLATED:Status:[END]

ADDRESS   :0x241ac
LEN_BYTES :15
ORIGINAL  :ステータス[END]
TRANSLATED:ステータス[END]

ADDRESS   :0x24240
LEN_BYTES :4
ORIGINAL  :/I.H[END]
TRANSLATED:/I.H[END]

ADDRESS   :0x2424c
LEN_BYTES :4
ORIGINAL  :-I+H[END]
TRANSLATED:-I+H[END]

ADDRESS   :0x24390
LEN_BYTES :6
ORIGINAL  :GKpAH[END]
TRANSLATED:GKpAH[END]

ADDRESS   :0x24724
LEN_BYTES :6
ORIGINAL  :%d.%dS[END]
TRANSLATED:%d.%dS[END]

ADDRESS   :0x24884
LEN_BYTES :5
ORIGINAL  :%3d%s[END]
TRANSLATED:%3d%s[END]

ADDRESS   :0x248c8
LEN_BYTES :6
ORIGINAL  :%d.%dS[END]
TRANSLATED:%d.%dS[END]

ADDRESS   :0x24e44
LEN_BYTES :10
ORIGINAL  :aHpaHp_H[END]
TRANSLATED:aHpaHp_H[END]

ADDRESS   :0x25aa8
LEN_BYTES :4
ORIGINAL  :!F [END]
TRANSLATED:!F [END]

ADDRESS   :0x25ad4
LEN_BYTES :4
ORIGINAL  :!F [END]
TRANSLATED:!F [END]

ADDRESS   :0x26554
LEN_BYTES :12
ORIGINAL  :#24d8a8 #[END]
TRANSLATED:#24d8a8 #[END]

ADDRESS   :0x26928
LEN_BYTES :29
ORIGINAL  :%s 计时器 
 %02d:%02d:%02d[END]
TRANSLATED:%s 计时器 
 %02d:%02d:%02d[END]

ADDRESS   :0x26948
LEN_BYTES :25
ORIGINAL  :%s Timer 
 %02d:%02d:%02d[END]
TRANSLATED:%s Timer 
 %02d:%02d:%02d[END]

ADDRESS   :0x26964
LEN_BYTES :30
ORIGINAL  :%s Minuterie..
 %02d:%02d:%02d[END]
TRANSLATED:%s Minuterie..
 %02d:%02d:%02d[END]

ADDRESS   :0x26984
LEN_BYTES :32
ORIGINAL  :%s タイマー 
 %02d:%02d:%02d[END]
TRANSLATED:%s タイマー 
 %02d:%02d:%02d[END]

ADDRESS   :0x269f8
LEN_BYTES :8
ORIGINAL  :1Hh1Hh[END]
TRANSLATED:1Hh1Hh[END]

ADDRESS   :0x27274
LEN_BYTES :6
ORIGINAL  : pdH[END]
TRANSLATED: pdH[END]

ADDRESS   :0x2727c
LEN_BYTES :6
ORIGINAL  : pd~H[END]
TRANSLATED: pd~H[END]

ADDRESS   :0x272ac
LEN_BYTES :6
ORIGINAL  : pdwH[END]
TRANSLATED: pdwH[END]

ADDRESS   :0x272bc
LEN_BYTES :6
ORIGINAL  : pdtH[END]
TRANSLATED: pdtH[END]

ADDRESS   :0x272cc
LEN_BYTES :6
ORIGINAL  : pdqH[END]
TRANSLATED: pdqH[END]

ADDRESS   :0x272f4
LEN_BYTES :6
ORIGINAL  : pdjH[END]
TRANSLATED: pdjH[END]

ADDRESS   :0x272fc
LEN_BYTES :6
ORIGINAL  : pdiH[END]
TRANSLATED: pdiH[END]

ADDRESS   :0x27304
LEN_BYTES :6
ORIGINAL  : pdhH[END]
TRANSLATED: pdhH[END]

ADDRESS   :0x2730c
LEN_BYTES :6
ORIGINAL  : pdgH[END]
TRANSLATED: pdgH[END]

ADDRESS   :0x2731c
LEN_BYTES :6
ORIGINAL  : pdeH[END]
TRANSLATED: pdeH[END]

ADDRESS   :0x2732c
LEN_BYTES :6
ORIGINAL  : pdbH[END]
TRANSLATED: pdbH[END]

ADDRESS   :0x27334
LEN_BYTES :6
ORIGINAL  : pdaH[END]
TRANSLATED: pdaH[END]

ADDRESS   :0x27344
LEN_BYTES :6
ORIGINAL  : pd_H[END]
TRANSLATED: pd_H[END]

ADDRESS   :0x2735c
LEN_BYTES :6
ORIGINAL  : pd\H[END]
TRANSLATED: pd\H[END]

ADDRESS   :0x274ec
LEN_BYTES :4
ORIGINAL  :dAH[END]
TRANSLATED:dAH[END]

ADDRESS   :0x275a4
LEN_BYTES :4
ORIGINAL  :d!H[END]
TRANSLATED:d!H[END]

ADDRESS   :0x275ac
LEN_BYTES :4
ORIGINAL  :d H[END]
TRANSLATED:d H[END]

ADDRESS   :0x276f8
LEN_BYTES :6
ORIGINAL  : pd8H[END]
TRANSLATED: pd8H[END]

ADDRESS   :0x27700
LEN_BYTES :6
ORIGINAL  : pd7H[END]
TRANSLATED: pd7H[END]

ADDRESS   :0x27708
LEN_BYTES :6
ORIGINAL  : pd6H[END]
TRANSLATED: pd6H[END]

ADDRESS   :0x27718
LEN_BYTES :6
ORIGINAL  : pd4H[END]
TRANSLATED: pd4H[END]

ADDRESS   :0x27720
LEN_BYTES :6
ORIGINAL  : pd3H[END]
TRANSLATED: pd3H[END]

ADDRESS   :0x27728
LEN_BYTES :6
ORIGINAL  : pd2H[END]
TRANSLATED: pd2H[END]

ADDRESS   :0x27730
LEN_BYTES :6
ORIGINAL  : pd1H[END]
TRANSLATED: pd1H[END]

ADDRESS   :0x27738
LEN_BYTES :6
ORIGINAL  : pd0H[END]
TRANSLATED: pd0H[END]

ADDRESS   :0x27740
LEN_BYTES :6
ORIGINAL  : pd/H[END]
TRANSLATED: pd/H[END]

ADDRESS   :0x27748
LEN_BYTES :6
ORIGINAL  : pd.H[END]
TRANSLATED: pd.H[END]

ADDRESS   :0x27750
LEN_BYTES :6
ORIGINAL  : pd-H[END]
TRANSLATED: pd-H[END]

ADDRESS   :0x27758
LEN_BYTES :6
ORIGINAL  : pd,H[END]
TRANSLATED: pd,H[END]

ADDRESS   :0x27760
LEN_BYTES :6
ORIGINAL  : pd+H[END]
TRANSLATED: pd+H[END]

ADDRESS   :0x27768
LEN_BYTES :6
ORIGINAL  : pd*H[END]
TRANSLATED: pd*H[END]

ADDRESS   :0x2785c
LEN_BYTES :6
ORIGINAL  :A!hx[END]
TRANSLATED:A!hx[END]

ADDRESS   :0x284e8
LEN_BYTES :4
ORIGINAL  :PCbl[END]
TRANSLATED:PCbl[END]

ADDRESS   :0x28504
LEN_BYTES :4
ORIGINAL  :PCbl[END]
TRANSLATED:PCbl[END]

ADDRESS   :0x28548
LEN_BYTES :4
ORIGINAL  :HCal[END]
TRANSLATED:HCal[END]

ADDRESS   :0x28564
LEN_BYTES :6
ORIGINAL  :HHCal[END]
TRANSLATED:HHCal[END]

ADDRESS   :0x28768
LEN_BYTES :4
ORIGINAL  :AhB[END]
TRANSLATED:AhB[END]

ADDRESS   :0x2a6a0
LEN_BYTES :4
ORIGINAL  :!F0F[END]
TRANSLATED:!F0F[END]

ADDRESS   :0x2a75c
LEN_BYTES :4
ORIGINAL  :!F0F[END]
TRANSLATED:!F0F[END]

ADDRESS   :0x2a814
LEN_BYTES :4
ORIGINAL  :!E[END]
TRANSLATED:!E[END]

ADDRESS   :0x2b410
LEN_BYTES :4
ORIGINAL  :ihp[END]
TRANSLATED:ihp[END]

ADDRESS   :0x2b524
LEN_BYTES :6
ORIGINAL  :ihUhh[END]
TRANSLATED:ihUhh[END]

ADDRESS   :0x2b558
LEN_BYTES :6
ORIGINAL  :ihUhh[END]
TRANSLATED:ihUhh[END]

ADDRESS   :0x2b5e0
LEN_BYTES :6
ORIGINAL  :ihUhh[END]
TRANSLATED:ihUhh[END]

ADDRESS   :0x2d8d8
LEN_BYTES :4
ORIGINAL  :0D[END]
TRANSLATED:0D[END]

ADDRESS   :0x2d8e8
LEN_BYTES :4
ORIGINAL  :0D[END]
TRANSLATED:0D[END]

ADDRESS   :0x2d904
LEN_BYTES :4
ORIGINAL  :2D[END]
TRANSLATED:2D[END]

ADDRESS   :0x2d914
LEN_BYTES :4
ORIGINAL  :2D[END]
TRANSLATED:2D[END]

ADDRESS   :0x2ef7c
LEN_BYTES :4
ORIGINAL  :4D[END]
TRANSLATED:4D[END]

ADDRESS   :0x2ef8c
LEN_BYTES :4
ORIGINAL  :6D[END]
TRANSLATED:6D[END]

ADDRESS   :0x2ef9c
LEN_BYTES :4
ORIGINAL  :4D[END]
TRANSLATED:4D[END]

ADDRESS   :0x2efac
LEN_BYTES :4
ORIGINAL  :6D[END]
TRANSLATED:6D[END]

ADDRESS   :0x2f49c
LEN_BYTES :4
ORIGINAL  :6D[END]
TRANSLATED:6D[END]

ADDRESS   :0x2f4cc
LEN_BYTES :4
ORIGINAL  :4D[END]
TRANSLATED:4D[END]

ADDRESS   :0x2f514
LEN_BYTES :4
ORIGINAL  :4D[END]
TRANSLATED:4D[END]

ADDRESS   :0x313bc
LEN_BYTES :4
ORIGINAL  :3Y[END]
TRANSLATED:3Y[END]

ADDRESS   :0x32e54
LEN_BYTES :4
ORIGINAL  :FH[END]
TRANSLATED:FH[END]

ADDRESS   :0x32fd8
LEN_BYTES :4
ORIGINAL  :ID[END]
TRANSLATED:ID[END]

ADDRESS   :0x33140
LEN_BYTES :4
ORIGINAL  : DHD[END]
TRANSLATED: DHD[END]

ADDRESS   :0x33710
LEN_BYTES :4
ORIGINAL  :4FH[END]
TRANSLATED:4FH[END]

ADDRESS   :0x33aac
LEN_BYTES :4
ORIGINAL  :0HD[END]
TRANSLATED:0HD[END]

ADDRESS   :0x33adc
LEN_BYTES :4
ORIGINAL  :8HD[END]
TRANSLATED:8HD[END]

ADDRESS   :0x34504
LEN_BYTES :8
ORIGINAL  :dH!hbH[END]
TRANSLATED:dH!hbH[END]

ADDRESS   :0x34524
LEN_BYTES :8
ORIGINAL  :\H!hZH[END]
TRANSLATED:\H!hZH[END]

ADDRESS   :0x3453c
LEN_BYTES :8
ORIGINAL  :VH!hTH[END]
TRANSLATED:VH!hTH[END]

ADDRESS   :0x345c8
LEN_BYTES :4
ORIGINAL  : !2H[END]
TRANSLATED: !2H[END]

ADDRESS   :0x348b8
LEN_BYTES :6
ORIGINAL  : !hvH[END]
TRANSLATED: !hvH[END]

ADDRESS   :0x349ac
LEN_BYTES :8
ORIGINAL  :;H!h9H[END]
TRANSLATED:;H!h9H[END]

ADDRESS   :0x34cb8
LEN_BYTES :10
ORIGINAL  :hHh!bhab[END]
TRANSLATED:hHh!bhab[END]

ADDRESS   :0x34d90
LEN_BYTES :8
ORIGINAL  :3H!h1H[END]
TRANSLATED:3H!h1H[END]

ADDRESS   :0x35268
LEN_BYTES :4
ORIGINAL  :!FH[END]
TRANSLATED:!FH[END]

ADDRESS   :0x35440
LEN_BYTES :4
ORIGINAL  :ADD[END]
TRANSLATED:ADD[END]

ADDRESS   :0x36d58
LEN_BYTES :4
ORIGINAL  :vB7F[END]
TRANSLATED:vB7F[END]

ADDRESS   :0x36ff0
LEN_BYTES :4
ORIGINAL  :pGF[END]
TRANSLATED:pGF[END]

ADDRESS   :0x370b0
LEN_BYTES :4
ORIGINAL  :8Faj[END]
TRANSLATED:8Faj[END]

ADDRESS   :0x38144
LEN_BYTES :9
ORIGINAL  :Check box[END]
TRANSLATED:Check box[END]

ADDRESS   :0x398fc
LEN_BYTES :6
ORIGINAL  :QapGH[END]
TRANSLATED:QapGH[END]

ADDRESS   :0x39b44
LEN_BYTES :4
ORIGINAL  :II[END]
TRANSLATED:II[END]

ADDRESS   :0x39f78
LEN_BYTES :7
ORIGINAL  :No
data[END]
TRANSLATED:No
data[END]

ADDRESS   :0x3a9dc
LEN_BYTES :4
ORIGINAL  :2FQF[END]
TRANSLATED:2FQF[END]

ADDRESS   :0x3ac10
LEN_BYTES :6
ORIGINAL  :+F2FQF[END]
TRANSLATED:+F2FQF[END]

ADDRESS   :0x3ac80
LEN_BYTES :4
ORIGINAL  :2FQF[END]
TRANSLATED:2FQF[END]

ADDRESS   :0x3b080
LEN_BYTES :6
ORIGINAL  :0F.FF[END]
TRANSLATED:0F.FF[END]

ADDRESS   :0x3ca2c
LEN_BYTES :4
ORIGINAL  : ! F[END]
TRANSLATED: ! F[END]

ADDRESS   :0x3cab0
LEN_BYTES :26
ORIGINAL  :Option 1
Option 2
Option 3[END]
TRANSLATED:Option 1
Option 2
Option 3[END]

ADDRESS   :0x3cc90
LEN_BYTES :6
ORIGINAL  :PjpGF[END]
TRANSLATED:PjpGF[END]

ADDRESS   :0x3d24c
LEN_BYTES :8
ORIGINAL  :pGFHhpG[END]
TRANSLATED:pGFHhpG[END]

ADDRESS   :0x3d3ec
LEN_BYTES :6
ORIGINAL  :myh[END]
TRANSLATED:myh[END]

ADDRESS   :0x3d718
LEN_BYTES :6
ORIGINAL  :BF9F F[END]
TRANSLATED:BF9F F[END]

ADDRESS   :0x3e5a0
LEN_BYTES :4
ORIGINAL  :pGF[END]
TRANSLATED:pGF[END]

ADDRESS   :0x3e5ec
LEN_BYTES :4
ORIGINAL  :pGF[END]
TRANSLATED:pGF[END]

ADDRESS   :0x3edec
LEN_BYTES :8
ORIGINAL  :CF:F1F F[END]
TRANSLATED:CF:F1F F[END]

ADDRESS   :0x3ee28
LEN_BYTES :6
ORIGINAL  ::F1F F[END]
TRANSLATED::F1F F[END]

ADDRESS   :0x3ee60
LEN_BYTES :8
ORIGINAL  :CF:F1F F[END]
TRANSLATED:CF:F1F F[END]

ADDRESS   :0x3f344
LEN_BYTES :8
ORIGINAL  :𵅰F%F[END]
TRANSLATED:𵅰F%F[END]

ADDRESS   :0x3f358
LEN_BYTES :4
ORIGINAL  :pC[END]
TRANSLATED:pC[END]

ADDRESS   :0x3f7d8
LEN_BYTES :4
ORIGINAL  :pGh[END]
TRANSLATED:pGh[END]

ADDRESS   :0x3f7f8
LEN_BYTES :4
ORIGINAL  :pGh[END]
TRANSLATED:pGh[END]

ADDRESS   :0x3f8b8
LEN_BYTES :4
ORIGINAL  :TH[END]
TRANSLATED:TH[END]

ADDRESS   :0x3f9a4
LEN_BYTES :4
ORIGINAL  :pq0h[END]
TRANSLATED:pq0h[END]

ADDRESS   :0x3fe10
LEN_BYTES :5
ORIGINAL  :Enter[END]
TRANSLATED:Enter[END]

ADDRESS   :0x3fe44
LEN_BYTES :4
ORIGINAL  :=P F[END]
TRANSLATED:=P F[END]

ADDRESS   :0x3ff90
LEN_BYTES :4
ORIGINAL  :Text[END]
TRANSLATED:Text[END]

ADDRESS   :0x405c8
LEN_BYTES :6
ORIGINAL  :PjpGF[END]
TRANSLATED:PjpGF[END]

ADDRESS   :0x40754
LEN_BYTES :6
ORIGINAL  :90KF[END]
TRANSLATED:90KF[END]

ADDRESS   :0x4078c
LEN_BYTES :6
ORIGINAL  :90KF[END]
TRANSLATED:90KF[END]

ADDRESS   :0x40b40
LEN_BYTES :6
ORIGINAL  :IBF[END]
TRANSLATED:IBF[END]

ADDRESS   :0x40bd0
LEN_BYTES :8
ORIGINAL  :RIBF[END]
TRANSLATED:RIBF[END]

ADDRESS   :0x40cfc
LEN_BYTES :4
ORIGINAL  :ND[END]
TRANSLATED:ND[END]

ADDRESS   :0x40d6c
LEN_BYTES :10
ORIGINAL  :9wOwL[END]
TRANSLATED:9wOwL[END]

ADDRESS   :0x40fec
LEN_BYTES :4
ORIGINAL  :G8F[END]
TRANSLATED:G8F[END]

ADDRESS   :0x4139c
LEN_BYTES :4
ORIGINAL  :P! F[END]
TRANSLATED:P! F[END]

ADDRESS   :0x417fc
LEN_BYTES :4
ORIGINAL  :!FH[END]
TRANSLATED:!FH[END]

ADDRESS   :0x41ab0
LEN_BYTES :4
ORIGINAL  :Rm[END]
TRANSLATED:Rm[END]

ADDRESS   :0x41b68
LEN_BYTES :6
ORIGINAL  :IRm[END]
TRANSLATED:IRm[END]

ADDRESS   :0x41c10
LEN_BYTES :4
ORIGINAL  :dR[END]
TRANSLATED:dR[END]

ADDRESS   :0x41cf0
LEN_BYTES :4
ORIGINAL  :RI[END]
TRANSLATED:RI[END]

ADDRESS   :0x41ecc
LEN_BYTES :4
ORIGINAL  :1F6H[END]
TRANSLATED:1F6H[END]

ADDRESS   :0x41f94
LEN_BYTES :8
ORIGINAL  :h505[END]
TRANSLATED:h505[END]

ADDRESS   :0x41fa0
LEN_BYTES :7
ORIGINAL  :G
[END]
TRANSLATED:G
[END]

ADDRESS   :0x41fc8
LEN_BYTES :6
ORIGINAL  :PkpGF[END]
TRANSLATED:PkpGF[END]

ADDRESS   :0x42b5c
LEN_BYTES :4
ORIGINAL  :%h h[END]
TRANSLATED:%h h[END]

ADDRESS   :0x435bc
LEN_BYTES :4
ORIGINAL  :!F0F[END]
TRANSLATED:!F0F[END]

ADDRESS   :0x440cc
LEN_BYTES :4
ORIGINAL  :8DPD[END]
TRANSLATED:8DPD[END]

ADDRESS   :0x45640
LEN_BYTES :4
ORIGINAL  : a i[END]
TRANSLATED: a i[END]

ADDRESS   :0x4583c
LEN_BYTES :4
ORIGINAL  :pG~[END]
TRANSLATED:pG~[END]

ADDRESS   :0x46930
LEN_BYTES :4
ORIGINAL  :9F0F[END]
TRANSLATED:9F0F[END]

ADDRESS   :0x46938
LEN_BYTES :6
ORIGINAL  :*F!F0F[END]
TRANSLATED:*F!F0F[END]

ADDRESS   :0x46e84
LEN_BYTES :4
ORIGINAL  :e!0F[END]
TRANSLATED:e!0F[END]

ADDRESS   :0x46ebc
LEN_BYTES :4
ORIGINAL  :Q!0F[END]
TRANSLATED:Q!0F[END]

ADDRESS   :0x46ef0
LEN_BYTES :4
ORIGINAL  :jA0F[END]
TRANSLATED:jA0F[END]

ADDRESS   :0x46f60
LEN_BYTES :6
ORIGINAL  :+F!!0F[END]
TRANSLATED:+F!!0F[END]

ADDRESS   :0x46f98
LEN_BYTES :6
ORIGINAL  :+F1!0F[END]
TRANSLATED:+F1!0F[END]

ADDRESS   :0x46fb4
LEN_BYTES :4
ORIGINAL  :20F[END]
TRANSLATED:20F[END]

ADDRESS   :0x47044
LEN_BYTES :6
ORIGINAL  :+FH!0F[END]
TRANSLATED:+FH!0F[END]

ADDRESS   :0x47060
LEN_BYTES :4
ORIGINAL  :i0F[END]
TRANSLATED:i0F[END]

ADDRESS   :0x4724c
LEN_BYTES :4
ORIGINAL  :YA0F[END]
TRANSLATED:YA0F[END]

ADDRESS   :0x476bc
LEN_BYTES :4
ORIGINAL  :AHH[END]
TRANSLATED:AHH[END]

ADDRESS   :0x47940
LEN_BYTES :4
ORIGINAL  :9F F[END]
TRANSLATED:9F F[END]

ADDRESS   :0x47964
LEN_BYTES :4
ORIGINAL  :AF F[END]
TRANSLATED:AF F[END]

ADDRESS   :0x47ba8
LEN_BYTES :4
ORIGINAL  :dH[END]
TRANSLATED:dH[END]

ADDRESS   :0x47bb8
LEN_BYTES :4
ORIGINAL  :mH[END]
TRANSLATED:mH[END]

ADDRESS   :0x47e1c
LEN_BYTES :4
ORIGINAL  :4F0F[END]
TRANSLATED:4F0F[END]

ADDRESS   :0x484a0
LEN_BYTES :4
ORIGINAL  :IF0F[END]
TRANSLATED:IF0F[END]

ADDRESS   :0x484f0
LEN_BYTES :4
ORIGINAL  :IF0F[END]
TRANSLATED:IF0F[END]

ADDRESS   :0x48858
LEN_BYTES :4
ORIGINAL  :B
 [END]
TRANSLATED:B
 [END]

ADDRESS   :0x489c8
LEN_BYTES :4
ORIGINAL  : nD[END]
TRANSLATED: nD[END]

ADDRESS   :0x48a18
LEN_BYTES :4
ORIGINAL  :LF
/[END]
TRANSLATED:LF
/[END]

ADDRESS   :0x49af8
LEN_BYTES :4
ORIGINAL  :Gm[END]
TRANSLATED:Gm[END]

ADDRESS   :0x49de4
LEN_BYTES :4
ORIGINAL  :AF0F[END]
TRANSLATED:AF0F[END]

ADDRESS   :0x4a040
LEN_BYTES :4
ORIGINAL  :QF F[END]
TRANSLATED:QF F[END]

ADDRESS   :0x4a250
LEN_BYTES :6
ORIGINAL  :\9F[END]
TRANSLATED:\9F[END]

ADDRESS   :0x4a274
LEN_BYTES :6
ORIGINAL  :PkpGF[END]
TRANSLATED:PkpGF[END]

ADDRESS   :0x4ae20
LEN_BYTES :7
ORIGINAL  : ,.;:-_[END]
TRANSLATED: ,.;:-_[END]

ADDRESS   :0x4b11c
LEN_BYTES :6
ORIGINAL  :iFh\[END]
TRANSLATED:iFh\[END]

ADDRESS   :0x4b2c4
LEN_BYTES :4
ORIGINAL  :pGx[END]
TRANSLATED:pGx[END]

ADDRESS   :0x4b300
LEN_BYTES :6
ORIGINAL  :3F*F!F[END]
TRANSLATED:3F*F!F[END]

ADDRESS   :0x4b3f0
LEN_BYTES :16
ORIGINAL  :DDF10CH Start!

[END]
TRANSLATED:DDF10CH Start!

[END]

ADDRESS   :0x4b408
LEN_BYTES :8
ORIGINAL  :KEY_task[END]
TRANSLATED:KEY_task[END]

ADDRESS   :0x4b41c
LEN_BYTES :9
ORIGINAL  :MENU_task[END]
TRANSLATED:MENU_task[END]

ADDRESS   :0x4b430
LEN_BYTES :8
ORIGINAL  :LED_task[END]
TRANSLATED:LED_task[END]

ADDRESS   :0x4b444
LEN_BYTES :13
ORIGINAL  :RF_START_task[END]
TRANSLATED:RF_START_task[END]

ADDRESS   :0x4bd30
LEN_BYTES :5
ORIGINAL  :%d/%d[END]
TRANSLATED:%d/%d[END]

ADDRESS   :0x4bf44
LEN_BYTES :6
ORIGINAL  :jHhoH[END]
TRANSLATED:jHhoH[END]

ADDRESS   :0x4bf78
LEN_BYTES :4
ORIGINAL  :bIcH[END]
TRANSLATED:bIcH[END]

ADDRESS   :0x4c004
LEN_BYTES :4
ORIGINAL  :;IGH[END]
TRANSLATED:;IGH[END]

ADDRESS   :0x4c034
LEN_BYTES :4
ORIGINAL  :2!;H[END]
TRANSLATED:2!;H[END]

ADDRESS   :0x4c11c
LEN_BYTES :5
ORIGINAL  :%d/%d[END]
TRANSLATED:%d/%d[END]

ADDRESS   :0x4c24c
LEN_BYTES :5
ORIGINAL  :%d/%d[END]
TRANSLATED:%d/%d[END]

ADDRESS   :0x4c46c
LEN_BYTES :6
ORIGINAL  :mHhrH[END]
TRANSLATED:mHhrH[END]

ADDRESS   :0x4c4a0
LEN_BYTES :4
ORIGINAL  :eIfH[END]
TRANSLATED:eIfH[END]

ADDRESS   :0x4c500
LEN_BYTES :4
ORIGINAL  :2!PH[END]
TRANSLATED:2!PH[END]

ADDRESS   :0x4c550
LEN_BYTES :4
ORIGINAL  :6IAH[END]
TRANSLATED:6IAH[END]

ADDRESS   :0x4c650
LEN_BYTES :5
ORIGINAL  :%d/%d[END]
TRANSLATED:%d/%d[END]

ADDRESS   :0x4c780
LEN_BYTES :5
ORIGINAL  :%d/%d[END]
TRANSLATED:%d/%d[END]

ADDRESS   :0x4c968
LEN_BYTES :6
ORIGINAL  :_HhdH[END]
TRANSLATED:_HhdH[END]

ADDRESS   :0x4c99c
LEN_BYTES :4
ORIGINAL  :WIXH[END]
TRANSLATED:WIXH[END]

ADDRESS   :0x4c9bc
LEN_BYTES :4
ORIGINAL  :SIRH[END]
TRANSLATED:SIRH[END]

ADDRESS   :0x4ca58
LEN_BYTES :4
ORIGINAL  :2!0H[END]
TRANSLATED:2!0H[END]

ADDRESS   :0x4cb14
LEN_BYTES :5
ORIGINAL  :%d/%d[END]
TRANSLATED:%d/%d[END]

ADDRESS   :0x4cc44
LEN_BYTES :5
ORIGINAL  :%d/%d[END]
TRANSLATED:%d/%d[END]

ADDRESS   :0x4ce40
LEN_BYTES :6
ORIGINAL  :dHhiH[END]
TRANSLATED:dHhiH[END]

ADDRESS   :0x4ce94
LEN_BYTES :4
ORIGINAL  :XIWH[END]
TRANSLATED:XIWH[END]

ADDRESS   :0x4cf00
LEN_BYTES :4
ORIGINAL  :5IAH[END]
TRANSLATED:5IAH[END]

ADDRESS   :0x4cf24
LEN_BYTES :4
ORIGINAL  :-I8H[END]
TRANSLATED:-I8H[END]

ADDRESS   :0x4cf30
LEN_BYTES :4
ORIGINAL  :2!5H[END]
TRANSLATED:2!5H[END]

ADDRESS   :0x4d000
LEN_BYTES :5
ORIGINAL  :%d/%d[END]
TRANSLATED:%d/%d[END]

ADDRESS   :0x4d3a0
LEN_BYTES :4
ORIGINAL  : H!I[END]
TRANSLATED: H!I[END]

ADDRESS   :0x4d440
LEN_BYTES :4
ORIGINAL  :!FH[END]
TRANSLATED:!FH[END]

ADDRESS   :0x4d48c
LEN_BYTES :4
ORIGINAL  :!FH[END]
TRANSLATED:!FH[END]

ADDRESS   :0x4d4c0
LEN_BYTES :4
ORIGINAL  :!FH[END]
TRANSLATED:!FH[END]

ADDRESS   :0x4d770
LEN_BYTES :4
ORIGINAL  :s!iH[END]
TRANSLATED:s!iH[END]

ADDRESS   :0x4d848
LEN_BYTES :6
ORIGINAL  :3HhVH[END]
TRANSLATED:3HhVH[END]

ADDRESS   :0x4d8e4
LEN_BYTES :4
ORIGINAL  :A!2H[END]
TRANSLATED:A!2H[END]

ADDRESS   :0x4d920
LEN_BYTES :25
ORIGINAL  :#3df3ff # 数据回传[END]
TRANSLATED:#3df3ff # 数据回传[END]

ADDRESS   :0x4d93c
LEN_BYTES :23
ORIGINAL  :#3df3ff # Telemetrie[END]
TRANSLATED:#3df3ff # Telemetrie[END]

ADDRESS   :0x4d954
LEN_BYTES :26
ORIGINAL  :#3df3ff # Télémétrie[END]
TRANSLATED:#3df3ff # Télémétrie[END]

ADDRESS   :0x4d970
LEN_BYTES :31
ORIGINAL  :#3df3ff # テレメトリー[END]
TRANSLATED:#3df3ff # テレメトリー[END]

ADDRESS   :0x4d990
LEN_BYTES :22
ORIGINAL  :#3df3ff # Telemetry[END]
TRANSLATED:#3df3ff # Telemetry[END]

ADDRESS   :0x4d9b4
LEN_BYTES :12
ORIGINAL  :剩余电量[END]
TRANSLATED:剩余电量[END]

ADDRESS   :0x4d9c4
LEN_BYTES :8
ORIGINAL  :Batterie[END]
TRANSLATED:Batterie[END]

ADDRESS   :0x4d9d0
LEN_BYTES :12
ORIGINAL  :電池残量[END]
TRANSLATED:電池残量[END]

ADDRESS   :0x4d9e0
LEN_BYTES :7
ORIGINAL  :Battery[END]
TRANSLATED:Battery[END]

ADDRESS   :0x4dc68
LEN_BYTES :4
ORIGINAL  :s!kH[END]
TRANSLATED:s!kH[END]

ADDRESS   :0x4dd14
LEN_BYTES :6
ORIGINAL  :hHhiH[END]
TRANSLATED:hHhiH[END]

ADDRESS   :0x4ddc4
LEN_BYTES :6
ORIGINAL  :AHhAH[END]
TRANSLATED:AHhAH[END]

ADDRESS   :0x4de20
LEN_BYTES :25
ORIGINAL  :#3df3ff # 通道状态[END]
TRANSLATED:#3df3ff # 通道状态[END]

ADDRESS   :0x4de3c
LEN_BYTES :25
ORIGINAL  :#3df3ff # Kanal Status[END]
TRANSLATED:#3df3ff # Kanal Status[END]

ADDRESS   :0x4de58
LEN_BYTES :25
ORIGINAL  :#3df3ff # Statut du CH[END]
TRANSLATED:#3df3ff # Statut du CH[END]

ADDRESS   :0x4de74
LEN_BYTES :43
ORIGINAL  :#3df3ff # チャンネルステータス[END]
TRANSLATED:#3df3ff # チャンネルステータス[END]

ADDRESS   :0x4dea0
LEN_BYTES :21
ORIGINAL  :#3df3ff # CH State[END]
TRANSLATED:#3df3ff # CH State[END]

ADDRESS   :0x4e150
LEN_BYTES :4
ORIGINAL  :gIqH[END]
TRANSLATED:gIqH[END]

ADDRESS   :0x4e15c
LEN_BYTES :4
ORIGINAL  :eInH[END]
TRANSLATED:eInH[END]

ADDRESS   :0x4e1f0
LEN_BYTES :4
ORIGINAL  :?ILH[END]
TRANSLATED:?ILH[END]

ADDRESS   :0x4e1fc
LEN_BYTES :4
ORIGINAL  :JIIH[END]
TRANSLATED:JIIH[END]

ADDRESS   :0x4e218
LEN_BYTES :6
ORIGINAL  :AHhAH[END]
TRANSLATED:AHhAH[END]

ADDRESS   :0x4e568
LEN_BYTES :6
ORIGINAL  :HhH[END]
TRANSLATED:HhH[END]

ADDRESS   :0x4e668
LEN_BYTES :6
ORIGINAL  :AHhAH[END]
TRANSLATED:AHhAH[END]

ADDRESS   :0x4e948
LEN_BYTES :4
ORIGINAL  :y!yH[END]
TRANSLATED:y!yH[END]

ADDRESS   :0x4e9d8
LEN_BYTES :4
ORIGINAL  :IIWH[END]
TRANSLATED:IIWH[END]

ADDRESS   :0x4e9e4
LEN_BYTES :4
ORIGINAL  :GITH[END]
TRANSLATED:GITH[END]

ADDRESS   :0x4ea00
LEN_BYTES :6
ORIGINAL  :HHhLH[END]
TRANSLATED:HHhLH[END]

ADDRESS   :0x4ea80
LEN_BYTES :4
ORIGINAL  : I1H[END]
TRANSLATED: I1H[END]

ADDRESS   :0x4eb18
LEN_BYTES :4
ORIGINAL  :-100[END]
TRANSLATED:-100[END]

ADDRESS   :0x4ec6c
LEN_BYTES :8
ORIGINAL  :Ʋ
.ѰH[END]
TRANSLATED:Ʋ
.ѰH[END]

ADDRESS   :0x4eec0
LEN_BYTES :4
ORIGINAL  :5эH[END]
TRANSLATED:5эH[END]

ADDRESS   :0x4ef3c
LEN_BYTES :12
ORIGINAL  :基础设置[END]
TRANSLATED:基础设置[END]

ADDRESS   :0x4ef54
LEN_BYTES :12
ORIGINAL  :高级设置[END]
TRANSLATED:高级设置[END]

ADDRESS   :0x4ef68
LEN_BYTES :15
ORIGINAL  :遥控器设置[END]
TRANSLATED:遥控器设置[END]

ADDRESS   :0x4ef7c
LEN_BYTES :15
ORIGINAL  :接收机设置[END]
TRANSLATED:接收机设置[END]

ADDRESS   :0x4ef90
LEN_BYTES :10
ORIGINAL  :Hauptmenü[END]
TRANSLATED:Hauptmenü[END]

ADDRESS   :0x4ef9c
LEN_BYTES :20
ORIGINAL  :Modell Einstellungen[END]
TRANSLATED:Modell Einstellungen[END]

ADDRESS   :0x4efb4
LEN_BYTES :28
ORIGINAL  :Fernsteuerungs Einstellungen[END]
TRANSLATED:Fernsteuerungs Einstellungen[END]

ADDRESS   :0x4efd4
LEN_BYTES :21
ORIGINAL  :Receiver installiert.[END]
TRANSLATED:Receiver installiert.[END]

ADDRESS   :0x4efec
LEN_BYTES :14
ORIGINAL  :Menu général[END]
TRANSLATED:Menu général[END]

ADDRESS   :0x4effc
LEN_BYTES :15
ORIGINAL  :Menu du modèle[END]
TRANSLATED:Menu du modèle[END]

ADDRESS   :0x4f00c
LEN_BYTES :22
ORIGINAL  :parametre transmetteur[END]
TRANSLATED:parametre transmetteur[END]

ADDRESS   :0x4f024
LEN_BYTES :23
ORIGINAL  :Réglages du récepteur[END]
TRANSLATED:Réglages du récepteur[END]

ADDRESS   :0x4f03c
LEN_BYTES :18
ORIGINAL  :基本メニュー[END]
TRANSLATED:基本メニュー[END]

ADDRESS   :0x4f050
LEN_BYTES :21
ORIGINAL  :モデルメニュー[END]
TRANSLATED:モデルメニュー[END]

ADDRESS   :0x4f068
LEN_BYTES :27
ORIGINAL  :送信機セッティング[END]
TRANSLATED:送信機セッティング[END]

ADDRESS   :0x4f084
LEN_BYTES :15
ORIGINAL  :受信機設定[END]
TRANSLATED:受信機設定[END]

ADDRESS   :0x4f094
LEN_BYTES :12
ORIGINAL  :General menu[END]
TRANSLATED:General menu[END]

ADDRESS   :0x4f0a4
LEN_BYTES :10
ORIGINAL  :Model menu[END]
TRANSLATED:Model menu[END]

ADDRESS   :0x4f0b0
LEN_BYTES :20
ORIGINAL  :Transmitter Settings[END]
TRANSLATED:Transmitter Settings[END]

ADDRESS   :0x4f0c8
LEN_BYTES :16
ORIGINAL  :Receiver setting[END]
TRANSLATED:Receiver setting[END]

ADDRESS   :0x4f0dc
LEN_BYTES :6
ORIGINAL  :语言[END]
TRANSLATED:语言[END]

ADDRESS   :0x4f0ec
LEN_BYTES :6
ORIGINAL  :言語[END]
TRANSLATED:言語[END]

ADDRESS   :0x4f3d8
LEN_BYTES :4
ORIGINAL  :XIuH[END]
TRANSLATED:XIuH[END]

ADDRESS   :0x4f554
LEN_BYTES :12
ORIGINAL  :基础设置[END]
TRANSLATED:基础设置[END]

ADDRESS   :0x4f564
LEN_BYTES :10
ORIGINAL  :Hauptmenü[END]
TRANSLATED:Hauptmenü[END]

ADDRESS   :0x4f570
LEN_BYTES :14
ORIGINAL  :Menu général[END]
TRANSLATED:Menu général[END]

ADDRESS   :0x4f580
LEN_BYTES :18
ORIGINAL  :基本メニュー[END]
TRANSLATED:基本メニュー[END]

ADDRESS   :0x4f594
LEN_BYTES :12
ORIGINAL  :General menu[END]
TRANSLATED:General menu[END]

ADDRESS   :0x4f5b4
LEN_BYTES :12
ORIGINAL  :高级设置[END]
TRANSLATED:高级设置[END]

ADDRESS   :0x4f5c4
LEN_BYTES :20
ORIGINAL  :Modell Einstellungen[END]
TRANSLATED:Modell Einstellungen[END]

ADDRESS   :0x4f5dc
LEN_BYTES :15
ORIGINAL  :Menu du modèle[END]
TRANSLATED:Menu du modèle[END]

ADDRESS   :0x4f5ec
LEN_BYTES :21
ORIGINAL  :モデルメニュー[END]
TRANSLATED:モデルメニュー[END]

ADDRESS   :0x4f604
LEN_BYTES :10
ORIGINAL  :Model menu[END]
TRANSLATED:Model menu[END]

ADDRESS   :0x4f9f4
LEN_BYTES :4
ORIGINAL  :VIUH[END]
TRANSLATED:VIUH[END]

ADDRESS   :0x4fa00
LEN_BYTES :4
ORIGINAL  :d!RH[END]
TRANSLATED:d!RH[END]

ADDRESS   :0x4fa30
LEN_BYTES :15
ORIGINAL  :遥控器设置[END]
TRANSLATED:遥控器设置[END]

ADDRESS   :0x4fa40
LEN_BYTES :28
ORIGINAL  :Fernsteuerungs Einstellungen[END]
TRANSLATED:Fernsteuerungs Einstellungen[END]

ADDRESS   :0x4fa60
LEN_BYTES :22
ORIGINAL  :parametre transmetteur[END]
TRANSLATED:parametre transmetteur[END]

ADDRESS   :0x4fa78
LEN_BYTES :27
ORIGINAL  :送信機セッティング[END]
TRANSLATED:送信機セッティング[END]

ADDRESS   :0x4fa94
LEN_BYTES :20
ORIGINAL  :Transmitter Settings[END]
TRANSLATED:Transmitter Settings[END]

ADDRESS   :0x4facc
LEN_BYTES :15
ORIGINAL  :接收机设置[END]
TRANSLATED:接收机设置[END]

ADDRESS   :0x4fadc
LEN_BYTES :21
ORIGINAL  :Receiver installiert.[END]
TRANSLATED:Receiver installiert.[END]

ADDRESS   :0x4faf4
LEN_BYTES :23
ORIGINAL  :Réglages du récepteur[END]
TRANSLATED:Réglages du récepteur[END]

ADDRESS   :0x4fb0c
LEN_BYTES :15
ORIGINAL  :受信機設定[END]
TRANSLATED:受信機設定[END]

ADDRESS   :0x4fb1c
LEN_BYTES :16
ORIGINAL  :Receiver setting[END]
TRANSLATED:Receiver setting[END]

ADDRESS   :0x4fb38
LEN_BYTES :6
ORIGINAL  :语言[END]
TRANSLATED:语言[END]

ADDRESS   :0x4fb44
LEN_BYTES :6
ORIGINAL  :言語[END]
TRANSLATED:言語[END]

ADDRESS   :0x4fcfc
LEN_BYTES :44
ORIGINAL  :English
简体中文
Germany
French
Japanese[END]
TRANSLATED:English
简体中文
Germany
French
Japanese[END]

ADDRESS   :0x500b4
LEN_BYTES :4
ORIGINAL  :𵍰[END]
TRANSLATED:𵍰[END]

ADDRESS   :0x509f8
LEN_BYTES :10
ORIGINAL  :model %02d[END]
TRANSLATED:model %02d[END]

ADDRESS   :0x50a10
LEN_BYTES :61
ORIGINAL  :请将手轮移动至#9f2f34 最右侧#,然后按下OK按键
[END]
TRANSLATED:请将手轮移动至#9f2f34 最右侧#,然后按下OK按键
[END]

ADDRESS   :0x50a50
LEN_BYTES :61
ORIGINAL  :Bewegen Sie das Lenkrad ganz nach rechts und drücken Sie OK
[END]
TRANSLATED:Bewegen Sie das Lenkrad ganz nach rechts und drücken Sie OK
[END]

ADDRESS   :0x50aac
LEN_BYTES :34
ORIGINAL  :xtrême droite et appuyez sur OK.
[END]
TRANSLATED:xtrême droite et appuyez sur OK.
[END]

ADDRESS   :0x50adc
LEN_BYTES :61
ORIGINAL  :请将扳机移动至#9f2f34 最上方#,然后按下OK按键
[END]
TRANSLATED:请将扳机移动至#9f2f34 最上方#,然后按下OK按键
[END]

ADDRESS   :0x50b1c
LEN_BYTES :55
ORIGINAL  :Schieben Sie den Trigger nach oben und drücken Sie OK
[END]
TRANSLATED:Schieben Sie den Trigger nach oben und drücken Sie OK
[END]

ADDRESS   :0x50b54
LEN_BYTES :55
ORIGINAL  :Déplacez la gâchette vers le haut et appuyez sur OK.
[END]
TRANSLATED:Déplacez la gâchette vers le haut et appuyez sur OK.
[END]

ADDRESS   :0x50b98
LEN_BYTES :50
ORIGINAL  :请#9f2f34 按住K10按键#,然后按下OK按键.
[END]
TRANSLATED:请#9f2f34 按住K10按键#,然后按下OK按键.
[END]

ADDRESS   :0x50be0
LEN_BYTES :62
ORIGINAL  :请将手轮移动至#9f7b34 中心点 #,然后按下OK按键
[END]
TRANSLATED:请将手轮移动至#9f7b34 中心点 #,然后按下OK按键
[END]

ADDRESS   :0x50c24
LEN_BYTES :57
ORIGINAL  :Placez le volant en position centrale et appuyez sur OK.
[END]
TRANSLATED:Placez le volant en position centrale et appuyez sur OK.
[END]

ADDRESS   :0x50c6c
LEN_BYTES :62
ORIGINAL  :请将扳机移动至#9f2f34 中心点 #,然后按下OK按键
[END]
TRANSLATED:请将扳机移动至#9f2f34 中心点 #,然后按下OK按键
[END]

ADDRESS   :0x50cb0
LEN_BYTES :59
ORIGINAL  :Placez la gâchette en position centrale et appuyez sur OK
[END]
TRANSLATED:Placez la gâchette en position centrale et appuyez sur OK
[END]

ADDRESS   :0x50cf8
LEN_BYTES :58
ORIGINAL  :请#9f2f34 同时按住K9和K10键#,然后按下OK按键.
[END]
TRANSLATED:请#9f2f34 同时按住K9和K10键#,然后按下OK按键.
[END]

ADDRESS   :0x510e8
LEN_BYTES :15
ORIGINAL  :正在校准...[END]
TRANSLATED:正在校准...[END]

ADDRESS   :0x51100
LEN_BYTES :14
ORIGINAL  :Kalibrieren...[END]
TRANSLATED:Kalibrieren...[END]

ADDRESS   :0x51110
LEN_BYTES :11
ORIGINAL  :Calibrer...[END]
TRANSLATED:Calibrer...[END]

ADDRESS   :0x5111c
LEN_BYTES :30
ORIGINAL  :キャリブレーション...[END]
TRANSLATED:キャリブレーション...[END]

ADDRESS   :0x5113c
LEN_BYTES :19
ORIGINAL  :Being calibrated...[END]
TRANSLATED:Being calibrated...[END]

ADDRESS   :0x51154
LEN_BYTES :7
ORIGINAL  :警告![END]
TRANSLATED:警告![END]

ADDRESS   :0x5115c
LEN_BYTES :8
ORIGINAL  :Warnung![END]
TRANSLATED:Warnung![END]

ADDRESS   :0x51168
LEN_BYTES :7
ORIGINAL  :Alarme![END]
TRANSLATED:Alarme![END]

ADDRESS   :0x51170
LEN_BYTES :8
ORIGINAL  :Warning![END]
TRANSLATED:Warning![END]

ADDRESS   :0x51180
LEN_BYTES :62
ORIGINAL  :请将手轮移动至#3df3ff 最左侧#,然后按下OK按键.
[END]
TRANSLATED:请将手轮移动至#3df3ff 最左侧#,然后按下OK按键.
[END]

ADDRESS   :0x511c0
LEN_BYTES :60
ORIGINAL  :Bewegen Sie das Lenkrad ganz nach links und drücken Sie OK
[END]
TRANSLATED:Bewegen Sie das Lenkrad ganz nach links und drücken Sie OK
[END]

ADDRESS   :0x51200
LEN_BYTES :61
ORIGINAL  :Move the steering wheel all the way to the left and press OK
[END]
TRANSLATED:Move the steering wheel all the way to the left and press OK
[END]

ADDRESS   :0x51240
LEN_BYTES :70
ORIGINAL  :xDD:请将扳机移动至#3df3ff 最下方#,然后按下OK按键.
[END]
TRANSLATED:xDD:请将扳机移动至#3df3ff 最下方#,然后按下OK按键.
[END]

ADDRESS   :0x51288
LEN_BYTES :55
ORIGINAL  :Bewegen Sie den Trigger nach unten und drücken Sie OK
[END]
TRANSLATED:Bewegen Sie den Trigger nach unten und drücken Sie OK
[END]

ADDRESS   :0x512c0
LEN_BYTES :53
ORIGINAL  :Déplacez la gâchette vers le bas et appuyez sur OK
[END]
TRANSLATED:Déplacez la gâchette vers le bas et appuyez sur OK
[END]

ADDRESS   :0x51300
LEN_BYTES :49
ORIGINAL  :请#3df3ff 按住K9按键#,然后按下OK按键.
[END]
TRANSLATED:请#3df3ff 按住K9按键#,然后按下OK按键.
[END]

ADDRESS   :0x51334
LEN_BYTES :59
ORIGINAL  :Halten Sie die Taste K9 gedrückt und drücken Sie dann OK
[END]
TRANSLATED:Halten Sie die Taste K9 gedrückt und drücken Sie dann OK
[END]

ADDRESS   :0x51370
LEN_BYTES :55
ORIGINAL  :Maintenez la touche K9 enfoncée, puis appuyez sur OK.
[END]
TRANSLATED:Maintenez la touche K9 enfoncée, puis appuyez sur OK.
[END]

ADDRESS   :0x516a8
LEN_BYTES :4
ORIGINAL  : CH[END]
TRANSLATED: CH[END]

ADDRESS   :0x517f4
LEN_BYTES :29
ORIGINAL  :..\STM32_Lib\FreeRTOS\tasks.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\tasks.c[END]

ADDRESS   :0x51814
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x5195c
LEN_BYTES :50
ORIGINAL  :..\STM32_Lib\FreeRTOS\portable\RVDS\ARM_CM3\port.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\portable\RVDS\ARM_CM3\port.c[END]

ADDRESS   :0x51990
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x51ab0
LEN_BYTES :47
ORIGINAL  :..\STM32_Lib\FreeRTOS\portable\MemMang\heap_4.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\portable\MemMang\heap_4.c[END]

ADDRESS   :0x51ae0
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x53518
LEN_BYTES :4
ORIGINAL  :GIBH[END]
TRANSLATED:GIBH[END]

ADDRESS   :0x53524
LEN_BYTES :4
ORIGINAL  :#!?H[END]
TRANSLATED:#!?H[END]

ADDRESS   :0x538a4
LEN_BYTES :6
ORIGINAL  :gHigH[END]
TRANSLATED:gHigH[END]

ADDRESS   :0x538e8
LEN_BYTES :6
ORIGINAL  :VHiVH[END]
TRANSLATED:VHiVH[END]

ADDRESS   :0x53e50
LEN_BYTES :4
ORIGINAL  :!H[END]
TRANSLATED:!H[END]

ADDRESS   :0x54404
LEN_BYTES :5
ORIGINAL  :05 [END]
TRANSLATED:05 [END]

ADDRESS   :0x547d8
LEN_BYTES :4
ORIGINAL  :p0F[END]
TRANSLATED:p0F[END]

ADDRESS   :0x54844
LEN_BYTES :5
ORIGINAL  :\9[END]
TRANSLATED:\9[END]

ADDRESS   :0x54c3c
LEN_BYTES :6
ORIGINAL  :2FAF h[END]
TRANSLATED:2FAF h[END]

ADDRESS   :0x54ff4
LEN_BYTES :50
ORIGINAL  :..\STM32_Lib\FreeRTOS\portable\RVDS\ARM_CM3\port.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\portable\RVDS\ARM_CM3\port.c[END]

ADDRESS   :0x55028
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x5506c
LEN_BYTES :50
ORIGINAL  :..\STM32_Lib\FreeRTOS\portable\RVDS\ARM_CM3\port.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\portable\RVDS\ARM_CM3\port.c[END]

ADDRESS   :0x550a0
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x5512c
LEN_BYTES :47
ORIGINAL  :..\STM32_Lib\FreeRTOS\portable\MemMang\heap_4.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\portable\MemMang\heap_4.c[END]

ADDRESS   :0x5515c
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x551c8
LEN_BYTES :29
ORIGINAL  :..\STM32_Lib\FreeRTOS\tasks.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\tasks.c[END]

ADDRESS   :0x551e8
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x552e0
LEN_BYTES :29
ORIGINAL  :..\STM32_Lib\FreeRTOS\tasks.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\tasks.c[END]

ADDRESS   :0x55300
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x5537c
LEN_BYTES :4
ORIGINAL  :IDLE[END]
TRANSLATED:IDLE[END]

ADDRESS   :0x55384
LEN_BYTES :5
ORIGINAL  :!gX[END]
TRANSLATED:!gX[END]

ADDRESS   :0x55394
LEN_BYTES :29
ORIGINAL  :..\STM32_Lib\FreeRTOS\tasks.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\tasks.c[END]

ADDRESS   :0x553b4
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x55454
LEN_BYTES :29
ORIGINAL  :..\STM32_Lib\FreeRTOS\tasks.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\tasks.c[END]

ADDRESS   :0x55474
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x555a0
LEN_BYTES :6
ORIGINAL  :!FpF[END]
TRANSLATED:!FpF[END]

ADDRESS   :0x55688
LEN_BYTES :50
ORIGINAL  :..\STM32_Lib\FreeRTOS\portable\RVDS\ARM_CM3\port.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\portable\RVDS\ARM_CM3\port.c[END]

ADDRESS   :0x556bc
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x557d4
LEN_BYTES :6
ORIGINAL  :7HhCH[END]
TRANSLATED:7HhCH[END]

ADDRESS   :0x558b8
LEN_BYTES :29
ORIGINAL  :..\STM32_Lib\FreeRTOS\tasks.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\tasks.c[END]

ADDRESS   :0x558d8
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x559e4
LEN_BYTES :29
ORIGINAL  :..\STM32_Lib\FreeRTOS\tasks.c[END]
TRANSLATED:..\STM32_Lib\FreeRTOS\tasks.c[END]

ADDRESS   :0x55a04
LEN_BYTES :13
ORIGINAL  :Error:%s,%d

[END]
TRANSLATED:Error:%s,%d

[END]

ADDRESS   :0x55e64
LEN_BYTES :6
ORIGINAL  :pG+Ŀ[END]
TRANSLATED:pG+Ŀ[END]

ADDRESS   :0x56508
LEN_BYTES :4
ORIGINAL  :ϸc[END]
TRANSLATED:ϸc[END]

ADDRESS   :0x58060
LEN_BYTES :4
ORIGINAL  :AtA[END]
TRANSLATED:AtA[END]

ADDRESS   :0x59050
LEN_BYTES :4
ORIGINAL  :DDA%[END]
TRANSLATED:DDA%[END]

ADDRESS   :0x59994
LEN_BYTES :4
ORIGINAL  :pˀ[END]
TRANSLATED:pˀ[END]

ADDRESS   :0x59b4c
LEN_BYTES :5
ORIGINAL  :00
[END]
TRANSLATED:00
[END]

ADDRESS   :0x5a750
LEN_BYTES :6
ORIGINAL  :vffffc[END]
TRANSLATED:vffffc[END]

ADDRESS   :0x5aea8
LEN_BYTES :4
ORIGINAL  :y[END]
TRANSLATED:y[END]

ADDRESS   :0x5af08
LEN_BYTES :5
ORIGINAL  :?wwS[END]
TRANSLATED:?wwS[END]

ADDRESS   :0x5b510
LEN_BYTES :5
ORIGINAL  :D:DBB[END]
TRANSLATED:D:DBB[END]

ADDRESS   :0x5b5d4
LEN_BYTES :5
ORIGINAL  :33tCt[END]
TRANSLATED:33tCt[END]

ADDRESS   :0x5b75c
LEN_BYTES :4
ORIGINAL  :wwwt[END]
TRANSLATED:wwwt[END]

ADDRESS   :0x5b784
LEN_BYTES :5
ORIGINAL  :ʎ#__[END]
TRANSLATED:ʎ#__[END]

ADDRESS   :0x5bb84
LEN_BYTES :6
ORIGINAL  :4P[END]
TRANSLATED:4P[END]

ADDRESS   :0x5bb9c
LEN_BYTES :6
ORIGINAL  :f 	[END]
TRANSLATED:f 	[END]

ADDRESS   :0x5bbcc
LEN_BYTES :6
ORIGINAL  :! 	[END]
TRANSLATED:! 	[END]

ADDRESS   :0x5bbd4
LEN_BYTES :6
ORIGINAL  :A 	[END]
TRANSLATED:A 	[END]

ADDRESS   :0x5bbdc
LEN_BYTES :6
ORIGINAL  :a 	[END]
TRANSLATED:a 	[END]

ADDRESS   :0x5bc4c
LEN_BYTES :6
ORIGINAL  :+p	[END]
TRANSLATED:+p	[END]

ADDRESS   :0x5bc94
LEN_BYTES :6
ORIGINAL  :Qp			[END]
TRANSLATED:Qp			[END]

ADDRESS   :0x5bc9c
LEN_BYTES :6
ORIGINAL  :zp	[END]
TRANSLATED:zp	[END]

ADDRESS   :0x5bcc4
LEN_BYTES :6
ORIGINAL  :9 			[END]
TRANSLATED:9 			[END]

ADDRESS   :0x5bd4c
LEN_BYTES :6
ORIGINAL  :=p
[END]
TRANSLATED:=p
[END]

ADDRESS   :0x5bddc
LEN_BYTES :6
ORIGINAL  :0
p[END]
TRANSLATED:0
p[END]

ADDRESS   :0x5be5c
LEN_BYTES :6
ORIGINAL  :z0
[END]
TRANSLATED:z0
[END]

ADDRESS   :0x5c1b4
LEN_BYTES :6
ORIGINAL  :b-
[END]
TRANSLATED:b-
[END]

ADDRESS   :0x5c440
LEN_BYTES :4
ORIGINAL  :p _[END]
TRANSLATED:p _[END]

ADDRESS   :0x5c6f8
LEN_BYTES :4
ORIGINAL  : ͷ[END]
TRANSLATED: ͷ[END]

ADDRESS   :0x5cdbc
LEN_BYTES :4
ORIGINAL  :Э	P[END]
TRANSLATED:Э	P[END]

ADDRESS   :0x5cff4
LEN_BYTES :4
ORIGINAL  :OP[END]
TRANSLATED:OP[END]

ADDRESS   :0x5df6c
LEN_BYTES :5
ORIGINAL  :0P5[END]
TRANSLATED:0P5[END]

ADDRESS   :0x5e09c
LEN_BYTES :5
ORIGINAL  :0
pYt[END]
TRANSLATED:0
pYt[END]

ADDRESS   :0x5f950
LEN_BYTES :6
ORIGINAL  :wwwwwq[END]
TRANSLATED:wwwwwq[END]

ADDRESS   :0x5fe0c
LEN_BYTES :5
ORIGINAL  :wwwwt[END]
TRANSLATED:wwwwt[END]

ADDRESS   :0x5ff04
LEN_BYTES :5
ORIGINAL  :wwwwr[END]
TRANSLATED:wwwwr[END]

ADDRESS   :0x60880
LEN_BYTES :6
ORIGINAL  :PPJop[END]
TRANSLATED:PPJop[END]

ADDRESS   :0x60bb4
LEN_BYTES :4
ORIGINAL  :ppf[END]
TRANSLATED:ppf[END]

ADDRESS   :0x60c60
LEN_BYTES :5
ORIGINAL  :6PP[END]
TRANSLATED:6PP[END]

ADDRESS   :0x61130
LEN_BYTES :4
ORIGINAL  :Pv[END]
TRANSLATED:Pv[END]

ADDRESS   :0x62030
LEN_BYTES :5
ORIGINAL  :bya[END]
TRANSLATED:bya[END]

ADDRESS   :0x62214
LEN_BYTES :4
ORIGINAL  :y
~p[END]
TRANSLATED:y
~p[END]

ADDRESS   :0x63530
LEN_BYTES :4
ORIGINAL  :wwws[END]
TRANSLATED:wwws[END]

ADDRESS   :0x63b48
LEN_BYTES :4
ORIGINAL  :o[END]
TRANSLATED:o[END]

ADDRESS   :0x64350
LEN_BYTES :6
ORIGINAL  :pwww [END]
TRANSLATED:pwww [END]

ADDRESS   :0x644a0
LEN_BYTES :6
ORIGINAL  :p 	P[END]
TRANSLATED:p 	P[END]

ADDRESS   :0x64a40
LEN_BYTES :4
ORIGINAL  :N0o[END]
TRANSLATED:N0o[END]

ADDRESS   :0x64f14
LEN_BYTES :4
ORIGINAL  : Q[END]
TRANSLATED: Q[END]

ADDRESS   :0x650fc
LEN_BYTES :4
ORIGINAL  :Lck0[END]
TRANSLATED:Lck0[END]

ADDRESS   :0x65204
LEN_BYTES :4
ORIGINAL  :Pp5[END]
TRANSLATED:Pp5[END]

ADDRESS   :0x655c4
LEN_BYTES :5
ORIGINAL  :N~PN[END]
TRANSLATED:N~PN[END]

ADDRESS   :0x655d4
LEN_BYTES :5
ORIGINAL  :N
PN[END]
TRANSLATED:N
PN[END]

ADDRESS   :0x6581c
LEN_BYTES :5
ORIGINAL  :wPe[END]
TRANSLATED:wPe[END]

ADDRESS   :0x65a54
LEN_BYTES :4
ORIGINAL  :0*r[END]
TRANSLATED:0*r[END]

ADDRESS   :0x65cb0
LEN_BYTES :7
ORIGINAL  :~pϐL[END]
TRANSLATED:~pϐL[END]

ADDRESS   :0x65ed8
LEN_BYTES :7
ORIGINAL  :0S0JT[END]
TRANSLATED:0S0JT[END]

ADDRESS   :0x66524
LEN_BYTES :12
ORIGINAL  :337wwwtr-Bp[END]
TRANSLATED:337wwwtr-Bp[END]

ADDRESS   :0x66e7c
LEN_BYTES :4
ORIGINAL  :NFq[END]
TRANSLATED:NFq[END]

ADDRESS   :0x66f2c
LEN_BYTES :4
ORIGINAL  :Fy0[END]
TRANSLATED:Fy0[END]

ADDRESS   :0x66f38
LEN_BYTES :4
ORIGINAL  :Uvs[END]
TRANSLATED:Uvs[END]

ADDRESS   :0x66fb8
LEN_BYTES :4
ORIGINAL  :3FQ:[END]
TRANSLATED:3FQ:[END]

ADDRESS   :0x67230
LEN_BYTES :4
ORIGINAL  :EVr[END]
TRANSLATED:EVr[END]

ADDRESS   :0x672a8
LEN_BYTES :4
ORIGINAL  :3Ea[END]
TRANSLATED:3Ea[END]

ADDRESS   :0x67900
LEN_BYTES :4
ORIGINAL  :%P [END]
TRANSLATED:%P [END]

ADDRESS   :0x67d94
LEN_BYTES :4
ORIGINAL  :m0W [END]
TRANSLATED:m0W [END]

ADDRESS   :0x683b8
LEN_BYTES :6
ORIGINAL  :w[END]
TRANSLATED:w[END]

ADDRESS   :0x68518
LEN_BYTES :6
ORIGINAL  :C
0[END]
TRANSLATED:C
0[END]

ADDRESS   :0x68598
LEN_BYTES :6
ORIGINAL  :!
 [END]
TRANSLATED:!
 [END]

ADDRESS   :0x685d0
LEN_BYTES :6
ORIGINAL  :K[END]
TRANSLATED:K[END]

ADDRESS   :0x685f8
LEN_BYTES :6
ORIGINAL  :E[END]
TRANSLATED:E[END]

ADDRESS   :0x68600
LEN_BYTES :6
ORIGINAL  :aP[END]
TRANSLATED:aP[END]

ADDRESS   :0x686b0
LEN_BYTES :6
ORIGINAL  :4P[END]
TRANSLATED:4P[END]

ADDRESS   :0x693cc
LEN_BYTES :7
ORIGINAL  :+,-./01[END]
TRANSLATED:+,-./01[END]

ADDRESS   :0x693d8
LEN_BYTES :5
ORIGINAL  :45678[END]
TRANSLATED:45678[END]

ADDRESS   :0x69ce0
LEN_BYTES :9
ORIGINAL  :UUUUUUUUS[END]
TRANSLATED:UUUUUUUUS[END]

ADDRESS   :0x69e48
LEN_BYTES :5
ORIGINAL  :fffeQ[END]
TRANSLATED:fffeQ[END]

ADDRESS   :0x6dfac
LEN_BYTES :4
ORIGINAL  :x/[END]
TRANSLATED:x/[END]

ADDRESS   :0x6e184
LEN_BYTES :4
ORIGINAL  :IK[END]
TRANSLATED:IK[END]

ADDRESS   :0x6e194
LEN_BYTES :6
ORIGINAL  :d 2 [END]
TRANSLATED:d 2 [END]

ADDRESS   :0x6e29c
LEN_BYTES :12
ORIGINAL  :pG0HHH[END]
TRANSLATED:pG0HHH[END]

ADDRESS   :0x6e4ec
LEN_BYTES :5
ORIGINAL  :4F[END]
TRANSLATED:4F[END]

ADDRESS   :0x6e518
LEN_BYTES :4
ORIGINAL  :5a[END]
TRANSLATED:5a[END]

ADDRESS   :0x6e524
LEN_BYTES :5
ORIGINAL  :ua[END]
TRANSLATED:ua[END]

ADDRESS   :0x6e718
LEN_BYTES :4
ORIGINAL  :B![END]
TRANSLATED:B![END]

ADDRESS   :0x6e7f8
LEN_BYTES :4
ORIGINAL  :ž[END]
TRANSLATED:ž[END]

ADDRESS   :0x6e8a8
LEN_BYTES :4
ORIGINAL  :Y[END]
TRANSLATED:Y[END]

ADDRESS   :0x6e9b4
LEN_BYTES :65
ORIGINAL  :Maintenez la touche #9f2f34 K10# enfoncée, puis appuyez sur OK.
[END]
TRANSLATED:Maintenez la touche #9f2f34 K10# enfoncée, puis appuyez sur OK.
[END]

ADDRESS   :0x6e9f8
LEN_BYTES :72
ORIGINAL  :Please move the trigger to the #3df3ff bottom# and press the OK button.
[END]
TRANSLATED:Please move the trigger to the #3df3ff bottom# and press the OK button.
[END]

ADDRESS   :0x6ea44
LEN_BYTES :85
ORIGINAL  :Please move the handwheel to the #3df3ff far# #3df3ff left# and press the OK button.
[END]
TRANSLATED:Please move the handwheel to the #3df3ff far# #3df3ff left# and press the OK button.
[END]

ADDRESS   :0x6ea9c
LEN_BYTES :69
ORIGINAL  :Please move the trigger to the #9f2f34 top #and press the OK button.
[END]
TRANSLATED:Please move the trigger to the #9f2f34 top #and press the OK button.
[END]

ADDRESS   :0x6eae4
LEN_BYTES :103
ORIGINAL  :Please press and #9f2f34 hold# #9f2f34 the# #9f2f34 K10# #9f2f34 button# and then press the OK button.
[END]
TRANSLATED:Please press and #9f2f34 hold# #9f2f34 the# #9f2f34 K10# #9f2f34 button# and then press the OK button.
[END]

ADDRESS   :0x6eb4c
LEN_BYTES :102
ORIGINAL  :Please press and #3df3ff hold# #3df3ff the# #3df3ff K9# #3df3ff button# and then press the OK button.
[END]
TRANSLATED:Please press and #3df3ff hold# #3df3ff the# #3df3ff K9# #3df3ff button# and then press the OK button.
[END]

ADDRESS   :0x6ebb4
LEN_BYTES :91
ORIGINAL  :按 #9f2f34 OK# 重置遥控器设置以及所有模型设置,按 #1b806d HOME+OK# 退出.
[END]
TRANSLATED:按 #9f2f34 OK# 重置遥控器设置以及所有模型设置,按 #1b806d HOME+OK# 退出.
[END]

ADDRESS   :0x6ec10
LEN_BYTES :64
ORIGINAL  :按 #9f2f34 OK# 重置模型设置,按 #1b806d HOME+OK# 退出.
[END]
TRANSLATED:按 #9f2f34 OK# 重置模型设置,按 #1b806d HOME+OK# 退出.
[END]

ADDRESS   :0x6ec54
LEN_BYTES :66
ORIGINAL  :Bringen Sie das Lenkrad in die Mittelstellung und drücken Sie OK
[END]
TRANSLATED:Bringen Sie das Lenkrad in die Mittelstellung und drücken Sie OK
[END]

ADDRESS   :0x6ec98
LEN_BYTES :69
ORIGINAL  :Bringen Sie den Trigger in die mittlere Position und drücken Sie OK
[END]
TRANSLATED:Bringen Sie den Trigger in die mittlere Position und drücken Sie OK
[END]

ADDRESS   :0x6ece0
LEN_BYTES :69
ORIGINAL  :Halten Sie die Taste #9f2f34 K10# gedrückt und drücken Sie dann OK
[END]
TRANSLATED:Halten Sie die Taste #9f2f34 K10# gedrückt und drücken Sie dann OK
[END]

ADDRESS   :0x6ed28
LEN_BYTES :82
ORIGINAL  :Please move the handwheel to the #9f7b34 center position# and press the OK button
[END]
TRANSLATED:Please move the handwheel to the #9f7b34 center position# and press the OK button
[END]

ADDRESS   :0x6ed7c
LEN_BYTES :80
ORIGINAL  :Please move the trigger to the #9f7b34 center position# and press the OK button
[END]
TRANSLATED:Please move the trigger to the #9f7b34 center position# and press the OK button
[END]

ADDRESS   :0x6edd0
LEN_BYTES :76
ORIGINAL  :Please move the handwheel to the #9f2f34 far right# and press the OK button
[END]
TRANSLATED:Please move the handwheel to the #9f2f34 far right# and press the OK button
[END]

ADDRESS   :0x6ee20
LEN_BYTES :76
ORIGINAL  :Maintenez les touches K9 et K10 enfoncées simultanément et appuyez sur OK.[END]
TRANSLATED:Maintenez les touches K9 et K10 enfoncées simultanément et appuyez sur OK.[END]

ADDRESS   :0x6ee70
LEN_BYTES :111
ORIGINAL  :Drücken Sie #9f2f34 OK#, um alle Einstellungen zurückzusetzen, und drücken Sie #1b806d HOME+OK# zum Beenden.[END]
TRANSLATED:Drücken Sie #9f2f34 OK#, um alle Einstellungen zurückzusetzen, und drücken Sie #1b806d HOME+OK# zum Beenden.[END]

ADDRESS   :0x6eee0
LEN_BYTES :87
ORIGINAL  :#9f2f34 OK#, um die Einstellungen zurückzusetzen, danach #1b806d HOME+OK# zum Beenden.[END]
TRANSLATED:#9f2f34 OK#, um die Einstellungen zurückzusetzen, danach #1b806d HOME+OK# zum Beenden.[END]

ADDRESS   :0x6ef38
LEN_BYTES :110
ORIGINAL  :Appuyez sur #9f2f34 OK# pour réinitialiser tous les paramètres et appuyez sur #1b806d HOME+OK# pour quitter.[END]
TRANSLATED:Appuyez sur #9f2f34 OK# pour réinitialiser tous les paramètres et appuyez sur #1b806d HOME+OK# pour quitter.[END]

ADDRESS   :0x6efa8
LEN_BYTES :84
ORIGINAL  :#9f2f34 OK# pour réinitialiser les paramètres, puis #1b806d HOME+OK# pour quitter.[END]
TRANSLATED:#9f2f34 OK# pour réinitialiser les paramètres, puis #1b806d HOME+OK# pour quitter.[END]

ADDRESS   :0x6f000
LEN_BYTES :82
ORIGINAL  :Press #9f2f34 OK# to reset the model Settings, and press #1b806d HOME+OK# to exit.[END]
TRANSLATED:Press #9f2f34 OK# to reset the model Settings, and press #1b806d HOME+OK# to exit.[END]

ADDRESS   :0x6f054
LEN_BYTES :114
ORIGINAL  :Press #9f2f34 OK# to reset the remote control Settings and all model Settings, and press #1b806d HOME+OK# to exit.[END]
TRANSLATED:Press #9f2f34 OK# to reset the remote control Settings and all model Settings, and press #1b806d HOME+OK# to exit.[END]

ADDRESS   :0x6f0c8
LEN_BYTES :70
ORIGINAL  :À propos de nous:
www.dumborc.com
Matériel: V1.0.0
Logiciels: V1.1.9[END]
TRANSLATED:À propos de nous:
www.dumborc.com
Matériel: V1.0.0
Logiciels: V1.1.9[END]

ADDRESS   :0x6f110
LEN_BYTES :83
ORIGINAL  :サポート:
www.dumborc.com
ハードウェア: V1.0.0
ソフトウェア: V1.1.9[END]
TRANSLATED:サポート:
www.dumborc.com
ハードウェア: V1.0.0
ソフトウェア: V1.1.9[END]

ADDRESS   :0x6f164
LEN_BYTES :75
ORIGINAL  :Halten Sie die Tasten K9 und K10 gleichzeitig gedrückt und drücken Sie OK[END]
TRANSLATED:Halten Sie die Tasten K9 und K10 gleichzeitig gedrückt und drücken Sie OK[END]

ADDRESS   :0x6f1b4
LEN_BYTES :144
ORIGINAL  :Please #9f2f34 hold# #9f2f34 down# #9f2f34 the# #9f2f34 K9# #9f2f34 and# #9f2f34 K10# #9f2f34 button# at the same time, then press the OK button[END]
TRANSLATED:Please #9f2f34 hold# #9f2f34 down# #9f2f34 the# #9f2f34 K9# #9f2f34 and# #9f2f34 K10# #9f2f34 button# at the same time, then press the OK button[END]

ADDRESS   :0x6f248
LEN_BYTES :75
ORIGINAL  :トリガーを奥に押しながらOKボダンを
押してください。[END]
TRANSLATED:トリガーを奥に押しながらOKボダンを
押してください。[END]

ADDRESS   :0x6f294
LEN_BYTES :75
ORIGINAL  :ステアリングを右に回してOKボダンを
押してください。[END]
TRANSLATED:ステアリングを右に回してOKボダンを
押してください。[END]

ADDRESS   :0x6f2e0
LEN_BYTES :69
ORIGINAL  :K10ボダンを押したままOKボダンを
押してください。[END]
TRANSLATED:K10ボダンを押したままOKボダンを
押してください。[END]

ADDRESS   :0x6f328
LEN_BYTES :78
ORIGINAL  :トリガーを手前に引きながらOKボタンを
押してください。[END]
TRANSLATED:トリガーを手前に引きながらOKボタンを
押してください。[END]

ADDRESS   :0x6f378
LEN_BYTES :68
ORIGINAL  :K9ボタンを押しながらOKボタンを
押してください。[END]
TRANSLATED:K9ボタンを押しながらOKボタンを
押してください。[END]

ADDRESS   :0x6f3c0
LEN_BYTES :81
ORIGINAL  :トリガーをニュートラルのまま
OKボダンを押してください。[END]
TRANSLATED:トリガーをニュートラルのまま
OKボダンを押してください。[END]

ADDRESS   :0x6f414
LEN_BYTES :99
ORIGINAL  :ステアリングホイールをニュートラルの
ままOKボダンを押してください。[END]
TRANSLATED:ステアリングホイールをニュートラルの
ままOKボダンを押してください。[END]

ADDRESS   :0x6f478
LEN_BYTES :87
ORIGINAL  :ステアリングホイールを左に回して
OKボタンを押してください。[END]
TRANSLATED:ステアリングホイールを左に回して
OKボタンを押してください。[END]

ADDRESS   :0x6f4d0
LEN_BYTES :80
ORIGINAL  :K9とK10ボタン同時に押したまま
OKボタンを押してください。[END]
TRANSLATED:K9とK10ボタン同時に押したまま
OKボタンを押してください。[END]

ADDRESS   :0x6f524
LEN_BYTES :128
ORIGINAL  :OKボタンを押してプロボ設定と
全てモデル設定をリセットします。
HOME+OKを押して終了します。[END]
TRANSLATED:OKボタンを押してプロボ設定と
全てモデル設定をリセットします。
HOME+OKを押して終了します。[END]

ADDRESS   :0x6f5a8
LEN_BYTES :139
ORIGINAL  :OKボタン押すとモデルセッティングがリセットされます。
HOMEボタン+OKボダンの順でキャンセルします。[END]
TRANSLATED:OKボタン押すとモデルセッティングがリセットされます。
HOMEボタン+OKボダンの順でキャンセルします。[END]

ADDRESS   :0x6f638
LEN_BYTES :80
ORIGINAL  :Kanal 1
Kanal 2
Kanal 3
Kanal 4
Kanal 5
Kanal 6
Kanal 7
Kanal 8
Kanal 9
Kanal 10[END]
TRANSLATED:Kanal 1
Kanal 2
Kanal 3
Kanal 4
Kanal 5
Kanal 6
Kanal 7
Kanal 8
Kanal 9
Kanal 10[END]

ADDRESS   :0x6f68c
LEN_BYTES :80
ORIGINAL  :通道1
通道2
通道3
通道4
通道5
通道6
通道7
通道8
通道9
通道10[END]
TRANSLATED:通道1
通道2
通道3
通道4
通道5
通道6
通道7
通道8
通道9
通道10[END]

ADDRESS   :0x6f6e0
LEN_BYTES :125
ORIGINAL  :P シリーズ受信機のみがこのインターフェイスでのパラメーター調整をサポートしています。[END]
TRANSLATED:P シリーズ受信機のみがこのインターフェイスでのパラメーター調整をサポートしています。[END]

ADDRESS   :0x6f8f4
LEN_BYTES :4
ORIGINAL  :Btn1[END]
TRANSLATED:Btn1[END]

ADDRESS   :0x6f8fc
LEN_BYTES :4
ORIGINAL  :Btn2[END]
TRANSLATED:Btn2[END]

ADDRESS   :0x6f904
LEN_BYTES :4
ORIGINAL  :Btn3[END]
TRANSLATED:Btn3[END]

ADDRESS   :0x6f90c
LEN_BYTES :4
ORIGINAL  :Btn4[END]
TRANSLATED:Btn4[END]

ADDRESS   :0x6f914
LEN_BYTES :4
ORIGINAL  :Btn5[END]
TRANSLATED:Btn5[END]

ADDRESS   :0x6f92c
LEN_BYTES :6
ORIGINAL  :\Kp[END]
TRANSLATED:\Kp[END]

