ADDRESS   :0x4f094
LEN_BYTES :12
ORIGINAL  :General menu[END]
TRANSLATED:General[END]

ADDRESS   :0x4f0a4
LEN_BYTES :10
ORIGINAL  :Model menu[END]
TRANSLATED:Model[END]

ADDRESS   :0x4f0b0
LEN_BYTES :20
ORIGINAL  :Transmitter Settings[END]
TRANSLATED:Transmitter[END]

ADDRESS   :0x4f0c8
LEN_BYTES :16
ORIGINAL  :Receiver setting[END]
TRANSLATED:Receiver[END]

ADDRESS   :0x4f594
LEN_BYTES :12
ORIGINAL  :General menu[END]
TRANSLATED:General[END]

ADDRESS   :0x4f604
LEN_BYTES :10
ORIGINAL  :Model menu[END]
TRANSLATED:Model[END]

ADDRESS   :0x4fa94
LEN_BYTES :20
ORIGINAL  :Transmitter Settings[END]
TRANSLATED:Transmitter[END]

ADDRESS   :0x4fb1c
LEN_BYTES :16
ORIGINAL  :Receiver setting[END]
TRANSLATED:Receiver[END]

ADDRESS   :0x8214
LEN_BYTES :14
ORIGINAL  :Model Settings[END]
TRANSLATED:Model[END]

ADDRESS   :0x7c6c
LEN_BYTES :14
ORIGINAL  :Rudder reading[END]
TRANSLATED:Channel Values[END]

ADDRESS   :0xce28
LEN_BYTES :9
ORIGINAL  :END Point[END]
TRANSLATED:Endpoints[END]

ADDRESS   :0xd78c
LEN_BYTES :4
ORIGINAL  :Back[END]
TRANSLATED:Back[END]

ADDRESS   :0xd7c4
LEN_BYTES :5
ORIGINAL  :Front[END]
TRANSLATED:Fwd[END]

ADDRESS   :0x136f4
LEN_BYTES :8
ORIGINAL  :SUB Trim[END]
TRANSLATED:Subtrims[END]

ADDRESS   :0x18bdc
LEN_BYTES :45
ORIGINAL  :Self-locking
Momentary
Three-speed
Four-speed[END]
TRANSLATED:Toggle
Push
Tri-state
Four-state[END]

ADDRESS   :0x1a26c
LEN_BYTES :9
ORIGINAL  :Remapping[END]
TRANSLATED:Mapping[END]

ADDRESS   :0x9278
LEN_BYTES :13
ORIGINAL  :mode 1
mode 2[END]
TRANSLATED:Mode 1
Mode 2[END]

ADDRESS   :0xbc7c
LEN_BYTES :7
ORIGINAL  :Presets[END]
TRANSLATED:Preset [END]

ADDRESS   :0xf944
LEN_BYTES :7
ORIGINAL  :Presets[END]
TRANSLATED:Preset [END]

ADDRESS   :0xf4e0
LEN_BYTES :20
ORIGINAL  :Throttle/Brake Curve[END]
TRANSLATED:Throttle Curve[END]

ADDRESS   :0x11d8c
LEN_BYTES :10
ORIGINAL  :Enable Key[END]
TRANSLATED:Start[END]

ADDRESS   :0x12218
LEN_BYTES :14
ORIGINAL  :Adjusting Knob[END]
TRANSLATED:Setting[END]

ADDRESS   :0x14e44
LEN_BYTES :11
ORIGINAL  :Front Ratio[END]
TRANSLATED:Fwd Rate[END]

ADDRESS   :0x14e90
LEN_BYTES :11
ORIGINAL  :Break Ratio[END]
TRANSLATED:Back Rate[END]

ADDRESS   :0x14ee0
LEN_BYTES :10
ORIGINAL  :Left Ratio[END]
TRANSLATED:Left
Rate[END]

ADDRESS   :0x14f30
LEN_BYTES :11
ORIGINAL  :Right Ratio[END]
TRANSLATED:Right
Rate[END]

ADDRESS   :0x17804
LEN_BYTES :12
ORIGINAL  :Rising ratio[END]
TRANSLATED:Rise rate[END]

ADDRESS   :0x17b60
LEN_BYTES :13
ORIGINAL  :Decline ratio[END]
TRANSLATED:Drop rate[END]

ADDRESS   :0x871c
LEN_BYTES :14
ORIGINAL  :Model renaming[END]
TRANSLATED:Model Rename[END]

ADDRESS   :0xa824
LEN_BYTES :14
ORIGINAL  :Coaching model[END]
TRANSLATED:Trainer mode[END]

ADDRESS   :0xb298
LEN_BYTES :17
ORIGINAL  :Stop/Reset button[END]
TRANSLATED:Stop/Reset btn[END]

ADDRESS   :0xe7ac
LEN_BYTES :18
ORIGINAL  :Power_on/off sound[END]
TRANSLATED:On/Off Sound[END]

ADDRESS   :0xe818
LEN_BYTES :9
ORIGINAL  :Tone Type[END]
TRANSLATED:Sounds[END]

ADDRESS   :0xf034
LEN_BYTES :36
ORIGINAL  :Close 
1 min 
3 min 
10 min 
30 min [END]
TRANSLATED:Off
1 min
3 min
10 min
30 min[END]

ADDRESS   :0x1d7e0
LEN_BYTES :29
ORIGINAL  :Close 
15 min 
30 min 
60 min[END]
TRANSLATED:Off
15 min
30 min
60 min[END]

ADDRESS   :0x1dcec
LEN_BYTES :43
ORIGINAL  :Close 
Idle 5 min 
Idle 10 min 
Idle 20 min[END]
TRANSLATED:Off
Idle 5 min
Idle 10 min
Idle 20 min[END]

ADDRESS   :0x13108
LEN_BYTES :15
ORIGINAL  :Current Voltage[END]
TRANSLATED:Voltage Curr.[END]

ADDRESS   :0x1e318
LEN_BYTES :18
ORIGINAL  :Voltage Calibrator[END]
TRANSLATED:Voltage Calib.[END]

ADDRESS   :0xb3a8
LEN_BYTES :20
ORIGINAL  :Close
Bright
Dynamic[END]
TRANSLATED:Off
Static
Dynamic[END]

ADDRESS   :0x10cd8
LEN_BYTES :12
ORIGINAL  :Double ratio[END]
TRANSLATED:Dual rates[END]

ADDRESS   :0x12294
LEN_BYTES :13
ORIGINAL  :Current Value[END]
TRANSLATED:Value[END]

ADDRESS   :0x199b8
LEN_BYTES :10
ORIGINAL  :Left Ratio[END]
TRANSLATED:Left[END]

ADDRESS   :0x19a74
LEN_BYTES :11
ORIGINAL  :Right Ratio[END]
TRANSLATED:Right[END]

ADDRESS   :0x23794
LEN_BYTES :19
ORIGINAL  :Servo Swing Control[END]
TRANSLATED:Servo Sweep[END]

ADDRESS   :0x23c90
LEN_BYTES :6
ORIGINAL  :Switch[END]
TRANSLATED:Start[END]
