<template #introduction>

:::info
The Loongson 2K0300 "Pioneer" is a development board launched based on Loongson 2K0300.
:::

</template>

<template #spec>

| Category | Specification |
| ---- | ---- |
| Manufacturer | Loongson Technology |
| Form Factor | 85×56mm |
| Processor | 2K0300 @ 1.0GHz |
| Memory | 512MiB DDR4 (onboard) |
| Interfaces (USB) | 4 × USB 2.0, 1 × USB-C† |
| Interfaces (Storage) | 1 × microSD card slot, 8GB eMMC (onboard) |
| Interfaces (Network) | 1 × GbE, onboard Wi-Fi module |
| Interfaces (Video) | 1 × LCD output |
| Interfaces (Other) | 1 × 3.5mm headphone/microphone jack, 1 × USB hub, 1 × JTAG debug interface, 1 × ADC/TTL debug interface, 40-pin GPIO |

†: USB-C for power and serial.

</template>

<template #known-issues>

None noted.

</template>

<template #image>

![](/images/devices/loongson-2k0300-pioneer-evb.webp)
Source: Loongson Technology

</template>
