<template #introduction>

:::info
The ALIENTEK 2K0300 Development Board is a development board based on Loongson 2K0300.
:::

</template>

<template #spec>

| Category | Specification |
| ---- | ---- |
| Manufacturer | ALIENTEK |
| Form Factor | 42×37mm (core board), 180×100mm (base board) |
| Processor | 2K0300 @ 1.0GHz |
| Memory | 512MiB DDR4 (onboard) |
| Interfaces (USB) | 2 × USB 2.0, 2 × USB-C (1 × OTG, 1 × serial port) |
| Interfaces (Storage) | 1 × microSD card slot, 8GB eMMC (onboard) |
| Interfaces (Network) | 2 × GbE, Wi-Fi + Bluetooth module (onboard) |
| Interfaces (Video) | 1 × LCD output |
| Interfaces (Other) | 1 × 3.5mm headphone/microphone jack, 1 × speaker, 1 × mPCIe interface (available for 4G LTE), 1 × SIM card slot, 1 × microphone, 1 × ADC, 1 × RS-232 serial port (DB-9), 2 × CAN-FD, 2 × RS-485, 14-pin user expansion I/O |

</template>

<template #known-issues>

None noted.

</template>

<template #image>

![Front-side view of the ALIENTEK 2K0300 EVB, with interfaces annotated](/images/devices/alientek-2k0300-evb-1.webp)
![Back-side view of the ALIENTEK 2K0300 EVB](/images/devices/alientek-2k0300-evb-2.webp)
Source: ALIENTEK

</template>
