# Page 185–188 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 185–188 of 434

# Page 185 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| COIL (n) | A sequence of loops | MAKE SURE THAT THE COILS OF THE OXYGEN HOSE DO NOT RUB TOGETHER. | |
| coil (v) — UNNAPPROVED | WIND (v) | WIND THE CABLES CAREFULLY. | Coil the cables carefully. |
| coincide (v) — UNNAPPROVED | ALIGN (v) | THE FASTENERS MUST ALIGN WITH THE HOLES IN THE TRACK. | The fasteners must coincide with the holes in the track. |
| coincident (adj) — UNNAPPROVED | SYNCHRONIZED (adj) | MAKE SURE THAT THE MOVEMENT OF THE TWO SURFACES IS SYNCHRONIZED. | Make sure that the movement of the two surfaces is coincident. |
| coincident (adj) — UNNAPPROVED | ALIGN (v) | MAKE SURE THAT THE TWO SURFACES ALIGN. | Make sure that the two surfaces are coincident. |
| COLD (adj) (COLDER, COLDEST) | At low temperature | MAKE SURE THAT COLD AIR COMES OUT OF THE OUTLETS. | |
| collapse (v) — UNNAPPROVED | CLOSE (v) | CLOSE THE BOX. | Collapse the box. |
| collapse (v) — UNNAPPROVED | FALL (v) | THE BOARDING BRIDGE FELL. | The boarding bridge collapsed. |
| COLLECT (v), COLLECTS, COLLECTED, COLLECTED | To come, or cause to come, together in one location | FLUID COLLECTS IN THE BOTTOM OF THE COWLING. | |
| COLLECT (v), COLLECTS, COLLECTED, COLLECTED | | COLLECT ALL LOOSE ITEMS AND PUT THEM IN THE CONTAINER. | |
| COLOR (n) | A property of light | THE COLOR CHANGES FROM BLUE TO RED. | |
| color code (v) — UNNAPPROVED | IDENTIFY (v) | IDENTIFY THE ASSEMBLY WITH THE CORRECT COLOR. | The assembly must be color coded. |
| color code (v) — UNNAPPROVED | CODE (n) | PUT A COLOR CODE ON EACH OF THE ASSEMBLIES. | Color code the assemblies. |
| colored (adj) — UNNAPPROVED | COLOR (n) | THE SCALE HAS TWO AREAS OF DIFFERENT COLOR. | The scale is divided into two colored areas. |

# Page 186 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| combine (v) — UNNAPPROVED | MIX (v) | MIX THE WATER AND THE GLYCOL. | Combine water and glycol. |
| combine (v) — UNNAPPROVED | PUT TOGETHER | DO NOT PUT DIFFERENT HPT SEGMENTS TOGETHER. | Do not combine different HPT segments. |
| combustible (adj) — UNNAPPROVED | FLAMMABLE (adj) | KEEP FLAMMABLE MATERIALS AT A MINIMUM DISTANCE OF 50 FEET FROM THE WORK AREA. | |
| COME (v), COMES, CAME | No other verb forms. To move to your location | FUMES MUST NOT COME INTO THE CABIN. | |
| COME ON (v), COMES ON, CAME ON | No other verb forms. To become bright with light when an internal power source is energized | THE LIGHTS MUST COME ON. | |
| commencement (n) — UNNAPPROVED | START (v) | AFTER THE TEST STARTS, MONITOR THE RESULTS ON THE SCREEN. | After the test commencement, monitor the results on the screen. |
| common (adj) — UNNAPPROVED | SAME (adv) | THE REMOVAL PROCEDURE IS THE SAME FOR THE TWO ITEMS. | The removal procedure is common to both items. |

# Page 187 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| communicate (v) — UNNAPPROVED | CONTACT (v) | FOR MORE INFORMATION, CONTACT THE MANUFACTURER. | For more information, communicate with the manufacturer. |
| communicate (v) — UNNAPPROVED | SPEAK (v) | USE A TELEPHONE TO SPEAK WITH THE LINE MANAGER. | Use a telephone to communicate with the line manager. |
| communicate (v) — UNNAPPROVED | HEAR (v) | MAKE SURE THAT AIR TRAFFIC CONTROL CAN HEAR YOU. | Make sure that you communicate with ATC. |
| communicate (v) — UNNAPPROVED | COMMUNICATION (n) | MAKE SURE THAT THERE IS COMMUNICATION BETWEEN THE SERVER AND THE PC. | Make sure that the server and the PC can communicate. |
| COMMUNICATION (n) | The exchange of information through a common system of symbols, signs, or sounds | COMMUNICATION BETWEEN THESE TWO SYSTEMS IS ENCRYPTED. | |
| COMPARE (v), COMPARES, COMPARED, COMPARED | To examine for differences | COMPARE THE TWO VALUES. | |
| comparison (n) — UNNAPPROVED | COMPARE (v) | COMPARE THE TWO INDICATIONS. | Make a comparison of the two readings. |
| COMPATIBLE (adj) | That can operate together satisfactorily or be used together safely | THIS SOFTWARE IS COMPATIBLE ONLY WITH THE SPECIFIED OPERATING SYSTEM. | |
| COMPATIBLE (adj) | | THE COOLANT IS COMPATIBLE WITH HIGH-PERFORMANCE ALLOYS. | |
| compile (v) — UNNAPPROVED | MAKE A LIST | MAKE A LIST OF THE NECESSARY TOOLS. | Compile a list of the required tools. |
| compile (v) — UNNAPPROVED | RECORD (v) | RECORD THE AILERON MOVEMENTS ON FORM B. | |
| compilation (n) — UNNAPPROVED | COLLECT (v) | COLLECT ALL INSPECTION RECORDS FOR THE COMPONENT. | Compile all inspection records for the component. |

# Page 188 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| complete (adj) — UNNAPPROVED | FULL (adj) | EXTEND AND RETRACT THE ACTUATOR THROUGH THREE FULL CYCLES. | Extend and retract the actuator through three complete cycles. |
| complete (adj) — UNNAPPROVED | ALL (adj) | SEND ALL THE TEST RESULTS TO THE MANUFACTURER. | The complete test results must be sent to the manufacturer. |
| complete (adj) — UNNAPPROVED | COMPLETED (adj) | THE GREEN INDICATION SHOWS THAT SERVICING IS COMPLETED. | The green indication shows that servicing is complete. |
| COMPLETE (v), COMPLETES, COMPLETED, COMPLETED | To bring to an end | COMPLETE THE FUNCTIONAL TEST. | |
| COMPLETED (adj) | Successfully brought to an end | SEND THE COMPLETED REPORT TO THE SUPERVISOR FOR APPROVAL. | |
| completely (adv) — UNNAPPROVED | FULLY (adv) | BEFORE YOU APPLY THE SECOND LAYER, LET THE FIRST LAYER OF PAINT DRY FULLY. | |
| completion (n) — UNNAPPROVED | END (n) | AT THE END OF THIS PROCEDURE, REFER TO 72-00-00, TEST 001. | See 72-00-00, Testing 001 upon completion of this procedure. |
| completion (n) — UNNAPPROVED | COMPLETE (v) | TWO HOURS ARE NECESSARY TO COMPLETE THIS TASK. | Completion of the task will require two hours. |
| complicated (adj) — UNNAPPROVED | NOT EASY | THIS TEST PROCEDURE IS NOT EASY WITHOUT THE CORRECT EQUIPMENT. | This test procedure is complicated without the right equipment. |
| comply (v) — UNNAPPROVED | OBEY (v) | WHEN YOU ASSEMBLE THE UNIT, OBEY THIS PROCEDURE. | When you assemble the unit, comply with this procedure. |
| comply (v) — UNNAPPROVED | Used in law and regulations. Refer to rule 1.12. | THE SHIP CERTIFICATE MUST COMPLY WITH ALL THE REQUIREMENTS OF THE AUTHORITIES. | |
