# Page 337 of 434

**Page 2-1-P17**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**<br>**Non-STE example**|
|---|---|---|
|**PUSH (v),**<br>**PUSHES,**<br>**PUSHED,**<br>**PUSHED**|1.To apply a force to<br>something to move it<br>away from the<br>source of the force|PUSH THE INSERT<br>DOWN UNTIL IT<br>TOUCHES THE<br>BOTTOM OF THE<br>HOLE.|
|||2.To move with a force<br>against something<br>Use this word<br>together with a<br>preposition or an<br>adverb to show<br>direction.|THE SPRING UNIT<br>PUSHES AGAINST THE<br>BRAKE PEDAL.|
|**PUT (v),**<br>**PUTS,**<br>**PUT**<br>No other verb<br>forms.|To cause something to<br>move or to be in a<br>specified position or<br>condition|PUT THE ADAPTER IN<br>POSITION AGAINST<br>ITS SUPPORT.|
||||PUT THE LEVER BACK<br>TO ITS INITIAL<br>POSITION.|
|**PUT ON (v),**<br>**PUTS ON,**<br>**PUT ON**<br>No other verb<br>forms.|To cover your skin or<br>face with clothing, or<br>other items that give<br>protection|PUT ON SAFETY<br>GOGGLES AND<br>PROTECTIVE<br>CLOTHING.|

# Page 338 of 434

**Page 2-1-P18**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**qualified (adj) — UNNAPPROVED**|APPROVED (adj)|AN APPROVED<br>PERSON MUST DO<br>THE IMPORTANT<br>CHECKS.|A qualified person must<br>do the important checks.|
|**QUALITY (n)**|Condition, property,<br>or type|THIS MEDICAL<br>EQUIPMENT MUST BE<br>OF GOOD QUALITY.|
|**QUANTITY (n)**|A specified amount or<br>number|APPLY A SMALL<br>QUANTITY OF<br>LUBRICATING OIL ON<br>THE THREADS OF THE<br>BOLTS.|
|For an amount<br>that you can<br>count, use<br>NUMBER (n).|MAKE SURE THAT<br>YOU HAVE THE<br>CORRECT NUMBER<br>OF SHIMS AVAILABLE.|
|**quarterly (adv) — UNNAPPROVED**|INTERVAL (n)|SEND REPORTS TO<br>THE AUTHORITIES AT<br>INTERVALS OF THREE<br>MONTHS.|Send reports to the<br>authorities quarterly.|
|**questionable (adj) — UNNAPPROVED**|NOT SURE|IF YOU ARE NOT SURE<br>OF THEIR CONDITION,<br>REJECT THE PARTS.|Reject the parts that are<br>in a questionable<br>condition.|
|**quick (adj) — UNNAPPROVED**|QUICKLY (adv)|MAKE SURE THAT THE<br>ROD DOES NOT MOVE<br>QUICKLY.|Make sure that there is<br>no quick movement of<br>the rod.|
|**QUICKLY (adv)**|In a fast manner|MAKE SURE THAT THE<br>PRESSURE<br>DECREASES QUICKLY.|
|**quit (v) — UNNAPPROVED**|GO (v)|BEFORE YOU START<br>THE ENGINE, MAKE<br>SURE THAT ALL<br>PERSONS GO AWAY<br>FROM THE DANGER<br>AREA.|Before you start the<br>engine, make sure that<br>all persons quit the<br>danger area.|
|STOP (v)|IF THE RED LIGHT<br>COMES ON, STOP THE<br>REFUEL PROCEDURE.|If the red light comes on,<br>quit the refuel procedure.|
|**quote (v) — UNNAPPROVED**|GIVE (v)|THE TABLE GIVES THE<br>MAXIMUM<br>TOLERANCE FOR THE<br>HOLE.|The table quotes the<br>maximum tolerance for<br>the hole.|

# Page 339 of 434

**Page 2-1-Q1**

Issue 9 Part 2 - Dictionary 2025-01-15

**ASD-STE100 Simplified Technical English**

**Word Approved meaning/** **<u>(part of speech) ALTERNATIVES STE EXAMPLE</u>**

**<u>Non-STE example</u>**

Blank Page

# Page 340 of 434

**Page 2-1-Q2**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**RADIAL (adj)**|Along a radius|DO A CHECK FOR<br>RADIAL CUTS,<br>CRACKS, OR SPLITS.|
|**RADIALLY (adv)**|Along a radius|THE FAN BLADES ARE<br>INSTALLED RADIALLY.|
|**RADIOACTIVE**<br>**(adj)**|Related to radioactivity|DO A CHECK FOR<br>RADIOACTIVE<br>CONTAMINATION.|
|**raise (v) — UNNAPPROVED**|LIFT (v)|DO NOT LIFT THE<br>COVER MORE THAN<br>THE SPECIFIED<br>CLEARANCE.|Do not raise the cover<br>more than the specified<br>clearance.|
|INCREASE (v)|INCREASE THE<br>TEMPERATURE BY<br>10 DEG.|Raise the temperature<br>10 deg.|
|RETRACT (v)|RETRACT THE<br>LANDING GEAR.|Raise the landing gear.|
|**RANDOM (adj)**|Not regular|DURING THIS<br>PROCEDURE, DO<br>RANDOM CHECKS OF<br>THE TIRE PRESSURE.|
|**RANDOMLY (adv)**|Not regularly|DO THESE CHECKS<br>RANDOMLY.|
|**RANGE (n)**|The limits within which<br>something operates|THE AUDIO<br>SPECTRUM IS THE<br>FREQUENCY RANGE<br>AT WHICH HUMANS<br>CAN HEAR.|
|**rapid (adj) — UNNAPPROVED**|FAST (adj)|CHEMICAL AGENTS<br>CAUSE FAST<br>DETERIORATION OF<br>PAINTED SURFACES.|Chemical agents cause<br>rapid deterioration of<br>painted surfaces.|
|**rapidly (adv) — UNNAPPROVED**|QUICKLY (adv)|QUICKLY TURN THE<br>HANDLE CLOCKWISE.|Rapidly turn the handle<br>clockwise.|
|**RATE (n)**|A measurement of how<br>frequently or how quickly<br>something occurs|MAKE SURE THAT THE<br>FLOW RATE IS<br>CORRECT.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
