# Page 421 of 434

**Page 2-1-W5**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**WITH (prep)**|Function word that<br>shows association or<br>relationship, help or<br>sharing, a means or<br>instrument|ALIGN THE MARK<br>WITH THE<br>LONGITUDINAL AXIS.||
|||Refer to<br>section 9, GR-2.|ATTACH THE FLANGE<br>(10) WITH THE FOUR<br>BOLTS (15).||
||||REMOVE THE<br>VALVE (2) WITH THE<br>EXTRACTOR.||
|**withdraw (v) — UNNAPPROVED**|REMOVE (v)|REMOVE THE<br>INDICATOR FROM THE<br>INSTRUMENT PANEL.|Withdraw the indicator<br>from the instrument<br>panel.|
|**within (prep) — UNNAPPROVED**|IN (prep)|A FILTER PREVENTS<br>CONTAMINATION OF<br>THE COMPONENTS IN<br>THE SYSTEM.|A filter prevents<br>contamination of the<br>components within the<br>system.|
|||IN ... OR LESS|LIGHT L4 COMES ON<br>IN 5 SECONDS OR<br>LESS.|Light L4 illuminates<br>within 5 seconds.|
|||IN LESS THAN|MAKE SURE THAT THE<br>WARNING LIGHT<br>COMES ON IN LESS<br>THAN 3 SECONDS.|Make sure that the<br>warning light illuminates<br>within 3 seconds.|
|**WITHOUT (prep)**|Not with|SMALL DAMAGE IS<br>PERMITTED WITHOUT<br>REPAIR. REFER TO<br>TABLE 1 FOR THE<br>APPLICABLE LIMITS.||
|**withstand (v) — UNNAPPROVED**|RESISTANT (adj)|THIS MATERIAL IS<br>RESISTANT TO FIRE.|This material can<br>withstand fire.|
|**WORK (n)**|That which you do when<br>you use physical<br>strength, or mental<br>power|DO THE WORK IN A<br>CLEAN AREA.||
|**work (v) — UNNAPPROVED**|WORK (n)|BE CAREFUL WHEN<br>YOU DO WORK NEAR<br>FUEL TANKS.|Be careful when you<br>work near fuel tanks.|
|**would (v) — UNNAPPROVED**|CAN (v)|SOLVENTS THAT STAY<br>ON THE PART CAN<br>CAUSE CORROSION.|<br>Solvents left on the part<br>would corrode the part.|

# Page 422 of 434

**Page 2-1-W6**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**wrap (v) — UNNAPPROVED**|PUT (v)|PUT THE PART IN<br>OILPAPER.|Wrap the part in<br>oilpaper.|
|||WIND (v)|WIND MASKING TAPE<br>AROUND THE PART.|Wrap masking tape<br>around the part.|
|**WRITE (v),**<br>**WRITES,**<br>**WROTE,**<br>**WRITTEN**|To record data or<br>information as words,<br>letters, or symbols|WRITE THE TEST<br>DATE ON THE<br>CERTIFICATE.||
|**wrong (adj) — UNNAPPROVED**|INCORRECT (adj)|IDENTIFY THE<br>BELLCRANK AND<br>SHAFT WITH MARKS.<br>THESE MARKS WILL<br>PREVENT AN<br>INCORRECT<br>INSTALLATION.|Mark the bellcrank and<br>shaft to prevent wrong<br>installation.|
|**wrongly (adv) — UNNAPPROVED**|INCORRECTLY (adv)|IF THE HOSES ARE<br>INCORRECTLY<br>INSTALLED, DAMAGE<br>CAN OCCUR.|Damage can occur if<br>hoses are wrongly<br>installed.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 423 of 434

**Page 2-1-W7**

**ASD-STE100 Simplified Technical English**

**Word Approved meaning/** **<u>(part of speech) ALTERNATIVES</u>**

**<u>STE EXAMPLE</u>**

**<u>Non-STE example</u>**

Blank Page

# Page 424 of 434

**Page 2-1-W8**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**YES (adv)**|Function word that<br>shows the positive<br>answer to a question|DOES THE LIGHT<br>COME ON? YES OR<br>NO?||
|**yet (conj) — UNNAPPROVED**|BUT (conj)|TIGHTEN THE NUTS,<br>BUT KEEP THEM<br>SUFFICIENTLY LOOSE<br>TO REMOVE THEM<br>WITH YOUR HAND.|The nuts should be<br>tightened, yet loose<br>enough to remove by<br>hand.|
|**yet (adv) — UNNAPPROVED**|AT THIS TIME|DO NOT REMOVE THE<br>FIXTURE COVER AT<br>THIS TIME.|Do not remove the<br>fixture cover yet.|
|**YOU (pron)**|The reader or the user|YOU CAN CONTINUE<br>THE TEST.||
||||HOT SURFACES CAN<br>BURN YOU.||
|**YOUR (adj)**|Related to the reader or<br>the user|IF YOU GET SOLVENT<br>IN YOUR EYES, FLUSH<br>THEM IMMEDIATELY<br>WITH WATER.||
|**yourself (pron) — UNNAPPROVED**|YOU (pron)|DO NOT USE YOUR<br>HANDS TO PREVENT<br>MOVEMENT OF THE<br>LP COMPRESSOR. IF<br>YOU DO, THE LP<br>COMPRESSOR CAN<br>CAUSE YOU INJURY<br>AND CAN CAUSE<br>DAMAGE TO THE<br>EQUIPMENT.|Do not use your hands<br>to prevent movement of<br>the LP compressor. If<br>you do, you can cause<br>injury to yourself and<br>damage to the<br>equipment.|
|**zero (v) — UNNAPPROVED**|ZERO (TN)|ADJUST THE METER<br>TO ZERO.|Zero the meter.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
