<!-- section: DICT_Q-Z | pages: 345-348 | verified: true -->

# Page 345 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **providing (that) — UNNAPROVED** | IF (conj) IF A NEW PART IS Providing that a new part is (conj) INSTALLED, YOU CAN installed, you can continue CONTINUE THE the operation of the OPERATION OF THE machine. MACHINE. |
| **proximity (n) — UNNAPROVED** | NEAR (prep) DO NOT DO Do not do maintenance MAINTENANCE WORK work in proximity to a NEAR AN ENGINE running engine. THAT IS IN OPERATION. |
| **PULL (v)** | , To use a force on PULL THE CABLE PULLS, something to move it DOWN AND AWAY PULLED, toward the source of the FROM THE BRACKET. PULLED force Use this word together with a preposition or an adverb to show direction. |
| **pump (v) — UNNAPROVED** | REMOVE (v) OPEN THE VALVE. Open the valve and then (WITH A PUMP [TN]) THEN, REMOVE THE pump oil from the tank. OIL FROM THE TANK AN APPLICABLE PUMP. |
| **MOVE (v)** | WHEN THE VALVE IS When the valve is open, (WITH A PUMP [TN]) OPEN, MOVE OIL pump oil from the tank to FROM THE TANK TO the circuit lines. THE CIRCUIT LINE WITH AN APPLICABLE PUMP. |
| **puncture (v) — UNNAPROVED** | HOLE (n) MAKE SURE THAT Take care not to YOU DO NOT MAKE A puncture the bladder. HOLE IN THE BLADDER. |
| **purge (v) — UNNAPROVED** | REMOVE (v) REMOVE UNWANTED Purge the system. MATERIAL FROM THE SYSTEM. |
| **purify (v) — UNNAPROVED** | CLEAN (v) CLEAN THE WATER. Purify the water. |

# Page 346 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| 1. To apply a force to |
| --- |
| something to move it |
| away from the |
| source of the force |

### HOLE.

| THE SPRING UNIT |
| --- |
| PUSHES AGAINST THE |
| BRAKE PEDAL. |

Use this word
together with a
preposition or an
adverb to show
direction.

| PUT THE ADAPTER IN |
| --- |
| POSITION AGAINST |
| ITS SUPPORT. |

condition
No other verb
forms.

### PUT THE LEVER BACK

### TO ITS INITIAL

### POSITION.

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **PUT ON (v)** | , To cover your skin or PUT ON SAFETY PUTS ON, face with clothing, or GOGGLES AND PUT ON other items that give PROTECTIVE protection CLOTHING. No other verb forms. |

# Page 347 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **qualified (adj) — UNNAPROVED** | APPROVED (adj) AN APPROVED A qualified person must PERSON MUST DO do the important checks. THE IMPORTANT CHECKS. |
| **QUALITY (n)** | Condition, property, THIS MEDICAL or type EQUIPMENT MUST BE OF GOOD QUALITY. |
| **QUANTITY (n)** | A specified amount or APPLY A SMALL number QUANTITY OF LUBRICATING OIL ON THE THREADS OF THE BOLTS. For an amount MAKE SURE THAT that you can YOU HAVE THE count, use CORRECT NUMBER |
| **NUMBER (n)** | . OF SHIMS AVAILABLE. |
| **quarterly (adv) — UNNAPROVED** | INTERVAL (n) SEND REPORTS TO Send reports to the THE AUTHORITIES AT authorities quarterly. INTERVALS OF THREE MONTHS. |
| **questionable (adj) — UNNAPROVED** | NOT SURE IF YOU ARE NOT SURE Reject the parts that are OF THEIR CONDITION, in a questionable REJECT THE PARTS. condition. |
| **quick (adj) — UNNAPROVED** | QUICKLY (adv) MAKE SURE THAT THE Make sure that there is ROD DOES NOT MOVE no quick movement of QUICKLY. the rod. |
| **QUICKLY (adv)** | In a fast manner MAKE SURE THAT THE PRESSURE DECREASES QUICKLY. |
| **quit (v) — UNNAPROVED** | GO (v) BEFORE YOU START Before you start the THE ENGINE, MAKE engine, make sure that SURE THAT ALL all persons quit the PERSONS GO AWAY danger area. FROM THE DANGER AREA. |
| **STOP (v)** | IF THE RED LIGHT If the red light comes on, COMES ON, STOP THE quit the refuel procedure. REFUEL PROCEDURE. |
| **quote (v) — UNNAPROVED** | GIVE (v) THE TABLE GIVES THE The table quotes the MAXIMUM maximum tolerance for TOLERANCE FOR THE the hole. HOLE. |

# Page 348 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example
Blank Page
Page 2-1-Q2 Part 2 - Dictionary Issue 9
2025-01-15
