<!-- section: APPENDIX | pages: 433-434 | verified: true -->

# Page 433 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **YES (adv)** | Function word that DOES THE LIGHT shows the positive COME ON? YES OR answer to a question NO? |
| **yet (conj) — UNNAPROVED** | BUT (conj) TIGHTEN THE NUTS, The nuts should be BUT KEEP THEM tightened, yet loose SUFFICIENTLY LOOSE enough to remove by TO REMOVE THEM hand. WITH YOUR HAND. |
| **yet (adv) — UNNAPROVED** | AT THIS TIME DO NOT REMOVE THE Do not remove the FIXTURE COVER AT fixture cover yet. THIS TIME. |
| **YOU (pron)** | The reader or the user YOU CAN CONTINUE THE TEST. HOT SURFACES CAN BURN YOU. |
| **YOUR (adj)** | Related to the reader or IF YOU GET SOLVENT the user IN YOUR EYES, FLUSH THEM IMMEDIATELY WITH WATER. |
| **yourself (pron) — UNNAPROVED** | YOU (pron) DO NOT USE YOUR Do not use your hands HANDS TO PREVENT to prevent movement of MOVEMENT OF THE the LP compressor. If LP COMPRESSOR. IF you do, you can cause YOU DO, THE LP injury to yourself and COMPRESSOR CAN damage to the CAUSE YOU INJURY equipment. AND CAN CAUSE DAMAGE TO THE EQUIPMENT. |
| **zero (v) — UNNAPROVED** | ZERO (TN) ADJUST THE METER Zero the meter. TO ZERO. |

# Page 434 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example
Blank Page
Page 2-1-Y2 Part 2 - Dictionary Issue 9
2025-01-15
