# Page 337–340 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 337–340 of 434

# Page 337 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE**<br>**Non-STE example** |
|---|---|---|
| **PUSH (v),**<br>**PUSHES,**<br>**PUSHED,**<br>**PUSHED** | 1.To apply a force to<br>something to move it<br>away from the<br>source of the force<br><br>2.To move with a force<br>against something<br>Use this word<br>together with a<br>preposition or an<br>adverb to show<br>direction. | PUSH THE INSERT<br>DOWN UNTIL IT<br>TOUCHES THE<br>BOTTOM OF THE<br>HOLE.<br><br>THE SPRING UNIT<br>PUSHES AGAINST THE<br>BRAKE PEDAL. |
| **PUT (v),**<br>**PUTS,**<br>**PUT**<br>No other verb<br>forms. | To cause something to<br>move or to be in a<br>specified position or<br>condition | PUT THE ADAPTER IN<br>POSITION AGAINST<br>ITS SUPPORT.<br><br>PUT THE LEVER BACK<br>TO ITS INITIAL<br>POSITION. |
| **PUT ON (v),**<br>**PUTS ON,**<br>**PUT ON**<br>No other verb<br>forms. | To cover your skin or<br>face with clothing, or<br>other items that give<br>protection | PUT ON SAFETY<br>GOGGLES AND<br>PROTECTIVE<br>CLOTHING. |

# Page 338 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **qualified (adj) — UNNAPPROVED** | APPROVED (adj) | AN APPROVED<br>PERSON MUST DO<br>THE IMPORTANT<br>CHECKS. | A qualified person must<br>do the important checks. |
| **QUALITY (n)** | Condition, property,<br>or type | THIS MEDICAL<br>EQUIPMENT MUST BE<br>OF GOOD QUALITY. |  |
| **QUANTITY (n)** | A specified amount or<br>number<br><br>For an amount<br>that you can<br>count, use<br>NUMBER (n). | APPLY A SMALL<br>QUANTITY OF<br>LUBRICATING OIL ON<br>THE THREADS OF THE<br>BOLTS.<br><br>MAKE SURE THAT<br>YOU HAVE THE<br>CORRECT NUMBER<br>OF SHIMS AVAILABLE. |  |
| **quarterly (adv) — UNNAPPROVED** | INTERVAL (n) | SEND REPORTS TO<br>THE AUTHORITIES AT<br>INTERVALS OF THREE<br>MONTHS. | Send reports to the<br>authorities quarterly. |
| **questionable (adj) — UNNAPPROVED** | NOT SURE | IF YOU ARE NOT SURE<br>OF THEIR CONDITION,<br>REJECT THE PARTS. | Reject the parts that are<br>in a questionable<br>condition. |
| **quick (adj) — UNNAPPROVED** | QUICKLY (adv) | MAKE SURE THAT THE<br>ROD DOES NOT MOVE<br>QUICKLY. | Make sure that there is<br>no quick movement of<br>the rod. |
| **QUICKLY (adv)** | In a fast manner | MAKE SURE THAT THE<br>PRESSURE<br>DECREASES QUICKLY. |  |
| **quit (v) — UNNAPPROVED** | GO (v) | BEFORE YOU START<br>THE ENGINE, MAKE<br>SURE THAT ALL<br>PERSONS GO AWAY<br>FROM THE DANGER<br>AREA. | Before you start the<br>engine, make sure that<br>all persons quit the<br>danger area. |
| **STOP (v)** | IF THE RED LIGHT<br>COMES ON, STOP THE<br>REFUEL PROCEDURE. |  | If the red light comes on,<br>quit the refuel procedure. |
| **quote (v) — UNNAPPROVED** | GIVE (v) | THE TABLE GIVES THE<br>MAXIMUM<br>TOLERANCE FOR THE<br>HOLE. | The table quotes the<br>maximum tolerance for<br>the hole. |

# Page 339 of 434

**Word Approved meaning/** **<u>(part of speech) ALTERNATIVES STE EXAMPLE</u>**

**<u>Non-STE example</u>**

Blank Page

# Page 340 of 434

| **Word**<br>**(part of speech)** | **Approved meaning/**<br>**ALTERNATIVES** | **STE EXAMPLE** | **Non-STE example** |
|---|---|---|---|
| **RADIAL (adj)** | Along a radius | DO A CHECK FOR<br>RADIAL CUTS,<br>CRACKS, OR SPLITS. |  |
| **RADIALLY (adv)** | Along a radius | THE FAN BLADES ARE<br>INSTALLED RADIALLY. |  |
| **RADIOACTIVE**<br>**(adj)** | Related to radioactivity | DO A CHECK FOR<br>RADIOACTIVE<br>CONTAMINATION. |  |
| **raise (v) — UNNAPPROVED** | LIFT (v) | DO NOT LIFT THE<br>COVER MORE THAN<br>THE SPECIFIED<br>CLEARANCE. | Do not raise the cover<br>more than the specified<br>clearance. |
| **INCREASE (v)** | INCREASE THE<br>TEMPERATURE BY<br>10 DEG. | Raise the temperature<br>10 deg. |  |
| **RETRACT (v)** | RETRACT THE<br>LANDING GEAR. | Raise the landing gear. |  |
| **RANDOM (adj)** | Not regular | DURING THIS<br>PROCEDURE, DO<br>RANDOM CHECKS OF<br>THE TIRE PRESSURE. |  |
| **RANDOMLY (adv)** | Not regularly | DO THESE CHECKS<br>RANDOMLY. |  |
| **RANGE (n)** | The limits within which<br>something operates | THE AUDIO<br>SPECTRUM IS THE<br>FREQUENCY RANGE<br>AT WHICH HUMANS<br>CAN HEAR. |  |
| **rapid (adj) — UNNAPPROVED** | FAST (adj) | CHEMICAL AGENTS<br>CAUSE FAST<br>DETERIORATION OF<br>PAINTED SURFACES. | Chemical agents cause<br>rapid deterioration of<br>painted surfaces. |
| **rapidly (adv) — UNNAPPROVED** | QUICKLY (adv) | QUICKLY TURN THE<br>HANDLE CLOCKWISE. | Rapidly turn the handle<br>clockwise. |
| **RATE (n)** | A measurement of how<br>frequently or how quickly<br>something occurs | MAKE SURE THAT THE<br>FLOW RATE IS<br>CORRECT. |  |
