// Module included in the following assemblies:
//
// microshift_networking/microshift-sriov.adoc

:_mod-docs-content-type: REFERENCE
[id="supported-devices_{context}"]
= SR-IOV Network Operator supported devices

[role="_abstract"]
The `config.yaml` file lists the supported network devices for the SR-IOV Network Operator.

.SR-IOV Network Operator configuration file

[source,yaml]
----
apiVersion: v1
kind: ConfigMap
metadata:
  name: supported-nic-ids
data:
  Intel_i40e_XXV710: "8086 158a 154c"
  Intel_i40e_25G_SFP28: "8086 158b 154c"
  Intel_i40e_10G_X710_SFP: "8086 1572 154c"
  Intel_ixgbe_10G_X550: "8086 1563 1565"
  Intel_ixgbe_82576: "8086 10c9 10ca"
  Intel_i40e_X710_X557_AT_10G: "8086 1589 154c"
  Intel_i40e_10G_X710_BACKPLANE: "8086 1581 154c"
  Intel_i40e_10G_X710_BASE_T: "8086 15ff 154c"
  Intel_i40e_XXV710_N3000: "8086 0d58 154c"
  Intel_i40e_40G_XL710_QSFP: "8086 1583 154c"
  Intel_ice_Columbiaville_E810-CQDA2_2CQDA2: "8086 1592 1889"
  Intel_ice_Columbiaville_E810-XXVDA4: "8086 1593 1889"
  Intel_ice_Columbiaville_E810-XXVDA2: "8086 159b 1889"
  Intel_ice_Columbiaville_E810-XXV_BACKPLANE: "8086 1599 1889"
  Intel_ice_Columbiaville_E810: "8086 1591 1889"
  Intel_ice_Columbiapark_E823C: "8086 188a 1889"
  Intel_ice_Columbiapark_E823L_SFP: "8086 124d 1889"
  Intel_ice_Columbiapark_E823L_BACKPLANE: "8086 124c 1889"
  Intel_ice_Columbiapark_E825C_BACKPLANE: "8086 579c 1889"
  Intel_ice_Columbiapark_E825C_QSFP: "8086 579d 1889"
  Intel_ice_Columbiapark_E825C_SFP: "8086 579e 1889"
  Intel_ice_Connorsville_E830_QSFP: "8086 12d2 1889"
  Intel_ice_Connorsville_E830_SFP: "8086 12d3 1889"
  Intel_ice_Connorsville_E835CC_QSFP: "8086 1249 1889"
  Intel_ice_Connorsville_E835CC_SFP: "8086 124a 1889"
  Nvidia_mlx5_ConnectX-4: "15b3 1013 1014"
  Nvidia_mlx5_ConnectX-4LX: "15b3 1015 1016"
  Nvidia_mlx5_ConnectX-5: "15b3 1017 1018"
  Nvidia_mlx5_ConnectX-5_Ex: "15b3 1019 101a"
  Nvidia_mlx5_ConnectX-6: "15b3 101b 101c"
  Nvidia_mlx5_ConnectX-6_Dx: "15b3 101d 101e"
  Nvidia_mlx5_ConnectX-6_Lx: "15b3 101f 101e"
  Nvidia_mlx5_ConnectX-7: "15b3 1021 101e"
  Nvidia_mlx5_ConnectX-8: "15b3 1023 101e"
  Nvidia_mlx5_MT42822_BlueField-2_integrated_ConnectX-6_Dx: "15b3 a2d6 101e"
  Nvidia_mlx5_MT43244_BlueField-3_integrated_ConnectX-7_Dx: "15b3 a2dc 101e"
  Broadcom_bnxt_BCM57414_2x25G: "14e4 16d7 16dc"
  Broadcom_bnxt_BCM75508_2x100G: "14e4 1750 1806"
  Qlogic_qede_QL45000_50G: "1077 1654 1664"
  Red_Hat_Virtio_network_device: "1af4 1000 1000"
  Red_Hat_Virtio_1_0_network_device: "1af4 1041 1041"
  Marvell_OCTEON_TX2_CN96XX: "177d b200 b203"
  Marvell_OCTEON_TX2_CN98XX: "177d b100 b103"
  Marvell_OCTEON_Fusion_CNF95XX: "177d b600 b603"
  Marvell_OCTEON10_CN10XXX: "177d b900 b903"
  Marvell_OCTEON_Fusion_CNF105XX: "177d ba00 ba03"
  Amazon_Elastic_Network_Adapter: "1d0f ec20 ec20"
----

[NOTE]
====
For the most up-to-date list of supported cards and compatible {product-title} versions available, see link:https://access.redhat.com/articles/6954499[Openshift Single Root I/O Virtualization (SR-IOV) and PTP hardware networks Support Matrix].
====
