- Settings
- Tasks
- EMA
- Download

Recorder Options:
Select what sensor/data you want to record and average each minute:
Steps Optical Heart Rate Accelerometry (per minute magnitude) Battery Movement Temperature/Pressure Bluetooth HRM (Uses BTHRM app/module) CORE Sensor (Uses coretemp app/module)
High Resolution Accelerometer Data:
If you want to record high temporal resolution accelerometer data (magnitude of x,y,z; can store up to 4 days of data at 1 second, will rollover).
High Temporal Accelerometry √(x² + y² + z²) Interval (seconds)

Interval for logging averaged magnitude and sum from accelerometer - default is 1 second

GPS PSMOO Options:
Option to have GPS work in PSMOO (uses GPSSetup app/module)
Turn GPS On Scan Time (mins)

The time spent scanning for a GPS signal.

Scan Interval (mins)

The time between scans when a signal is not acquired.

Adaptive Time (mins)

The time between scans when a signal is acquired.

Extras: Fall Detection (beta)

Will detect falls.

Randomize EMA questions

Enable this if you want your questions to be shuffled at random each time.

Swipe to Launch HeatSuite App

On by default. Will enable quick access to the HeatSuite app for participants by simply swiping right on the screen.

Study ID:

For communicating with HeatSuite Nodes. Maximum of 4 (no special) characters.

File Prefix

ONLY CHANGE IF YOU KNOW WHAT YOU ARE DOING.

Edit your Task JSON File Editor:
Read the Docs on how to properly format the JSON file. GUI coming soon to BangleApps.
Ecological Momentary Assessment (EMA) JSON File Editor:
Read the Docs on how to properly format the JSON file. GUI coming soon to BangleApps.

File name | Actions
--- | ---