# Atmel EDBG-based Tools Protocols
Events

Sidebar | Prev | Up | Next

### Event: Break

Indicates that the target has stopped

Table 133. Event: Break event format

Field | Size | Description
--- | --- | ---
EVT_AVR8_BREAK | 1 byte | Event ID
Version (0x00) | 1 byte | Event version
PC | 4 byte | Program Counter value (word address)
Break cause | 1 byte | 0x00 = unspecified 0x01 = program breakpoint
Extended info | 2 bytes | N/A

Prev | Up | Next
| Home |