# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Software Breakpoint Clear All

Removes all software breakpoints immediately. Useful if you have forgotten where you put them.

Table 127. Software Breakpoint Clear All command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_SW_BREAKPOINT_CLR_ALL | 1 byte | Command ID
Version (0x00) | 1 byte | Command version

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |