# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### QUERY

Used to discover the capabilities of the tool.

For lists of valid query types, see the section called “AVR8 QUERY contexts”

Table 94. Query

Field | Size | Description
--- | --- | ---
QUERY (0x00) | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Query context | 1 byte | Type of query to execute

Responses:

- LIST

- FAILED

Prev | Up | Next
| Home |