---
tag: m0165
title: Set Mix
brief: Set all mix factors for the mixing extruder.
author: thinkyhead

group: mixing
requires: MIXING_EXTRUDER, DIRECT_MIXING_IN_G1

codes: [ M165 ]
related: [ M163, M164, M166 ]

notes: Requires `MIXING_EXTRUDER` and `DIRECT_MIXING_IN_G1`.

parameters:

- tag: A
  optional: true
  description: Mix factor 1
  values:
  - tag: factor
    type: float

- tag: B
  optional: true
  description: Mix factor 2
  values:
  - tag: factor
    type: float

- tag: C
  optional: true
  description: Mix factor 3
  values:
  - tag: factor
    type: float

- tag: D
  optional: true
  description: Mix factor 4
  values:
  - tag: factor
    type: float

- tag: H
  optional: true
  description: Mix factor 5
  values:
  - tag: factor
    type: float

- tag: I
  optional: true
  description: Mix factor 6
  values:
  - tag: factor
    type: float

examples:
- pre: Set a colorful mix
  code: M165 A0.2 B0.4 C0.3 D0.1

---

Set the mix for the active virtual extruder all at once. Any factors left out are set to 0.0. This is based on a reference implementation by Pìa Taubert.
