---
tag: m0145
title: Set Material Preset
brief: Set material presets in the LCD menu.
author: thinkyhead

group: lcd
requires: NEWPANEL
eeprom: true

codes: [ M145 ]

notes:
  - Requires an LCD controller.
  - View the current settings with [`M503`](/docs/gcode/M503.html).
  - If `EEPROM_SETTINGS` is enabled, these settings are saved with [`M500`](/docs/gcode/M500.html), loaded with [`M501`](/docs/gcode/M501.html), and reset with [`M502`](/docs/gcode/M502.html).

parameters:

- tag: S
  optional: true
  description: Material index
  values:
  - tag: index
    type: int

- tag: H
  optional: true
  description: Hotend temperature
  values:
  - tag: temp
    type: int

- tag: B
  optional: true
  description: Bed temperature
  values:
  - tag: temp
    type: int

- tag: F
  optional: true
  description: Fan speed
  values:
  - tag: speed
    type: int

example:
- pre: Set heatup presets for material 1
  code: M145 S0 H190 B70 F50

---

Set the preheating presets for materials in the LCD menu.
