---
tag: m0363
title: SCARA Psi-B
brief: Move to Psi-B
author: thinkyhead

group: control
requires: MORGAN_SCARA

codes: [ M363 ]
related: [ M360, M361, M362, M364 ]

---

Move the nozzle to SCARA Psi-B calibration position Psi 90 (A50 B90) for calibration of "90 degrees steps-per-degree."
