Mesa 25.1.8 Release Notes / 2025-08-13
======================================

Mesa 25.1.8 is a bug fix release which fixes bugs found since the 25.1.7 release.

Mesa 25.1.8 implements the OpenGL 4.6 API, but the version reported by
glGetString(GL_VERSION) or glGetIntegerv(GL_MAJOR_VERSION) /
glGetIntegerv(GL_MINOR_VERSION) depends on the particular driver being used.
Some drivers don't support all the features required in OpenGL 4.6. OpenGL
4.6 is **only** available if requested at context creation.
Compatibility contexts may report a lower version depending on each driver.

Mesa 25.1.8 implements the Vulkan 1.4 API, but the version reported by
the apiVersion property of the VkPhysicalDeviceProperties struct
depends on the particular driver being used.

SHA checksums
-------------

::

    SHA256: 5cf1571d0d646d90047f3d93f57acc787cf88ec7e95efe172c555b492c30fb71  mesa-25.1.8.tar.xz
    SHA512: 98435d52a2855c71b15060785c225dc674b3565545a8581a5dd501605a04f9d597636282f1bce61e7a2e8ee98c31ecf7fbccab594571e31bc8b827e18e98aaa5  mesa-25.1.8.tar.xz


New features
------------

- None


Bug fixes
---------

- Build dependency on intel_wa.h missing in Intel vulkan driver
- \`vn_ring`: use-after-release crash after \`vn_ring_destroy` on Virtio-Vulkan
- venus: vkmark --winsys headless segfault (regression)
- Vulkan headless WSI crashes when initializing swapchain on Asahi Linux running Apple M1 Max
- [RADV] Graphical glitches in Ghost of Tsushima on Polaris
- Segfault when activating DPMS on i915 hardware
- radv: regression: commit a7291074c800 break lighting in Like a Dragon: Infinite Wealth


Changes
-------

Alyssa Rosenzweig (2):

- asahi: enable virtgpu support
- agx: gate scratch opt on internal shaders

Caio Oliveira (1):

- brw: Remove extra iteration on instructions from brw_opt_address_reg_load

Christian Gmeiner (2):

- etnaviv: blt: Clear only requested color buffers
- etnaviv: rs: Clear only requested color buffers

Dave Airlie (1):

- spirv: move cmat store barrier after the store.

David Rosca (3):

- vulkan/video: Fix h265 level values
- radv: Add timeout to video encode query
- rusticl/ptr: Fix hidden lifetime warning

Emma Anholt (1):

- i915: Avoid calling drm_intel_get_aperture_sizes().

Eric Engestrom (7):

- docs: add sha sum for 25.1.7
- .pick_status.json: Update to 20171f23d6b89c8fdcb2b6a56de4d8293995af64
- .pick_status.json: Mark 0cd745c386a342e2bc8b1cc5cfd26f33b771910d as denominated
- .pick_status.json: Mark 9ced3148ca18e8b057e7f2a7e773c701b95c8741 as denominated
- .pick_status.json: Mark 5649a0aa06e7f436a7f010e733e60366b471da79 as denominated
- .pick_status.json: Mark 71c4f136607eeb50b8aa08ad1a8efb8412385b96 as denominated
- ci: track changes to new src/x11/ folder

Eric R. Smith (1):

- panvk: fix a NULL pointer dereference in occlusion queries

Erico Nunes (1):

- lima: ppir: fix store_output optimization for modifiers

Gert Wollny (3):

- r600/sfn: check number of fsat64 source uses properly
- r600: Update GPR count when adding a GDS instruction
- r00/sfn: Fix copy propagation into buffer load address

Hans-Kristian Arntzen (1):

- ac/nir: Avoid 0/0 when computing texel buffer size on Polaris.

Job Noorman (1):

- ir3/legalize: prevent infinite loop when inserting (ss)nop

Jordan Justen (1):

- intel/dev: Add BMG 0xe209 PCI ID

Karol Herbst (11):

- rusticl: use pipe_sampler_view_release
- rusticl/mesa: wire up fence_server
- rusticl/gl: store the mesa_glinterop_export_in
- st/interup: flushing objects is a no-op when no context is bound
- rusticl/gl: only flush objects on import if we get a valid fd
- rusticl/gl: flush and wait on gl objects inside clEnqueueAcquireGLObjects
- zink: fix data race in descriptor_util_pool_key_get
- rusticl: silence warnings in generated sources
- rusticl: silence new warnings from rustc versions above our rustc target
- anv: do not map from_host_ptr bos in image_bind_address
- zink: set zink_bo is_user_ptr on creation

Kenneth Graunke (4):

- brw: Refactor copy propagation checks for EOT send restrictions
- brw: Fix units in copy propagation EOT restriction size calculation
- brw: Update copy propagation into EOT sends handling for Xe2 units
- intel: Disable 16x MSAA support on Xe3

Lars-Ivar Hesselberg Simonsen (1):

- u_trace: Indirect capture fixes

Lionel Landwerlin (2):

- anv: fix wsi image aliasing
- anv: fix missing meson dep

Mary Guillemard (2):

- panvk: Always use varying_count in emit_varying_attrs
- panvk: track oq write jobs in JM

Mike Blumenkrantz (5):

- zink: also add access stage sync when rebinding buffers
- zink: fix tc buffer replacement rebind condition
- zink: trigger multi-context buffer invalidate on internal buffer invalidate
- zink: don't access ctx in submit_queue
- perfetto: unify init

Patrick Lerda (3):

- r600: refactor r600_is_buffer_format_supported() for the next update
- r600: fix remaining pbo issues
- r600: fix arb_shader_image_load_store incomplete

Rhys Perry (2):

- nir/load_store_vectorize: check for interfering shared2 before vectorizing
- nir/load_store_vectorize: set is_store for shared append/consume

Ricardo Garcia (1):

- radv: Ignore image barrier queue families if equal

Rob Clark (1):

- freedreno: Remove obsolete comment

Rohan Garg (1):

- intel/compiler: use the WA framework when emitting WA 14014595444

Samuel Pitoiset (3):

- radv: fix fbfetch output with compresed FMASK on <= GFX9
- ac,radv,radeonsi: fix programming PA_SU_PRIM_FILTER_CNTL on GFX12
- radv/amdgpu: fix creation with different but unused RADV_PERFTEST flags

Thomas H.P. Andersen (1):

- zink: do not overwrite existing error for miptail on uncommit

Yiwei Zhang (4):

- util/perf: amend missing atrace_init
- vulkan/wsi/headless: allow explicit modifiers
- venus: fix a race condition in ring shmem reuse
- vulkan/util: add missing vulkan header
