Mesa 21.1.4 Release Notes / 2021-06-30
======================================

Mesa 21.1.4 is a bug fix release which fixes bugs found since the 21.1.3 release.

Mesa 21.1.4 implements the OpenGL 4.6 API, but the version reported by
glGetString(GL_VERSION) or glGetIntegerv(GL_MAJOR_VERSION) /
glGetIntegerv(GL_MINOR_VERSION) depends on the particular driver being used.
Some drivers don't support all the features required in OpenGL 4.6. OpenGL
4.6 is **only** available if requested at context creation.
Compatibility contexts may report a lower version depending on each driver.

Mesa 21.1.4 implements the Vulkan 1.2 API, but the version reported by
the apiVersion property of the VkPhysicalDeviceProperties struct
depends on the particular driver being used.

SHA256 checksum
---------------

::

    1f177f44098164b65731c5ded4c928fd58b14f6c9d2087aa0e37bc79bf79e90b  mesa-21.1.4.tar.xz


New features
------------

- None


Bug fixes
---------

- [anv] GravityMark (benchmark) crashes on ANV
- [opengl] We happy few not being rendered correctly
- Factorio: GPU hang when opening machine inventory
- RuneScape on Mesa 21.1.1 (VEGA10) has bad performance and leaks memory
- Supraland: flickering black bars on ground
- radv: GPU hang in Cyberpunk 2077 on Big Navi
- [amdgpu][renoir][rx5500m]: [drm:0xffffffff8198ad5e] \*ERROR* ring gfx timeout, signaled seq=10952, emitted seq=10954
- [spirv-fuzz] SPIR-V parsing FAILED: Invalid back or cross-edge in the CFG
- panfrost Mount and Blade: Warband (glitches)
- anv: dEQP-VK.robustness.robustness2*no_fmt_qual.null_descriptor.samples* fail


Changes
-------

Bas Nieuwenhuizen (3):

- util/fossilize_db: Pull seek into lock.
- util/fossilize_db: Split out reading the index.
- util/fossilize_db: Do not lock the fossilize db permanently.

Caio Marcelo de Oliveira Filho (2):

- spirv: Fix handling of OpBranchConditional with same THEN and ELSE
- nir/opt_if: Don't split ALU for single block infinite loops

Daniel Stone (1):

- llvmpipe: Add handle export for resource_get_param

Dave Airlie (1):

- i965: fix regression in pipe control on g45

Eric Engestrom (2):

- .pick_status.json: Update to 977355c6e5efd781dde85d834172dd23cd4852f1
- .pick_status.json: Update to 40b67a292297606f0a7576e3ef4087028d5edd17

Erik Faye-Lund (7):

- zink: do not unmap dt-buffers twice
- zink: drop repeated usage-bit
- zink: do not check buffer-format for usage-bits
- zink: remove unused moltenvk functions
- libgl-gdi: add missing include
- aux/trace: fix bool argument
- ci/windows: work around meson encoding issues

Francisco Jerez (2):

- intel/fs: Teach IR about EOT instruction writing the accumulator implicitly on TGL+.
- intel/fs: Fix synchronization of accumulator-clearing W/A move on TGL+.

Icecream95 (5):

- pan/mdg: Add a bundle ID to instructions
- pan/mdg: Reorder some code in mir_spill_register
- pan/mdg: Fill from TLS before spilling non-SSA nodes
- pan/mdg: Fix reading a spilt register in the bundle it's written
- pan/mdg: Add 16 bytes of padding to the end of shaders

Iván Briano (1):

- intel/nir: Fix txs for null surfaces

Faith Ekstrand (1):

- spirv: Create acceleration structure and shader record variables

Karol Herbst (1):

- nv50/ir: fix surface lowering when values get shared accross operations

Kenneth Graunke (1):

- anv: Fix dynamic primitive topology for tess on Gfx7.x too

Lionel Landwerlin (1):

- anv: allocate bigger batches as we grow command buffers

Marek Olšák (1):

- mesa: unreference zombie buffers when creating buffers to lower memory usage

Martin Krastev (1):

- compiler/glsl: Use mutex lock while freeing up mem_ctx

Mike Blumenkrantz (2):

- anv: fix dynamic primitive topology for tess
- zink: handle custom border color without matching wrap mode case

Pierre-Eric Pelloux-Prayer (2):

- radeonsi: skip instance_count==0 draws on <= GFX9
- radeonsi: disable ngg culling on llvm < 12

Samuel Pitoiset (2):

- radv: reject binding buffer/image when the device memory is too small
- radv: always decompress both aspects of a depth/stencil image

Simon Ser (1):

- amd/addrlib: remove Meson debug message()

Thong Thai (1):

- radeon/vcn/enc: Add missing line to HEVC SPS header code

Timothy Arceri (1):

- util: add work around for the game We Happy Few

Timur Kristóf (4):

- ac/nir: Update TCS output barriers with nir_var_mem_shared.
- radv/llvm: Emit s_barrier at the beginning of NGG non-GS shaders.
- aco/gfx10: NGG zero output workaround for conservative rasterization.
- aco/gfx10: Emit barrier at the start of NGG VS and TES.
